(kicad_pcb (version 4) (host pcbnew 4.0.1-3.201512221402+6198~38~ubuntu14.04.1-stable)
  (general
    (links 27)
    (no_connects 0)
    (area 87.554999 64.694999 158.825001 118.185001)
    (thickness 1.6)
    (drawings 38)
    (tracks 108)
    (zones 0)
    (modules 15)
    (nets 16)
  )
  (page A4)
  (title_block
    (company "Released under the CERN Open Hardware License v1.2")
    (comment 1 jeh.wicker@gmail.com)
    (comment 2 "Jenner Hanni")
    (comment 3 "Wickerbox Electronics")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3302)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 1.27)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 0.762 0.4064)
    (user_via 0.8636 0.508)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.54 2.54)
    (pad_drill 2.032)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEDF7D)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(LED1-Pad1)")
  (net 4 "Net-(LED2-Pad1)")
  (net 5 /A4_PLAYBACK_LED)
  (net 6 /RESET)
  (net 7 "Net-(RV1-Pad2)")
  (net 8 /D7_KEY1)
  (net 9 /D5_KEY3)
  (net 10 /D6_KEY2)
  (net 11 /D2_PWM)
  (net 12 /D3_DIG_SPEAKER_OUT)
  (net 13 /A5_RECORD_LED)
  (net 14 /D9_BTN_PLAYBACK)
  (net 15 /D8_BTN_RECORD)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +5V)
    (add_net /A4_PLAYBACK_LED)
    (add_net /A5_RECORD_LED)
    (add_net /D2_PWM)
    (add_net /D3_DIG_SPEAKER_OUT)
    (add_net /D5_KEY3)
    (add_net /D6_KEY2)
    (add_net /D7_KEY1)
    (add_net /D8_BTN_RECORD)
    (add_net /D9_BTN_PLAYBACK)
    (add_net /RESET)
    (add_net GND)
    (add_net "Net-(LED1-Pad1)")
    (add_net "Net-(LED2-Pad1)")
    (add_net "Net-(RV1-Pad2)")
  )
  (module Wickerlib:SW-B3F-10XX (layer F.Cu) (tedit 5724F748)
    (at 126.08 103.378)
    (descr SW-B3F-10XX)
    (tags "Omron B3F-10xx")
    (fp_text reference RESET (at -2.763 1.651 90) (layer F.SilkS))
    (fp_text value B3F-1000 (at 2.95 -2.05) (layer F.Fab))
    (pad 4 thru_hole circle (at 6 4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 6 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /RESET))
  )
  (module Wickerlib:CAPSENSE-CIRCLE-D10 (layer F.Cu) (tedit 5724F609)
    (at 145.6055 103.886)
    (fp_text reference A (at 0.0635 -0.508 90) (layer F.SilkS))
    (fp_text value KEY1 (at 0.025 7.325) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 10.16 10.16) (layers F.Cu)
      (net 8 /D7_KEY1) (clearance 0.508))
  )
  (module Wickerlib:CAPSENSE-CIRCLE-D10 (layer F.Cu) (tedit 5724FA4A)
    (at 145.288 78.9305)
    (fp_text reference F (at 0.508 0.1905 90) (layer F.SilkS))
    (fp_text value KEY3 (at 0.025 7.325) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 10.16 10.16) (layers F.Cu)
      (net 9 /D5_KEY3) (clearance 0.508))
  )
  (module Wickerlib:CAPSENSE-CIRCLE-D10 (layer F.Cu) (tedit 5724F5F7)
    (at 138.684 91.186)
    (fp_text reference C (at -0.127 -0.381 90) (layer F.SilkS))
    (fp_text value KEY2 (at 0.025 7.325) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 10.16 10.16) (layers F.Cu)
      (net 10 /D6_KEY2) (clearance 0.508))
  )
  (module Wickerlib:LV_EZ1_Rangefinder (layer F.Cu) (tedit 5724FD34)
    (at 108.585 97.79)
    (descr http://maxbotix.com/uploads/LV-MaxSonar-EZ1-Datasheet.pdf)
    (tags "Rangefinder Module Breakout Board")
    (fp_text reference LV-EZ1-RANGEFINDER (at 1.27 -13.081 90) (layer F.SilkS))
    (fp_text value LV-EZ1-RANGEFINDER (at 1.375 -13.65 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 15.494 -19.558) (size 3.1496 3.1496) (drill 3.1496) (layers F.Cu))
    (pad 1 thru_hole rect (at 18.669 -16.891) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 18.669 -14.351) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 18.669 -11.811) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 18.669 -9.271) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 18.669 -6.731) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 18.669 -4.191) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /D2_PWM))
    (pad 7 thru_hole oval (at 18.669 -1.651) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 -2.54) (size 3.1496 3.1496) (drill 3.1496) (layers F.Cu))
  )
  (module Wickerlib:LED-5MM-2PIN (layer F.Cu) (tedit 5724F759)
    (at 92.456 110.236)
    (descr "LED 5mm round vertical")
    (tags "LED 5mm round vertical")
    (fp_text reference REC (at 5.588 -0.127 90) (layer F.SilkS))
    (fp_text value RECORD (at 1.524 -3.937) (layer F.Fab))
    (fp_text user K (at -1.905 1.905) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(LED1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.9 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A5_RECORD_LED))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:LED-5MM-2PIN (layer F.Cu) (tedit 5724F74F)
    (at 105.664 109.728)
    (descr "LED 5mm round vertical")
    (tags "LED 5mm round vertical")
    (fp_text reference PLAY (at 5.461 0.762 90) (layer F.SilkS))
    (fp_text value PLAYBACK (at 1.524 -3.937) (layer F.Fab))
    (fp_text user K (at -1.905 1.905) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(LED2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.9 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A4_PLAYBACK_LED))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 110.871 101.346)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R1 (at 3.81 0) (layer F.SilkS))
    (fp_text value 220 (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(LED1-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
  )
  (module Wickerlib:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 110.871 105.9815)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R2 (at 3.937 -0.0635) (layer F.SilkS))
    (fp_text value 220 (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(LED2-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
  )
  (module Wickerlib:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 103.505 82.7405 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R3 (at 3.7465 0 90) (layer F.SilkS))
    (fp_text value 10K (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 14 /D9_BTN_PLAYBACK))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
  )
  (module Wickerlib:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 103.6 86.48 270)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R4 (at 4.05892 -0.032 270) (layer F.SilkS))
    (fp_text value 10K (at 3.81 3.81 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 15 /D8_BTN_RECORD))
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
  )
  (module Wickerlib:P160-TRIMPOT (layer F.Cu) (tedit 5724FA2F)
    (at 99.4 77.47)
    (descr P160-TRIMPOT)
    (tags "Rotary Pot Trimpot Variable Resistor")
    (fp_text reference VOLUME (at -3.642 6.477 90) (layer F.SilkS))
    (fp_text value 10K (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 12 /D3_DIG_SPEAKER_OUT))
    (pad 2 thru_hole circle (at 0 5.08) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(RV1-Pad2)"))
    (pad 3 thru_hole circle (at 0 10.16) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Wickerlib:SW-100SP3 (layer F.Cu) (tedit 5724FC91)
    (at 100.838 102.87 270)
    (descr "Three-position through-hole board mount switch.")
    (tags "ON-OFF-ON switch")
    (fp_text reference S1 (at 2.667 0.127 360) (layer F.SilkS) hide)
    (fp_text value "100SP3 ON-OFF-ON" (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.54 2.54) (drill 2.032) (layers *.Cu *.Mask F.SilkS)
      (net 15 /D8_BTN_RECORD))
    (pad 2 thru_hole circle (at 0 4.699 270) (size 2.54 2.54) (drill 2.032) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 3 thru_hole circle (at 0 9.398 270) (size 2.54 2.54) (drill 2.032) (layers *.Cu *.Mask F.SilkS)
      (net 14 /D9_BTN_PLAYBACK))
  )
  (module Wickerlib:ARDU-UNOSHIELD locked (layer F.Cu) (tedit 5724F58D)
    (at 87.63 118.11)
    (descr none)
    (fp_text reference U1 (at 5.715 -57.15) (layer F.SilkS) hide)
    (fp_text value ARDUINO-UNO-SHIELD (at 10.16 -54.61) (layer F.SilkS) hide)
    (fp_text user IOREF (at 30.353 -6.604 90) (layer F.SilkS))
    (fp_text user NC (at 27.793 -5.461 90) (layer F.SilkS))
    (fp_text user RST (at 32.893 -5.715 90) (layer F.SilkS))
    (fp_text user 3.3V (at 35.56 -6.096 90) (layer F.SilkS))
    (fp_text user 5V (at 37.953 -5.461 90) (layer F.SilkS))
    (fp_text user GND (at 40.493 -5.969 90) (layer F.SilkS))
    (fp_text user GND (at 43.068 -5.969 90) (layer F.SilkS))
    (fp_text user VIN (at 45.743 -5.894 90) (layer F.SilkS))
    (fp_text user A5 (at 63.523 -5.386 90) (layer F.SilkS))
    (fp_text user A4 (at 60.848 -5.461 90) (layer F.SilkS))
    (fp_text user A3 (at 58.273 -5.461 90) (layer F.SilkS))
    (fp_text user A2 (at 55.733 -5.461 90) (layer F.SilkS))
    (fp_text user A1 (at 53.32 -5.461 90) (layer F.SilkS))
    (fp_text user A0 (at 50.8 -5.461 90) (layer F.SilkS))
    (fp_text user SCL (at 18.903 -47.371 90) (layer F.SilkS))
    (fp_text user SDA (at 21.316 -47.371 90) (layer F.SilkS))
    (fp_text user ARE (at 23.856 -47.371 90) (layer F.SilkS))
    (fp_text user GND (at 26.396 -47.371 90) (layer F.SilkS))
    (fp_text user D13 (at 29.063 -47.371 90) (layer F.SilkS))
    (fp_text user D12 (at 31.603 -47.371 90) (layer F.SilkS))
    (fp_text user D11 (at 34.143 -47.371 90) (layer F.SilkS))
    (fp_text user D10 (at 36.556 -47.371 90) (layer F.SilkS))
    (fp_text user D9 (at 39.223 -47.752 90) (layer F.SilkS))
    (fp_text user D8 (at 41.763 -47.752 90) (layer F.SilkS))
    (fp_text user D7 (at 45.827 -47.625 90) (layer F.SilkS))
    (fp_text user D6 (at 48.24 -47.625 90) (layer F.SilkS))
    (fp_text user D5 (at 50.78 -47.625 90) (layer F.SilkS))
    (fp_text user D4 (at 53.447 -47.625 90) (layer F.SilkS))
    (fp_text user D3 (at 55.86 -47.625 90) (layer F.SilkS))
    (fp_text user D2 (at 58.4 -47.625 90) (layer F.SilkS))
    (fp_text user D1 (at 60.975 -47.625 90) (layer F.SilkS))
    (fp_text user D0 (at 63.65 -47.55 90) (layer F.SilkS))
    (pad A5 thru_hole oval (at 63.5 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A5_RECORD_LED))
    (pad A4 thru_hole oval (at 60.96 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A4_PLAYBACK_LED))
    (pad A3 thru_hole oval (at 58.42 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad A0 thru_hole oval (at 50.8 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad A1 thru_hole oval (at 53.34 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad A2 thru_hole oval (at 55.88 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad VIN thru_hole oval (at 45.72 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad GND2 thru_hole oval (at 43.18 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad GND1 thru_hole oval (at 40.64 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3V3 thru_hole oval (at 35.56 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad RST thru_hole oval (at 33.02 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /RESET))
    (pad D0 thru_hole oval (at 63.5 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad D1 thru_hole oval (at 60.96 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad D2 thru_hole oval (at 58.42 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /D2_PWM))
    (pad D3 thru_hole oval (at 55.88 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /D3_DIG_SPEAKER_OUT))
    (pad D4 thru_hole oval (at 53.34 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad D5 thru_hole oval (at 50.8 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /D5_KEY3))
    (pad D6 thru_hole oval (at 48.26 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /D6_KEY2))
    (pad D7 thru_hole oval (at 45.72 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /D7_KEY1))
    (pad D8 thru_hole oval (at 41.656 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /D8_BTN_RECORD))
    (pad D9 thru_hole oval (at 39.116 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /D9_BTN_PLAYBACK))
    (pad D10 thru_hole oval (at 36.576 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad D11 thru_hole oval (at 34.036 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad D12 thru_hole oval (at 31.496 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad D13 thru_hole oval (at 28.956 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad GND3 thru_hole oval (at 26.416 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad AREF thru_hole oval (at 23.876 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5V thru_hole oval (at 38.1 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad "" np_thru_hole circle (at 66.04 -7.62 90) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 66.04 -35.56 90) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 15.24 -50.8 90) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 13.97 -2.54 90) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad SDA thru_hole oval (at 21.336 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad SCL thru_hole oval (at 18.796 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad IO thru_hole oval (at 30.48 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad NC thru_hole oval (at 27.94 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  )
  (module Wickerlib:OSTVN02A150 (layer F.Cu) (tedit 5737D30F)
    (at 95.5294 68.4276 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference SPEAKER (at 4.2418 1.2954 360) (layer F.SilkS))
    (fp_text value "8 OHM" (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(RV1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text RECORD (at 91.821 99.187 90) (layer F.SilkS))
  (gr_text PWM (at 123.323048 93.726) (layer F.SilkS))
  (gr_text "5V\n" (at 124.072953 83.566) (layer F.SilkS))
  (gr_text GND (at 123.444 81.28) (layer F.SilkS))
  (gr_text "Arduino Theremin Shield \nDemo Board v1.3\n\nOSH Park 2016" (at 140.208 91.186 90) (layer B.SilkS))
  (gr_text - (at 89.916 68.072) (layer F.SilkS))
  (gr_text + (at 98.2 68.2) (layer F.SilkS))
  (gr_text PLAYBACK (at 100.7745 99.3 90) (layer F.SilkS))
  (gr_text STOP (at 96.52 99.1235 90) (layer F.SilkS))
  (gr_line (start 152.4 64.77) (end 87.63 64.77) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.67 66.04) (end 152.4 64.77) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.67 77.47) (end 153.67 66.04) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.75 82.55) (end 153.67 77.47) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.75 110.49) (end 158.75 82.55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.67 115.57) (end 158.75 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.67 118.11) (end 153.67 115.57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.63 118.11) (end 153.67 118.11) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.63 64.77) (end 87.63 118.11) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.67 66.04) (xy 158.75 82.55) (xy 158.75 110.49) (xy 153.67 118.11) (xy 87.63 118.11)
        (xy 87.63 64.77) (xy 152.4 64.77) (xy 153.67 66.04)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.67 66.04) (xy 153.67 77.47) (xy 158.75 82.55) (xy 158.75 110.49) (xy 153.67 115.57)
        (xy 153.67 118.11) (xy 87.63 118.11) (xy 87.63 64.77) (xy 152.4 64.77) (xy 153.67 66.04)
      )
    )
  )
)
