(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 1)
    (no_connects 1)
    (area 83.199999 156.149999 137.330001 198.160001)
    (thickness 1.6)
    (drawings 49)
    (tracks 79)
    (zones 0)
    (modules 5)
    (nets 24)
  )
  (page USLetter portrait)
  (title_block
    (title "Atari 2600 1MiB PROM bank-switched cartridge")
    (date 2017-08-30)
    (rev 17.242)
    (company "Fabulous Production Company")
    (comment 1 "Bruce-Robert Fenn Pocock")
    (comment 2 "Initial Game: Skyline 2600")
  )
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk true)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(AddrHi1-Pad3)")
  (net 2 "Net-(AddrHi1-Pad13)")
  (net 3 "Net-(AddrHi1-Pad4)")
  (net 4 "Net-(AddrHi1-Pad14)")
  (net 5 "Net-(AddrHi1-Pad7)")
  (net 6 "Net-(AddrHi1-Pad17)")
  (net 7 "Net-(AddrHi1-Pad8)")
  (net 8 "Net-(AddrHi1-Pad18)")
  (net 9 "Net-(AddrNAND1-Pad2)")
  (net 10 "Net-(AddrNAND1-Pad10)")
  (net 11 "Net-(AddrNAND1-Pad3)")
  (net 12 "Net-(AddrNAND1-Pad11)")
  (net 13 "Net-(AddrNAND1-Pad4)")
  (net 14 "Net-(AddrNAND1-Pad5)")
  (net 15 "Net-(AddrNAND1-Pad13)")
  (net 16 "Net-(AddrNAND1-Pad6)")
  (net 17 "Net-(AddrNAND1-Pad14)")
  (net 18 "Net-(AddrNAND1-Pad7)")
  (net 19 "Net-(AddrNAND1-Pad15)")
  (net 20 "Net-(CartConn1-Pad5)")
  (net 21 Earth_Protective)
  (net 22 +5V)
  (net 23 "Net-(AddrNAND1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(AddrHi1-Pad13)")
    (add_net "Net-(AddrHi1-Pad14)")
    (add_net "Net-(AddrHi1-Pad17)")
    (add_net "Net-(AddrHi1-Pad18)")
    (add_net "Net-(AddrHi1-Pad3)")
    (add_net "Net-(AddrHi1-Pad4)")
    (add_net "Net-(AddrHi1-Pad7)")
    (add_net "Net-(AddrHi1-Pad8)")
    (add_net "Net-(AddrNAND1-Pad1)")
    (add_net "Net-(AddrNAND1-Pad10)")
    (add_net "Net-(AddrNAND1-Pad11)")
    (add_net "Net-(AddrNAND1-Pad13)")
    (add_net "Net-(AddrNAND1-Pad14)")
    (add_net "Net-(AddrNAND1-Pad15)")
    (add_net "Net-(AddrNAND1-Pad2)")
    (add_net "Net-(AddrNAND1-Pad3)")
    (add_net "Net-(AddrNAND1-Pad4)")
    (add_net "Net-(AddrNAND1-Pad5)")
    (add_net "Net-(AddrNAND1-Pad6)")
    (add_net "Net-(AddrNAND1-Pad7)")
    (add_net "Net-(CartConn1-Pad5)")
  )
  (net_class +5V ""
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
  )
  (net_class Ground ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net Earth_Protective)
  )
  (module Housings_DIP:DIP-24_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 59A7268C)
    (at 99.06 167.64 90)
    (descr "24-lead dip package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference Socket24 (at 3.81 -2.39 90) (layer F.SilkS))
    (fp_text value "Breakout Socket" (at 3.81 30.33 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 7.62 27.94 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 7.62 25.4 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 7.62 22.86 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 7.62 20.32 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 7.62 17.78 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 7.62 15.24 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 7.62 12.7 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at 7.62 10.16 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 21 thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 22 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 23 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 24 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model Housings_DIP.3dshapes/DIP-24_W7.62mm_Socket_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Parts:BUS_ATARI_CX2600 (layer F.Cu) (tedit 59CC181A)
    (at 110.49 195.58)
    (descr "Atari CX-2600 cartridge edge connector")
    (tags "conn bus cart atari edge")
    (fp_text reference "This side toward couch" (at -5.08 -11.43) (layer F.SilkS))
    (fp_text value CONN_CX2600_CART (at 0 -8.89) (layer F.Fab))
    (pad 13 connect rect (at 13.97 -2.54) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 7 "Net-(AddrHi1-Pad8)"))
    (pad 14 connect rect (at 11.43 -2.54) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 2 "Net-(AddrHi1-Pad13)"))
    (pad 15 connect rect (at 8.89 -2.54) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 4 "Net-(AddrHi1-Pad14)"))
    (pad 16 connect rect (at 6.35 -2.54) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 6 "Net-(AddrHi1-Pad17)"))
    (pad 17 connect rect (at 3.81 -2.54) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 8 "Net-(AddrHi1-Pad18)"))
    (pad 18 connect rect (at 1.27 -2.54) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 23 "Net-(AddrNAND1-Pad1)"))
    (pad 19 connect rect (at -1.27 -2.54) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 11 "Net-(AddrNAND1-Pad3)"))
    (pad 20 connect rect (at -3.81 -2.54) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 9 "Net-(AddrNAND1-Pad2)"))
    (pad 21 connect rect (at -6.35 -2.54) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 13 "Net-(AddrNAND1-Pad4)"))
    (pad 22 connect rect (at -8.89 -2.54) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 14 "Net-(AddrNAND1-Pad5)"))
    (pad 23 connect rect (at -11.43 -2.54) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 22 +5V))
    (pad 24 connect rect (at -13.97 -2.54) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 21 Earth_Protective))
    (pad 12 connect rect (at 13.97 -2.54) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 21 Earth_Protective))
    (pad 11 connect rect (at 11.43 -2.54) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 5 "Net-(AddrHi1-Pad7)"))
    (pad 10 connect rect (at 8.89 -2.54) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 3 "Net-(AddrHi1-Pad4)"))
    (pad 9 connect rect (at 6.35 -2.54) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 1 "Net-(AddrHi1-Pad3)"))
    (pad 8 connect rect (at 3.81 -2.54) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 19 "Net-(AddrNAND1-Pad15)"))
    (pad 7 connect rect (at 1.27 -2.54) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 17 "Net-(AddrNAND1-Pad14)"))
    (pad 6 connect rect (at -1.27 -2.54) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 15 "Net-(AddrNAND1-Pad13)"))
    (pad 5 connect rect (at -3.81 -2.54) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 20 "Net-(CartConn1-Pad5)"))
    (pad 4 connect rect (at -6.35 -2.54) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 12 "Net-(AddrNAND1-Pad11)"))
    (pad 3 connect rect (at -8.89 -2.54) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 10 "Net-(AddrNAND1-Pad10)"))
    (pad 2 connect rect (at -11.43 -2.54) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 18 "Net-(AddrNAND1-Pad7)"))
    (pad 1 connect rect (at -13.97 -2.54) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 16 "Net-(AddrNAND1-Pad6)"))
  )
  (module Measurement_Points:Measurement_Point_Square-TH_Big (layer F.Cu) (tedit 59A72A42)
    (at 133.35 168.91)
    (descr "Mesurement Point, Square, Trough Hole,  3mm x 3mm, Drill 1.5mm,")
    (tags "Mesurement Point Square Trough Hole 3x3mm Drill 1.5mm")
    (attr virtual)
    (fp_text reference GND13 (at 0 -3) (layer F.SilkS))
    (fp_text value Ground (at 0 3) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module Measurement_Points:Measurement_Point_Square-TH_Big (layer F.Cu) (tedit 59A72A55)
    (at 86.36 168.91)
    (descr "Mesurement Point, Square, Trough Hole,  3mm x 3mm, Drill 1.5mm,")
    (tags "Mesurement Point Square Trough Hole 3x3mm Drill 1.5mm")
    (attr virtual)
    (fp_text reference VCC2 (at 0 -3) (layer F.SilkS))
    (fp_text value +5V (at 0 3) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module Measurement_Points:Measurement_Point_Square-TH_Big (layer F.Cu) (tedit 59A72A4E)
    (at 91.44 168.91)
    (descr "Mesurement Point, Square, Trough Hole,  3mm x 3mm, Drill 1.5mm,")
    (tags "Mesurement Point Square Trough Hole 3x3mm Drill 1.5mm")
    (attr virtual)
    (fp_text reference GND1 (at 0 -3) (layer F.SilkS))
    (fp_text value Ground (at 0 3) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
  )
  (gr_text ... (at 111.25 170.5) (layer B.SilkS))
  (gr_text ... (at 105 170.5) (layer B.SilkS))
  (gr_text ... (at 121.75 170.25) (layer B.SilkS))
  (gr_text ... (at 122 162.25) (layer B.SilkS))
  (gr_text D4 (at 127 163.25 90) (layer B.SilkS))
  (gr_text D8 (at 117 163.25 90) (layer B.SilkS))
  (gr_text A12 (at 114.25 163.75 90) (layer B.SilkS))
  (gr_text A10 (at 112 163.75 90) (layer B.SilkS))
  (gr_text A11 (at 109.25 163.75 90) (layer B.SilkS))
  (gr_text A9 (at 106.75 163.25 90) (layer B.SilkS))
  (gr_text A8 (at 104 163 90) (layer B.SilkS))
  (gr_text +5V (at 101.75 163.5 90) (layer B.SilkS))
  (gr_text GND (at 99 163.75 90) (layer B.SilkS))
  (gr_text GND (at 127.5 172 90) (layer B.SilkS))
  (gr_text D3 (at 124.25 171 90) (layer B.SilkS))
  (gr_text D1 (at 119.5 171.25 90) (layer B.SilkS))
  (gr_text A0 (at 116.75 171.25 90) (layer B.SilkS))
  (gr_text A7 (at 99 171 90) (layer B.SilkS))
  (gr_line (start 126.25 185.5) (end 130.75 181) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 126.25 198) (end 126.25 185.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.75 198) (end 126.25 198) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.75 185.5) (end 94.75 198) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.25 181) (end 94.75 185.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 84 181) (end 90.25 181) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.25 180.25) (end 84 181) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.25 156.25) (end 83.25 180.25) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.25 156.25) (end 83.25 156.25) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.25 181) (end 137.25 156.25) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.75 181) (end 137.25 181) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.63 198.11) (end 94.64 198.11) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.26 156.2) (end 137.28 156.2) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text 12↑ (at 128 170.5) (layer F.SilkS))
  (gr_text ←13 (at 132.08 160.02) (layer F.SilkS))
  (gr_text 24→ (at 93.98 160.02) (layer F.SilkS))
  (gr_text "↑1\n" (at 101.25 170.25) (layer F.SilkS))
  (gr_text "Atari 2600 Cartridge Port Breakout Card\nRevision 2017.270" (at 110.49 179.07) (layer F.SilkS))
  (dimension 6.330506 (width 0.3) (layer Dwgs.User)
    (gr_text "6.331 mm" (at 115.992451 104.722073 0.7240787271) (layer Dwgs.User))
    (feature1 (pts (xy 119.37 121.5) (xy 119.140391 103.332181)))
    (feature2 (pts (xy 113.04 121.58) (xy 112.810391 103.412181)))
    (crossbar (pts (xy 112.844511 106.111965) (xy 119.174511 106.031965)))
    (arrow1a (pts (xy 119.174511 106.031965) (xy 118.055508 106.632575)))
    (arrow1b (pts (xy 119.174511 106.031965) (xy 118.040686 105.459827)))
    (arrow2a (pts (xy 112.844511 106.111965) (xy 113.978336 106.684103)))
    (arrow2b (pts (xy 112.844511 106.111965) (xy 113.963514 105.511355)))
  )
  (dimension 4.61 (width 0.3) (layer Dwgs.User)
    (gr_text "4.610 mm" (at 116.185 110.78) (layer Dwgs.User))
    (feature1 (pts (xy 118.49 121.27) (xy 118.49 109.43)))
    (feature2 (pts (xy 113.88 121.27) (xy 113.88 109.43)))
    (crossbar (pts (xy 113.88 112.13) (xy 118.49 112.13)))
    (arrow1a (pts (xy 118.49 112.13) (xy 117.363496 112.716421)))
    (arrow1b (pts (xy 118.49 112.13) (xy 117.363496 111.543579)))
    (arrow2a (pts (xy 113.88 112.13) (xy 115.006504 112.716421)))
    (arrow2b (pts (xy 113.88 112.13) (xy 115.006504 111.543579)))
  )
  (dimension 6.820066 (width 0.3) (layer Dwgs.User)
    (gr_text "6.820 mm" (at 134.480718 199.345039 0.2520325952) (layer Dwgs.User))
    (feature1 (pts (xy 137.81 180.98) (xy 137.896657 200.680026)))
    (feature2 (pts (xy 130.99 181.01) (xy 131.076657 200.710026)))
    (crossbar (pts (xy 131.06478 198.010052) (xy 137.88478 197.980052)))
    (arrow1a (pts (xy 137.88478 197.980052) (xy 136.760867 198.571422)))
    (arrow1b (pts (xy 137.88478 197.980052) (xy 136.755708 197.398592)))
    (arrow2a (pts (xy 131.06478 198.010052) (xy 132.193852 198.591512)))
    (arrow2b (pts (xy 131.06478 198.010052) (xy 132.188693 197.418682)))
  )
  (dimension 4.45018 (width 0.3) (layer Dwgs.User)
    (gr_text "4.450 mm" (at 128.883045 207.442521 0.5150043727) (layer Dwgs.User))
    (feature1 (pts (xy 130.87 180.94) (xy 131.12018 208.772467)))
    (feature2 (pts (xy 126.42 180.98) (xy 126.67018 208.812467)))
    (crossbar (pts (xy 126.645911 206.112576) (xy 131.095911 206.072576)))
    (arrow1a (pts (xy 131.095911 206.072576) (xy 129.974724 206.669099)))
    (arrow1b (pts (xy 131.095911 206.072576) (xy 129.964182 205.496304)))
    (arrow2a (pts (xy 126.645911 206.112576) (xy 127.77764 206.688848)))
    (arrow2b (pts (xy 126.645911 206.112576) (xy 127.767098 205.516053)))
  )
  (dimension 4.39 (width 0.3) (layer Dwgs.User)
    (gr_text "4.390 mm" (at 85.385 111) (layer Dwgs.User))
    (feature1 (pts (xy 87.58 116.84) (xy 87.58 109.65)))
    (feature2 (pts (xy 83.19 116.84) (xy 83.19 109.65)))
    (crossbar (pts (xy 83.19 112.35) (xy 87.58 112.35)))
    (arrow1a (pts (xy 87.58 112.35) (xy 86.453496 112.936421)))
    (arrow1b (pts (xy 87.58 112.35) (xy 86.453496 111.763579)))
    (arrow2a (pts (xy 83.19 112.35) (xy 84.316504 112.936421)))
    (arrow2b (pts (xy 83.19 112.35) (xy 84.316504 111.763579)))
  )
  (dimension 4.410102 (width 0.3) (layer Dwgs.User)
    (gr_text "4.410 mm" (at 60.247322 119.180902 270.3897612) (layer Dwgs.User))
    (feature1 (pts (xy 83.18 121.23) (xy 58.912353 121.395086)))
    (feature2 (pts (xy 83.15 116.82) (xy 58.882353 116.985086)))
    (crossbar (pts (xy 61.582291 116.966719) (xy 61.612291 121.376719)))
    (arrow1a (pts (xy 61.612291 121.376719) (xy 61.018221 120.25423)))
    (arrow1b (pts (xy 61.612291 121.376719) (xy 62.191035 120.246252)))
    (arrow2a (pts (xy 61.582291 116.966719) (xy 61.003547 118.097186)))
    (arrow2b (pts (xy 61.582291 116.966719) (xy 62.176361 118.089208)))
  )
  (dimension 12.650668 (width 0.3) (layer Dwgs.User)
    (gr_text "12.651 mm" (at 79.86944 191.947049 270.5887897) (layer Dwgs.User))
    (feature1 (pts (xy 94.73 198.12) (xy 78.584512 198.285922)))
    (feature2 (pts (xy 94.6 185.47) (xy 78.454512 185.635922)))
    (crossbar (pts (xy 81.154369 185.608176) (xy 81.284369 198.258176)))
    (arrow1a (pts (xy 81.284369 198.258176) (xy 80.686403 197.137758)))
    (arrow1b (pts (xy 81.284369 198.258176) (xy 81.859183 197.125706)))
    (arrow2a (pts (xy 81.154369 185.608176) (xy 80.579555 186.740646)))
    (arrow2b (pts (xy 81.154369 185.608176) (xy 81.752335 186.728594)))
  )
  (dimension 4.381381 (width 0.3) (layer Dwgs.User)
    (gr_text "4.381 mm" (at 47.92501 184.344588 271.4386327) (layer Dwgs.User))
    (feature1 (pts (xy 94.75 185.36) (xy 46.630436 186.568482)))
    (feature2 (pts (xy 94.64 180.98) (xy 46.520436 182.188482)))
    (crossbar (pts (xy 49.219585 182.120695) (xy 49.329585 186.500695)))
    (arrow1a (pts (xy 49.329585 186.500695) (xy 48.715067 185.389269)))
    (arrow1b (pts (xy 49.329585 186.500695) (xy 49.887539 185.359824)))
    (arrow2a (pts (xy 49.219585 182.120695) (xy 48.661631 183.261566)))
    (arrow2b (pts (xy 49.219585 182.120695) (xy 49.834103 183.232121)))
  )
  (dimension 64.050282 (width 0.3) (layer Dwgs.User)
    (gr_text "64.050 mm" (at 51.031745 149.010409 270.1699636) (layer Dwgs.User))
    (feature1 (pts (xy 83.29 180.94) (xy 49.776751 181.039414)))
    (feature2 (pts (xy 83.1 116.89) (xy 49.586751 116.989414)))
    (crossbar (pts (xy 52.286739 116.981405) (xy 52.476739 181.031405)))
    (arrow1a (pts (xy 52.476739 181.031405) (xy 51.886979 179.906646)))
    (arrow1b (pts (xy 52.476739 181.031405) (xy 53.059815 179.903167)))
    (arrow2a (pts (xy 52.286739 116.981405) (xy 51.703663 118.109643)))
    (arrow2b (pts (xy 52.286739 116.981405) (xy 52.876499 118.106164)))
  )
  (dimension 81.880005 (width 0.3) (layer Dwgs.User)
    (gr_text "81.880 mm" (at 42.575182 157.804882 270.0209926) (layer Dwgs.User))
    (feature1 (pts (xy 83.21 198.73) (xy 41.240182 198.745377)))
    (feature2 (pts (xy 83.18 116.85) (xy 41.210182 116.865377)))
    (crossbar (pts (xy 43.910182 116.864388) (xy 43.940182 198.744388)))
    (arrow1a (pts (xy 43.940182 198.744388) (xy 43.353349 197.618099)))
    (arrow1b (pts (xy 43.940182 198.744388) (xy 44.52619 197.617669)))
    (arrow2a (pts (xy 43.910182 116.864388) (xy 43.324174 117.991107)))
    (arrow2b (pts (xy 43.910182 116.864388) (xy 44.497015 117.990677)))
  )
  (dimension 54.630045 (width 0.3) (layer Dwgs.User)
    (gr_text "54.630 mm" (at 110.52391 211.311658 0.07341574906) (layer Dwgs.User))
    (feature1 (pts (xy 137.8 180.91) (xy 137.84064 212.626657)))
    (feature2 (pts (xy 83.17 180.98) (xy 83.21064 212.696657)))
    (crossbar (pts (xy 83.20718 209.996659) (xy 137.83718 209.926659)))
    (arrow1a (pts (xy 137.83718 209.926659) (xy 136.711429 210.514523)))
    (arrow1b (pts (xy 137.83718 209.926659) (xy 136.709926 209.341682)))
    (arrow2a (pts (xy 83.20718 209.996659) (xy 84.334434 210.581636)))
    (arrow2b (pts (xy 83.20718 209.996659) (xy 84.332931 209.408795)))
  )
  (dimension 31.740191 (width 0.3) (layer Dwgs.User)
    (gr_text "31.740 mm" (at 110.501934 205.969472 0.1985668089) (layer Dwgs.User))
    (feature1 (pts (xy 126.34 196.7) (xy 126.376613 207.264464)))
    (feature2 (pts (xy 94.6 196.81) (xy 94.636613 207.374464)))
    (crossbar (pts (xy 94.627256 204.67448) (xy 126.367256 204.56448)))
    (arrow1a (pts (xy 126.367256 204.56448) (xy 125.242791 205.154801)))
    (arrow1b (pts (xy 126.367256 204.56448) (xy 125.238727 203.981967)))
    (arrow2a (pts (xy 94.627256 204.67448) (xy 95.755785 205.256993)))
    (arrow2b (pts (xy 94.627256 204.67448) (xy 95.751721 204.084159)))
  )
)
