(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 0)
    (no_connects 0)
    (area 133.574999 85.924999 166.375001 123.600001)
    (thickness 1.6)
    (drawings 8)
    (tracks 25)
    (zones 0)
    (modules 11)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1526)
    (trace_clearance 0.01)
    (zone_clearance 0.02548)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.2606 2.2606)
    (pad_drill 2.2606)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010c0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../../../../../../../../5/))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.01)
    (trace_width 0.1526)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module bribrary:female_mdm_small (layer F.Cu) (tedit 5AC69E04)
    (at 161.4932 104.9274 270)
    (fp_text reference J1 (at 0 0.5 270) (layer F.SilkS) hide)
    (fp_text value DB25_FEMALE (at 0.127 -3.556 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 7.62 -0.6096 270) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 6.35 -0.6096 270) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 -0.6096 270) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 3.81 -0.6096 270) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 2.54 -0.6096 270) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 1.27 -0.6096 270) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 0 -0.6096 270) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -1.27 -0.6096 270) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at -2.54 -0.6096 270) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at -3.81 -0.6096 270) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at -5.08 -0.6096 270) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at -6.35 -0.6096 270) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 8.255 0.508 270) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 6.985 0.508 270) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 5.715 0.508 270) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 4.445 0.508 270) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at 3.175 0.508 270) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 18 thru_hole circle (at 1.905 0.508 270) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 0.635 0.508 270) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at -0.635 0.508 270) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 21 thru_hole circle (at -1.905 0.508 270) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 22 thru_hole circle (at -3.175 0.508 270) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at -4.445 0.508 270) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 24 thru_hole circle (at -5.715 0.508 270) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 25 thru_hole circle (at -6.985 0.508 270) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -11.6332 0 270) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 12.8778 0.0508 270) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask))
  )
  (module aruj:2hole (layer F.Cu) (tedit 5AAA8E85)
    (at 136.025 88.35)
    (fp_text reference * (at 0 0.5) (layer F.SilkS))
    (fp_text value "#2 hole" (at -28.1 0.1) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.2606 2.2606) (drill 2.2606) (layers *.Cu *.Mask))
  )
  (module aruj:2hole (layer F.Cu) (tedit 5AAA8EA5)
    (at 164.275 88.275)
    (fp_text reference * (at 0 0.5) (layer F.SilkS))
    (fp_text value "#2 hole" (at 32.65 1.95) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.2 0.075) (size 2.2606 2.2606) (drill 2.2606) (layers *.Cu *.Mask))
  )
  (module aruj:2hole (layer F.Cu) (tedit 5AAA8E9C)
    (at 164.475 121.25)
    (fp_text reference * (at 0 0.5) (layer F.SilkS))
    (fp_text value "#2 hole" (at 34.925 -1.15) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0.175) (size 2.2606 2.2606) (drill 2.2606) (layers *.Cu *.Mask))
  )
  (module aruj:2hole (layer F.Cu) (tedit 5AAA8E98)
    (at 135.925 121.425)
    (fp_text reference * (at 0 0.5) (layer F.SilkS))
    (fp_text value "#2 hole" (at -27.825 1.775) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.1 0) (size 2.2606 2.2606) (drill 2.2606) (layers *.Cu *.Mask))
  )
  (module aruj:2hole (layer F.Cu) (tedit 5AAA8EAF)
    (at 145.525 88.275)
    (fp_text reference * (at 0 0.5) (layer F.SilkS))
    (fp_text value "#2 hole" (at -0.175 -5.425) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0.075) (size 2.2606 2.2606) (drill 2.2606) (layers *.Cu *.Mask))
  )
  (module aruj:2hole (layer F.Cu) (tedit 5AAA8EAA)
    (at 155.125 88.375)
    (fp_text reference * (at 0 0.5) (layer F.SilkS))
    (fp_text value "#2 hole" (at 4.525 -7.4) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 -0.025) (size 2.2606 2.2606) (drill 2.2606) (layers *.Cu *.Mask))
  )
  (module aruj:2hole (layer F.Cu) (tedit 5AAA8E88)
    (at 139.55 96.175)
    (fp_text reference * (at 0 0.5) (layer F.SilkS))
    (fp_text value "#2 hole" (at -22.225 -1.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.2606 2.2606) (drill 2.2606) (layers *.Cu *.Mask))
  )
  (module aruj:2hole (layer F.Cu) (tedit 5AAA8E90)
    (at 139.475 105.25)
    (fp_text reference * (at 0 0.5) (layer F.SilkS))
    (fp_text value "#2 hole" (at -20.8 2.85) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.2606 2.2606) (drill 2.2606) (layers *.Cu *.Mask))
  )
  (module aruj:2hole (layer F.Cu) (tedit 5AAA8E94)
    (at 139.475 113.875)
    (fp_text reference * (at 0 0.5) (layer F.SilkS))
    (fp_text value "#2 hole" (at -25.425 -0.35) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.2606 2.2606) (drill 2.2606) (layers *.Cu *.Mask))
  )
  (module bribrary:female_mdm_small (layer F.Cu) (tedit 5AC69E04)
    (at 148.8948 106.1974 90)
    (fp_text reference J1 (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value DB25_FEMALE (at 0.127 -3.556 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 7.62 -0.6096 90) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 6.35 -0.6096 90) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 -0.6096 90) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 3.81 -0.6096 90) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 2.54 -0.6096 90) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 1.27 -0.6096 90) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 0 -0.6096 90) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -1.27 -0.6096 90) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at -2.54 -0.6096 90) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at -3.81 -0.6096 90) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at -5.08 -0.6096 90) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at -6.35 -0.6096 90) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 8.255 0.508 90) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 6.985 0.508 90) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 5.715 0.508 90) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 4.445 0.508 90) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at 3.175 0.508 90) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 18 thru_hole circle (at 1.905 0.508 90) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 0.635 0.508 90) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at -0.635 0.508 90) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 21 thru_hole circle (at -1.905 0.508 90) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 22 thru_hole circle (at -3.175 0.508 90) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at -4.445 0.508 90) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 24 thru_hole circle (at -5.715 0.508 90) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad 25 thru_hole circle (at -6.985 0.508 90) (size 1 1) (drill 0.61) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -11.6332 0 90) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 12.8778 0.0508 90) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask))
  )
  (gr_line (start 138.65 123.475) (end 133.625 123.475) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.625 123.425) (end 133.625 123.55) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.625 85.975) (end 133.625 123.45) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.6 85.975) (end 133.625 85.975) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.325 85.975) (end 166.325 88.375) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.6 85.975) (end 166.325 85.975) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.325 123.475) (end 166.325 87.825) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.6 123.475) (end 166.325 123.475) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.02548))
    (min_thickness 0.02548)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 1) (thermal_bridge_width 0.02549))
    (polygon
      (pts
        (xy 166.25 114.475) (xy 144.275 114.475) (xy 144.275 96.425) (xy 166.25 96.425)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.02548))
    (min_thickness 0.02548)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 1) (thermal_bridge_width 0.02549))
    (polygon
      (pts
        (xy 166.25 114.475) (xy 144.275 114.475) (xy 144.275 96.425) (xy 166.25 96.425)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads no (clearance 0.02548))
    (min_thickness 0.02548)
    (fill yes (arc_segments 16) (thermal_gap 1) (thermal_bridge_width 0.02549))
    (polygon
      (pts
        (xy 166.325 123.5) (xy 133.65 123.5) (xy 133.65 85.975) (xy 166.325 85.975)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads no (clearance 0.02548))
    (min_thickness 0.02548)
    (fill yes (arc_segments 16) (thermal_gap 1) (thermal_bridge_width 0.02549))
    (polygon
      (pts
        (xy 166.325 123.5) (xy 133.65 123.5) (xy 133.65 85.975) (xy 166.325 85.975)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads no (clearance 0.02548))
    (min_thickness 0.02548)
    (fill yes (arc_segments 16) (thermal_gap 1) (thermal_bridge_width 0.02549))
    (polygon
      (pts
        (xy 133.625 85.975) (xy 133.625 123.475) (xy 166.325 123.475) (xy 166.325 85.95) (xy 133.625 85.95)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads no (clearance 0.02548))
    (min_thickness 0.02548)
    (fill yes (arc_segments 16) (thermal_gap 1) (thermal_bridge_width 0.02549))
    (polygon
      (pts
        (xy 133.625 85.975) (xy 133.625 123.475) (xy 166.325 123.475) (xy 166.325 85.95) (xy 133.625 85.95)
      )
    )
  )
)
