(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 33)
    (no_connects 0)
    (area 25.324999 25.324999 115.645001 80.085001)
    (thickness 1.6)
    (drawings 30)
    (tracks 70)
    (zones 0)
    (modules 22)
    (nets 13)
  )
  (page A4)
  (layers
    (0 Top mixed)
    (31 Bottom power)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.381)
    (user_trace_width 0.4572)
    (user_trace_width 0.5588)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.762)
    (via_drill 0.381)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 0.762 0.381)
    (user_via 0.889 0.4572)
    (user_via 1.016 0.508)
    (user_via 1.27 0.635)
    (user_via 1.524 0.762)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VIN)
  (net 2 "Net-(F1-Pad2)")
  (net 3 GND)
  (net 4 JOY_X)
  (net 5 +5V)
  (net 6 JOY_Y)
  (net 7 SW1)
  (net 8 SW2)
  (net 9 SW_JOY)
  (net 10 VCC)
  (net 11 RX)
  (net 12 TX)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net JOY_X)
    (add_net JOY_Y)
    (add_net RX)
    (add_net SW1)
    (add_net SW2)
    (add_net SW_JOY)
    (add_net TX)
  )
  (net_class Min ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
  )
  (net_class Power ""
    (clearance 0.254)
    (trace_width 0.762)
    (via_dia 1.016)
    (via_drill 0.508)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(F1-Pad2)")
    (add_net VCC)
    (add_net VIN)
  )
  (module Sparkfun_Modules_BG:Microview (layer Top) (tedit 5A51DE6F)
    (at 63.5 46.99 90)
    (fp_text reference U3 (at 6.35 8.89 180) (layer F.SilkS))
    (fp_text value Module_Sparkfun_Microview (at 8.89 0 90) (layer F.Fab) hide)
    (fp_text user SCREEN (at 12.7 8.89 360) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 SW_JOY))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 JOY_Y))
    (pad 5 thru_hole circle (at 0 10.16 90) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 JOY_X))
    (pad 6 thru_hole circle (at 0 12.7 90) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 0 15.24 90) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 0 17.78 90) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 9 thru_hole circle (at 17.78 17.78 90) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 RX))
    (pad 10 thru_hole circle (at 17.78 15.24 90) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 TX))
    (pad 11 thru_hole circle (at 17.78 12.7 90) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 SW2))
    (pad 12 thru_hole circle (at 17.78 10.16 90) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 17.78 7.62 90) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 SW1))
    (pad 14 thru_hole circle (at 17.78 5.08 90) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 17.78 2.54 90) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 16 thru_hole circle (at 17.78 0 90) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 VCC))
  )
  (module Hardware_BG:SW_PUSH-12mm (layer Top) (tedit 5A51DE69)
    (at 91.44 68.58)
    (descr "SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
    (tags "tact sw push 12mm")
    (fp_text reference SW2 (at 6.08 2.54 180) (layer F.SilkS))
    (fp_text value SW_Push (at 6.62 9.93) (layer F.Fab) hide)
    (fp_text user %R (at 6.35 2.54) (layer F.Fab))
    (pad 1 thru_hole oval (at 12.5 0) (size 5.08 3.048) (drill 1.5494) (layers *.Cu *.Mask)
      (net 8 SW2))
    (pad 2 thru_hole oval (at 12.5 5) (size 5.08 3.048) (drill 1.5494) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole oval (at 0 0) (size 5.08 3.048) (drill 1.5494) (layers *.Cu *.Mask)
      (net 8 SW2))
    (pad 2 thru_hole oval (at 0 5) (size 5.08 3.048) (drill 1.5494) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0.248 -0.1 0))
      (scale (xyz 3.93701 3.93701 3.93701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.5mm (layer Top) (tedit 5A51D856)
    (at 29.21 29.21)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01_Pitch2.54mm (layer Top) (tedit 5A51D5E2)
    (at 105.41 30.48)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Socket_Strip_Straight_1x01_Pitch2.54mm (at 0 2.33) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Mounting_Holes:MountingHole_3mm (layer Top) (tedit 5A51D5CF)
    (at 110.49 57.15)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0 4) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3mm (layer Top) (tedit 5A51D5CD)
    (at 87.63 57.15)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0 4) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3mm (layer Top) (tedit 5A51D5CA)
    (at 110.49 29.21)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0 4) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_1-5mmDrill (layer Top) (tedit 5A51D397)
    (at 59.055 71.0946)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value "" (at -0.635 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at -0.635 0.3302) (size 4.0005 4.0005) (drill 1.5494) (layers *.Cu *.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_1-5mmDrill (layer Top) (tedit 5A51D397)
    (at 43.815 71.0946)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value "" (at -0.635 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at -0.635 0.3302) (size 4.0005 4.0005) (drill 1.5494) (layers *.Cu *.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_1-5mmDrill (layer Top) (tedit 5A51D397)
    (at 59.055 57.785)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value "" (at -0.635 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at -0.635 0.3302) (size 4.0005 4.0005) (drill 1.5494) (layers *.Cu *.Mask))
  )
  (module Capacitors_THT:C_Disc_D7.0mm_W2.5mm_P5.00mm (layer Top) (tedit 5A51DE4E)
    (at 53.34 45.72 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7mm width 2.5mm Capacitor")
    (fp_text reference F1 (at 2.5 0 180) (layer F.SilkS))
    (fp_text value Polyfuse_Small (at 2.5 2.56 180) (layer F.Fab) hide)
    (fp_text user %R (at 2.5 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VIN))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(F1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x05_Pitch2.54mm (layer Top) (tedit 5A51D84A)
    (at 35.56 31.75)
    (descr "Through hole straight socket strip, 1x05, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x05 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value USB_OTG (at 0 12.49) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(F1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Potentiometers:Potentiometer_WirePads_Small (layer Top) (tedit 5A51DE63)
    (at 53.34 74.93 270)
    (descr "Potentiometer, Wire Pads only, small, RevA, 02 Aug 2010,")
    (tags "Potentiometer Wire Pads only small RevA 02 Aug 2010 ")
    (fp_text reference RV1 (at 1.3 -1.9 270) (layer F.SilkS) hide)
    (fp_text value POT (at 1.35 7.15 270) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 0 2.54 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 JOY_X))
    (pad 3 thru_hole circle (at 0 5.08 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module Potentiometers:Potentiometer_WirePads_Small (layer Top) (tedit 5A51DE60)
    (at 40.64 67.31 180)
    (descr "Potentiometer, Wire Pads only, small, RevA, 02 Aug 2010,")
    (tags "Potentiometer Wire Pads only small RevA 02 Aug 2010 ")
    (fp_text reference RV2 (at 1.3 -1.9 180) (layer F.SilkS) hide)
    (fp_text value POT (at 1.35 7.15 180) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 0 2.54 180) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 JOY_Y))
    (pad 3 thru_hole circle (at 0 5.08 180) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module Hardware_BG:SW_PUSH-12mm (layer Top) (tedit 5A51DE66)
    (at 71.12 68.66)
    (descr "SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
    (tags "tact sw push 12mm")
    (fp_text reference SW1 (at 6.08 2.54 180) (layer F.SilkS))
    (fp_text value SW_Push (at 6.62 9.93) (layer F.Fab) hide)
    (fp_text user %R (at 6.35 2.54) (layer F.Fab))
    (pad 1 thru_hole oval (at 12.5 0) (size 5.08 3.048) (drill 1.5494) (layers *.Cu *.Mask)
      (net 7 SW1))
    (pad 2 thru_hole oval (at 12.5 5) (size 5.08 3.048) (drill 1.5494) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole oval (at 0 0) (size 5.08 3.048) (drill 1.5494) (layers *.Cu *.Mask)
      (net 7 SW1))
    (pad 2 thru_hole oval (at 0 5) (size 5.08 3.048) (drill 1.5494) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0.248 -0.1 0))
      (scale (xyz 3.93701 3.93701 3.93701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hardware_BG:Joy_SW (layer Top) (tedit 5A51DE5D)
    (at 47.625 52.07)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=4.3mm")
    (tags "tact sw push 6mm")
    (fp_text reference SW3 (at 3.25 2.54) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7) (layer F.Fab) hide)
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 5.08 90) (size 1.778 1.778) (drill 0.889) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.778 1.778) (drill 0.889) (layers *.Cu *.Mask)
      (net 9 SW_JOY))
    (pad 2 thru_hole circle (at 6.35 5.08 90) (size 1.778 1.778) (drill 0.889) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 6.35 0 90) (size 1.778 1.778) (drill 0.889) (layers *.Cu *.Mask)
      (net 9 SW_JOY))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm_h4.3mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pololu_BG:Pololu_2810_2811 (layer Top) (tedit 5A51DE58)
    (at 44.45 29.21)
    (fp_text reference U1 (at 6.35 11.43) (layer F.SilkS))
    (fp_text value PowerModule_Pololu_281x (at 6.35 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 5 thru_hole circle (at 0 10.16) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 VCC))
    (pad 6 thru_hole circle (at 0 12.7) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 VCC))
    (pad 7 thru_hole circle (at 12.7 12.7) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 VIN))
    (pad 8 thru_hole circle (at 12.7 10.16) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 VIN))
    (pad 9 thru_hole circle (at 12.7 7.62) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 10 thru_hole circle (at 12.7 5.08) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 11 thru_hole circle (at 12.7 2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 3.81 8.255) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 6.35 8.255) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 8.89 8.255) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x04_Pitch2.54mm (layer Top) (tedit 5A51DE6B)
    (at 95.25 58.42 90)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference U2 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value XbeeExplorer (at 0 9.95 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 RX))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 TX))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Wire_Pads:SolderWirePad_single_1-5mmDrill (layer Top) (tedit 5A51D397)
    (at 43.815 57.785)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value "" (at -0.635 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at -0.635 0.3302) (size 4.0005 4.0005) (drill 1.5494) (layers *.Cu *.Mask))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01_Pitch2.54mm (layer Top) (tedit 5A51D5E2)
    (at 92.71 30.48)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Socket_Strip_Straight_1x01_Pitch2.54mm (at 0 2.33) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Mounting_Holes:MountingHole_3mm (layer Top) (tedit 5A51D5DF)
    (at 87.63 29.21)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0 4) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.5mm (layer Top) (tedit 5A51D85B)
    (at 29.21 44.45)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (gr_text "Zumo Remote" (at 30.48 60.96 90) (layer F.SilkS))
  (gr_text "Rev B    Jan 2018\nDesigned by Blake Garner" (at 26.67 77.47) (layer F.SilkS))
  (gr_text "Power\nProtection\nModule" (at 50.8 34.29) (layer F.SilkS))
  (gr_text "USB Connector" (at 33.02 36.83 90) (layer F.SilkS))
  (gr_arc (start 27.94 77.47) (end 27.94 80.01) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 27.94 27.94) (end 25.4 27.94) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 113.03 27.94) (end 113.03 25.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 113.03 77.47) (end 115.57 77.47) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.57 27.94) (end 115.57 77.47) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 113.03 25.4) (end 27.94 25.4) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 25.4 77.47) (end 25.4 27.94) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 113.03 80.01) (end 27.94 80.01) (layer Edge.Cuts) (width 0.15))
  (gr_text XBEE (at 99.06 41.91) (layer F.SilkS))
  (gr_text "LED\nON/OFF" (at 97.79 62.23) (layer F.SilkS))
  (gr_text "LINE\nFOLLOW" (at 77.47 62.23) (layer F.SilkS))
  (gr_text "Thumb\nJoystick" (at 50.8 64.77) (layer F.SilkS))
  (zone (net 3) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.27))
    (polygon
      (pts
        (xy 26.67 26.67) (xy 114.3 26.67) (xy 114.3 78.74) (xy 26.67 78.74)
      )
    )
  )
)
