(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (date "2022-10-17")
    (rev "0.0.01")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 127 76.2)
    (pcbplotparams
      (layerselection 0x00310f0_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/media/adamw/data/programming/bq/gerbers/")
    )
  )
  (net 0 "")
  (footprint "Library:55fdc74f-a520-4e50-91cd-2504150caa4f" (layer "F.Cu")
    (tedit 0)
    (at 142.561913 105.618997)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -2.8625 -2.75) (layer "F.Fab"))
    (pad "1" smd roundrect (at -5.725 -8) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "2" smd roundrect (at -5.725 -7.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "3" smd roundrect (at -5.725 -7) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "4" smd roundrect (at -5.725 -6.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "5" smd roundrect (at -5.725 -6) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "6" smd roundrect (at -5.725 -5.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "7" smd roundrect (at -5.725 -5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "8" smd roundrect (at -5.725 -4.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "9" smd roundrect (at -5.725 -4) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "10" smd roundrect (at -5.725 -3.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "11" smd roundrect (at -5.725 -3) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "12" smd roundrect (at -5.725 -2.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "13" smd roundrect (at -5.725 -2) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "14" smd roundrect (at -5.725 -1.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "15" smd roundrect (at -5.725 -1) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "16" smd roundrect (at -5.725 -0.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "17" smd roundrect (at -5.725 0) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "18" smd roundrect (at -5.725 0.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "19" smd roundrect (at -5.725 1) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "20" smd roundrect (at -5.725 1.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "21" smd roundrect (at -5.725 2) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "22" smd roundrect (at -5.725 2.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "23" smd roundrect (at 0 2.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "24" smd roundrect (at 0 2) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "25" smd roundrect (at 0 1.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "26" smd roundrect (at 0 1) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "27" smd roundrect (at 0 0.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "28" smd roundrect (at 0 0) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "29" smd roundrect (at 0 -0.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "30" smd roundrect (at 0 -1) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "31" smd roundrect (at 0 -1.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "32" smd roundrect (at 0 -2) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "33" smd roundrect (at 0 -2.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "34" smd roundrect (at 0 -3) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "35" smd roundrect (at 0 -3.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "36" smd roundrect (at 0 -4) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "37" smd roundrect (at 0 -4.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "38" smd roundrect (at 0 -5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "39" smd roundrect (at 0 -5.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "40" smd roundrect (at 0 -6) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "41" smd roundrect (at 0 -6.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "42" smd roundrect (at 0 -7) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "43" smd roundrect (at 0 -7.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "44" smd roundrect (at 0 -8) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  )
  (footprint "Library:DIP-48_W15.24mm_LongPads" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 127 76.2)
    (descr "48-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil LongPads")
    (attr through_hole)
    (fp_text reference "REF**" (at 12.59 -0.1) (layer "F.SilkS") hide)
    (fp_text value "TSSOP44toDIP-44_28x56.15mm_1.1023x2.2893in_LongPads" (at 20.82 29.69 90) (layer "F.Fab") hide)
    (fp_line (start 26.86 -1.55) (end -1.5 -1.55) (layer "Edge.Cuts") (width 0.05))
    (fp_line (start -1.5 -1.55) (end -1.5 54.6) (layer "Edge.Cuts") (width 0.05))
    (fp_line (start -1.5 54.6) (end 26.88 54.6) (layer "Edge.Cuts") (width 0.05))
    (fp_line (start 26.88 54.6) (end 26.86 -1.55) (layer "Edge.Cuts") (width 0.05))
    (pad "1" thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "2" thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "3" thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "4" thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "5" thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "6" thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "7" thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "8" thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "9" thru_hole oval (at 0 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "10" thru_hole oval (at 0 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "11" thru_hole oval (at 0 25.4) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "12" thru_hole oval (at 0 27.94) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "13" thru_hole oval (at 0 30.48) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "14" thru_hole oval (at 0 33.02) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "15" thru_hole oval (at 0 35.56) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "16" thru_hole oval (at 0 38.1) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "17" thru_hole oval (at 0 40.64) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "18" thru_hole oval (at 0 43.18) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "19" thru_hole oval (at 0 45.72) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "20" thru_hole oval (at 0 48.26) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "21" thru_hole oval (at 0 50.8) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "22" thru_hole oval (at 0 53.34) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "23" thru_hole oval (at 25.4 53.34) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "24" thru_hole oval (at 25.4 50.8) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "25" thru_hole oval (at 25.4 48.26) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "26" thru_hole oval (at 25.4 45.72) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "27" thru_hole oval (at 25.4 43.18) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "28" thru_hole oval (at 25.4 40.64) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "29" thru_hole oval (at 25.4 38.1) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "30" thru_hole oval (at 25.4 35.56) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "31" thru_hole oval (at 25.4 33.02) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "32" thru_hole oval (at 25.4 30.48) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "33" thru_hole oval (at 25.4 27.94) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "34" thru_hole oval (at 25.4 25.4) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "35" thru_hole oval (at 25.4 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "36" thru_hole oval (at 25.4 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "37" thru_hole oval (at 25.4 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "38" thru_hole oval (at 25.4 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "39" thru_hole oval (at 25.4 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "40" thru_hole oval (at 25.4 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "41" thru_hole oval (at 25.4 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "42" thru_hole oval (at 25.4 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "43" thru_hole oval (at 25.4 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "44" thru_hole oval (at 25.4 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-48_W15.24mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
)
