(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "Compaq Portable III Battery Module")
    (date "2022-05-23")
    (rev "1.1")
    (company "Designed by Sergey Kiselev")
    (comment 2 "Licensed under CERN-OHL-S: https://cern-ohl.web.cern.ch")
    (comment 3 "Documentation and design files: https://github.com/skiselev/compaq-portable-iii-battery")
    (comment 4 "Compaq Portable III Battery Module is an open source hardware project")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber")
    )
  )
  (net 0 "")
  (net 1 "VMEM")
  (net 2 "GND")
  (footprint "My_Components:Conn_Pin_Header_1x1_2.54mm_NoKey" (layer "F.Cu")
    (tedit 603D245E)
    (at 133.35 77.47)
    (descr "Pin Header, 1x1, 2.54mm pitch, No Key")
    (tags "CONN 1x1")
    (property "Sheetfile" "Compaq_Portable_III_Battery.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.54) (layer "F.SilkS") hide)
    (fp_text value "-" (at 2.54 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (model "pin_array/pins_array_8x2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Conn_Pin_Header_1x1_2.54mm" (layer "F.Cu")
    (tedit 603D244E)
    (at 107.95 77.47)
    (descr "Pin Header, 1x1, 2.54mm pitch")
    (tags "CONN 1x1")
    (property "Sheetfile" "Compaq_Portable_III_Battery.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.54) (layer "F.SilkS") hide)
    (fp_text value "+" (at -2.54 0) (layer "F.SilkS"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "VMEM") (pinfunction "Pin_1") (pintype "passive"))
    (model "pin_array/pins_array_8x2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Conn_Pin_Header_1x1_2.54mm" (layer "F.Cu")
    (tedit 603D244E)
    (at 133.35 105.41)
    (descr "Pin Header, 1x1, 2.54mm pitch")
    (tags "CONN 1x1")
    (property "Sheetfile" "Compaq_Portable_III_Battery.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 0 2.54) (layer "F.SilkS") hide)
    (fp_text value "+" (at 2.54 0) (layer "F.SilkS"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "VMEM") (pinfunction "Pin_1") (pintype "passive"))
    (model "pin_array/pins_array_8x2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Conn_Pin_Header_1x1_2.54mm_NoKey" (layer "F.Cu")
    (tedit 603D245E)
    (at 107.95 105.41)
    (descr "Pin Header, 1x1, 2.54mm pitch, No Key")
    (tags "CONN 1x1")
    (property "Sheetfile" "Compaq_Portable_III_Battery.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 2.54) (layer "F.SilkS") hide)
    (fp_text value "-" (at -2.54 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (model "pin_array/pins_array_8x2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Battery_Holder_Renata_SMTU2477N-LF_Hand_Soldering" (layer "F.Cu")
    (tedit 627AA63F)
    (at 120.65 91.44)
    (descr "Battery Holder, CR2030, Links BAT-HLD-001-SMT")
    (tags "BATTERY HOLDER CR2032")
    (property "Sheetfile" "Compaq_Portable_III_Battery.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "BT1" (at -5.08 13.97) (layer "F.SilkS"))
    (fp_text value "CR2477N" (at 5.08 13.97) (layer "F.SilkS"))
    (fp_text user "-" (at 15.24 4.445 unlocked) (layer "F.SilkS"))
    (fp_text user "+" (at -15.24 4.445 unlocked) (layer "F.SilkS"))
    (pad "1" smd rect (at -17.1 0) (size 3 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "VMEM") (pinfunction "+") (pintype "passive"))
    (pad "2" smd rect (at 17.1 0) (size 3 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "-") (pintype "passive"))
  )
  (gr_line (start 101.6 105.41) (end 101.6 77.47) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 102.87 106.68) (mid 101.971974 106.308026) (end 101.6 105.41) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 102.87 76.2) (end 138.43 76.2) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 139.7 105.41) (mid 139.328026 106.308026) (end 138.43 106.68) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 138.43 106.68) (end 102.87 106.68) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 101.6 77.47) (mid 101.971974 76.571974) (end 102.87 76.2) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 138.43 76.2) (mid 139.328026 76.571974) (end 139.7 77.47) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 139.7 77.47) (end 139.7 105.41) (layer "Edge.Cuts") (width 0.1))
  (gr_text "Compaq Portable III Battery Module\nCopyright (C) 2022 Sergey Kiselev" (at 120.65 77.978) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.7 106.68)
        (xy 115.57 106.68)
        (xy 107.95 99.06)
        (xy 107.95 76.2)
        (xy 139.7 76.2)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.7 106.68)
        (xy 101.6 106.68)
        (xy 101.6 76.2)
        (xy 139.7 76.2)
      )
    )
  )
)
