(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 97)
    (no_connects 0)
    (area 90.679199 65.202999 137.920801 137.997001)
    (thickness 1.6)
    (drawings 20)
    (tracks 331)
    (zones 0)
    (modules 52)
    (nets 36)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.1778)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.2 3.2)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 114.3 101.6)
    (grid_origin 114.3 101.6)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /USBDP)
  (net 3 /USBDM)
  (net 4 +5V)
  (net 5 "Net-(D1-Pad2)")
  (net 6 +3V3)
  (net 7 "Net-(D2-Pad1)")
  (net 8 "Net-(J1-Pad2)")
  (net 9 "Net-(J1-Pad3)")
  (net 10 /RF_MOD)
  (net 11 /RTS)
  (net 12 /GPIO2)
  (net 13 /CH_PD)
  (net 14 /GPIO15)
  (net 15 /DTR)
  (net 16 /USB_RX)
  (net 17 /RESET)
  (net 18 /GPIO0)
  (net 19 /TX)
  (net 20 "Net-(Q1-Pad2)")
  (net 21 "Net-(Q1-Pad5)")
  (net 22 /AC-N)
  (net 23 /AC-L)
  (net 24 "Net-(AE1-Pad1)")
  (net 25 "Net-(C4-Pad1)")
  (net 26 "Net-(C9-Pad1)")
  (net 27 "Net-(C14-Pad1)")
  (net 28 "Net-(R9-Pad2)")
  (net 29 /RF_CLK)
  (net 30 "Net-(C17-Pad2)")
  (net 31 "Net-(C15-Pad2)")
  (net 32 "Net-(C15-Pad1)")
  (net 33 "Net-(C16-Pad2)")
  (net 34 "Net-(C16-Pad1)")
  (net 35 "Net-(C17-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /AC-L)
    (add_net /AC-N)
    (add_net /CH_PD)
    (add_net /DTR)
    (add_net /GPIO0)
    (add_net /GPIO15)
    (add_net /GPIO2)
    (add_net /RESET)
    (add_net /RF_CLK)
    (add_net /RF_MOD)
    (add_net /RTS)
    (add_net /TX)
    (add_net /USBDM)
    (add_net /USBDP)
    (add_net /USB_RX)
    (add_net GND)
    (add_net "Net-(AE1-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C16-Pad2)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C17-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q1-Pad5)")
    (add_net "Net-(R9-Pad2)")
  )
  (module Connectors_USB:USB_Micro-B_Vertical_Molex-105133-0001 (layer F.Cu) (tedit 5A72AA58)
    (at 132.759145 107.652891 180)
    (descr "Molex Vertical Micro USB Typ-B (http://www.molex.com/pdm_docs/sd/1051330001_sd.pdf)")
    (tags "Micro-USB SMD Typ-B Vertical")
    (attr smd)
    (fp_text reference J1 (at -3.384855 2.496891 180) (layer F.SilkS))
    (fp_text value USB_OTG (at -0.025 3 180) (layer F.Fab))
    (fp_text user %R (at 0 -0.375 180) (layer F.Fab))
    (pad 3 smd rect (at 0 -0.825 180) (size 0.45 1.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at 0.65 -0.825 180) (size 0.45 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.65 -0.825 180) (size 0.45 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad2)"))
    (pad 5 smd rect (at 1.3 -0.825 180) (size 0.45 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.3 -0.825 180) (size 0.45 1.5) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C9-Pad1)"))
    (pad 6 thru_hole circle (at -2.8 -1.075 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 2.8 -1.075 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 0 1.075 180) (size 1.905 1.905) (drill 1.397) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connectors_USB.3dshapes/USB_Micro-B_Vertical_Molex-105133-0001.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ESP8266:ESP-12E_SMD (layer F.Cu) (tedit 5A700E39)
    (at 117.348 88.392)
    (descr "Module, ESP-8266, ESP-12, 16 pad, SMD")
    (tags "Module ESP-8266 ESP8266")
    (fp_text reference U4 (at -1.524 -1.778 90) (layer F.SilkS))
    (fp_text value ESP-12E (at 5.08 6.35 90) (layer F.Fab) hide)
    (fp_text user "No Copper" (at 6.892 -5.4) (layer F.CrtYd))
    (pad 1 smd rect (at 0 0) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 17 /RESET))
    (pad 2 smd rect (at 0 2) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0 4) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 13 /CH_PD))
    (pad 4 smd rect (at 0 6) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 10 /RF_MOD))
    (pad 5 smd rect (at 0 8) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 29 /RF_CLK))
    (pad 6 smd rect (at 0 10) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 0 12) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 0 14) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 9 smd rect (at 14 14) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 14 12) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 14 /GPIO15))
    (pad 11 smd rect (at 14 10) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 12 /GPIO2))
    (pad 12 smd rect (at 14 8) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 18 /GPIO0))
    (pad 13 smd rect (at 14 6) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 14 4) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 14 2) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R9-Pad2)"))
    (pad 16 smd rect (at 14 0) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 19 /TX))
    (model ${ESPLIB}/ESP8266.3dshapes/ESP-12.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x03 (layer F.Cu) (tedit 5A76AC68)
    (at 130.556 129.286 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J2 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /RF_MOD))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 135.329145 111.271891)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 1.322855 0.996109) (layer F.SilkS))
    (fp_text value 10n (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 129.487145 111.271891 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 2.051891 -0.963145 90) (layer F.SilkS))
    (fp_text value 47p (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /USBDP))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 129.487145 114.319891 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 1.250109 1.217145 270) (layer F.SilkS))
    (fp_text value 47p (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 /USBDM))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 120.089145 107.207891 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 0 1.543891 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 123.137145 107.207891)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at 0 -1.543891) (layer F.SilkS))
    (fp_text value 4.7u (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 126.185145 107.207891 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 0 1.543891 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 135.382 93.218 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at -0.254 1.524 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Inductors_SMD:L_0805 (layer F.Cu) (tedit 58307B54)
    (at 134.567145 113.811891 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference L1 (at 0.488109 -1.576855 270) (layer F.SilkS))
    (fp_text value Ferrite_Bead (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (model Inductors_SMD.3dshapes\L_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 117.041145 111.271891 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 2.012109 -0.052855 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(Q1-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 /RTS))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 135.382 98.806 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.524 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 /GPIO2))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 116.078 105.156 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -2.032 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 /CH_PD))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 135.382 101.6 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 1.524 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 /GPIO15))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 115.263145 111.271891 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -2.012109 0.052855 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(Q1-Pad5)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /DTR))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 131.519145 112.033891)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0.052855 -1.289891) (layer F.SilkS))
    (fp_text value 27 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 /USBDP))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 135.382 90.424 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 1.524 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 /USB_RX))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R9-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 131.519145 113.557891)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0.052855 1.504109) (layer F.SilkS))
    (fp_text value 27 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 /USBDM))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 118.872 111.264 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 2.528 0 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 /RESET))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 135.382 96.024 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0 1.524 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 /GPIO0))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Converters_DCDC_ACDC:ACDC-Converter_MeanWell-IRM-02-x (layer F.Cu) (tedit 58388E98)
    (at 110.196 85.03 270)
    (descr "ACDC-Converter, 2W, Meanwell, IRM-02, THT")
    (fp_text reference U1 (at -4.512 18.248 270) (layer F.SilkS))
    (fp_text value IRM-02-5 (at 14.15 20.7 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.29 2.29) (drill 0.76) (layers *.Cu *.Mask)
      (net 22 /AC-N))
    (pad 2 thru_hole circle (at 0 15.2 270) (size 2.29 2.29) (drill 0.76) (layers *.Cu *.Mask)
      (net 23 /AC-L))
    (pad 3 thru_hole circle (at 28 0 270) (size 2.29 2.29) (drill 0.76) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 28 7.6 270) (size 2.29 2.29) (drill 0.76) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)"))
  )
  (module SMD_Packages:SSOP-20 (layer F.Cu) (tedit 0)
    (at 124.407145 112.541891)
    (descr "SSOP 20 pins")
    (tags "CMS SSOP SMD")
    (attr smd)
    (fp_text reference U5 (at -2.995145 4.298109) (layer F.SilkS))
    (fp_text value FT231XS (at 0 0.635) (layer F.Fab))
    (pad 1 smd rect (at -2.921 2.667) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 15 /DTR))
    (pad 2 smd rect (at -2.286 2.667) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 11 /RTS))
    (pad 3 smd rect (at -1.6256 2.667) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 4 smd rect (at -0.9652 2.667) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 19 /TX))
    (pad 5 smd rect (at -0.3302 2.667) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 0.3302 2.667) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 0.9906 2.667) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 1.6256 2.667) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 2.286 2.667) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 2.921 2.667) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 2.921 -2.667) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 /USBDP))
    (pad 12 smd rect (at 2.286 -2.667) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 /USBDM))
    (pad 13 smd rect (at 1.6256 -2.667) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C14-Pad1)"))
    (pad 14 smd rect (at 0.9906 -2.667) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C14-Pad1)"))
    (pad 15 smd rect (at 0.3302 -2.667) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 16 smd rect (at -0.3302 -2.667) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at -0.9652 -2.667) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -1.6256 -2.667) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at -2.286 -2.667) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at -2.921 -2.667) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 16 /USB_RX))
    (model SMD_Packages.3dshapes/SSOP-20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.255 0.33 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-363_SC-70-6 (layer F.Cu) (tedit 585EA0FD)
    (at 116.025145 107.715891 90)
    (descr "SOT-363, SC-70-6")
    (attr smd)
    (fp_text reference Q1 (at 0.019891 1.830855 90) (layer F.SilkS))
    (fp_text value MBT2222ADW1T1 (at 0 2 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 -0.65 90) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 /DTR))
    (pad 3 smd rect (at -0.95 0.65 90) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 17 /RESET))
    (pad 5 smd rect (at 0.95 0 90) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(Q1-Pad5)"))
    (pad 2 smd rect (at -0.95 0 90) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(Q1-Pad2)"))
    (pad 4 smd rect (at 0.95 0.65 90) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /RTS))
    (pad 6 smd rect (at 0.95 -0.65 90) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 18 /GPIO0))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A76AC73)
    (at 93.6498 77.7748)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference MK3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A76AC80)
    (at 134.9502 77.7748)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference MK4 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A76AC6C)
    (at 134.9502 125.4252)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference MK5 (at -0.0762 2.8448) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A76AC63)
    (at 93.660594 125.422834)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference MK6 (at 0 2.847166) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 5A76AC77)
    (at 114.3 73.66)
    (fp_text reference MK1 (at 0 -3.81) (layer F.SilkS))
    (fp_text value Mounting_Hole_PAD (at -0.6604 5.715) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 23 /AC-L))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 5A76AC7B)
    (at 101.854 73.66)
    (fp_text reference MK2 (at 0 -3.81) (layer F.SilkS))
    (fp_text value Mounting_Hole_PAD (at -0.5334 5.334) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 22 /AC-N))
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 583F3A3F)
    (at 133.35 117.856 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at 0 -2.9 180) (layer F.SilkS))
    (fp_text value AP2127K-3.3 (at 0 2.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 136.398 118.11 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.032 0 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 130.302 118.11 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 102.87 117.094 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -2.286 0 180) (layer F.SilkS))
    (fp_text value DNP (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 100.838 117.856 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -0.762 1.27 90) (layer F.SilkS))
    (fp_text value 220p (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C4-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 99.568 117.856 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0.508 -1.524 270) (layer F.SilkS))
    (fp_text value 0.01u (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C4-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 98.806 125.222)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at -2.286 0) (layer F.SilkS))
    (fp_text value 12p (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(AE1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 95.504 120.65 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 12p (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C17-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 103.632 124.46)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0 1.524) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603 (layer F.Cu) (tedit 58307A47)
    (at 98.044 119.38 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L2 (at 0 1.27 270) (layer F.SilkS))
    (fp_text value 27nH (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603 (layer F.Cu) (tedit 58307A47)
    (at 98.044 123.444 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L3 (at 0 1.524 270) (layer F.SilkS))
    (fp_text value 16nH (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C17-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(AE1-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Trimmer_Vishay_TS53YL (layer F.Cu) (tedit 5A76ACA0)
    (at 108.204 121.368 270)
    (descr "Spindle Trimmer Potentiometer, Vishay TS53YL, https://www.bourns.com/pdfs/3224.pdf")
    (tags "Spindle Trimmer Potentiometer   Vishay TS53YL")
    (attr smd)
    (fp_text reference R6 (at 4.362 -1.778 540) (layer F.SilkS))
    (fp_text value R_Variable (at -0.18 3.75 270) (layer F.Fab) hide)
    (pad 1 smd rect (at 2.75 -1.15 270) (size 1.3 1.3) (layers F.Cu F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at -2.75 0 270) (size 2 1.3) (layers F.Cu F.Mask)
      (net 25 "Net-(C4-Pad1)"))
    (pad 3 smd rect (at 2.75 1.15 270) (size 1.3 1.3) (layers F.Cu F.Mask))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_Vishay_TS53YL.wrl
      (at (xyz 0.04 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-8 (layer F.Cu) (tedit 58CE4E7E)
    (at 102.362 121.412 270)
    (descr "8-pin SOT-23 package, http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/sot-23rj/rj_8.pdf")
    (tags SOT-23-8)
    (attr smd)
    (fp_text reference U3 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value MAX7044 (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.98 270) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C15-Pad2)"))
    (pad 2 smd rect (at -1.1 -0.33 270) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.33 270) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -1.1 0.98 270) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C17-Pad1)"))
    (pad 5 smd rect (at 1.1 0.98 270) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 /RF_CLK))
    (pad 6 smd rect (at 1.1 0.33 270) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 /RF_MOD))
    (pad 7 smd rect (at 1.1 -0.33 270) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 8 smd rect (at 1.1 -0.98 270) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C16-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-U_Vertical (layer F.Cu) (tedit 58CD2E9C)
    (at 117.348 117.802 270)
    (descr "Crystal THT HC-49/U http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49/U")
    (fp_text reference Y1 (at 2.44 -3.525 270) (layer F.SilkS))
    (fp_text value Crystal (at 2.44 3.525 270) (layer F.Fab))
    (fp_text user %R (at 2.44 0 450) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(C15-Pad1)"))
    (pad 2 thru_hole circle (at 4.88 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(C16-Pad2)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_HC49-U_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module esp433:W3127 (layer F.Cu) (tedit 5A76977C)
    (at 97.663 130.302)
    (fp_text reference AE1 (at -2.413 0) (layer F.SilkS))
    (fp_text value Antenna (at 0 -5.588) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(AE1-Pad1)"))
    (pad "" np_thru_hole circle (at 4.15 0) (size 3 3) (drill 2.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 29.15 0) (size 3 3) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Buttons_Switches_SMD:SW_SPST_B3U-1000P (layer F.Cu) (tedit 5A76AC8B)
    (at 135.636 84.582 270)
    (descr "Ultra-small-sized Tactile Switch with High Contact Reliability, Top-actuated Model, without Ground Terminal, without Boss")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at -3.81 0 270) (layer F.SilkS))
    (fp_text value SW_Push (at 0 2.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.5 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.7 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 /RESET))
    (pad 2 smd rect (at 1.7 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3U-1000P.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 112.776 119.634 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at 0 -4.318 180) (layer F.SilkS))
    (fp_text value 12p (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C15-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C15-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 112.776 121.158)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at 0 4.064) (layer F.SilkS))
    (fp_text value 12p (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C16-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C16-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 97.802 121.412 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C17 (at -2.274 0 270) (layer F.SilkS))
    (fp_text value 15p (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C17-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C17-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123F (layer F.Cu) (tedit 587F7769)
    (at 128.016 120.396 180)
    (descr D_SOD-123F)
    (tags D_SOD-123F)
    (attr smd)
    (fp_text reference D1 (at -0.127 -1.905 180) (layer F.SilkS))
    (fp_text value D (at 0 2.1 180) (layer F.Fab))
    (fp_text user %R (at -0.127 -1.905 180) (layer F.Fab))
    (pad 1 smd rect (at -1.4 0 180) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 1.4 0 180) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 112.776 118.11 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C18 (at 0 1.27 180) (layer F.SilkS))
    (fp_text value DNP (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C15-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 112.776 122.682 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C19 (at 0 -3.81 180) (layer F.SilkS))
    (fp_text value DNP (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C16-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 131.4958 131.572) (end 137.8458 131.572) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.4958 137.922) (end 131.4958 131.572) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.1042 131.572) (end 97.1042 137.922) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.7542 131.572) (end 97.1042 131.572) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.1042 71.628) (end 90.7542 71.628) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.1042 65.278) (end 97.1042 71.628) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.4958 71.628) (end 131.4958 65.278) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.8458 71.628) (end 131.4958 71.628) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.4628 77.8764) (end 119.126 77.8764) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.4628 69.9516) (end 121.4628 77.8764) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.126 77.8764) (end 119.126 69.9516) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.126 69.9516) (end 121.4628 69.9516) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.1372 77.8764) (end 107.1372 69.9516) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.474 77.8764) (end 107.1372 77.8764) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.474 69.9516) (end 109.474 77.8764) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.1372 69.9516) (end 109.474 69.9516) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.8458 131.572) (end 137.8458 71.628) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.7542 71.628) (end 90.7542 131.572) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.1042 137.922) (end 131.4958 137.922) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.1042 65.278) (end 131.4958 65.278) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.678 86.868) (xy 96.5835 86.868) (xy 102.489 86.868) (xy 114.3 86.868) (xy 137.922 86.868)
        (xy 137.922 125.984) (xy 90.678 125.984)
      )
    )
  )
  (zone (net 6) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.648 91.694) (xy 137.922 91.694) (xy 137.922 125.984) (xy 104.648 125.984)
      )
    )
  )
)
