(kicad_pcb (version 20170123) (host pcbnew no-vcs-found-7613~57~ubuntu16.04.1)
  (general
    (links 63)
    (no_connects 0)
    (area 102.572599 96.172599 121.7749 121.277401)
    (thickness 1.6)
    (drawings 19)
    (tracks 301)
    (zones 0)
    (modules 32)
    (nets 23)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.8128)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (pad_to_paste_clearance -0.15)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x210fc_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 /D0_Sense)
  (net 4 /D0_Assert)
  (net 5 /D1_Sense)
  (net 6 /D1_Assert)
  (net 7 /LED_Sense)
  (net 8 /LED_Assert)
  (net 9 /Reader_+5-18v)
  (net 10 "Net-(C2-Pad1)")
  (net 11 "Net-(C2-Pad2)")
  (net 12 /Reader_D0)
  (net 13 /Reader_D1)
  (net 14 /Reader_LED)
  (net 15 "Net-(R1-Pad1)")
  (net 16 "Net-(R4-Pad2)")
  (net 17 "Net-(R5-Pad2)")
  (net 18 "Net-(R6-Pad2)")
  (net 19 "Net-(R7-Pad2)")
  (net 20 "Net-(R8-Pad2)")
  (net 21 "Net-(D1-Pad1)")
  (net 22 "Net-(C3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +3V3)
    (add_net /D0_Assert)
    (add_net /D0_Sense)
    (add_net /D1_Assert)
    (add_net /D1_Sense)
    (add_net /LED_Assert)
    (add_net /LED_Sense)
    (add_net /Reader_+5-18v)
    (add_net /Reader_D0)
    (add_net /Reader_D1)
    (add_net /Reader_LED)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 576410FF)
    (at 106.697 113.015 90)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 0 0 90) (layer F.SilkS))
    (fp_text value RT6212A/B (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C2-Pad1)"))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 /Reader_+5-18v))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C3-Pad1)"))
    (pad 6 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C2-Pad2)"))
    (pad 5 smd rect (at 1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R1-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 576410DB)
    (at 109 119.2 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R8 (at 0 0 90) (layer F.SilkS))
    (fp_text value 12k7 (at 0 -0.2 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R8-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 57641162)
    (at 112.5 106.1 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 0 0 270) (layer F.SilkS))
    (fp_text value 2N7002 (at 0 0.4 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 8 /LED_Assert))
    (pad 2 smd rect (at 0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -0.99822 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 14 /Reader_LED))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 587FFCEB)
    (at 105.4 105.2 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 0 180) (layer F.SilkS))
    (fp_text value PWR (at 0 0.3 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connector_IDC_SMD:SSL_DW_IDC_02 (layer F.Cu) (tedit 56CC14AC)
    (at 117.0178 116.0145 90)
    (fp_text reference P1 (at 0 0.0022 180) (layer F.SilkS))
    (fp_text value Power (at 0 3.7122 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 3 5.4) (layers F.Cu F.Paste F.Mask)
      (net 9 /Reader_+5-18v))
    (pad 2 smd rect (at 2 0 90) (size 3 5.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Connector_IDC_SMD:SSL_DW_IDC_03 (layer F.Cu) (tedit 56CC155B)
    (at 117.0178 106 270)
    (fp_text reference P2 (at -1.96 -0.0022) (layer F.SilkS))
    (fp_text value Wiegand (at 0 -3.7 270) (layer F.Fab))
    (pad 1 smd rect (at -4 0 270) (size 3 5.4) (layers F.Cu F.Paste F.Mask)
      (net 14 /Reader_LED))
    (pad 2 smd rect (at 0 0 270) (size 3 5.4) (layers F.Cu F.Paste F.Mask)
      (net 13 /Reader_D1))
    (pad 3 smd rect (at 4 0 270) (size 3 5.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Reader_D0))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57641137)
    (at 111.8 114.99 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -0.0075 180) (layer F.SilkS))
    (fp_text value 22u (at 0.0215 0.3925 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /Reader_+5-18v))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57641141)
    (at 104.6 113.4 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 0 90) (layer F.SilkS))
    (fp_text value 100n (at 0 -0.2 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 576410F3)
    (at 110.3 118.4 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 0 90) (layer F.SilkS))
    (fp_text value 22u (at 0 -0.4 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 576410EA)
    (at 111.75 118.7 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 0 90) (layer F.SilkS))
    (fp_text value 100n (at 0 -0.2 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 57641116)
    (at 112.5 112.7 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 0 270) (layer F.SilkS))
    (fp_text value 2N7002 (at 0 0.4 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 4 /D0_Assert))
    (pad 2 smd rect (at 0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -0.99822 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 12 /Reader_D0))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 576411FA)
    (at 112.5 109.4 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 0 270) (layer F.SilkS))
    (fp_text value 2N7002 (at 0 0.4 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 6 /D1_Assert))
    (pad 2 smd rect (at 0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -0.99822 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 13 /Reader_D1))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 57641176)
    (at 106.2 107.25 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at 0 0 90) (layer F.SilkS))
    (fp_text value 12k7 (at -0.05 -0.2 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5764121E)
    (at 108.6 107 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at 0 0 90) (layer F.SilkS))
    (fp_text value 12k7 (at 0 -0.2 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 57641123)
    (at 109.05 115 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at 0 0 180) (layer F.SilkS))
    (fp_text value 12k7 (at 0 0.2 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5764112D)
    (at 109.05 116.25 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at 0 0 270) (layer F.SilkS))
    (fp_text value 12k7 (at 0 0.2 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R7-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5764120E)
    (at 110.2 112.1 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R9 (at 0 0 180) (layer F.SilkS))
    (fp_text value 12k7 (at 0 0.2 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /D0_Assert))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 57641216)
    (at 110.2 111.1 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R10 (at 0 0 180) (layer F.SilkS))
    (fp_text value 12k7 (at 0 0.2 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 /Reader_D0))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /D0_Sense))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 57641205)
    (at 110.2 110)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R11 (at 0 0) (layer F.SilkS))
    (fp_text value 22k (at 0 -0.2) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /D0_Sense))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5764122A)
    (at 110.2 108.9 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R12 (at 0 0 180) (layer F.SilkS))
    (fp_text value 12k7 (at 0 0.2 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /D1_Assert))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5764119F)
    (at 110.2 107.8 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R13 (at 0 0 180) (layer F.SilkS))
    (fp_text value 12k7 (at 0 0.2 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /Reader_D1))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /D1_Sense))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 57641233)
    (at 110.2 106.7)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R14 (at -0.1 0) (layer F.SilkS))
    (fp_text value 22k (at 0 -0.2) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /D1_Sense))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 57641192)
    (at 107.4 106)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R15 (at -0.1 0) (layer F.SilkS))
    (fp_text value 12k7 (at 0 -0.2) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /LED_Assert))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5764116A)
    (at 110.5 105.3 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R16 (at -0.1 0 90) (layer F.SilkS))
    (fp_text value 12k7 (at 0 -0.2 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /Reader_LED))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /LED_Sense))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5764115A)
    (at 109.5 105.3 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R17 (at 0.1 0 270) (layer F.SilkS))
    (fp_text value 22k (at 0 0.2 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /LED_Sense))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5764117F)
    (at 107.4 105)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R18 (at 1 -0.2) (layer F.SilkS))
    (fp_text value 330 (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ESP8266:ESP-12-SMD locked (layer B.Cu) (tedit 569A764B)
    (at 119 105.1 180)
    (descr "Module, ESP-8266, ESP-12, 16 pad, SMD")
    (tags "Module ESP-8266 ESP8266")
    (fp_text reference U2 (at 1.7 -1.1 180) (layer B.SilkS))
    (fp_text value ESP-12 (at 6.992 -1 180) (layer B.Fab))
    (fp_text user "No Copper" (at 6.892 5.4 180) (layer B.CrtYd))
    (pad 1 smd rect (at 0 0 180) (size 2.5 1.1) (drill (offset -0.7 0)) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(R5-Pad2)"))
    (pad 2 smd oval (at 0 -2 180) (size 2.5 1.1) (drill (offset -0.7 0)) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd oval (at 0 -4 180) (size 2.5 1.1) (drill (offset -0.7 0)) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(R4-Pad2)"))
    (pad 4 smd oval (at 0 -6 180) (size 2.5 1.1) (drill (offset -0.7 0)) (layers B.Cu B.Paste B.Mask)
      (net 6 /D1_Assert))
    (pad 5 smd oval (at 0 -8 180) (size 2.5 1.1) (drill (offset -0.7 0)) (layers B.Cu B.Paste B.Mask)
      (net 5 /D1_Sense))
    (pad 6 smd oval (at 0 -10 180) (size 2.5 1.1) (drill (offset -0.7 0)) (layers B.Cu B.Paste B.Mask)
      (net 4 /D0_Assert))
    (pad 7 smd oval (at 0 -12 180) (size 2.5 1.1) (drill (offset -0.7 0)) (layers B.Cu B.Paste B.Mask)
      (net 3 /D0_Sense))
    (pad 8 smd oval (at 0 -14 180) (size 2.5 1.1) (drill (offset -0.7 0)) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 9 smd oval (at 14 -14 180) (size 2.5 1.1) (drill (offset 0.7 0)) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 10 smd oval (at 14 -12 180) (size 2.5 1.1) (drill (offset 0.6 0)) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(R8-Pad2)"))
    (pad 11 smd oval (at 14 -10 180) (size 2.5 1.1) (drill (offset 0.7 0)) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(R7-Pad2)"))
    (pad 12 smd oval (at 14 -8 180) (size 2.5 1.1) (drill (offset 0.7 0)) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(R6-Pad2)"))
    (pad 13 smd oval (at 14 -6 180) (size 2.5 1.1) (drill (offset 0.7 0)) (layers B.Cu B.Paste B.Mask)
      (net 8 /LED_Assert))
    (pad 14 smd oval (at 14 -4 180) (size 2.5 1.1) (drill (offset 0.7 0)) (layers B.Cu B.Paste B.Mask)
      (net 7 /LED_Sense))
    (pad 15 smd oval (at 14 -2 180) (size 2.5 1.1) (drill (offset 0.7 0)) (layers B.Cu B.Paste B.Mask))
    (pad 16 smd oval (at 14 0 180) (size 2.5 1.1) (drill (offset 0.7 0)) (layers B.Cu B.Paste B.Mask))
    (model ${ESPLIB}/ESP8266.3dshapes/ESP-12.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 57641109)
    (at 106.45 110.7 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at 0 0 180) (layer F.SilkS))
    (fp_text value 75k (at 0 0.2 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /Reader_+5-18v))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom_Inductors:ELL4_M-small (layer F.Cu) (tedit 5782E4A1)
    (at 106.3 117.7 270)
    (descr "Panasonic ELL4_M")
    (tags Inductor)
    (attr smd)
    (fp_text reference L1 (at 0 0 180) (layer F.SilkS))
    (fp_text value 3.6uH (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.5 0 270) (size 1.15 4.2) (drill (offset -0.575 0)) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.5 0 270) (size 1.15 4.2) (drill (offset 0.575 0)) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd trapezoid (at 1.65 0 270) (size 0.45 3.75) (rect_delta 0.45 0 ) (drill (offset 0.225 0)) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 1 smd trapezoid (at -1.65 0 270) (size 0.45 3.75) (rect_delta -0.45 0 ) (drill (offset -0.225 0)) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C2-Pad1)"))
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 57830700)
    (at 107.2 108.7 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at 0 0 180) (layer F.SilkS))
    (fp_text value np (at 0 0.2 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 57830714)
    (at 107.2 109.7)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at 0 0) (layer F.SilkS))
    (fp_text value 75k (at 0 -0.2) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 57830722)
    (at 108.1 110.7)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at 0 0) (layer F.SilkS))
    (fp_text value 24k (at 0 -0.2) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text octosavvi.com (at 105.3 108.6 90) (layer F.SilkS))
  (gr_text "ESPKey v1.3.2" (at 104.6 109.05 90) (layer F.SilkS))
  (gr_text G (at 113.8 110.5) (layer F.SilkS))
  (gr_text O (at 113.7 105.2) (layer F.SilkS))
  (gr_text W (at 113.8 107.2) (layer F.SilkS))
  (gr_text K (at 113.8 114) (layer F.SilkS))
  (gr_text R (at 113.8 118) (layer F.SilkS))
  (gr_line (start 114 104) (end 113.5 104.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104 104.5) (end 113.5 104.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114 100) (end 114 104) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120 120) (end 104 120) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104 104.5) (end 104 120) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120 100) (end 114 100) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120 100) (end 120 120) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104 104.5) (xy 113.5 104.5) (xy 114 104) (xy 114 100) (xy 120 100)
        (xy 120 120) (xy 104 120) (xy 104 112.25)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114 100) (xy 120 100) (xy 120 120) (xy 104 120) (xy 104 104.5)
        (xy 113.5 104.5) (xy 114 104)
      )
    )
  )
)
