(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu16.04.1)
  (general
    (links 12)
    (no_connects 4)
    (area 83.235714 83.1 191.164286 109.825)
    (thickness 1.6)
    (drawings 10)
    (tracks 80)
    (zones 0)
    (modules 10)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user hide)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.00001)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.8 3.8)
    (pad_drill 2.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00000_00000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../../../../Desktop/bp/))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(bp1-Pad2)")
  (net 3 "Net-(bp2-Pad2)")
  (net 4 "Net-(bp3-Pad2)")
  (net 5 "Net-(J2-Pad1)")
  (net 6 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(bp1-Pad2)")
    (add_net "Net-(bp2-Pad2)")
    (add_net "Net-(bp3-Pad2)")
  )
  (module BP_pcb_lib:BP2,4GHz_1 (layer F.Cu) (tedit 5A53AFC5)
    (at 112.008766 97.355155 14)
    (fp_text reference bp1 (at 0 6.25 14) (layer F.SilkS) hide)
    (fp_text value BP2,4GHz1 (at 0 -4.75 14) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -1.295 14) (size 16.4 2.17) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 0 1.295 14) (size 16.4 2.17) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(bp1-Pad2)"))
  )
  (module BP_pcb_lib:BP2,4GHz_2 (layer F.Cu) (tedit 5A53AFD3)
    (at 128.7522 97.380299 14)
    (fp_text reference bp2 (at 0 -6 14) (layer F.SilkS) hide)
    (fp_text value BP2,4GHz1 (at 0 5.75 14) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -2.615 14) (size 16.09 2.85) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(bp1-Pad2)"))
    (pad 2 smd rect (at 0 2.615 14) (size 16.09 2.85) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(bp2-Pad2)"))
  )
  (module BP_pcb_lib:BP2,4GHz_2 (layer F.Cu) (tedit 5A53AFDA)
    (at 145.62951 98.562422 14)
    (fp_text reference bp3 (at 0 -6 14) (layer F.SilkS) hide)
    (fp_text value BP2,4GHz1 (at 0 5.75 14) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -2.615 14) (size 16.09 2.85) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(bp2-Pad2)"))
    (pad 2 smd rect (at 0 2.615 14) (size 16.09 2.85) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(bp3-Pad2)"))
  )
  (module BP_pcb_lib:BP2,4GHz_1 (layer F.Cu) (tedit 5A53AFDF)
    (at 162.36 98.6 14)
    (fp_text reference bp4 (at 0 6.25 14) (layer F.SilkS) hide)
    (fp_text value BP2,4GHz1 (at 0 -4.75 14) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -1.295 14) (size 16.4 2.17) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(bp3-Pad2)"))
    (pad 2 smd rect (at 0 1.295 14) (size 16.4 2.17) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad1)"))
  )
  (module BP_pcb_lib:SMA (layer F.Cu) (tedit 5A53B1C9)
    (at 95.65 97.7)
    (fp_text reference J1 (at 2.25 7.5) (layer F.SilkS) hide)
    (fp_text value Conn_Coaxial (at 2 -8) (layer F.Fab) hide)
    (pad 1 smd rect (at 2 0) (size 4 2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 2 -3.775) (size 4 3) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 3 smd rect (at 2 3.775) (size 4 3) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
  )
  (module BP_pcb_lib:SMA (layer F.Cu) (tedit 5A53B1D0)
    (at 174.75 98.3)
    (fp_text reference J2 (at 2.25 7.5) (layer F.SilkS) hide)
    (fp_text value Conn_Coaxial (at 2 -8) (layer F.Fab) hide)
    (pad 1 smd rect (at 2 0) (size 4 2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at 2 -3.775) (size 4 3) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 3 smd rect (at 2 3.775) (size 4 3) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 5A54BBF9)
    (at 97.65 89.15)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965_Pad (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask)
      (net 6 GND))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 5A54A557)
    (at 176.75 89.15)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965_Pad (at 0 2.9) (layer F.Fab) hide)
    (fp_text user e%R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask)
      (net 6 GND))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 5A54BC31)
    (at 176.75 105.85)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965_Pad (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask)
      (net 6 GND))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 5A54A7E2)
    (at 97.65 105.8)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965_Pad (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask)
      (net 6 GND))
  )
  (dimension 83.4 (width 0.3) (layer Dwgs.User)
    (gr_text "83.400 mm" (at 137.2 84.45) (layer Dwgs.User))
    (feature1 (pts (xy 178.9 87) (xy 178.9 83.1)))
    (feature2 (pts (xy 95.5 87) (xy 95.5 83.1)))
    (crossbar (pts (xy 95.5 85.8) (xy 178.9 85.8)))
    (arrow1a (pts (xy 178.9 85.8) (xy 177.773496 86.386421)))
    (arrow1b (pts (xy 178.9 85.8) (xy 177.773496 85.213579)))
    (arrow2a (pts (xy 95.5 85.8) (xy 96.626504 86.386421)))
    (arrow2b (pts (xy 95.5 85.8) (xy 96.626504 85.213579)))
  )
  (dimension 21 (width 0.3) (layer Dwgs.User)
    (gr_text "21.000 mm" (at 91.65 97.5 90) (layer Dwgs.User))
    (feature1 (pts (xy 95.5 87) (xy 90.3 87)))
    (feature2 (pts (xy 95.5 108) (xy 90.3 108)))
    (crossbar (pts (xy 93 108) (xy 93 87)))
    (arrow1a (pts (xy 93 87) (xy 93.586421 88.126504)))
    (arrow1b (pts (xy 93 87) (xy 92.413579 88.126504)))
    (arrow2a (pts (xy 93 108) (xy 93.586421 106.873496)))
    (arrow2b (pts (xy 93 108) (xy 92.413579 106.873496)))
  )
  (gr_text "8% BW" (at 169.5 105.5) (layer B.SilkS))
  (gr_text "DB4UM DB9MAT" (at 135 103.5) (layer B.SilkS))
  (gr_text 2018 (at 104 105.5) (layer B.SilkS))
  (gr_text "2.400 GHz BP" (at 135 94) (layer B.SilkS))
  (gr_line (start 95.5 87) (end 178.9 87) (layer Edge.Cuts) (width 0.00001))
  (gr_line (start 178.9 108) (end 95.5 108) (layer Edge.Cuts) (width 0.00001))
  (gr_line (start 178.9 87) (end 178.9 108) (layer Edge.Cuts) (width 0.00001))
  (gr_line (start 95.5 108) (end 95.5 87) (layer Edge.Cuts) (width 0.00001))
  (zone (net 5) (net_name "Net-(J2-Pad1)") (layer F.Cu) (hatch full 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.026)
    (fill yes (arc_segments 32) (thermal_gap 0) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 178.9 97.7) (xy 178.9 97.3) (xy 173.85 96.8) (xy 170.4 96.8) (xy 170.3 96.85)
        (xy 166.175 99.775) (xy 173.85 99.775) (xy 178.9 99.3) (xy 178.9 98.5)
      )
    )
  )
  (zone (net 1) (net_name "Net-(J1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.05)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 95.5 96.7) (xy 100.5 96.2) (xy 107.325 96.2) (xy 107.35 97.6) (xy 103.975 99.15)
        (xy 100.5 99.15) (xy 95.5 98.7) (xy 95.5 98)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.05)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 174.75 96) (xy 174.75 87) (xy 178.9 87) (xy 178.9 96)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.05)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 95.5 95.4) (xy 95.5 87) (xy 99.65 87) (xy 99.65 95.4)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.05)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 174.75 100.6) (xy 174.75 108) (xy 178.9 108) (xy 178.9 100.6)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.05)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 99.65 99.95) (xy 99.65 107.95) (xy 95.5 108) (xy 95.5 100)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.05)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 95.5 86.95) (xy 95.5 108) (xy 178.9 108) (xy 178.9 87)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.05)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 102.5 87) (xy 102.5 108) (xy 172 108) (xy 172 87)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.05)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 95.05 87) (xy 101.5 87) (xy 101.5 108) (xy 95.05 108)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.05)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 173 108) (xy 173 87) (xy 179 87) (xy 179 108)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.05)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 170.5 87) (xy 175 87) (xy 175 96) (xy 171.5 96)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.05)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 171.5 100.5) (xy 174 100.5) (xy 174 108) (xy 171.5 108)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.05)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 101.5 100) (xy 102.5 100) (xy 102.5 108) (xy 101.5 108)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.05)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 101.5 95.5) (xy 102.5 95.5) (xy 102.5 87) (xy 101.5 87)
      )
    )
  )
  (zone (net 4) (net_name "Net-(bp3-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.35 98.65) (xy 145.25 100.6) (xy 145.85 101.85) (xy 153.6 100.45) (xy 154.25 100.4)
        (xy 155 100.2) (xy 154.25 98.2)
      )
    )
  )
)
