(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen") (color "White"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Purple") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Purple") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen") (color "White"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+1V8")
  (net 2 "GND")
  (net 3 "/P11")
  (net 4 "/P12")
  (net 5 "/P01")
  (net 6 "/P02")
  (net 7 "/P03")
  (net 8 "/P04")
  (net 9 "/P06")
  (net 10 "/P08")
  (net 11 "/P09")
  (net 12 "/P10")
  (net 13 "/P13")
  (net 14 "/P14")
  (net 15 "/P15")
  (net 16 "/P16")
  (net 17 "/P18")
  (net 18 "/P20")
  (net 19 "/P21")
  (net 20 "/P22")
  (net 21 "/P23")
  (net 22 "/P24")
  (net 23 "/P25")
  (net 24 "/P26")
  (net 25 "/P27")
  (net 26 "/P28")
  (net 27 "/P29")
  (net 28 "/P30")
  (net 29 "GNDA")
  (net 30 "/P32")
  (net 31 "/P33")
  (net 32 "/P34")
  (net 33 "/P35")
  (net 34 "/P36")
  (net 35 "/P37")
  (net 36 "/P38")
  (net 37 "/P39")
  (net 38 "/P41")
  (net 39 "/P42")
  (net 40 "/P44")
  (net 41 "/P45")
  (net 42 "/P46")
  (net 43 "/P47")
  (net 44 "/P48")
  (net 45 "unconnected-(U201-Pad4)")
  (net 46 "+3V3")
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 115.824 106.68)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Digikey" "TCR2EF18LM(CTCT-ND")
    (property "Mouser" "MIC5317-1.8YD5-TR")
    (property "Purpose" "Regulator 3.3V->1.8V")
    (property "Sheetfile" "../../rollercoasterometer/kicad/regulator_1v8.kicad_sch")
    (property "Sheetname" "1V8 Regulator")
    (attr smd)
    (fp_text reference "U201" (at 0 -2.4) (layer "F.SilkS") hide)
    (fp_text value "TCR2EF 1.8V" (at 0 2.4) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "+3V3") (pinfunction "IN") (pintype "power_in"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "+3V3") (pinfunction "EN") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "unconnected-(U201-Pad4)") (pinfunction "P4") (pintype "no_connect"))
    (pad "5" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+1V8") (pinfunction "OUT") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (tedit 5C745284)
    (at 144.78 106.68 90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "net tie solder jumper bridged")
    (property "Sheetfile" "LPC210x breakout.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "JP131" (at 0 -1.8 90) (layer "F.SilkS") hide)
    (fp_text value "AnalogGround" (at 0 1.9 90) (layer "F.Fab") hide)
    (pad "1" smd custom (at -0.65 0 90) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0 90) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 29 "GNDA") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (tedit 5C745284)
    (at 108.712 106.68 -90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "net tie solder jumper bridged")
    (property "Sheetfile" "LPC210x breakout.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "JP142" (at 0 -1.8 90) (layer "F.SilkS") hide)
    (fp_text value "VDDA" (at 0 1.9 90) (layer "F.Fab") hide)
    (pad "1" smd custom (at -0.65 0 270) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 46 "+3V3") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0 270) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 39 "/P42") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 118.618 106.68 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Dielectric" "X5R")
    (property "Digikey" "399-C0402C105K9PAC7800CT-ND")
    (property "Max Voltage" "6.3V")
    (property "Mouser" "187-CL05A105KP5NNWC")
    (property "Precision" "10%")
    (property "Purpose" "1.8V Regulator output")
    (property "Sheetfile" "../../rollercoasterometer/kicad/regulator_1v8.kicad_sch")
    (property "Sheetname" "1V8 Regulator")
    (attr smd)
    (fp_text reference "C205" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at 0 1.16 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+1V8") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 152.4 106.68 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Mouser" "667-ERJ-2RKF1002X")
    (property "Sheetfile" "LPC210x breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R106" (at 0 -1.17 -90) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.17 -90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/P06") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "+3V3") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 122.77 106.68 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Digikey" "399-17554-1-ND")
    (property "Mouser" "187-CL05C220JB5NNNC")
    (property "Sheetfile" "LPC210x breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C112" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "22pF" (at 0 1.16 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/P12") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_SMD_Abracon_ABM8G-4Pin_3.2x2.5mm" (layer "F.Cu")
    (tedit 5A0FD1B2)
    (at 125.31 106.68 -90)
    (descr "Abracon Miniature Ceramic Smd Crystal ABM8G http://www.abracon.com/Resonators/ABM8G.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (property "Digikey" "535-14128-1-ND")
    (property "Freq Stability" "Y - +/-30ppm")
    (property "Freq Tolerance" "2 - +/-20ppm")
    (property "Load Capacitance" "18pF")
    (property "Mouser" "815-ABM8G-12-18D2Y")
    (property "Part Number" "ABM8G-12.000MHZ-17-D2Y")
    (property "Sheetfile" "LPC210x breakout.kicad_sch")
    (property "Sheetname" "")
    (property "Temperature Range" "D - -40C ~ +85C")
    (attr smd)
    (fp_text reference "Y101" (at 0 -2.45 -270) (layer "F.SilkS") hide)
    (fp_text value "12MHz" (at 0 2.45 -270) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd rect (at -1.1 0.85 270) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/P12") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 1.1 0.85 270) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 1.1 -0.85 270) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/P11") (pinfunction "3") (pintype "passive"))
    (pad "4" smd rect (at -1.1 -0.85 270) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_Abracon_ABM8G-4Pin_3.2x2.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KwanSystems:SW_SPST_B3U-1000P-B" (layer "F.Cu")
    (tedit 6358498D)
    (at 149.352 106.68)
    (descr "Ultra-small-sized Tactile Switch with High Contact Reliability, Top-actuated Model, without Ground Terminal, with Boss")
    (tags "Tactile Switch")
    (property "Mouser" "653-B3U-1000P")
    (property "Sheetfile" "LPC210x breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "S106" (at 0 -2.5) (layer "F.Fab"))
    (fp_text value "B3U-1000" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.75 0.75) (drill 0.75) (layers *.Mask))
    (pad "1" smd rect (at -1.7 0) (size 0.9 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at 1.7 0) (size 0.9 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/P06") (pinfunction "B") (pintype "passive"))
    (model ":KWAN_KICAD_LIB:wrl/B3U1000P.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 129.54 106.68 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Digikey" "399-C0402C104K4RAC7411CT-ND")
    (property "Mouser" "187-CL05A105KP5NNWC")
    (property "Sheetfile" "LPC210x breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C105" (at 0 -1.16) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at 0 1.16) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+1V8") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (tedit 5C745284)
    (at 111.252 106.68 -90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "net tie solder jumper bridged")
    (property "Sheetfile" "LPC210x breakout.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "JP104" (at 0 -1.8 90) (layer "F.SilkS") hide)
    (fp_text value "VBAT" (at 0 1.9 90) (layer "F.Fab") hide)
    (pad "1" smd custom (at -0.65 0 270) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 46 "+3V3") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0 270) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 8 "/P04") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "KwanSystems:StKwansSoldermask" (layer "F.Cu")
    (tedit 62597235)
    (at 161.29 106.68)
    (property "Sheetfile" "LPC210x breakout.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (attr through_hole exclude_from_bom)
    (fp_text reference "G101" (at -3.683 -2.7432) (layer "F.Mask") hide)
    (fp_text value "KwanSystems" (at 4.2926 3.7084) (layer "F.Mask") hide)
    (fp_text user "github.com/kwan3217/kicad" (at -2.54 4.318 unlocked) (layer "B.SilkS"))
    (fp_text user "stkwans.blogspot.com" (at -3.81 2.794 unlocked) (layer "B.SilkS"))
    (fp_text user "St Kwan's Home for" (at -17.526 -3.81 unlocked) (layer "F.SilkS"))
    (fp_text user "a division of Kwan Systems" (at -20.066 2.794 unlocked) (layer "F.SilkS"))
    (fp_text user "the Terminally ADD" (at -17.018 -2.286 unlocked) (layer "F.SilkS"))
  )
  (footprint "Package_QFP:LQFP-48_7x7mm_P0.5mm" (layer "F.Cu")
    (tedit 5D9F72AF)
    (at 135.89 106.68 45)
    (descr "LQFP, 48 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ltc2358-16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "LQFP QFP")
    (property "Digikey" "568-LPC2103FBD48EL-ND")
    (property "Mouser" "771-LPC2102FBD48-S")
    (property "Sheetfile" "LPC210x breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U101" (at 0 -5.85 45) (layer "F.SilkS") hide)
    (fp_text value "LPC2103" (at 0 5.85 45) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -4.1625 -2.75 45) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/P01") (pinfunction "(MAT1.2/MISO1)P0.19") (pintype "bidirectional"))
    (pad "2" smd roundrect (at -4.1625 -2.25 45) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/P02") (pinfunction "(MAT1.3/MOSI1)P0.20") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -4.1625 -1.75 45) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/P03") (pinfunction "(SSEL1/MAT3.0)P0.21") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -4.1625 -1.25 45) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/P04") (pinfunction "VBAT") (pintype "power_in"))
    (pad "5" smd roundrect (at -4.1625 -0.75 45) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+1V8") (pinfunction "VDD(1V8)") (pintype "power_in"))
    (pad "6" smd roundrect (at -4.1625 -0.25 45) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/P06") (pinfunction "~{RST}") (pintype "bidirectional"))
    (pad "7" smd roundrect (at -4.1625 0.25 45) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "8" smd roundrect (at -4.1625 0.75 45) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/P08") (pinfunction "(~{TRST}/CAP2.0)P0.27") (pintype "bidirectional"))
    (pad "9" smd roundrect (at -4.1625 1.25 45) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/P09") (pinfunction "(TMS/CAP2.1)P0.28") (pintype "bidirectional"))
    (pad "10" smd roundrect (at -4.1625 1.75 45) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/P10") (pinfunction "(TCK/CAP2.2)P0.29") (pintype "bidirectional"))
    (pad "11" smd roundrect (at -4.1625 2.25 45) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/P11") (pinfunction "XTAL1") (pintype "input"))
    (pad "12" smd roundrect (at -4.1625 2.75 45) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/P12") (pinfunction "XTAL2") (pintype "output"))
    (pad "13" smd roundrect (at -2.75 4.1625 45) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/P13") (pinfunction "(TXD0/MAT3.1)P0.0") (pintype "bidirectional"))
    (pad "14" smd roundrect (at -2.25 4.1625 45) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/P14") (pinfunction "(RXD0/MAT3.2)P0.1") (pintype "bidirectional"))
    (pad "15" smd roundrect (at -1.75 4.1625 45) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/P15") (pinfunction "(TDI/MAT3.3)P0.30") (pintype "bidirectional"))
    (pad "16" smd roundrect (at -1.25 4.1625 45) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/P16") (pinfunction "(TDO)P0.31") (pintype "bidirectional"))
    (pad "17" smd roundrect (at -0.75 4.1625 45) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "+3V3") (pinfunction "VDD(3V3)") (pintype "power_in"))
    (pad "18" smd roundrect (at -0.25 4.1625 45) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/P18") (pinfunction "(SCL0/CAP0.0)P0.2") (pintype "bidirectional"))
    (pad "19" smd roundrect (at 0.25 4.1625 45) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "20" smd roundrect (at 0.75 4.1625 45) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/P20") (pinfunction "RTCX1") (pintype "input"))
    (pad "21" smd roundrect (at 1.25 4.1625 45) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/P21") (pinfunction "(SDA0/MAT0.0)P0.3") (pintype "bidirectional"))
    (pad "22" smd roundrect (at 1.75 4.1625 45) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/P22") (pinfunction "(SCK0/CAP0.1)P0.4") (pintype "bidirectional"))
    (pad "23" smd roundrect (at 2.25 4.1625 45) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/P23") (pinfunction "(MISO0/MAT0.1)P0.5") (pintype "bidirectional"))
    (pad "24" smd roundrect (at 2.75 4.1625 45) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/P24") (pinfunction "(MOSI0/CAP0.2)P0.6") (pintype "bidirectional"))
    (pad "25" smd roundrect (at 4.1625 2.75 45) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/P25") (pinfunction "RTCX2") (pintype "output"))
    (pad "26" smd roundrect (at 4.1625 2.25 45) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/P26") (pinfunction "RTCK") (pintype "bidirectional"))
    (pad "27" smd roundrect (at 4.1625 1.75 45) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "/P27") (pinfunction "DBGSEL") (pintype "input"))
    (pad "28" smd roundrect (at 4.1625 1.25 45) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/P28") (pinfunction "(SSEL0/MAT2.0)P0.7") (pintype "bidirectional"))
    (pad "29" smd roundrect (at 4.1625 0.75 45) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/P29") (pinfunction "(TXD1/MAT2.1)P0.8") (pintype "bidirectional"))
    (pad "30" smd roundrect (at 4.1625 0.25 45) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/P30") (pinfunction "(RXD1/MAT2.2)P0.9") (pintype "bidirectional"))
    (pad "31" smd roundrect (at 4.1625 -0.25 45) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDA") (pinfunction "VSSA") (pintype "power_in"))
    (pad "32" smd roundrect (at 4.1625 -0.75 45) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/P32") (pinfunction "(AD0.0)P0.22") (pintype "bidirectional"))
    (pad "33" smd roundrect (at 4.1625 -1.25 45) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/P33") (pinfunction "(AD0.1)P0.23") (pintype "bidirectional"))
    (pad "34" smd roundrect (at 4.1625 -1.75 45) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/P34") (pinfunction "(AD0.2)P0.24") (pintype "bidirectional"))
    (pad "35" smd roundrect (at 4.1625 -2.25 45) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/P35") (pinfunction "(RTS1/CAP1.0/AD0.3)P0.10") (pintype "bidirectional"))
    (pad "36" smd roundrect (at 4.1625 -2.75 45) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/P36") (pinfunction "(CTS1/CAP1.1/AD0.4)P0.11") (pintype "bidirectional"))
    (pad "37" smd roundrect (at 2.75 -4.1625 45) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/P37") (pinfunction "(DSR1/MAT1.0/AD0.5)P0.12") (pintype "bidirectional"))
    (pad "38" smd roundrect (at 2.25 -4.1625 45) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/P38") (pinfunction "(AD0.6)P0.25") (pintype "bidirectional"))
    (pad "39" smd roundrect (at 1.75 -4.1625 45) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "/P39") (pinfunction "(AD0.7)P0.26") (pintype "bidirectional"))
    (pad "40" smd roundrect (at 1.25 -4.1625 45) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "+3V3") (pinfunction "VDD(3V3)") (pintype "power_in"))
    (pad "41" smd roundrect (at 0.75 -4.1625 45) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/P41") (pinfunction "(DTR1/MAT1.1)P0.13") (pintype "bidirectional"))
    (pad "42" smd roundrect (at 0.25 -4.1625 45) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/P42") (pinfunction "VDDA") (pintype "power_in"))
    (pad "43" smd roundrect (at -0.25 -4.1625 45) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "44" smd roundrect (at -0.75 -4.1625 45) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/P44") (pinfunction "(DCD1/SCK1/EINT1)P0.14") (pintype "bidirectional"))
    (pad "45" smd roundrect (at -1.25 -4.1625 45) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/P45") (pinfunction "(RI1/EINT2)P0.15") (pintype "bidirectional"))
    (pad "46" smd roundrect (at -1.75 -4.1625 45) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "/P46") (pinfunction "(EINT0/MAT0.2)P0.16") (pintype "bidirectional"))
    (pad "47" smd roundrect (at -2.25 -4.1625 45) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "/P47") (pinfunction "(CAP1.2/SCL1)P0.17") (pintype "bidirectional"))
    (pad "48" smd roundrect (at -2.75 -4.1625 45) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "/P48") (pinfunction "(CAP1.3/SDA1)P0.18") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/LQFP-48_7x7mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.03 106.68 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Digikey" "399-C0402C105K9PAC7800CT-ND")
    (property "Mouser" "187-CL05A105KP5NNWC")
    (property "Purpose" "1.8V Regulator Input")
    (property "Sheetfile" "../../rollercoasterometer/kicad/regulator_1v8.kicad_sch")
    (property "Sheetname" "1V8 Regulator")
    (attr smd)
    (fp_text reference "C201" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at 0 1.16 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 120.65 106.68 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Digikey" "754-1123-1-ND")
    (property "Mouser" "604-APT1608SURC")
    (property "Purpose" "Power indicator")
    (property "Sheetfile" "../../rollercoasterometer/kicad/regulator_1v8.kicad_sch")
    (property "Sheetname" "1V8 Regulator")
    (attr smd)
    (fp_text reference "D201" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "RED" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+1V8") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 142.494 106.68)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Digikey" "399-C0402C104K4RAC7411CT-ND")
    (property "Mouser" "187-CL05A105KP5NNWC")
    (property "Sheetfile" "LPC210x breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C117" (at 0 -1.16) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at 0 1.16) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KwanSystems:Symbol_KiCAD-Logo_CopperAndSilkScreenTop_small" (layer "F.Cu")
    (tedit 6255721F)
    (at 109.728 110.49)
    (descr "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (tags "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (property "Sheetfile" "LPC210x breakout.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (attr through_hole exclude_from_bom)
    (fp_text reference "G102" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "DesignedWithKicad" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 127.85 106.68 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Digikey" "399-17554-1-ND")
    (property "Mouser" "187-CL05C220JB5NNNC")
    (property "Sheetfile" "LPC210x breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C111" (at 0 -1.16 -270) (layer "F.SilkS") hide)
    (fp_text value "22pF" (at 0 1.16 -270) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/P11") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KwanSystems:OSHW-Symbol_6.7x6mm_SolderMask" (layer "B.Cu")
    (tedit 6257683B)
    (at 161.29 106.426 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (property "Sheetfile" "LPC210x breakout.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G103" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "OSHW" (at 0.75 0) (layer "B.Fab") hide)
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x24_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 635FEC1E)
    (at 106.68 114.3 -90)
    (descr "Through hole straight pin header, 1x24, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x24 2.54mm single row")
    (property "Sheetfile" "LPC210x breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J101" (at 0 2.33 90) (layer "B.SilkS") hide)
    (fp_text value "Conn_01x24_Male" (at 0 -60.75 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -29.21 180) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "/P01") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/P02") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "/P03") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "/P04") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+1V8") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/P06") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "/P08") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/P09") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "/P10") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/P11") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/P12") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "/P13") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "/P14") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "/P15") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 0 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/P16") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "+3V3") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 0 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/P18") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 0 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "/P20") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole oval (at 0 -50.8 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/P21") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval (at 0 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/P22") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole oval (at 0 -55.88 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "/P23") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole oval (at 0 -58.42 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/P24") (pinfunction "Pin_24") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x24_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x24_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 635FEC4F)
    (at 165.1 99.06 90)
    (descr "Through hole straight pin header, 1x24, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x24 2.54mm single row")
    (property "Sheetfile" "LPC210x breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J102" (at 0 2.33 270) (layer "B.SilkS") hide)
    (fp_text value "Conn_01x24_Male" (at 0 -60.75 270) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -29.21) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "/P25") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "/P26") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "/P27") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "/P28") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "/P29") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "/P30") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "GNDA") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "/P32") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "/P33") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 -22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "/P34") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 -25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "/P35") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 -27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "/P36") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 -30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "/P37") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 -33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "/P38") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 -35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "/P39") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 0 -38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "+3V3") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 -40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "/P41") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 0 -43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "/P42") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 -45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 0 -48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "/P44") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole oval (at 0 -50.8 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "/P45") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval (at 0 -53.34 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "/P46") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole oval (at 0 -55.88 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "/P47") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole oval (at 0 -58.42 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "/P48") (pinfunction "Pin_24") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x24_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 165.1 97.79) (mid 165.998026 98.161974) (end 166.37 99.06) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 105.41 99.06) (mid 105.781974 98.161974) (end 106.68 97.79) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 166.37 99.06) (end 166.37 114.3) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 166.37 114.3) (mid 165.998026 115.198026) (end 165.1 115.57) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 106.68 115.57) (mid 105.781974 115.198026) (end 105.41 114.3) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 165.1 115.57) (end 106.68 115.57) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 105.41 114.3) (end 105.41 99.06) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 106.68 97.79) (end 165.1 97.79) (layer "Edge.Cuts") (width 0.1))
  (gr_text "23" (at 162.56 112.268 90) (layer "F.SilkS"))
  (gr_text "10" (at 129.54 112.268 90) (layer "F.SilkS"))
  (gr_text "47" (at 109.22 101.092 90) (layer "F.SilkS"))
  (gr_text "28" (at 157.48 101.092 90) (layer "F.SilkS"))
  (gr_text "27" (at 160.02 101.092 90) (layer "F.SilkS"))
  (gr_text "26" (at 162.56 101.092 90) (layer "F.SilkS"))
  (gr_text "18" (at 149.86 112.268 90) (layer "F.SilkS"))
  (gr_text "16" (at 144.78 112.268 90) (layer "F.SilkS"))
  (gr_text "22" (at 160.02 112.268 90) (layer "F.SilkS"))
  (gr_text "3" (at 111.76 112.268 90) (layer "F.SilkS"))
  (gr_text "LPC210x Breakout\n2022-10-31" (at 106.426 103.378) (layer "F.SilkS"))
  (gr_text "15" (at 142.24 112.268 90) (layer "F.SilkS"))
  (gr_text "32" (at 147.32 101.092 90) (layer "F.SilkS"))
  (gr_text "43" (at 119.38 101.092 90) (layer "F.SilkS"))
  (gr_text "20" (at 154.94 112.268 90) (layer "F.SilkS"))
  (gr_text "34" (at 142.24 101.092 90) (layer "F.SilkS"))
  (gr_text "38" (at 132.08 101.092 90) (layer "F.SilkS"))
  (gr_text "1" (at 106.68 112.268 90) (layer "F.SilkS"))
  (gr_text "29" (at 154.94 101.092 90) (layer "F.SilkS"))
  (gr_text "35" (at 139.7 101.092 90) (layer "F.SilkS"))
  (gr_text "6" (at 119.38 112.268 90) (layer "F.SilkS"))
  (gr_text "9" (at 127 112.268 90) (layer "F.SilkS"))
  (gr_text "19" (at 152.4 112.268 90) (layer "F.SilkS"))
  (gr_text "21" (at 157.48 112.268 90) (layer "F.SilkS"))
  (gr_text "42" (at 121.92 101.092 90) (layer "F.SilkS"))
  (gr_text "39" (at 129.54 101.092 90) (layer "F.SilkS"))
  (gr_text "44" (at 116.84 101.092 90) (layer "F.SilkS"))
  (gr_text "7" (at 121.92 112.268 90) (layer "F.SilkS"))
  (gr_text "46" (at 111.76 101.092 90) (layer "F.SilkS"))
  (gr_text "48" (at 106.68 101.092 90) (layer "F.SilkS"))
  (gr_text "4" (at 114.3 112.268 90) (layer "F.SilkS"))
  (gr_text "30" (at 152.4 101.092 90) (layer "F.SilkS"))
  (gr_text "25" (at 165.1 101.092 90) (layer "F.SilkS"))
  (gr_text "11" (at 132.08 112.268 90) (layer "F.SilkS"))
  (gr_text "33" (at 144.78 101.092 90) (layer "F.SilkS"))
  (gr_text "2" (at 109.22 112.268 90) (layer "F.SilkS"))
  (gr_text "5" (at 116.84 112.268 90) (layer "F.SilkS"))
  (gr_text "24" (at 165.1 112.268 90) (layer "F.SilkS"))
  (gr_text "14" (at 139.7 112.268 90) (layer "F.SilkS"))
  (gr_text "31" (at 149.86 101.092 90) (layer "F.SilkS"))
  (gr_text "8" (at 124.46 112.268 90) (layer "F.SilkS"))
  (gr_text "41" (at 124.46 101.092 90) (layer "F.SilkS"))
  (gr_text "45" (at 114.3 101.092 90) (layer "F.SilkS"))
  (gr_text "40" (at 127 101.092 90) (layer "F.SilkS"))
  (gr_text "17" (at 147.32 112.268 90) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.37 97.79)
        (xy 166.37 115.57)
        (xy 105.41 115.57)
        (xy 105.41 97.79)
      )
    )
  )
)
