(kicad_pcb (version 20171130) (host pcbnew "(5.1.9-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 24)
    (tracks 41)
    (zones 0)
    (modules 136)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu mixed)
    (31 B.Cu mixed)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.35)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.127)
    (zone_45_only yes)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.15)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.5 3.5)
    (pad_drill 3.5)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J103-Pad2)")
  (net 2 "Net-(J103-Pad1)")
  (net 3 "Net-(L101-Pad1)")
  (net 4 "Net-(C101-Pad1)")
  (net 5 "Net-(C101-Pad2)")
  (net 6 "Net-(L102-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C101-Pad1)")
    (add_net "Net-(C101-Pad2)")
    (add_net "Net-(L102-Pad2)")
  )
  (net_class rf ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 1)
    (via_drill 0.7)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J103-Pad1)")
    (add_net "Net-(J103-Pad2)")
    (add_net "Net-(L101-Pad1)")
  )
  (module Oddities:RG-174_Attachment (layer F.Cu) (tedit 60F1D955)
    (at 122.05 138.05)
    (tags "rod antenna")
    (clearance 0.1)
    (fp_text reference J103 (at -0.07 -9.53) (layer B.SilkS))
    (fp_text value CONN_01X03 (at 0.2286 -6.858) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 15.16002 -12.83796) (size 4 4) (drill 2.5) (layers *.Cu *.Mask)
      (net 1 "Net-(J103-Pad2)"))
    (pad 3 thru_hole circle (at 0.09488 0.08128) (size 5 5) (drill 3) (layers *.Cu *.Mask)
      (net 5 "Net-(C101-Pad2)"))
    (pad 1 smd rect (at 0 -22) (size 5 10) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(J103-Pad1)"))
    (pad 2 thru_hole circle (at 15 -7) (size 4 4) (drill 2.5) (layers *.Cu *.Mask)
      (net 1 "Net-(J103-Pad2)"))
    (pad 2 thru_hole circle (at 15 -19) (size 4 4) (drill 2.5) (layers *.Cu *.Mask)
      (net 1 "Net-(J103-Pad2)"))
    (pad 2 smd rect (at 15 -13) (size 10 20) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(J103-Pad2)"))
    (pad 3 smd rect (at 0 0) (size 15 5) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C101-Pad2)"))
    (pad 3 smd rect (at 0 0) (size 15 5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C101-Pad2)"))
    (pad 1 thru_hole circle (at 0 -25) (size 3 3) (drill 1.5) (layers *.Cu B.Mask)
      (net 2 "Net-(J103-Pad1)"))
    (pad "" np_thru_hole circle (at 3 13) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -3 13) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 3 6) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -3 6) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at 5.4 0) (size 4 4) (drill 2.5) (layers *.Cu *.Mask)
      (net 5 "Net-(C101-Pad2)"))
    (pad 2 smd rect (at 15 -13) (size 10 20) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J103-Pad2)"))
    (pad "" np_thru_hole circle (at 8.3439 -10.3886) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 8.3185 -14.859) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.2 -4) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -2.2 -4) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -2 -15) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
    (pad 1 smd rect (at 0 -22) (size 5 10) (layers F.Cu F.Paste)
      (net 2 "Net-(J103-Pad1)"))
    (pad "" np_thru_hole circle (at 2 -15) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at -5.4 0) (size 4 4) (drill 2.5) (layers *.Cu *.Mask)
      (net 5 "Net-(C101-Pad2)"))
  )
  (module Oddities:Wire_Strain_Relief_and_Attach (layer F.Cu) (tedit 60F1D8CC)
    (at 122.24 109.97)
    (tags "rod antenna")
    (clearance 0.1)
    (fp_text reference J101 (at -2.22 -38.67 90) (layer F.SilkS))
    (fp_text value "Thru Holes" (at -0.08382 -20.79244) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -27.5) (size 5 10) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C101-Pad1)"))
    (pad "" thru_hole circle (at 0 -38.39) (size 4 4) (drill 2.45) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.48666 -34.25952) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -2.43078 -34.25952) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
    (pad 1 smd rect (at 0 -27.5) (size 5 10) (layers F.Cu F.Paste)
      (net 4 "Net-(C101-Pad1)"))
    (pad 1 thru_hole circle (at 0 -28) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask)
      (net 4 "Net-(C101-Pad1)"))
  )
  (module Inductors:Manually_Wound_Coil (layer F.Cu) (tedit 60F1D682)
    (at 107.3 128.63 90)
    (descr "Inductor ")
    (tags INDUCTOR)
    (fp_text reference L102 (at 0.18 -0.04) (layer F.SilkS))
    (fp_text value 0.4-1.0uH (at 0.09906 -1.99898 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at -3.65 0 90) (size 3 3) (drill 2) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C101-Pad2)"))
    (pad 2 thru_hole circle (at 3.65 0 90) (size 3 3) (drill 2) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(L102-Pad2)"))
    (pad 1 thru_hole rect (at -8 0 90) (size 3 3) (drill 2) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C101-Pad2)"))
    (pad 2 thru_hole circle (at 8 0 90) (size 3 3) (drill 2) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(L102-Pad2)"))
    (model Inductors.3dshapes/INDUCTOR_V.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2 2 2))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D7.5_P5 (layer F.Cu) (tedit 5E1A7234)
    (at 117.77 131.05)
    (descr "Capacitor 7.5mm Disc, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C101 (at 3.84 -0.12 180) (layer F.SilkS))
    (fp_text value 470pF (at 2.5 3.5 180) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 8.7 0) (size 2 2) (drill 0.92) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C101-Pad2)") (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.92) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C101-Pad1)") (zone_connect 2))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D7.5_P5.wrl
      (offset (xyz 2.500000042453766 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Oddities:Core_150A_2_windings_Horiz_TH (layer F.Cu) (tedit 5E1D2221)
    (at 122.14 101.01)
    (descr "Through hole toroid")
    (tags toroid)
    (zone_connect 2)
    (fp_text reference T101 (at -0.11 -7.86) (layer F.SilkS))
    (fp_text value TRANSFO (at 0.3175 7.3914) (layer F.Fab) hide)
    (fp_text user S1 (at -6.7056 3.2766) (layer F.SilkS))
    (fp_text user S1' (at -19.5017 -4.0386) (layer F.SilkS))
    (fp_text user P (at 4.72186 5.24764) (layer F.SilkS))
    (fp_text user P' (at 17.3863 -11.7475) (layer F.SilkS))
    (pad 4 smd rect (at -8.05942 -0.47752) (size 1.524 5) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C101-Pad1)") (zone_connect 2))
    (pad 2 smd rect (at 6.39826 8.26516) (size 1.524 5) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(J103-Pad2)") (zone_connect 2))
    (pad 1 smd rect (at 17.64538 -7.35076) (size 1.524 5) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(L101-Pad1)") (zone_connect 2))
    (pad 1 thru_hole rect (at 17.5641 -9.7028) (size 3.5 3.5) (drill 2.1) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(L101-Pad1)") (zone_connect 2))
    (pad 2 thru_hole rect (at 6.34238 5.80644) (size 3.5 3.5) (drill 2.1) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(J103-Pad2)") (zone_connect 2))
    (pad 3 thru_hole circle (at -19.7303 -2.2098) (size 3.5 3.5) (drill 2.1) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(L102-Pad2)") (zone_connect 2))
    (pad 4 thru_hole circle (at -8.0391 1.9431) (size 3.5 3.5) (drill 2.1) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C101-Pad1)") (zone_connect 2))
    (pad 3 smd rect (at -19.6795 -4.61264) (size 1.524 5) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(L102-Pad2)") (zone_connect 2))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (offset (xyz 1.269999980926514 -2.539999961853027 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 5CCF1ADE)
    (at 112.2 134.4)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.SilkS) hide)
    (fp_text value MountingHole_3-5mm (at 0 5.00126) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 5CCF1ADE)
    (at 102.6 134.4)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.SilkS) hide)
    (fp_text value MountingHole_3-5mm (at 0 5.00126) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 5CCF1ADE)
    (at 112.2 148)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.SilkS) hide)
    (fp_text value MountingHole_3-5mm (at 0 5.00126) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_1mm_Outlined (layer F.Cu) (tedit 5E1C85DF)
    (at 105 62)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value MountingHole_1mm_Outlined (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 2.45) (layers *.Cu *.Mask))
  )
  (module Inductors:Toroid_T-60_2TH (layer B.Cu) (tedit 5DACC4D9)
    (at 135.45 79.21 120)
    (descr "T-60 Toroid")
    (tags "toroid inductor")
    (fp_text reference L101 (at 0.480833 5.840702 120) (layer B.SilkS))
    (fp_text value 3.2uH (at 0.444499 5.2324 120) (layer B.Fab))
    (pad 2 thru_hole circle (at -7.9121 1.1049 120) (size 2 2) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 "Net-(J103-Pad1)"))
    (pad 1 thru_hole circle (at -3.8862 -0.8382 120) (size 2 2) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 3 "Net-(L101-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (offset (xyz 1.269999980926514 -2.539999961853027 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 5CCF1ADE)
    (at 130.2 70.58)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.SilkS) hide)
    (fp_text value MountingHole_3-5mm (at 0 5.00126) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 5CCF1ADE)
    (at 134.17 77.39)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.SilkS) hide)
    (fp_text value MountingHole_3-5mm (at 0 5.00126) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 5CCF1ADE)
    (at 126.84 61.96)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.SilkS) hide)
    (fp_text value MountingHole_3-5mm (at 0 5.00126) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_1mm_Outlined (layer F.Cu) (tedit 5E1C860A)
    (at 117 62)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value MountingHole_1mm_Outlined (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 2.45) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_1mm_Outlined (layer F.Cu) (tedit 5E1C85FB)
    (at 111 62)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value MountingHole_1mm_Outlined (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 2.45) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 5CCF1ADE)
    (at 112.2 141.1)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.SilkS) hide)
    (fp_text value MountingHole_3-5mm (at 0 5.00126) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 5CCF1ADE)
    (at 102.6 141.1)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.SilkS) hide)
    (fp_text value MountingHole_3-5mm (at 0 5.00126) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 5CCF1ADE)
    (at 102.6 148)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.SilkS) hide)
    (fp_text value MountingHole_3-5mm (at 0 5.00126) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Capacitors_ThroughHole:C_Disc_D7.5_P5 (layer F.Cu) (tedit 5E1A7234)
    (at 117.77 125.36)
    (descr "Capacitor 7.5mm Disc, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C101 (at 3.84 -0.12 180) (layer F.SilkS))
    (fp_text value 470pF (at 2.5 3.5 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.92) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C101-Pad1)") (zone_connect 2))
    (pad 2 thru_hole circle (at 8.7 0) (size 2 2) (drill 0.92) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C101-Pad2)") (zone_connect 2))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D7.5_P5.wrl
      (offset (xyz 2.500000042453766 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 5E1D22C5)
    (at 122.15 100.99)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.SilkS) hide)
    (fp_text value MountingHole_3-5mm (at 0 5.00126) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 101.92 67)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 101.19 67)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 100.45 67)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 142.12 67.02 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012 180) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 142.86 67.02 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012 180) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 143.59 67 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012 180) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 5CCF1ADE)
    (at 132.48 61.84)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.SilkS) hide)
    (fp_text value MountingHole_3-5mm (at 0 5.00126) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 5CCF1ADE)
    (at 138.18 61.9)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.SilkS) hide)
    (fp_text value MountingHole_3-5mm (at 0 5.00126) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 141.42 153.27 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012 180) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 140.7 153.44 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012 180) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 142.1 152.96 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012 180) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 139.98 153.58 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012 180) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 142.68 152.51 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012 180) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 143.19 151.99 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012 180) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 143.6 151.37 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012 180) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer B.Cu) (tedit 5CCF1CB9)
    (at 100.41 151.36)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 3.50012) (layer B.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 -3.59918) (layer B.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer B.Cu) (tedit 5CCF1CB9)
    (at 100.82 151.98)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 3.50012) (layer B.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 -3.59918) (layer B.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer B.Cu) (tedit 5CCF1CB9)
    (at 101.33 152.5)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 3.50012) (layer B.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 -3.59918) (layer B.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer B.Cu) (tedit 5CCF1CB9)
    (at 104.03 153.57)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 3.50012) (layer B.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 -3.59918) (layer B.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer B.Cu) (tedit 5CCF1CB9)
    (at 101.91 152.95)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 3.50012) (layer B.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 -3.59918) (layer B.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer B.Cu) (tedit 5CCF1CB9)
    (at 103.31 153.43)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 3.50012) (layer B.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 -3.59918) (layer B.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer B.Cu) (tedit 5CCF1CB9)
    (at 102.59 153.26)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 3.50012) (layer B.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 -3.59918) (layer B.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 141.43 66.34 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012 180) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 140.71 66.51 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012 180) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 142.11 66.03 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012 180) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 139.99 66.65 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012 180) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 142.69 65.58 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012 180) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 143.2 65.06 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012 180) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 143.61 64.44 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012 180) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer B.Cu) (tedit 5CCF1CB9)
    (at 141.42 67.71 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 3.50012 180) (layer B.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 -3.59918 180) (layer B.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer B.Cu) (tedit 5CCF1CB9)
    (at 140.7 67.54 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 3.50012 180) (layer B.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 -3.59918 180) (layer B.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer B.Cu) (tedit 5CCF1CB9)
    (at 142.1 68.02 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 3.50012 180) (layer B.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 -3.59918 180) (layer B.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer B.Cu) (tedit 5CCF1CB9)
    (at 139.98 67.4 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 3.50012 180) (layer B.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 -3.59918 180) (layer B.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer B.Cu) (tedit 5CCF1CB9)
    (at 142.68 68.47 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 3.50012 180) (layer B.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 -3.59918 180) (layer B.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer B.Cu) (tedit 5CCF1CB9)
    (at 143.19 68.99 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 3.50012 180) (layer B.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 -3.59918 180) (layer B.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer B.Cu) (tedit 5CCF1CB9)
    (at 143.6 69.61 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 3.50012 180) (layer B.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 -3.59918 180) (layer B.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer B.Cu) (tedit 5CCF1CB9)
    (at 143.59 59.62 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 3.50012 180) (layer B.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 -3.59918 180) (layer B.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer B.Cu) (tedit 5CCF1CB9)
    (at 143.18 59 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 3.50012 180) (layer B.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 -3.59918 180) (layer B.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer B.Cu) (tedit 5CCF1CB9)
    (at 142.67 58.48 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 3.50012 180) (layer B.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 -3.59918 180) (layer B.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer B.Cu) (tedit 5CCF1CB9)
    (at 139.97 57.41 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 3.50012 180) (layer B.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 -3.59918 180) (layer B.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer B.Cu) (tedit 5CCF1CB9)
    (at 142.09 58.03 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 3.50012 180) (layer B.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 -3.59918 180) (layer B.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer B.Cu) (tedit 5CCF1CB9)
    (at 140.69 57.55 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 3.50012 180) (layer B.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 -3.59918 180) (layer B.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer B.Cu) (tedit 5CCF1CB9)
    (at 141.41 57.72 180)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 3.50012 180) (layer B.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 -3.59918 180) (layer B.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 102.56 57.7)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 103.28 57.53)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 101.88 58.01)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 104 57.39)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 101.3 58.46)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 100.79 58.98)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 100.38 59.6)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 100.4 69.23)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 100.42 64.73)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 100.81 68.61)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 100.88 65.3)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 101.4 68.17)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 101.43 65.81)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 104.02 67.02)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 102.04 67.83)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 125.03 67.02)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 125.78 67.02)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 126.53 67.02)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 127.28 67.02)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 130.28 67.03)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 129.53 67.03)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 128.78 67.03)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 128.03 67.03)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 134.03 67.03)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 134.78 67.03)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 135.53 67.03)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 136.28 67.03)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 133.28 67.02)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 132.53 67.02)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 131.78 67.02)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 131.03 67.02)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 139.31 67.05)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 138.56 67.05)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 137.81 67.05)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 137.06 67.05)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 113.03 67.03)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 113.78 67.03)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 114.53 67.03)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 115.28 67.03)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 118.28 67.04)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 117.53 67.04)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 116.78 67.04)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 116.03 67.04)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 122.03 67.04)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 122.78 67.04)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 123.53 67.04)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 124.28 67.04)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 121.28 67.03)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 120.53 67.03)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 119.78 67.03)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 119.03 67.03)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 107 67)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 107.75 67)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 108.5 67)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 109.25 67)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 112.25 67.01)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 111.5 67.01)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 110.75 67.01)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 110 67.01)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 103.41 67.39)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 104.75 67.01)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 105.5 67.01)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 106.25 67.01)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 102.72 67.57)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 102.72 66.48)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 102.05 66.21)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 5CCF1ADE)
    (at 111.66 116.9)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.SilkS) hide)
    (fp_text value MountingHole_3-5mm (at 0 5.00126) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 5CCF1ADE)
    (at 116.9 108.99)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.SilkS) hide)
    (fp_text value MountingHole_3-5mm (at 0 5.00126) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 5CCF1ADE)
    (at 141.17 101.26)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.SilkS) hide)
    (fp_text value MountingHole_3-5mm (at 0 5.00126) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 5CCF1ADE)
    (at 131.57 101.26)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.SilkS) hide)
    (fp_text value MountingHole_3-5mm (at 0 5.00126) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 5CCF1ADE)
    (at 111.3 85.26)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.SilkS) hide)
    (fp_text value MountingHole_3-5mm (at 0 5.00126) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 5CCF1ADE)
    (at 116.87 93.12)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.SilkS) hide)
    (fp_text value MountingHole_3-5mm (at 0 5.00126) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 5CCF1CB9)
    (at 103.42 66.65)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (gr_text "Upper\nElement" (at 114.22 79.57) (layer B.SilkS))
  (gr_text "Vertical Dipole Feedpoint\n16 Jul 2021\nVer 1.3" (at 107.48 69.08 90) (layer B.SilkS))
  (gr_text "Wire End Insulator" (at 122.43 58.26) (layer B.SilkS))
  (gr_text "Wire End Insulator" (at 122.43 58.26) (layer F.SilkS))
  (gr_text "Coax Center\nConductor" (at 117.32 116.06 90) (layer B.SilkS))
  (gr_text "Coax\nShield" (at 137.46 137.12) (layer B.SilkS))
  (gr_text "Lower\nElement" (at 132.37 141.97) (layer B.SilkS))
  (gr_text "Upper\nElement" (at 114.26 79.59) (layer F.SilkS))
  (gr_text "Coax Center\nConductor" (at 114.59 113.08) (layer F.SilkS))
  (gr_text "Coax\nShield" (at 137.86 137.13) (layer F.SilkS))
  (gr_text "Lower\nElement" (at 132.55 142.06) (layer F.SilkS))
  (gr_line (start 100 57) (end 144 57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 154) (end 100 57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144 154) (end 100 154) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144 57) (end 144 154) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name "Net-(C101-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 5))
    (polygon
      (pts
        (xy 126.87 86.14) (xy 124.74 88.27) (xy 119.82 88.27) (xy 117.54 85.99) (xy 117.54 68.24)
        (xy 126.87 68.24)
      )
    )
  )
  (zone (net 4) (net_name "Net-(C101-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 5))
    (polygon
      (pts
        (xy 126.87 86.14) (xy 124.74 88.27) (xy 119.82 88.27) (xy 117.54 85.99) (xy 117.54 68.24)
        (xy 126.87 68.24)
      )
    )
  )
  (zone (net 4) (net_name "Net-(C101-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 5))
    (polygon
      (pts
        (xy 115.25 102.34) (xy 111.71 102.34) (xy 111.71 113.54) (xy 114.18 116.01) (xy 114.305 127.23)
        (xy 118.195 127.23) (xy 118.07 115.78) (xy 114.66 112.37) (xy 114.66 108.02) (xy 115.28 107.4)
        (xy 115.28 102.37) (xy 115.34 102.37)
      )
    )
  )
  (zone (net 4) (net_name "Net-(C101-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 5))
    (polygon
      (pts
        (xy 115.25 102.34) (xy 111.71 102.34) (xy 111.71 113.54) (xy 114.18 116.01) (xy 114.305 127.19)
        (xy 118.195 127.19) (xy 118.07 115.78) (xy 114.66 112.37) (xy 114.66 108.02) (xy 115.28 107.4)
        (xy 115.28 102.37) (xy 115.34 102.37)
      )
    )
  )
  (zone (net 5) (net_name "Net-(C101-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 5))
    (polygon
      (pts
        (xy 116.81 135.39) (xy 117.41 138.96) (xy 114.53 139.03) (xy 105.08 139.03) (xy 105.08 129.69)
        (xy 115.71 129.78)
      )
    )
  )
  (zone (net 5) (net_name "Net-(C101-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 5))
    (polygon
      (pts
        (xy 116.87 135.44) (xy 117.09 139.03) (xy 114.53 139.03) (xy 105.08 139.03) (xy 105.08 129.69)
        (xy 115.71 129.89)
      )
    )
  )
  (zone (net 6) (net_name "Net-(L102-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 5))
    (polygon
      (pts
        (xy 100.36 97.9) (xy 100.36 116.51) (xy 103.55 119.7) (xy 103.55 127.18) (xy 110.2 127.18)
        (xy 110.2 119.53) (xy 107.68 117.01) (xy 107.68 113.55) (xy 105.17 111.04) (xy 105.17 97.96)
        (xy 100.42 97.96) (xy 100.42 97.9)
      )
    )
  )
  (zone (net 6) (net_name "Net-(L102-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 5))
    (polygon
      (pts
        (xy 100.36 97.9) (xy 100.36 116.51) (xy 103.55 119.7) (xy 103.55 127.18) (xy 110.2 127.18)
        (xy 110.2 119.53) (xy 107.68 117.01) (xy 107.68 113.55) (xy 105.17 111.04) (xy 105.17 97.96)
        (xy 100.42 97.96) (xy 100.42 97.9)
      )
    )
  )
)
