<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<text>16</text>
<text>17</text>
<text>32</text>
<wire x1="46.5" y1="21.25" x2="46.5" y2="1.75" width="0.2064" layer="20"/>
<wire x1="46.5" y1="1.75" x2="4.25" y2="1.75" width="0.2064" layer="20"/>
<wire x1="4.25" y1="1.75" x2="4.25" y2="21.25" width="0.2064" layer="20"/>
<text>     SNES
 4M-bit Flash 
      to
   Mask ROM </text>
<text>Bazz</text>
<text>www.Bazz1.com</text>
<wire x1="4.25" y1="21.25" x2="46.5" y2="21.25" width="0.2064" layer="20"/>
<text>
   OSH Park
</text>
<text>SNES 
Mask ROM 
Adaptor
4Mbit</text>
<text>Bazz1</text>
</plain>
<libraries>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X16">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="memory2_bazz">
<description>&lt;b&gt;Generic Memories&lt;/b&gt;&lt;p&gt;

This one has a modified TSOP32 (shorter SMD pad pitch thickness) for SST39VF040 also compatible with SST39SF040

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TSOP32">
<description>&lt;b&gt;Thin Small Outline Package&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SST39SF040" library="memory2_bazz" package="TSOP32" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="-" library="pinhead" package="1X16" value=""/>
<element name="1" library="pinhead" package="1X16" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="WE#" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S$1">
<contactref element="SST39SF040" pad="6"/>
<contactref element="1" pad="1"/>
</signal>
<signal name="S$2">
<contactref element="1" pad="2"/>
<contactref element="SST39SF040" pad="9"/>
</signal>
<signal name="S$3">
<contactref element="SST39SF040" pad="11"/>
<contactref element="1" pad="3"/>
</signal>
<signal name="S$4">
<contactref element="1" pad="4"/>
<contactref element="SST39SF040" pad="12"/>
</signal>
<signal name="S$5">
<contactref element="1" pad="5"/>
<contactref element="SST39SF040" pad="13"/>
</signal>
<signal name="S$6">
<contactref element="1" pad="6"/>
<contactref element="SST39SF040" pad="14"/>
</signal>
<signal name="S$7">
<contactref element="1" pad="7"/>
<contactref element="SST39SF040" pad="15"/>
</signal>
<signal name="S$8">
<contactref element="1" pad="8"/>
<contactref element="SST39SF040" pad="16"/>
</signal>
<signal name="S$9">
<contactref element="SST39SF040" pad="17"/>
<contactref element="1" pad="9"/>
</signal>
<signal name="S$10">
<contactref element="1" pad="10"/>
<contactref element="SST39SF040" pad="18"/>
</signal>
<signal name="S$11">
<contactref element="1" pad="11"/>
<contactref element="SST39SF040" pad="19"/>
</signal>
<signal name="S$12">
<contactref element="1" pad="12"/>
<contactref element="SST39SF040" pad="20"/>
</signal>
<signal name="S$13">
<contactref element="1" pad="13"/>
<contactref element="SST39SF040" pad="21"/>
</signal>
<signal name="S$14">
<contactref element="1" pad="14"/>
<contactref element="SST39SF040" pad="22"/>
</signal>
<signal name="S$15">
<contactref element="1" pad="15"/>
<contactref element="SST39SF040" pad="23"/>
</signal>
<signal name="S$16">
<contactref element="1" pad="16"/>
<contactref element="SST39SF040" pad="24"/>
</signal>
<signal name="S$17">
<contactref element="-" pad="16"/>
<contactref element="SST39SF040" pad="25"/>
</signal>
<signal name="S$18">
<contactref element="-" pad="15"/>
<contactref element="SST39SF040" pad="26"/>
</signal>
<signal name="S$19">
<contactref element="-" pad="14"/>
<contactref element="SST39SF040" pad="27"/>
</signal>
<signal name="S$20">
<contactref element="-" pad="13"/>
<contactref element="SST39SF040" pad="28"/>
</signal>
<signal name="S$21">
<contactref element="-" pad="12"/>
<contactref element="SST39SF040" pad="29"/>
</signal>
<signal name="S$22">
<contactref element="-" pad="11"/>
<contactref element="SST39SF040" pad="30"/>
</signal>
<signal name="S$23">
<contactref element="-" pad="10"/>
<contactref element="SST39SF040" pad="31"/>
</signal>
<signal name="S$24">
<contactref element="-" pad="9"/>
<contactref element="SST39SF040" pad="10"/>
</signal>
<signal name="S$25">
<contactref element="-" pad="8"/>
<contactref element="SST39SF040" pad="1"/>
</signal>
<signal name="S$26">
<contactref element="-" pad="7"/>
<contactref element="SST39SF040" pad="2"/>
</signal>
<signal name="S$27">
<contactref element="-" pad="6"/>
<contactref element="SST39SF040" pad="3"/>
</signal>
<signal name="S$28">
<contactref element="-" pad="5"/>
<contactref element="SST39SF040" pad="4"/>
</signal>
<signal name="S$29">
<contactref element="-" pad="4"/>
<contactref element="SST39SF040" pad="5"/>
</signal>
<signal name="S$30">
<contactref element="-" pad="2"/>
<contactref element="SST39SF040" pad="32"/>
</signal>
<signal name="S$31">
<contactref element="-" pad="1"/>
<contactref element="SST39SF040" pad="8"/>
</signal>
<signal name="S$32">
<contactref element="SST39SF040" pad="7"/>
<contactref element="WE#" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
