(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 33)
    (tracks 78)
    (zones 0)
    (modules 17)
    (nets 11)
  )
  (page User 149.708 105.004)
  (title_block
    (title "PIR Sensor for HMI 4.3 screen")
    (date 2019-10-24)
    (rev v1.0.0)
    (company NetwiZe.be)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.975 1.4)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 /3V0)
  (net 2 /OEN)
  (net 3 GND)
  (net 4 /ONTIME)
  (net 5 /SENS)
  (net 6 /RX)
  (net 7 /TX)
  (net 8 +5V)
  (net 9 /PIR)
  (net 10 /REL)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /3V0)
    (add_net /OEN)
    (add_net /ONTIME)
    (add_net /PIR)
    (add_net /REL)
    (add_net /SENS)
    (add_net GND)
  )
  (net_class +5V ""
    (clearance 0.25)
    (trace_width 0.75)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
  )
  (net_class Serial ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /RX)
    (add_net /TX)
  )
  (module "AliExpress:S16-L221D - Mini Pir Sensor" (layer F.Cu) (tedit 5DE9538C)
    (at 73.35 36.227)
    (fp_text reference U1 (at 4.35 -0.027 270) (layer F.SilkS))
    (fp_text value S16-L221D-2 (at 0 -11) (layer F.Fab))
    (pad 4 smd rect (at -2.1 2.4) (size 1 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V0))
    (pad 5 smd rect (at 0 2.4) (size 1 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 /SENS))
    (pad 6 smd rect (at 2.1 2.4) (size 1 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 2.1 -2.4) (size 1 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 /REL))
    (pad 2 smd rect (at 0 -2.4) (size 1 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 /ONTIME))
    (pad 3 smd rect (at -2.1 -2.4) (size 1 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 /OEN))
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5DB8B06B)
    (at 64.633332 38.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -2.4 0.05 90) (layer F.SilkS))
    (fp_text value 1M (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /OEN))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /3V0) (zone_connect 2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 64.633332 33.6 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -2.5 0.05 90) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /PIR))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /REL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 67.1 33.6 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -2.5 0.05 90) (layer F.SilkS))
    (fp_text value 39k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /ONTIME))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5DB8AFAE)
    (at 67.1 38.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -2.4 0.05 90) (layer F.SilkS))
    (fp_text value 1M (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /ONTIME))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /3V0) (zone_connect 2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5DB8B065)
    (at 62.166666 38.5 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 2.4 0.066666 90) (layer F.SilkS))
    (fp_text value 20k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /3V0) (zone_connect 2))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /SENS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 59.7 38.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -2.4 0.05 90) (layer F.SilkS))
    (fp_text value 160R (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /SENS))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 87.925542 38.5 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 2.4 -0.074458 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 85.15036 38.5 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -2.4 0.066306 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +5V))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 82.37518 38.5 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 2.4 -0.058153 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /3V0))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 79.6 38.5 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -2.4 0.05 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /3V0))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbol:OSHW-Logo2_7.3x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 63.1 38.8 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at -0.3 -12.6 180) (layer B.Fab) hide)
    (model "U:/Projects/KiCad/Models/Copyrighted/GrabCad/Nextion - NX4827T043_011 - 4.3inch HMI LCD Screen.wrl"
      (offset (xyz -7.3 -56 1.6))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 180 0 90))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer B.Cu) (tedit 5DB3992E)
    (at 74.945 29.745 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 0.045 -9.845 90) (layer B.SilkS))
    (fp_text value "Pin Header to HMI" (at 6.1495 0.034 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 -3.81) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND) (zone_connect 2))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /RX))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /TX))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (offset (xyz 0 0 -1.4))
      (scale (xyz 0.1 1 0.5))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Horizontal.wrl
      (offset (xyz 0 0 3.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5DB1F49C)
    (at 86.5 33.2)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H1 (at 0 6.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5DB1F494)
    (at 60.2 33.2)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H2 (at 0 6.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Connector_PinSocket_1.27mm:PinSocket_1x05_P1.27mm_Vertical (layer B.Cu) (tedit 5DB899ED)
    (at 78.7 29.364 270)
    (descr "Through hole straight socket strip, 1x05, 1.27mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x05 1.27mm single row")
    (fp_text reference J2 (at 0.036 1.5 90) (layer B.SilkS))
    (fp_text value "Ribbon Cable from MCU" (at 8 0 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 -2.54) (layer B.Fab))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 /PIR))
    (pad 4 thru_hole oval (at 0 -3.81 270) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 +5V))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 /TX))
    (pad 2 thru_hole oval (at 0 -1.27 270) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 /RX))
    (pad 1 thru_hole rect (at 0 0 270) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Connector_PinSocket_1.27mm.3dshapes/PinSocket_1x05_P1.27mm_Vertical.wrl
      (offset (xyz 2.54 0 -0.1))
      (scale (xyz 1 1 0))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5DB32315)
    (at 80.834 33.682)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U2 (at 1.651 1.651 90) (layer F.SilkS))
    (fp_text value XC6206P302 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V0))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text v1.0.1 (at 87.6 37.5 90) (layer B.SilkS))
  (gr_arc (start 88.2 40.5) (end 88.2 42) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 58.5 40.5) (end 57 40.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 84.6 33.1) (end 89.7 32.9) (angle -87.8) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 62.1 33.1) (end 61.9 28) (angle -87.8) (layer Edge.Cuts) (width 0.05))
  (dimension 26.1 (width 0.15) (layer Dwgs.User)
    (gr_text "26.100 mm" (at 73.35 17.3) (layer Dwgs.User))
    (feature1 (pts (xy 86.4 29.8) (xy 86.4 18.013579)))
    (feature2 (pts (xy 60.3 29.8) (xy 60.3 18.013579)))
    (crossbar (pts (xy 60.3 18.6) (xy 86.4 18.6)))
    (arrow1a (pts (xy 86.4 18.6) (xy 85.273496 19.186421)))
    (arrow1b (pts (xy 86.4 18.6) (xy 85.273496 18.013579)))
    (arrow2a (pts (xy 60.3 18.6) (xy 61.426504 19.186421)))
    (arrow2b (pts (xy 60.3 18.6) (xy 61.426504 18.013579)))
  )
  (dimension 32.7 (width 0.15) (layer Dwgs.User)
    (gr_text "32.700 mm" (at 73.35 48.6) (layer Dwgs.User))
    (feature1 (pts (xy 89.7 41.9715) (xy 89.7 47.886421)))
    (feature2 (pts (xy 57 41.9715) (xy 57 47.886421)))
    (crossbar (pts (xy 57 47.3) (xy 89.7 47.3)))
    (arrow1a (pts (xy 89.7 47.3) (xy 88.573496 47.886421)))
    (arrow1b (pts (xy 89.7 47.3) (xy 88.573496 46.713579)))
    (arrow2a (pts (xy 57 47.3) (xy 58.126504 47.886421)))
    (arrow2b (pts (xy 57 47.3) (xy 58.126504 46.713579)))
  )
  (dimension 14 (width 0.15) (layer Dwgs.User)
    (gr_text "14.000 mm" (at 45.6 35 270) (layer Dwgs.User))
    (feature1 (pts (xy 56.4 42) (xy 46.313579 42)))
    (feature2 (pts (xy 56.4 28) (xy 46.313579 28)))
    (crossbar (pts (xy 46.9 28) (xy 46.9 42)))
    (arrow1a (pts (xy 46.9 42) (xy 46.313579 40.873496)))
    (arrow1b (pts (xy 46.9 42) (xy 47.486421 40.873496)))
    (arrow2a (pts (xy 46.9 28) (xy 46.313579 29.126504)))
    (arrow2b (pts (xy 46.9 28) (xy 47.486421 29.126504)))
  )
  (gr_text 5V (at 82.752 30.031 90) (layer F.SilkS))
  (gr_text GND (at 78.627 30.031 90) (layer F.SilkS))
  (gr_text PIR (at 85 29.2 90) (layer F.SilkS))
  (gr_text RX (at 80.002 30.031 90) (layer F.SilkS))
  (gr_text TX (at 81.377 30.031 90) (layer F.SilkS))
  (gr_text PIR (at 85.2 28.1 90) (layer B.SilkS))
  (gr_text 5V (at 82.525 30.77 90) (layer B.SilkS))
  (gr_text TX (at 81.15 30.77 90) (layer B.SilkS))
  (gr_text RX (at 79.775 30.77 90) (layer B.SilkS))
  (gr_text Gnd (at 78.4 30.75 90) (layer B.SilkS))
  (gr_text RX (at 72.76 31.65 90) (layer B.SilkS))
  (gr_text Gnd (at 75.3 31.65 90) (layer B.SilkS))
  (gr_text 5V (at 67.7 31.65 90) (layer B.SilkS))
  (gr_text TX (at 70.22 31.65 90) (layer B.SilkS))
  (gr_text Gnd (at 74.9 31.52) (layer F.SilkS))
  (gr_text RX (at 72.36 31.52) (layer F.SilkS))
  (gr_text TX (at 69.82 31.52) (layer F.SilkS))
  (gr_text 5V (at 67.28 31.52) (layer F.SilkS))
  (gr_text "PCB design by NetwiZe.be\nCC-BY-SA 2019-10-24" (at 75 40.1) (layer B.SilkS))
  (gr_text "HMI Mini PIR sensor" (at 84.1 36.8) (layer B.SilkS))
  (gr_line (start 58.5 42) (end 88.2 42) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 89.7 32.9) (end 89.7 40.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 61.9 28) (end 84.595925 27.996082) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 57 40.5) (end 56.996082 33.104075) (layer Edge.Cuts) (width 0.05))
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.5 27.818) (xy 88.5 42.55) (xy 56.9 42.666) (xy 56.9 27.934)
      )
    )
  )
  (zone (net 1) (net_name /3V0) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 84.1 37.5) (xy 84.1 38.2) (xy 78.7 37.95) (xy 76.2 37.95) (xy 74.525 37.751)
        (xy 72.3 37.75) (xy 72.3 38.55) (xy 68.2 40.1) (xy 61.6 40.1) (xy 61.6 39.1)
        (xy 65.2 39.1) (xy 69.658 34.317) (xy 75.1 34.4) (xy 79.3 34.4) (xy 80.9 34)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57 27.815) (xy 57 41.785) (xy 88.4 42.058) (xy 88.4 27.961)
      )
    )
  )
)
