(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 8)
    (no_connects 0)
    (area 140.477142 93.224999 156.702858 106.275)
    (thickness 1.6)
    (drawings 5)
    (tracks 22)
    (zones 0)
    (modules 6)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 147.32 102.87)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad1)")
  (net 2 "Net-(U1-Pad2)")
  (net 3 "Net-(U1-Pad5)")
  (net 4 "Net-(U1-Pad6)")
  (net 5 "Net-(U1-Pad8)")
  (net 6 "Net-(U1-Pad9)")
  (net 7 "Net-(U1-Pad10)")
  (net 8 "Net-(U1-Pad12)")
  (net 9 "Net-(U1-Pad13)")
  (net 10 "Net-(U1-Pad14)")
  (net 11 "Net-(C1-Pad1)")
  (net 12 "Net-(C1-Pad2)")
  (net 13 "Net-(J1-Pad1)")
  (net 14 "Net-(J2-Pad1)")
  (net_class Default "Это класс цепей по умолчанию."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 148.59 99.06 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 1.75 180) (layer B.SilkS))
    (fp_text value C_Small (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5A875BD6)
    (at 147.32 95.25)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference A (at -1.905 -0.381) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5A875BD1)
    (at 149.86 95.25)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference B (at 1.778 -0.381) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5A9F2B5F)
    (at 149.86 102.87)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference 3V3 (at 2.54 0.381) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5A9F2B4E)
    (at 147.32 102.87)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference GND (at -2.54 0.381) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:SSOP-16_5.3x6.2mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 148.59 99.0675)
    (descr "SSOP16: plastic shrink small outline package; 16 leads; body width 5.3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot338-1_po.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at -0.889 -1.6585) (layer F.SilkS))
    (fp_text value AD5593R (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -3.45 -2.275) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at -3.45 -1.625) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -3.45 -0.975) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad1)"))
    (pad 4 smd rect (at -3.45 -0.325) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J2-Pad1)"))
    (pad 5 smd rect (at -3.45 0.325) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at -3.45 0.975) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at -3.45 1.625) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C1-Pad2)"))
    (pad 8 smd rect (at -3.45 2.275) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U1-Pad8)"))
    (pad 9 smd rect (at 3.45 2.275) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U1-Pad9)"))
    (pad 10 smd rect (at 3.45 1.625) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-Pad10)"))
    (pad 11 smd rect (at 3.45 0.975) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C1-Pad2)"))
    (pad 12 smd rect (at 3.45 0.325) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-Pad12)"))
    (pad 13 smd rect (at 3.45 -0.325) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U1-Pad13)"))
    (pad 14 smd rect (at 3.45 -0.975) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at 3.45 -1.625) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C1-Pad1)"))
    (pad 16 smd rect (at 3.45 -2.275) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/SSOP-16_5.3x6.2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 143.51 104.14) (end 153.67 104.14) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.67 104.14) (end 153.67 99.06) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.51 93.98) (end 143.51 104.14) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.67 93.98) (end 143.51 93.98) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.67 99.06) (end 153.67 93.98) (layer Edge.Cuts) (width 0.15))
)
