<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="75.87" y2="0" width="0" layer="20"/>
<wire x1="75.87" y1="0" x2="75.87" y2="60.95" width="0" layer="20"/>
<wire x1="75.87" y1="60.95" x2="0" y2="60.95" width="0" layer="20"/>
<wire x1="0" y1="60.95" x2="0" y2="0" width="0" layer="20"/>
<text>Aguaingo by Flatbox</text>
<text>v1.0</text>
</plain>
<libraries>
<library name="Teensy356">
<packages>
<package name="TEENSY_3.5/3.6_BASIC">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JST-3-PTH-VERT">
<description>&lt;h3&gt;JST 3 Pin Vertical Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/ePH.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-4-PTH-VERT">
<description>&lt;h3&gt;JST Vertical 4 Pin Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.jst-mfg.com/product/pdf/eng/ePH.pdf"&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X08">
<description>&lt;h3&gt;Plated Through Hole -8 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,0">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.0 mm with drill center</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA3216-KIT">
<description>&lt;h3&gt;EIA3216-KIT&lt;/h3&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has longer pads to make hand soldering easier.&lt;br&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="Teensy356" package="TEENSY_3.5/3.6_BASIC" value="TEENSY_3.5/3.6_BASIC"/>
<element name="J1" library="SparkFun-Connectors" package="JST-3-PTH-VERT" value="WFS">
<attribute name="PROD_ID" value="CONN-13230"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="JST-4-PTH-VERT" value="TOF">
<attribute name="PROD_ID" value="CONN-13251"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X08" value="2.8TFT">
<attribute name="PROD_ID" value="CONN-08438"/>
</element>
<element name="JP1" library="pinhead" package="1X02/90" value="5Vin"/>
<element name="H1" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="H2" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="H3" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="H4" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="JP2" library="adafruit" package="1X03" value="5v Relay"/>
<element name="R1" library="SparkFun-Resistors" package="1206" value="10K"/>
<element name="C1" library="SparkFun-Passives" package="EIA3216-KIT" value="0.1uF"/>
</elements>
<signals>
<signal name="5V">
<contactref element="U$1" pad="VIN"/>
<contactref element="JP1" pad="1"/>
<contactref element="J1" pad="3"/>
<contactref element="J3" pad="8"/>
<contactref element="R1" pad="2"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="2"/>
<contactref element="J3" pad="7"/>
<contactref element="JP2" pad="1"/>
<contactref element="C1" pad="C"/>
<contactref element="U$1" pad="GND"/>
<contactref element="J1" pad="2"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="D6">
<contactref element="U$1" pad="6"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="J2" pad="1"/>
<contactref element="U$1" pad="19/A5/SCL"/>
</signal>
<signal name="INT2">
<contactref element="U$1" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="C1" pad="A"/>
</signal>
<signal name="3V3">
<contactref element="U$1" pad="3V3"/>
<contactref element="J2" pad="4"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="J3" pad="2"/>
<contactref element="U$1" pad="13/SCK"/>
</signal>
<signal name="SDA">
<contactref element="U$1" pad="18/A4/SDA"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="CS">
<contactref element="U$1" pad="10/CS"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="A0">
<contactref element="U$1" pad="9/CS"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="RESET">
<contactref element="J3" pad="5"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="MOSI">
<contactref element="J3" pad="3"/>
<contactref element="U$1" pad="11/MOSI"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
