(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 10)
    (no_connects 0)
    (area 121.739353 101.22855 150.040648 119.1228)
    (thickness 1.6)
    (drawings 28)
    (tracks 32)
    (zones 0)
    (modules 7)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4826)
    (user_trace_width 0.7366)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 "Net-(HOLE1-Pad1)")
  (net 4 "Net-(HOLE2-Pad1)")
  (net 5 /SCL)
  (net 6 /SDA)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
    (add_net "Net-(HOLE1-Pad1)")
    (add_net "Net-(HOLE2-Pad1)")
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58864A9C)
    (at 140.97 109.22)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.4765 0.127 90) (layer F.SilkS))
    (fp_text value 1u (at 1.27 -1.5875 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Hole_2.5mm (layer F.Cu) (tedit 58864794)
    (at 129.54 104.14)
    (descr "Mounting Hole, 2.5mm")
    (tags "HOLE 2.5MM")
    (fp_text reference HOLE1 (at -5.08 -0.635) (layer F.SilkS) hide)
    (fp_text value M2.5 (at -5.08 0.635) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.556 3.556) (drill 2.54) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(HOLE1-Pad1)"))
  )
  (module my_components:Hole_2.5mm (layer F.Cu) (tedit 58864798)
    (at 142.24 104.14)
    (descr "Mounting Hole, 2.5mm")
    (tags "HOLE 2.5MM")
    (fp_text reference HOLE2 (at 5.08 -0.635) (layer F.SilkS) hide)
    (fp_text value M2.5 (at 5.08 0.635) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.556 3.556) (drill 2.54) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(HOLE2-Pad1)"))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58864A90)
    (at 135.89 109.22)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -2.4765 0 90) (layer F.SilkS))
    (fp_text value 10k (at -2.54 -1.5875) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 /SDA))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58864B87)
    (at 130.81 109.22 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0.635 1.5875 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 /SCL))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Conn_Pin_Header_4x1_2.54mm (layer F.Cu) (tedit 58864992)
    (at 135.89 114.3)
    (descr "Pin Header, 4x1, 2.54mm pitch")
    (tags "CONN 4x1")
    (fp_text reference P1 (at -6.0325 0 90) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 3.81) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -3.81 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SCL))
    (pad 2 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SDA))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +3V3))
    (pad 4 thru_hole circle (at 3.81 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:IC_TO-46-4 (layer F.Cu) (tedit 5886595E)
    (at 135.89 104.775 90)
    (descr TO-46-4)
    (tags "TO-46-4, TO-46, 4Pin")
    (fp_text reference U1 (at 0 -3.3655 90) (layer F.SilkS))
    (fp_text value MLX90615 (at -0.3175 3.4925 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 1.27 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SDA))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 +3V3))
    (pad 3 thru_hole circle (at 0 -1.27 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SCL))
    (pad 4 thru_hole circle (at -1.27 0 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (gr_text "MLX90615\nInfrared Temperature\nSensor V1 (C) 2017\nSergey Kiselev" (at 135.89 110.1725) (layer B.SilkS))
  (gr_text GND (at 139.7 111.4425 90) (layer F.SilkS))
  (gr_text VCC (at 137.16 111.4425 90) (layer F.SilkS))
  (gr_text SDA (at 134.62 111.4425 90) (layer F.SilkS))
  (gr_text SCL (at 132.08 111.4425 90) (layer F.SilkS))
  (gr_line (start 127 102.87) (end 127 115.57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 102.87) (end 144.78 115.57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.51 101.6) (end 128.27 101.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.27 116.84) (end 143.51 116.84) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 143.51 115.57) (end 144.78 115.57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 128.27 115.57) (end 128.27 116.84) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 128.27 102.87) (end 127 102.87) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 143.51 102.87) (end 143.51 101.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.78 116.84) (xy 127 116.84) (xy 127 101.6) (xy 144.78 101.6) (xy 144.78 116.84)
      )
    )
  )
)
