(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 147)
    (no_connects 0)
    (area 66.392599 91.32298 123.013353 202.949001)
    (thickness 1.6)
    (drawings 64)
    (tracks 684)
    (zones 0)
    (modules 56)
    (nets 55)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.16)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (user_trace_width 2)
    (trace_clearance 0.16)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.16)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.99898 1.99898)
    (pad_drill 1.00076)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x01008_00000000)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 "Net-(D4-Pad1)")
  (net 3 GND)
  (net 4 VBAT)
  (net 5 "Net-(Q1-Pad1)")
  (net 6 "Net-(D1-Pad1)")
  (net 7 /loadsharing/VSHARED)
  (net 8 /loadsharing/HALF_VDD)
  (net 9 /loadsharing/HALF_VBAT)
  (net 10 "Net-(R5-Pad2)")
  (net 11 "Net-(R6-Pad2)")
  (net 12 "Net-(U2-Pad6)")
  (net 13 "Net-(U2-Pad5)")
  (net 14 "Net-(C6-Pad1)")
  (net 15 "Net-(L1-Pad1)")
  (net 16 "Net-(L1-Pad2)")
  (net 17 "Net-(R8-Pad2)")
  (net 18 "Net-(R10-Pad1)")
  (net 19 "Net-(R11-Pad2)")
  (net 20 /VDDA)
  (net 21 /SWCLK)
  (net 22 /SWDIO)
  (net 23 /ADCIN_6)
  (net 24 /ADCIN_5)
  (net 25 /QSPI_CLK)
  (net 26 /QSPI_NCS)
  (net 27 /DAC1_OUT)
  (net 28 /ADCIN_10)
  (net 29 /QSPI_IO3)
  (net 30 /QSPI_IO2)
  (net 31 /QSPI_IO1)
  (net 32 /QSPI_IO0)
  (net 33 /GPIOOUT_PC14)
  (net 34 /GPIOOUT_PC15)
  (net 35 /GPIOIN_PA8)
  (net 36 /CAN1_RX)
  (net 37 /CAN1_TX)
  (net 38 /SPI3_SCK)
  (net 39 /GPIOIN_PA15)
  (net 40 /SPI3_MOSI)
  (net 41 /SPI3_MISO)
  (net 42 /USART1_RX)
  (net 43 /USART1_TX)
  (net 44 "Net-(P4-Pad1)")
  (net 45 "Net-(P5-Pad1)")
  (net 46 "Net-(P6-Pad1)")
  (net 47 "Net-(P7-Pad1)")
  (net 48 /voltageregulator/BUCKBOOST)
  (net 49 "Net-(J1-Pad1)")
  (net 50 /solarcharger/I2C_SDA)
  (net 51 /solarcharger/I2C_SCL)
  (net 52 /NRST)
  (net 53 "Net-(D3-Pad1)")
  (net 54 "Net-(D5-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.16)
    (trace_width 0.16)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ADCIN_10)
    (add_net /ADCIN_5)
    (add_net /ADCIN_6)
    (add_net /CAN1_RX)
    (add_net /CAN1_TX)
    (add_net /DAC1_OUT)
    (add_net /GPIOIN_PA15)
    (add_net /GPIOIN_PA8)
    (add_net /GPIOOUT_PC14)
    (add_net /GPIOOUT_PC15)
    (add_net /NRST)
    (add_net /QSPI_CLK)
    (add_net /QSPI_IO0)
    (add_net /QSPI_IO1)
    (add_net /QSPI_IO2)
    (add_net /QSPI_IO3)
    (add_net /QSPI_NCS)
    (add_net /SPI3_MISO)
    (add_net /SPI3_MOSI)
    (add_net /SPI3_SCK)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net /USART1_RX)
    (add_net /USART1_TX)
    (add_net /VDDA)
    (add_net /loadsharing/HALF_VBAT)
    (add_net /loadsharing/HALF_VDD)
    (add_net /loadsharing/VSHARED)
    (add_net /solarcharger/I2C_SCL)
    (add_net /solarcharger/I2C_SDA)
    (add_net /voltageregulator/BUCKBOOST)
    (add_net GND)
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P7-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net VBAT)
    (add_net VDD)
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 5A2DE13D)
    (at 101.7194 108.4072)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U7 (at -0.094 -1.4478) (layer F.SilkS))
    (fp_text value INA219 (at 4.5974 -4.3434) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 VBAT))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 /solarcharger/I2C_SCL))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 /solarcharger/I2C_SDA))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dics-exotic-footprints:Pin_Header_Angled_2x07 (layer F.Cu) (tedit 5A25EC57)
    (at 111.887 175.514 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at -2.032 0 360) (layer F.SilkS) hide)
    (fp_text value bottom (at 5.9436 7.0104 360) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /voltageregulator/BUCKBOOST))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /GPIOIN_PA8))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 /solarcharger/I2C_SDA))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 /solarcharger/I2C_SCL))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /CAN1_TX))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 /CAN1_RX))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /SPI3_SCK))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /GPIOIN_PA15))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /SPI3_MOSI))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /SPI3_MISO))
    (pad 13 thru_hole oval (at 0 15.24 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /USART1_RX))
    (pad 14 thru_hole oval (at 2.54 15.24 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 /USART1_TX))
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5A25ECB9)
    (at 98.4124 113.0046 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at 1.1812 1.2954 180) (layer F.SilkS))
    (fp_text value LED (at 4.191 -0.254 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5A25ED06)
    (at 109.5502 103.8352 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 1.524 -2.0828 270) (layer F.SilkS))
    (fp_text value SolarPanel (at 8.2296 9.6774 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5A25ED01)
    (at 111.8362 119.5832 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at 0.0762 5.0292 180) (layer F.SilkS))
    (fp_text value "LiFePo4 Battery" (at -3.048 5.334 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 VBAT))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A25ED0D)
    (at 101.4382 123.5608 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 2.429 -0.061 270) (layer F.SilkS))
    (fp_text value DMP1045U7 (at -1.3048 2.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 /loadsharing/VSHARED))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A25ED26)
    (at 103.7082 127.3302 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 2.159 0.1524 450) (layer F.SilkS))
    (fp_text value 100K (at -0.0134 3.6576 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /loadsharing/HALF_VDD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A25ED2B)
    (at 101.8794 127.8756 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -2.02 -0.4572 180) (layer F.SilkS))
    (fp_text value 100K (at -5.7792 1.3208 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /loadsharing/HALF_VDD))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A25ED1A)
    (at 110.49 126.3008 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 2.0962 0.2032 360) (layer F.SilkS))
    (fp_text value 100K (at -2.5774 -6.0198 360) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 VBAT))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 /loadsharing/HALF_VBAT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A25ED20)
    (at 112.2934 126.3396 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -2.032 0.3048 360) (layer F.SilkS))
    (fp_text value 100K (at -13.1198 2.54 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 /loadsharing/HALF_VBAT))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A25ECEF)
    (at 101.5492 113.0046)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 2.2098 0.8636) (layer F.SilkS))
    (fp_text value 1K (at 2.0962 0.1524 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.5882 0.0508 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A25ECF4)
    (at 106.16 112.776 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -0.7994 1.4478 360) (layer F.SilkS))
    (fp_text value 1.15K (at -10.9594 -0.7112 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5A25ED32)
    (at 106.8402 126.3548)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at 0.7034 2.474) (layer F.SilkS))
    (fp_text value TS391ILT (at 11.1174 0.5436) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 /loadsharing/HALF_VBAT))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 /loadsharing/HALF_VDD))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 VBAT))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dics-exotic-footprints:DFN10-3x3x0.9-MF (layer F.Cu) (tedit 5A25EB37)
    (at 101.108 115.544)
    (fp_text reference U2 (at 0.762 4.826) (layer F.SilkS))
    (fp_text value MCP73x23 (at 17.7894 -3.8094) (layer F.Fab) hide)
    (pad 10 smd rect (at 0 0) (size 0.28 0.63) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R6-Pad2)"))
    (pad 9 smd rect (at 0.5 0) (size 0.28 0.63) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 8 smd rect (at 1 0) (size 0.28 0.63) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 7 smd rect (at 1.5 0) (size 0.28 0.63) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R5-Pad2)"))
    (pad 6 smd rect (at 2 0) (size 0.28 0.63) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(U2-Pad6)"))
    (pad 5 smd rect (at 2 3.1) (size 0.28 0.63) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U2-Pad5)"))
    (pad 4 smd rect (at 1.5 3.1) (size 0.28 0.63) (layers F.Cu F.Paste F.Mask)
      (net 4 VBAT))
    (pad 3 smd rect (at 1 3.1) (size 0.28 0.63) (layers F.Cu F.Paste F.Mask)
      (net 4 VBAT))
    (pad 2 smd rect (at 0.5 3.1) (size 0.28 0.63) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 1 smd rect (at 0 3.1) (size 0.28 0.63) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 11 smd rect (at 1 1.55) (size 2.46 1.53) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module dics-exotic-footprints:SOD-323HE (layer F.Cu) (tedit 5A1BBD1D)
    (at 106.304 121.92 270)
    (fp_text reference D1 (at 0.254 2.032 270) (layer F.SilkS))
    (fp_text value D_Schottky (at 0.254 -3.302 270) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 270) (size 1.1 2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0 -1.9 270) (size 1.1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 VBAT))
  )
  (module dics-exotic-footprints:SOD-323HE (layer F.Cu) (tedit 5A1BBD25)
    (at 97.917 121.92 90)
    (fp_text reference D2 (at 1.4732 -0.3302 180) (layer F.SilkS))
    (fp_text value D_Schottky (at 0.254 -3.302 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 90) (size 1.1 2) (layers F.Cu F.Paste F.Mask)
      (net 7 /loadsharing/VSHARED))
    (pad 2 smd rect (at 0 -1.9 90) (size 1.1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
  )
  (module Capacitors_SMD:CP_Elec_4x5.7 (layer F.Cu) (tedit 5A25ECD1)
    (at 96.139 116.5352)
    (descr "SMT capacitor, aluminium electrolytic, 4x5.7")
    (attr smd)
    (fp_text reference C1 (at 3.302 2.1082 90) (layer F.SilkS))
    (fp_text value 4.7uF (at -0.0254 -3.0226) (layer F.Fab) hide)
    (fp_text user + (at -1.1 -0.08) (layer F.Fab))
    (fp_text user + (at -2.77 2.01) (layer F.SilkS))
    (fp_text user %R (at 3.302 2.1082 270) (layer F.Fab))
    (pad 1 smd rect (at -1.8 0 180) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.8 0 180) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_4x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_4x5.7 (layer F.Cu) (tedit 5A25ECD6)
    (at 107.0356 117.3734 90)
    (descr "SMT capacitor, aluminium electrolytic, 4x5.7")
    (attr smd)
    (fp_text reference C2 (at 3.1242 2.1844 180) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 -3.54 90) (layer F.Fab) hide)
    (fp_text user + (at -1.1 -0.08 90) (layer F.Fab))
    (fp_text user + (at -2.77 2.01 90) (layer F.SilkS))
    (fp_text user %R (at 4.0894 0.4064 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.8 0 270) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 VBAT))
    (pad 2 smd rect (at 1.8 0 270) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_4x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A25ED12)
    (at 107.2 123.698 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -2.274 -0.0762 360) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 VBAT))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:CP_Elec_4x5.7 (layer F.Cu) (tedit 5A25ECA0)
    (at 91.948 132.7692 270)
    (descr "SMT capacitor, aluminium electrolytic, 4x5.7")
    (attr smd)
    (fp_text reference C3 (at -0.0288 -3.2004 270) (layer F.SilkS))
    (fp_text value 10uF (at 1.8254 5.3594 360) (layer F.Fab) hide)
    (fp_text user + (at -1.1 -0.08 270) (layer F.Fab))
    (fp_text user + (at -2.77 2.01 270) (layer F.SilkS))
    (fp_text user %R (at 0 3.54 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.8 0 90) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /loadsharing/VSHARED))
    (pad 2 smd rect (at 1.8 0 90) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_4x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_4x5.7 (layer F.Cu) (tedit 5A25EC8A)
    (at 91.9226 124.3872 90)
    (descr "SMT capacitor, aluminium electrolytic, 4x5.7")
    (attr smd)
    (fp_text reference C4 (at 4.1182 -0.8128 180) (layer F.SilkS))
    (fp_text value 10uF (at 0.5554 6.2484 180) (layer F.Fab) hide)
    (fp_text user + (at -1.1 -0.08 90) (layer F.Fab))
    (fp_text user + (at -2.77 2.01 90) (layer F.SilkS))
    (fp_text user %R (at 0 3.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.8 0 270) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /loadsharing/VSHARED))
    (pad 2 smd rect (at 1.8 0 270) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_4x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_4x5.7 (layer F.Cu) (tedit 5A55CFDB)
    (at 97.1042 128.1938 90)
    (descr "SMT capacitor, aluminium electrolytic, 4x5.7")
    (attr smd)
    (fp_text reference C5 (at 4.1402 -0.254 180) (layer F.SilkS))
    (fp_text value 10uF (at 0.635 -11.7602 180) (layer F.Fab) hide)
    (fp_text user + (at -1.1 -0.08 90) (layer F.Fab))
    (fp_text user + (at -2.77 2.01 90) (layer F.SilkS))
    (fp_text user %R (at 0 3.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.8 0 270) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /loadsharing/VSHARED))
    (pad 2 smd rect (at 1.8 0 270) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_4x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A25ED3D)
    (at 97.1176 136.144 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0.4198 1.1938 360) (layer F.SilkS))
    (fp_text value 100nF (at 10.8592 -0.1016 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C6-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:CP_Elec_4x5.7 (layer F.Cu) (tedit 5A25EC1A)
    (at 110.7982 131.8006)
    (descr "SMT capacitor, aluminium electrolytic, 4x5.7")
    (attr smd)
    (fp_text reference C7 (at -3.8642 -0.4826 90) (layer F.SilkS))
    (fp_text value 10uF (at 5.4068 -3.4544) (layer F.Fab) hide)
    (fp_text user + (at -1.1 -0.08) (layer F.Fab))
    (fp_text user + (at -2.77 2.01) (layer F.SilkS))
    (fp_text user %R (at 4.7972 3.7846) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.8 0 180) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 48 /voltageregulator/BUCKBOOST))
    (pad 2 smd rect (at 1.8 0 180) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_4x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_4x5.7 (layer F.Cu) (tedit 5A25EC2C)
    (at 108.7916 144.2212)
    (descr "SMT capacitor, aluminium electrolytic, 4x5.7")
    (attr smd)
    (fp_text reference C8 (at 4.1622 0.1016 270) (layer F.SilkS))
    (fp_text value 22uF (at 7.5658 -0.1524) (layer F.Fab) hide)
    (fp_text user + (at -1.1 -0.08) (layer F.Fab))
    (fp_text user + (at -2.77 2.01) (layer F.SilkS))
    (fp_text user %R (at 8.8358 3.2004) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.8 0 180) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 48 /voltageregulator/BUCKBOOST))
    (pad 2 smd rect (at 1.8 0 180) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_4x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_4x5.7 (layer F.Cu) (tedit 5A25EC1E)
    (at 110.766 137.7188)
    (descr "SMT capacitor, aluminium electrolytic, 4x5.7")
    (attr smd)
    (fp_text reference C9 (at -3.959 1.2954 90) (layer F.SilkS))
    (fp_text value 22uF (at 5.8962 -3.81) (layer F.Fab) hide)
    (fp_text user + (at -1.1 -0.08) (layer F.Fab))
    (fp_text user + (at -2.77 2.01) (layer F.SilkS))
    (fp_text user %R (at 4.7532 3.937) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.8 0 180) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 48 /voltageregulator/BUCKBOOST))
    (pad 2 smd rect (at 1.8 0 180) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_4x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_4x5.7 (layer F.Cu) (tedit 5A25EC68)
    (at 101.9556 144.3194 270)
    (descr "SMT capacitor, aluminium electrolytic, 4x5.7")
    (attr smd)
    (fp_text reference C10 (at -3.9336 -0.8128 360) (layer F.SilkS))
    (fp_text value 22uF (at 4.042 14.8336 360) (layer F.Fab) hide)
    (fp_text user + (at -1.1 -0.08 270) (layer F.Fab))
    (fp_text user + (at -2.77 2.01 270) (layer F.SilkS))
    (fp_text user %R (at 1.248 -13.9446 360) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.8 0 90) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 48 /voltageregulator/BUCKBOOST))
    (pad 2 smd rect (at 1.8 0 90) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_4x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A25ED37)
    (at 97.1924 133.096)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 2.2486 -0.9144) (layer F.SilkS))
    (fp_text value 10K (at -10.807 4.8768) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 /loadsharing/VSHARED))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A25ED48)
    (at 99.3514 139.3444 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0.2152 1.4224 180) (layer F.SilkS))
    (fp_text value 274k (at 11.6198 -5.8928 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 /voltageregulator/BUCKBOOST))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A25ED5B)
    (at 98.552 141.5796 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0.0508 1.3208 270) (layer F.SilkS))
    (fp_text value 100K (at 9.5892 -0.762 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R10-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A25ED44)
    (at 94.1324 137.033)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at -3.2766 0.0254) (layer F.SilkS))
    (fp_text value 100K (at -4.953 -9.7282 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 /voltageregulator/BUCKBOOST))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Choke_Axial_ThroughHole:Choke_Horizontal_RM10mm (layer F.Cu) (tedit 5A5BCEE3)
    (at 105.156 135.2042 90)
    (descr "Choke, Axial, 10mm")
    (tags "Choke, Axial, 10mm")
    (fp_text reference L1 (at 0 -3.50012 90) (layer F.SilkS))
    (fp_text value 1.5uH (at 2.2352 11.7856 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -5.10126 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 15 "Net-(L1-Pad1)"))
    (pad 2 thru_hole circle (at 5.25874 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 16 "Net-(L1-Pad2)"))
  )
  (module dics-exotic-footprints:TPS63070 (layer F.Cu) (tedit 5A25ECA5)
    (at 99.8938 136.4912)
    (fp_text reference U3 (at 2.6206 -3.827) (layer F.SilkS))
    (fp_text value TPS63070 (at -14.9054 -5.5542) (layer F.Fab) hide)
    (pad 5 smd oval (at 0 0) (size 0.25 0.45) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R10-Pad1)"))
    (pad 6 smd oval (at 0.5 0) (size 0.25 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 7 smd oval (at 1 0) (size 0.25 0.45) (layers F.Cu F.Paste F.Mask)
      (net 48 /voltageregulator/BUCKBOOST))
    (pad 7 smd oval (at 1.5 0) (size 0.25 0.45) (layers F.Cu F.Paste F.Mask)
      (net 48 /voltageregulator/BUCKBOOST))
    (pad 12 smd rect (at 1.25 -2.44856) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /loadsharing/VSHARED))
    (pad 15 smd oval (at 0 -2.55) (size 0.25 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 14 smd oval (at 0.5 -2.55) (size 0.25 0.45) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R8-Pad2)"))
    (pad 12 smd oval (at 1 -2.55) (size 0.25 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 /loadsharing/VSHARED))
    (pad 12 smd oval (at 1.5 -2.55) (size 0.25 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 /loadsharing/VSHARED))
    (pad 7 smd rect (at 1.2446 -0.1016) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 48 /voltageregulator/BUCKBOOST))
    (pad 4 smd oval (at -0.275 -0.525) (size 0.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd oval (at -0.275 -1.025) (size 0.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C6-Pad1)"))
    (pad 2 smd oval (at -0.275 -1.525) (size 0.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R11-Pad2)"))
    (pad 1 smd rect (at -0.275 -2.025) (size 0.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R8-Pad2)"))
    (pad 11 smd oval (at 1.425 -1.775) (size 1.15 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(L1-Pad2)"))
    (pad 10 smd oval (at 1.25 -1.275) (size 1.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 9 smd oval (at 1.425 -0.775) (size 1.15 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(L1-Pad1)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A25EC81)
    (at 95.885 151.0792 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 0.4826 -2.0828 90) (layer F.SilkS))
    (fp_text value 100nF (at 8.8392 -13.9192 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 52 /NRST))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A25EC79)
    (at 95.885 154.305 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at -0.127 1.524 270) (layer F.SilkS))
    (fp_text value 100nF (at 10.0076 -14.6558 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 /VDDA))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A25EC3A)
    (at 105.803 158.2928 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at 3.1108 -0.1524 360) (layer F.SilkS))
    (fp_text value 100nF (at -13.4232 2.6162 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 48 /voltageregulator/BUCKBOOST))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-32-1EP_5x5mm_Pitch0.5mm (layer F.Cu) (tedit 5A25EC3F)
    (at 102.616 154.305)
    (descr "UH Package; 32-Lead Plastic QFN (5mm x 5mm); (see Linear Technology QFN_32_05-08-1693.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U4 (at 0.2032 -4.6482) (layer F.SilkS))
    (fp_text value STM32L432 (at 12.9286 6.477 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.4 -1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 48 /voltageregulator/BUCKBOOST))
    (pad 2 smd rect (at -2.4 -1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 /GPIOOUT_PC14))
    (pad 3 smd rect (at -2.4 -0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 /GPIOOUT_PC15))
    (pad 4 smd rect (at -2.4 -0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 52 /NRST))
    (pad 5 smd rect (at -2.4 0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 /VDDA))
    (pad 6 smd rect (at -2.4 0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 /ADCIN_5))
    (pad 7 smd rect (at -2.4 1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 /ADCIN_6))
    (pad 8 smd rect (at -2.4 1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /QSPI_NCS))
    (pad 9 smd rect (at -1.75 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /QSPI_CLK))
    (pad 10 smd rect (at -1.25 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /DAC1_OUT))
    (pad 11 smd rect (at -0.75 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /ADCIN_10))
    (pad 12 smd rect (at -0.25 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /QSPI_IO3))
    (pad 13 smd rect (at 0.25 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 /QSPI_IO2))
    (pad 14 smd rect (at 0.75 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 /QSPI_IO1))
    (pad 15 smd rect (at 1.25 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 /QSPI_IO0))
    (pad 16 smd rect (at 1.75 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 17 smd rect (at 2.4 1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 48 /voltageregulator/BUCKBOOST))
    (pad 18 smd rect (at 2.4 1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 /GPIOIN_PA8))
    (pad 19 smd rect (at 2.4 0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 51 /solarcharger/I2C_SCL))
    (pad 20 smd rect (at 2.4 0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 50 /solarcharger/I2C_SDA))
    (pad 21 smd rect (at 2.4 -0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 /CAN1_RX))
    (pad 22 smd rect (at 2.4 -0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 /CAN1_TX))
    (pad 23 smd rect (at 2.4 -1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 /SWDIO))
    (pad 24 smd rect (at 2.4 -1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 /SWCLK))
    (pad 25 smd rect (at 1.75 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 /GPIOIN_PA15))
    (pad 26 smd rect (at 1.25 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 /SPI3_SCK))
    (pad 27 smd rect (at 0.75 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 /SPI3_MISO))
    (pad 28 smd rect (at 0.25 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 /SPI3_MOSI))
    (pad 29 smd rect (at -0.25 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 43 /USART1_TX))
    (pad 30 smd rect (at -0.75 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 42 /USART1_RX))
    (pad 31 smd rect (at -1.25 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 32 smd rect (at -1.75 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 33 smd rect (at 0.8625 0.8625) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at 0.8625 -0.8625) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.8625 0.8625) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.8625 -0.8625) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-32-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A25ED70)
    (at 98.679 150.241)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 48 /voltageregulator/BUCKBOOST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dics-exotic-footprints:Pin_Header_Angled_2x07 (layer B.Cu) (tedit 5A2DE112)
    (at 93.8276 156.6418 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 5.1 180) (layer B.SilkS) hide)
    (fp_text value side (at 6.0198 -7.4422 270) (layer B.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 3 GND))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 48 /voltageregulator/BUCKBOOST))
    (pad 3 thru_hole oval (at 0 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 33 /GPIOOUT_PC14))
    (pad 4 thru_hole oval (at 2.54 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 34 /GPIOOUT_PC15))
    (pad 5 thru_hole oval (at 0 -5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 23 /ADCIN_6))
    (pad 6 thru_hole oval (at 2.54 -5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 24 /ADCIN_5))
    (pad 7 thru_hole oval (at 0 -7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 25 /QSPI_CLK))
    (pad 8 thru_hole oval (at 2.54 -7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 26 /QSPI_NCS))
    (pad 9 thru_hole oval (at 0 -10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 28 /ADCIN_10))
    (pad 10 thru_hole oval (at 2.54 -10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 27 /DAC1_OUT))
    (pad 11 thru_hole oval (at 0 -12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 30 /QSPI_IO2))
    (pad 12 thru_hole oval (at 2.54 -12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 29 /QSPI_IO3))
    (pad 13 thru_hole oval (at 0 -15.24 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 32 /QSPI_IO0))
    (pad 14 thru_hole oval (at 2.54 -15.24 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 31 /QSPI_IO1))
  )
  (module SMD_Packages:1Pin (layer F.Cu) (tedit 5A25EC53)
    (at 92 177)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P4 (at 0.3544 -3.2386) (layer F.SilkS) hide)
    (fp_text value H1 (at 0.2528 4.6862) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 3.5 3.5) (drill 2.7) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(P4-Pad1)"))
  )
  (module SMD_Packages:1Pin (layer F.Cu) (tedit 5A25ECE2)
    (at 92 109)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P5 (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value H2 (at 0.24892 3.74904) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.7) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(P5-Pad1)"))
  )
  (module SMD_Packages:1Pin (layer F.Cu) (tedit 5A25ECC6)
    (at 111 109)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P6 (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value H3 (at 0.24892 3.74904) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.7) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(P6-Pad1)"))
  )
  (module SMD_Packages:1Pin (layer F.Cu) (tedit 5A25EC44)
    (at 111 170)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P7 (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value H4 (at 4.4684 0.0784) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.7) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(P7-Pad1)"))
  )
  (module Downloads:bufnita_kicad (layer B.Cu) (tedit 0)
    (at 93.3958 128.70977 270)
    (fp_text reference U6 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value Bufnita_Logo (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM15mm (layer F.Cu) (tedit 5A55C18F)
    (at 105.6386 103.8606 180)
    (descr "Resistor, Axial, RM 15mm,")
    (tags "Resistor Axial RM 15mm")
    (fp_text reference R12 (at 7.6454 -0.0508 180) (layer F.SilkS))
    (fp_text value Shunt (at -5.193 3.2766 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.40076) (layers *.Cu *.SilkS *.Mask)
      (net 49 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 15 0 180) (size 1.99898 1.99898) (drill 1.40076) (layers *.Cu *.SilkS *.Mask)
      (net 1 VDD))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.2905 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A2DE0F6)
    (at 106.68 172.8978)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 2.794 0.6604) (layer F.SilkS))
    (fp_text value 10K (at 7.5826 0.3556) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 /solarcharger/I2C_SDA))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 /voltageregulator/BUCKBOOST))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A2DE0F3)
    (at 103.7971 172.8978 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 2.8956 -0.6604 180) (layer F.SilkS))
    (fp_text value 10K (at -8.013 0.9652 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 /voltageregulator/BUCKBOOST))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 /solarcharger/I2C_SCL))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 5A5BA3AC)
    (at 111.5568 148.4122)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -5.1) (layer F.SilkS))
    (fp_text value SWD (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /voltageregulator/BUCKBOOST))
    (pad 2 thru_hole oval (at 0.1 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 /NRST))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /SWCLK))
    (pad 4 thru_hole oval (at 0.1 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /SWDIO))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A5BA3A6)
    (at 93.6498 153.5938 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at -0.127 -1.4224 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 /VDDA))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A5B9BE2)
    (at 105.8164 160.0962 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at 3.1108 -0.0254 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 48 /voltageregulator/BUCKBOOST))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5A5C11D4)
    (at 108.5596 163.4236 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at -0.0635 1.3716 180) (layer F.SilkS))
    (fp_text value LED (at -7.3279 1.4732 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 37 /CAN1_TX))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(D3-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5A5C11DF)
    (at 108.5469 165.4302 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D5 (at -0.0508 -1.4224 180) (layer F.SilkS))
    (fp_text value LED (at -7.1628 1.1811 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 36 /CAN1_RX))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(D5-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A5C117D)
    (at 111.9251 163.4236 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 0.0381 1.4478 180) (layer F.SilkS))
    (fp_text value 1K (at 4.3568 3.0226 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(D3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A5C1183)
    (at 111.9251 165.4302 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at 0.0127 -1.4478 180) (layer F.SilkS))
    (fp_text value 1K (at 3.7465 1.4478 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(D5-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dics-exotic-footprints:SMD_Switch_B3FS-1015P (layer F.Cu) (tedit 5A5C1670)
    (at 91.0463 147.6121 270)
    (fp_text reference S1 (at -4.1783 -2.413 360) (layer F.SilkS))
    (fp_text value B3FS-1015P (at -3.5052 3.429 270) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 270) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 52 /NRST))
    (pad 2 smd rect (at 0 -4.5 270) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -8 0 270) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 52 /NRST))
    (pad 2 smd rect (at -8 -4.5 270) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module dics-exotic-footprints:Bufnita_LOGO_medium (layer F.Cu) (tedit 0)
    (at 101.3079 166.5351)
    (fp_text reference U5 (at 0 0) (layer F.SilkS) hide)
    (fp_text value Bufnita_Logo (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text Reset (at 93.2688 139.1158) (layer F.SilkS))
  (gr_arc (start 113.665 179.7812) (end 114.3 179.7812) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 89.535 179.7812) (end 89.535 180.4162) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 89.535 101.6) (end 88.9 101.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 113.665 101.6) (end 113.665 100.965) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "GND\n" (at 111.8616 173.9138) (layer B.SilkS))
  (gr_text GND (at 95.6818 156.5656 90) (layer B.SilkS))
  (gr_text Vcc (at 89.5096 156.7688 90) (layer B.SilkS))
  (gr_text PC14 (at 95.6818 159.258 90) (layer B.SilkS))
  (gr_text PC15 (at 89.5096 159.3342 90) (layer B.SilkS))
  (gr_text ADC6 (at 95.6818 161.7218 90) (layer B.SilkS))
  (gr_text ADC5 (at 89.5096 161.8234 90) (layer B.SilkS))
  (gr_text CLK (at 95.6818 164.2872 90) (layer B.SilkS))
  (gr_text NCS (at 89.5096 164.3888 90) (layer B.SilkS))
  (gr_text ADC10 (at 95.6818 166.878 90) (layer B.SilkS))
  (gr_text DAC1 (at 89.5096 166.8526 90) (layer B.SilkS))
  (gr_text IO2 (at 95.6818 169.2656 90) (layer B.SilkS))
  (gr_text IO3 (at 89.5096 169.3926 90) (layer B.SilkS))
  (gr_text IO0 (at 95.6818 171.9072 90) (layer B.SilkS))
  (gr_text IO1 (at 89.5096 171.958 90) (layer B.SilkS))
  (gr_text "GND\n" (at 109.2962 173.9138) (layer B.SilkS))
  (gr_text Vcc (at 111.9378 179.7558) (layer B.SilkS))
  (gr_text PA8 (at 109.22 179.7558) (layer B.SilkS))
  (gr_text SCL (at 106.7816 179.7558) (layer B.SilkS))
  (gr_text SDA (at 106.7816 173.9138) (layer B.SilkS))
  (gr_text CANrx (at 104.2924 179.7558) (layer B.SilkS))
  (gr_text CANtx (at 104.2416 173.9138) (layer B.SilkS))
  (gr_text sck (at 101.7016 173.9138) (layer B.SilkS))
  (gr_text PA15 (at 101.7016 179.7558) (layer B.SilkS))
  (gr_text mosi (at 99.187 173.9138) (layer B.SilkS))
  (gr_text RX (at 96.6724 173.9138) (layer B.SilkS))
  (gr_text TX (at 96.6978 179.7558) (layer B.SilkS))
  (gr_text miso (at 99.2378 179.7558) (layer B.SilkS))
  (gr_text gnd (at 113.3348 158.5468 90) (layer B.SilkS))
  (gr_text io (at 113.3348 156.0068 90) (layer B.SilkS))
  (gr_text clk (at 113.3348 153.5176 90) (layer B.SilkS))
  (gr_text rst (at 113.3348 150.9268 90) (layer B.SilkS))
  (gr_text vcc (at 113.3348 148.463 90) (layer B.SilkS))
  (gr_text SWD (at 108.8898 152.1206 90) (layer B.SilkS))
  (gr_line (start 88.9 106.0704) (end 88.9 101.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.3 106.0704) (end 114.3 101.6) (layer Edge.Cuts) (width 0.15))
  (gr_text Bufnita (at 100.076 128.6764 90) (layer B.SilkS))
  (gr_line (start 88.9 111.506) (end 88.9 106.0704) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.3 111.506) (end 114.3 106.0704) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.9 175.26) (end 88.9 179.7812) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.3 175.26) (end 114.3 179.7812) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.9 175.26) (end 88.9 147.701) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 113.665 180.4162) (end 89.535 180.4162) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.3 147.701) (end 114.3 175.26) (layer Edge.Cuts) (width 0.15))
  (gr_text Rev.5 (at 102.4128 128.67644 90) (layer B.SilkS))
  (gr_text 32bit.fun (at 97.4598 128.6764 90) (layer B.SilkS))
  (gr_text "+3.xV OUT" (at 91.5162 145.4912 90) (layer B.SilkS))
  (gr_text + (at 98.0186 145.4404) (layer B.SilkS))
  (gr_text + (at 98.1964 146.558) (layer F.SilkS))
  (gr_line (start 88.9 129.032) (end 88.9 147.701) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.3 129.032) (end 114.3 147.701) (layer Edge.Cuts) (width 0.15))
  (gr_text "+\n" (at 109.4994 101.9302) (layer B.SilkS))
  (gr_text + (at 111.76 121.3358) (layer B.SilkS))
  (gr_text "LiFePo4\nBattery" (at 108.8136 118.4148 90) (layer B.SilkS))
  (gr_text "Solar 6V" (at 107.5436 104.9274 90) (layer B.SilkS))
  (gr_text + (at 111.76 122.174) (layer F.SilkS))
  (gr_line (start 114.3 129.032) (end 114.3 111.506) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.9 111.506) (end 88.9 129.032) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 89.535 100.965) (end 113.665 100.965) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.9 100.965) (xy 114.3 100.965) (xy 114.3 179.8828) (xy 88.9 179.8828)
      )
    )
  )
)
