(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 25)
    (no_connects 0)
    (area 153.424999 97.924999 178.575001 112.075001)
    (thickness 1.6)
    (drawings 4)
    (tracks 121)
    (zones 0)
    (modules 12)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(64x32_OLED_Display1-Pad1)")
  (net 2 "Net-(64x32_OLED_Display1-Pad2)")
  (net 3 "Net-(64x32_OLED_Display1-Pad3)")
  (net 4 "Net-(64x32_OLED_Display1-Pad4)")
  (net 5 VCC)
  (net 6 Earth)
  (net 7 "Net-(64x32_OLED_Display1-Pad9)")
  (net 8 SCL_3.3V)
  (net 9 SDA_3.3V)
  (net 10 "Net-(64x32_OLED_Display1-Pad12)")
  (net 11 "Net-(64x32_OLED_Display1-Pad13)")
  (net 12 "Net-(64x32_OLED_Display1-Pad14)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net Earth)
    (add_net "Net-(64x32_OLED_Display1-Pad1)")
    (add_net "Net-(64x32_OLED_Display1-Pad12)")
    (add_net "Net-(64x32_OLED_Display1-Pad13)")
    (add_net "Net-(64x32_OLED_Display1-Pad14)")
    (add_net "Net-(64x32_OLED_Display1-Pad2)")
    (add_net "Net-(64x32_OLED_Display1-Pad3)")
    (add_net "Net-(64x32_OLED_Display1-Pad4)")
    (add_net "Net-(64x32_OLED_Display1-Pad9)")
    (add_net SCL_3.3V)
    (add_net SDA_3.3V)
    (add_net VCC)
  )
  (module Library:ZOIC-14 (layer F.Cu) (tedit 5962A524)
    (at 156.4371 105.2381 90)
    (fp_text reference 64x32_OLED_Display1 (at 0.4381 -2.4371 90) (layer F.SilkS))
    (fp_text value LCD1 (at -2.3619 -2.0371 90) (layer F.Fab))
    (pad 1 smd rect (at -4.55 0 90) (size 0.35 2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(64x32_OLED_Display1-Pad1)"))
    (pad 2 smd rect (at -3.85 0 90) (size 0.35 2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(64x32_OLED_Display1-Pad2)"))
    (pad 3 smd rect (at -3.15 0 90) (size 0.35 2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(64x32_OLED_Display1-Pad3)"))
    (pad 4 smd rect (at -2.45 0 90) (size 0.35 2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(64x32_OLED_Display1-Pad4)"))
    (pad 5 smd rect (at -1.75 0 90) (size 0.35 2) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 6 smd rect (at -1.05 0 90) (size 0.35 2) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -0.35 0 90) (size 0.35 2) (layers F.Cu F.Paste F.Mask)
      (net 6 Earth))
    (pad 8 smd rect (at 0.35 0 90) (size 0.35 2) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 9 smd rect (at 1.05 0 90) (size 0.35 2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(64x32_OLED_Display1-Pad9)"))
    (pad 10 smd rect (at 1.75 0 90) (size 0.35 2) (layers F.Cu F.Paste F.Mask)
      (net 8 SCL_3.3V))
    (pad 11 smd rect (at 2.45 0 90) (size 0.35 2) (layers F.Cu F.Paste F.Mask)
      (net 9 SDA_3.3V))
    (pad 12 smd rect (at 3.15 0 90) (size 0.35 2) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(64x32_OLED_Display1-Pad12)"))
    (pad 13 smd rect (at 3.85 0 90) (size 0.35 2) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(64x32_OLED_Display1-Pad13)"))
    (pad 14 smd rect (at 4.55 0 90) (size 0.35 2) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(64x32_OLED_Display1-Pad14)"))
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5962A41D)
    (at 171.3858 100.5022)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 2) (layer F.Fab))
    (fp_text user %R (at -1.8858 -1.5022) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 Earth))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(64x32_OLED_Display1-Pad9)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5962A422)
    (at 164.5691 100.5022)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at -2.5691 -1.5022) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(64x32_OLED_Display1-Pad14)"))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 Earth))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5962A4E0)
    (at 171.3956 102.8166 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at -4.0044 0.2166 180) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 2.8956 -0.1834 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(64x32_OLED_Display1-Pad13)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 Earth))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5962A4C0)
    (at 173.7792 107.5108 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at 3.6892 -0.0208 360) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 3.6892 -0.0208 360) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 Earth))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5962A465)
    (at 164.4134 106.0156 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at 0.2134 0.2156 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0.2134 0.2156 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(64x32_OLED_Display1-Pad3)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(64x32_OLED_Display1-Pad4)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5962A46A)
    (at 164.3486 108.9173)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C6 (at 0.0514 -0.1173) (layer F.SilkS))
    (fp_text value 1uF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0.0514 -0.1173) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(64x32_OLED_Display1-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(64x32_OLED_Display1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Angled_1x04_Pitch2.54mm (layer F.Cu) (tedit 5962A457)
    (at 176.85 108.925 180)
    (descr "Through hole angled socket strip, 1x04, 2.54mm pitch, 8.51mm socket length, single row")
    (tags "Through hole angled socket strip THT 1x04 2.54mm single row")
    (fp_text reference P1 (at 0.05 -2.275 180) (layer F.SilkS))
    (fp_text value CONN_01X04 (at -4.38 9.89 180) (layer F.Fab))
    (fp_text user %R (at 0.05 -2.275 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 Earth))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 SCL_3.3V))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 SDA_3.3V))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Angled_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5962A4BB)
    (at 171.4344 107.5145 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at -3.6855 -0.0344 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 SCL_3.3V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5962A4C4)
    (at 169.0377 107.5309 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at -3.6691 -0.0377 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 SDA_3.3V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5962A4A7)
    (at 159.7864 104.3261 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 4.2739 -0.0136 270) (layer F.SilkS))
    (fp_text value 10K (at -4.7261 -0.0136 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(64x32_OLED_Display1-Pad9)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5962A4D5)
    (at 164.5799 102.8644)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at -2.3799 1.5356) (layer F.SilkS))
    (fp_text value 390K (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(64x32_OLED_Display1-Pad12)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 Earth))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 178.5 112) (end 178.5 98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.5 112) (end 178.5 112) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.5 98) (end 153.5 112) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 178.5 98) (end 153.5 98) (angle 90) (layer Edge.Cuts) (width 0.15))
)
