(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.59)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (33 "F.Adhes" user "F.Adhesive")
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(J8-Pad1)")
  (net 2 "Net-(J9-Pad1)")
  (net 3 "Net-(J1-Pad1)")
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 83.566 35.56)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 81.534 35.56)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 88.646 39.624)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 90.678 39.624)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 91.694 39.624)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 87.122 37.592)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "graflex_helper_board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at 10.414 0) (layer "F.SilkS"))
    (fp_text value "Q_PMOS_GDS" (at 14.478 3.81) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(J1-Pad1)") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(J8-Pad1)") (pinfunction "D") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(J9-Pad1)") (pinfunction "S") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 82.55 35.56)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 83.566 39.624)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 87.63 39.624)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 90.678 35.56)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 86.614 39.624)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 89.662 35.56)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 92.71 35.56)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 91.694 35.56)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 83.312 41.656)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "graflex_helper_board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J8" (at -4.064 -2.54) (layer "F.SilkS"))
    (fp_text value "BATT+" (at -5.588 2.286) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers F&B.Cu *.Mask)
      (net 1 "Net-(J8-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 90.932 33.528)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "graflex_helper_board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J9" (at 5.588 -2.54) (layer "F.SilkS"))
    (fp_text value "PB+" (at 3.81 0.254) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J9-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 83.312 33.528 90)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "graflex_helper_board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J8" (at -4.064 -2.54 90) (layer "F.SilkS"))
    (fp_text value "BATT+" (at -5.588 2.286 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J8-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 87.63 35.56)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 90.932 37.592)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "graflex_helper_board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J9" (at 5.588 -2.54) (layer "F.SilkS"))
    (fp_text value "PB+" (at 3.81 0.254) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers F&B.Cu *.Mask)
      (net 2 "Net-(J9-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 88.646 35.56)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 87.122 41.656)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "graflex_helper_board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at 10.414 0) (layer "F.SilkS"))
    (fp_text value "Q_PMOS_GDS" (at 14.478 3.81) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(J1-Pad1)") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(J8-Pad1)") (pinfunction "D") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(J9-Pad1)") (pinfunction "S") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 92.71 39.624)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 87.122 33.528)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "graflex_helper_board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at 10.414 0) (layer "F.SilkS"))
    (fp_text value "Q_PMOS_GDS" (at 14.478 3.81) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(J1-Pad1)") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(J8-Pad1)") (pinfunction "D") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(J9-Pad1)") (pinfunction "S") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 84.582 35.56)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 81.534 39.624)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 84.582 39.624)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 89.662 39.624)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 86.614 35.56)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 83.312 37.592)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "graflex_helper_board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J8" (at -4.064 -2.54) (layer "F.SilkS"))
    (fp_text value "BATT+" (at -5.588 2.286) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers F&B.Cu *.Mask)
      (net 1 "Net-(J8-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 90.932 41.656)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "graflex_helper_board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J9" (at 5.588 -2.54) (layer "F.SilkS"))
    (fp_text value "PB+" (at 3.81 0.254) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers F&B.Cu *.Mask)
      (net 2 "Net-(J9-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 82.55 39.624)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 85.598 39.624)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 85.598 35.56)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm" (layer "B.Cu")
    (tedit 5DD6EB27)
    (at 88.392 33.528 180)
    (descr "Wire Pad, Square, SMD Pad,  1mm x 2mm,")
    (tags "MesurementPoint Square SMDPad 1mmx2mm ")
    (property "Sheetfile" "graflex_helper_board.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J1" (at -7.874 -1.524) (layer "B.SilkS"))
    (fp_text value "SW" (at 0 -2.54) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at 0 0 180) (size 1 2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 85.852 37.592 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "graflex_helper_board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 6.096 90) (layer "B.SilkS"))
    (fp_text value "100k" (at 0 -1.43 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(J1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(J8-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 85.852 33.528 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "graflex_helper_board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 6.096 90) (layer "B.SilkS"))
    (fp_text value "100k" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(J1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(J8-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm" (layer "B.Cu")
    (tedit 5DD6EB27)
    (at 88.392 37.592 180)
    (descr "Wire Pad, Square, SMD Pad,  1mm x 2mm,")
    (tags "MesurementPoint Square SMDPad 1mmx2mm ")
    (property "Sheetfile" "graflex_helper_board.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J1" (at -7.874 -1.524) (layer "B.SilkS"))
    (fp_text value "SW" (at 0 -2.54) (layer "B.Fab"))
    (pad "1" smd roundrect (at 0 0 180) (size 1 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm" (layer "B.Cu")
    (tedit 5DD6EB27)
    (at 88.392 41.656 180)
    (descr "Wire Pad, Square, SMD Pad,  1mm x 2mm,")
    (tags "MesurementPoint Square SMDPad 1mmx2mm ")
    (property "Sheetfile" "graflex_helper_board.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J1" (at -7.874 -1.524) (layer "B.SilkS"))
    (fp_text value "SW" (at 0 -2.54) (layer "B.Fab"))
    (pad "1" smd roundrect (at 0 0 180) (size 1 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 85.852 41.656 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "graflex_helper_board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 6.096 90) (layer "B.SilkS"))
    (fp_text value "100k" (at 0 -1.43 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(J1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(J8-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 92.456 31.75) (end 92.456 35.306) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 81.788 35.306) (end 81.788 31.75) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 92.456 35.306) (end 92.456 35.814) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 81.788 39.878) (end 81.788 39.37) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 81.788 35.814) (end 81.788 35.306) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 81.788 39.37) (end 81.788 35.814) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 81.788 31.75) (end 92.456 31.75) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 92.456 39.878) (end 92.456 43.434) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 92.456 35.814) (end 92.456 39.37) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 92.456 39.37) (end 92.456 39.878) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 92.456 43.434) (end 81.788 43.434) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 81.788 43.434) (end 81.788 39.878) (layer "Edge.Cuts") (width 0.15))
  (gr_text "BATT" (at 83.566 38.862) (layer "B.SilkS"))
  (gr_text "BRD" (at 90.678 34.798) (layer "B.SilkS"))
  (gr_text "BRD" (at 90.678 42.926) (layer "B.SilkS"))
  (gr_text "BATT" (at 83.566 42.926) (layer "B.SilkS"))
  (gr_text "BRD" (at 90.678 38.862) (layer "B.SilkS"))
  (gr_text "BATT" (at 83.566 34.798) (layer "B.SilkS"))
  (gr_text "SW" (at 87.376 37.846 90) (layer "B.SilkS"))
  (gr_text "SW" (at 87.376 33.782 90) (layer "B.SilkS"))
  (gr_text "SW" (at 87.376 41.91 90) (layer "B.SilkS"))
  (zone (net 2) (net_name "Net-(J9-Pad1)") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.948 39.116)
        (xy 87.884 39.116)
        (xy 87.376 38.608)
        (xy 87.376 37.338)
        (xy 88.138 36.576)
        (xy 91.948 36.576)
      )
    )
  )
  (zone (net 2) (net_name "Net-(J9-Pad1)") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.218 43.942)
        (xy 87.122 43.942)
        (xy 87.122 30.988)
        (xy 93.218 30.988)
      )
    )
  )
  (zone (net 1) (net_name "Net-(J8-Pad1)") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.09 37.338)
        (xy 86.36 37.338)
        (xy 87.122 38.1)
        (xy 87.122 39.116)
        (xy 82.296 39.116)
        (xy 82.296 36.576)
        (xy 84.328 36.576)
      )
    )
  )
  (zone (net 1) (net_name "Net-(J8-Pad1)") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.09 41.402)
        (xy 86.36 41.402)
        (xy 87.122 42.164)
        (xy 87.122 43.18)
        (xy 82.296 43.18)
        (xy 82.296 40.64)
        (xy 84.328 40.64)
      )
    )
  )
  (zone (net 2) (net_name "Net-(J9-Pad1)") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.948 43.18)
        (xy 87.884 43.18)
        (xy 87.376 42.672)
        (xy 87.376 41.402)
        (xy 88.138 40.64)
        (xy 91.948 40.64)
      )
    )
  )
  (zone (net 2) (net_name "Net-(J9-Pad1)") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.948 35.052)
        (xy 87.884 35.052)
        (xy 87.376 34.544)
        (xy 87.376 33.274)
        (xy 88.138 32.512)
        (xy 91.948 32.512)
      )
    )
  )
  (zone (net 1) (net_name "Net-(J8-Pad1)") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.09 33.274)
        (xy 86.36 33.274)
        (xy 87.122 34.036)
        (xy 87.122 35.052)
        (xy 82.296 35.052)
        (xy 82.296 32.512)
        (xy 84.328 32.512)
      )
    )
  )
)
