(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~87~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 16)
    (tracks 34)
    (zones 0)
    (modules 10)
    (nets 44)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 2.76)
    (user_trace_width 2.76)
    (user_trace_width 5.6)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 4.3)
    (pad_drill 0)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 "Net-(D1-Pad1)")
  (net 3 GND)
  (net 4 "Net-(D2-Pad1)")
  (net 5 "Net-(D2-Pad5)")
  (net 6 "Net-(D2-Pad2)")
  (net 7 "Net-(M1-Pad20)")
  (net 8 "Net-(M1-Pad19)")
  (net 9 "Net-(M1-Pad18)")
  (net 10 "Net-(M1-Pad17)")
  (net 11 "Net-(M1-Pad16)")
  (net 12 "Net-(M1-Pad15)")
  (net 13 "Net-(M1-Pad14)")
  (net 14 "Net-(M1-Pad13)")
  (net 15 "Net-(M1-Pad12)")
  (net 16 "Net-(M1-Pad11)")
  (net 17 "Net-(M1-Pad9)")
  (net 18 "Net-(M1-Pad8)")
  (net 19 "Net-(M1-Pad7)")
  (net 20 "Net-(M1-Pad6)")
  (net 21 "Net-(M1-Pad5)")
  (net 22 "Net-(M1-Pad4)")
  (net 23 "Net-(M1-Pad3)")
  (net 24 "Net-(M1-Pad2)")
  (net 25 "Net-(M1-Pad1)")
  (net 26 "Net-(U1-Pad14)")
  (net 27 "Net-(U1-Pad15)")
  (net 28 "Net-(U1-Pad24)")
  (net 29 "Net-(U1-Pad17)")
  (net 30 "Net-(U1-Pad13)")
  (net 31 "Net-(U1-Pad16)")
  (net 32 "Net-(U1-Pad22)")
  (net 33 "Net-(U1-Pad12)")
  (net 34 "Net-(U1-Pad11)")
  (net 35 "Net-(U1-Pad10)")
  (net 36 "Net-(U1-Pad9)")
  (net 37 "Net-(U1-Pad8)")
  (net 38 "Net-(U1-Pad7)")
  (net 39 "Net-(U1-Pad6)")
  (net 40 "Net-(U1-Pad5)")
  (net 41 "Net-(U1-Pad3)")
  (net 42 "Net-(U1-Pad2)")
  (net 43 "Net-(U1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D2-Pad5)")
    (add_net "Net-(M1-Pad1)")
    (add_net "Net-(M1-Pad11)")
    (add_net "Net-(M1-Pad12)")
    (add_net "Net-(M1-Pad13)")
    (add_net "Net-(M1-Pad14)")
    (add_net "Net-(M1-Pad15)")
    (add_net "Net-(M1-Pad16)")
    (add_net "Net-(M1-Pad17)")
    (add_net "Net-(M1-Pad18)")
    (add_net "Net-(M1-Pad19)")
    (add_net "Net-(M1-Pad2)")
    (add_net "Net-(M1-Pad20)")
    (add_net "Net-(M1-Pad3)")
    (add_net "Net-(M1-Pad4)")
    (add_net "Net-(M1-Pad5)")
    (add_net "Net-(M1-Pad6)")
    (add_net "Net-(M1-Pad7)")
    (add_net "Net-(M1-Pad8)")
    (add_net "Net-(M1-Pad9)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
  )
  (module propeller:PropellerMini-Throughole (layer F.Cu) (tedit 60091FBF)
    (at 112.268 54.356)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference U1 (at 1.27 -6.35) (layer F.SilkS) hide)
    (fp_text value Propeller_Mini (at 8.89 8.89 180) (layer F.Fab))
    (fp_text user %R (at 8.89 12.7) (layer F.Fab) hide)
    (pad 14 thru_hole oval (at 17.78 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(U1-Pad14)"))
    (pad 15 thru_hole oval (at 17.78 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(U1-Pad15)"))
    (pad 24 thru_hole circle (at 17.78 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(U1-Pad24)"))
    (pad 17 thru_hole oval (at 17.78 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad17)"))
    (pad 13 thru_hole oval (at 17.78 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(U1-Pad13)"))
    (pad 16 thru_hole oval (at 17.78 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(U1-Pad16)"))
    (pad 18 thru_hole oval (at 17.78 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(M1-Pad3)"))
    (pad 22 thru_hole oval (at 17.78 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(U1-Pad22)"))
    (pad 23 thru_hole oval (at 17.78 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 19 thru_hole oval (at 17.78 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(M1-Pad2)"))
    (pad 20 thru_hole oval (at 17.78 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (pad 21 thru_hole oval (at 17.78 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(U1-Pad12)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(U1-Pad11)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(U1-Pad10)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(U1-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(U1-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(U1-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(U1-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(U1-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(M1-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(U1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(U1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(U1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x12_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.5mm_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 107.442 53.34)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference "" (at 0 -3.5) (layer F.SilkS))
    (fp_text value MountingHole_2.5mm_Pad_TopBottom (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.9 2.9) (drill 2.5) (layers *.Cu *.Mask))
    (pad 1 connect circle (at 0 0) (size 5 5) (layers F.Cu F.Mask))
    (pad 1 connect circle (at 0 0) (size 5 5) (layers B.Cu B.Mask))
  )
  (module MountingHole:MountingHole_2.5mm_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 107.442 82.55)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm_Pad_TopBottom (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 connect circle (at 0 0) (size 5 5) (layers B.Cu B.Mask))
    (pad 1 connect circle (at 0 0) (size 5 5) (layers F.Cu F.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 2.9 2.9) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 161.29 82.55)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm_Pad_TopBottom (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.9 2.9) (drill 2.5) (layers *.Cu *.Mask))
    (pad 1 connect circle (at 0 0) (size 5 5) (layers F.Cu F.Mask))
    (pad 1 connect circle (at 0 0) (size 5 5) (layers B.Cu B.Mask))
  )
  (module MountingHole:MountingHole_2.5mm_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 161.29 53.34)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm_Pad_TopBottom (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 connect circle (at 0 0) (size 5 5) (layers B.Cu B.Mask))
    (pad 1 connect circle (at 0 0) (size 5 5) (layers F.Cu F.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 2.9 2.9) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module RF-Sparkfun:XBEE-SMD (layer F.Cu) (tedit 200000)
    (at 148.59 80.01)
    (descr "DIGI XBEE AND XBEE-PRO RF MODULES (SMD PADS)")
    (tags "DIGI XBEE AND XBEE-PRO RF MODULES (SMD PADS)")
    (attr smd)
    (fp_text reference M1 (at 8.89 3.81) (layer F.SilkS) hide)
    (fp_text value XBEE (at 0 -20.828) (layer F.SilkS))
    (fp_text user 1 (at -8.9916 -20.50796) (layer F.SilkS))
    (pad 20 smd rect (at 9.4996 -19.99996 90) (size 0.84836 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(M1-Pad20)") (solder_mask_margin 0.1016))
    (pad 19 smd rect (at 12.49934 -17.99844 90) (size 0.84836 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(M1-Pad19)") (solder_mask_margin 0.1016))
    (pad 18 smd rect (at 9.4996 -15.99946 90) (size 0.84836 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(M1-Pad18)") (solder_mask_margin 0.1016))
    (pad 17 smd rect (at 12.49934 -13.99794 90) (size 0.84836 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(M1-Pad17)") (solder_mask_margin 0.1016))
    (pad 16 smd rect (at 9.4996 -11.99896 90) (size 0.84836 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(M1-Pad16)") (solder_mask_margin 0.1016))
    (pad 15 smd rect (at 12.49934 -9.99998 90) (size 0.84836 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(M1-Pad15)") (solder_mask_margin 0.1016))
    (pad 14 smd rect (at 9.4996 -7.99846 90) (size 0.84836 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(M1-Pad14)") (solder_mask_margin 0.1016))
    (pad 13 smd rect (at 12.49934 -5.99948 90) (size 0.84836 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(M1-Pad13)") (solder_mask_margin 0.1016))
    (pad 12 smd rect (at 9.4996 -3.99796 90) (size 0.84836 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(M1-Pad12)") (solder_mask_margin 0.1016))
    (pad 11 smd rect (at 12.49934 -1.99898 90) (size 0.84836 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(M1-Pad11)") (solder_mask_margin 0.1016))
    (pad 10 smd rect (at -9.4996 -1.99898 90) (size 0.84836 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_mask_margin 0.1016))
    (pad 9 smd rect (at -12.49934 -3.99796 90) (size 0.84836 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(M1-Pad9)") (solder_mask_margin 0.1016))
    (pad 8 smd rect (at -9.4996 -5.99948 90) (size 0.84836 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(M1-Pad8)") (solder_mask_margin 0.1016))
    (pad 7 smd rect (at -12.49934 -7.99846 90) (size 0.84836 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(M1-Pad7)") (solder_mask_margin 0.1016))
    (pad 6 smd rect (at -9.4996 -9.99998 90) (size 0.84836 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(M1-Pad6)") (solder_mask_margin 0.1016))
    (pad 5 smd rect (at -12.49934 -11.99896 90) (size 0.84836 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(M1-Pad5)") (solder_mask_margin 0.1016))
    (pad 4 smd rect (at -9.4996 -13.99794 90) (size 0.84836 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(M1-Pad4)") (solder_mask_margin 0.1016))
    (pad 3 smd rect (at -12.49934 -15.99946 90) (size 0.84836 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(M1-Pad3)") (solder_mask_margin 0.1016))
    (pad 2 smd rect (at -9.4996 -17.99844 90) (size 0.84836 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(M1-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -12.49934 -19.99996 90) (size 0.84836 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(M1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 600C6320)
    (at 141.732 82.55 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value RGB (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND) (zone_connect 1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RobsDigiKeyLibs:WS2812_SMD (layer B.Cu) (tedit 600C6361)
    (at 120.396 55.626 180)
    (fp_text reference D2 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value WS2812-3in-3out (at 0 0.5) (layer B.Fab) hide)
    (pad 6 smd roundrect (at 2.54 -19.54 180) (size 2 4.3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 3 GND) (zone_connect 1) (thermal_width 2) (thermal_gap 2))
    (pad 1 smd roundrect (at 0 -19.54 180) (size 2 4.3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 4 "Net-(D2-Pad1)"))
    (pad 5 smd roundrect (at -2.54 -19.54 180) (size 2 4.3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 5 "Net-(D2-Pad5)"))
    (pad 4 smd roundrect (at 2.54 -2.54 180) (size 2 4.299999) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 3 GND))
    (pad 2 smd roundrect (at 0 -2.54 180) (size 2 4.3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 6 "Net-(D2-Pad2)"))
    (pad 3 smd roundrect (at -2.54 -2.54 180) (size 2 4.3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 2 "Net-(D1-Pad1)"))
  )
  (module digi_footprints:CUI_PJ-037AH (layer F.Cu) (tedit 600C6338)
    (at 151.892 71.12 270)
    (fp_text reference J1 (at 2.675 -5.635 90) (layer F.SilkS))
    (fp_text value Barrel_Jack (at 7.12 5.635 270) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 6 0 270) (size 2.25 4.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 3 GND) (zone_connect 1))
    (pad 1 thru_hole oval (at 0 0 270) (size 2.5 5) (drill oval 1 3.5) (layers *.Cu *.Mask)
      (net 1 +5V))
  )
  (module RobsDigiKeyLibs:RRE02VTM4SFHTR (layer F.Cu) (tedit 0)
    (at 120.65 67.31)
    (fp_text reference D1 (at 0 2.54) (layer F.SilkS))
    (fp_text value D_Small (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text user 0.033in/0.838mm (at 3.7592 0) (layer Dwgs.User))
    (fp_text user * (at -1.9304 0) (layer F.SilkS))
    (fp_text user * (at -0.7493 0) (layer F.Fab))
    (fp_text user 0.018in/0.457mm (at -1.3208 -3.4163) (layer Dwgs.User))
    (fp_text user * (at -0.7493 0) (layer F.Fab))
    (fp_text user * (at -1.9304 0) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 2 smd rect (at 1.3208 0) (size 0.4572 0.8382) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at -1.3208 0) (size 0.4572 0.8382) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad1)"))
  )
  (gr_line (start 165.1 49.53) (end 103.632 49.53) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 165.1 86.36) (end 165.1 49.53) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 103.632 86.36) (end 165.1 86.36) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 103.632 49.53) (end 103.632 86.36) (layer Edge.Cuts) (width 0.05))
  (gr_text DO (at 120.396 78.994 270) (layer B.SilkS))
  (gr_text +5 (at 123.19 78.994 270) (layer B.SilkS))
  (gr_text +5 (at 122.936 54.356 270) (layer B.SilkS))
  (gr_text DIN (at 120.396 54.102 270) (layer B.SilkS))
  (gr_text GND (at 117.856 54.102 270) (layer B.SilkS))
  (gr_text GND (at 117.856 79.502 270) (layer B.SilkS))
  (gr_text GND (at 117.856 79.248) (layer B.Cu))
  (gr_text GND (at 141.732 80.772) (layer F.SilkS))
  (gr_text DAT (at 139.192 80.772) (layer F.SilkS))
  (gr_text +5 (at 136.398 80.772) (layer F.SilkS))
  (gr_text GND (at 147.828 75.184) (layer F.SilkS))
  (gr_text +5v (at 148.59 68.58) (layer F.SilkS))
  (zone (net 0) (net_name "") (layer Dwgs.User) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 165.1 86.36) (xy 104.14 86.36) (xy 104.14 49.53) (xy 165.1 49.53)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 165.1 86.36) (xy 103.632 86.36) (xy 103.632 49.53) (xy 165.1 49.53)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 165.1 86.36) (xy 103.632 86.36) (xy 103.632 49.53) (xy 165.1 49.53)
      )
    )
  )
)
