(kicad_pcb (version 20171130) (host pcbnew "(5.1.8)-1")
  (general
    (thickness 1.6)
    (drawings 39)
    (tracks 117)
    (zones 0)
    (modules 14)
    (nets 23)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user hide)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad2)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(J1-Pad14)")
  (net 7 "Net-(J1-Pad13)")
  (net 8 "Net-(J1-Pad12)")
  (net 9 "Net-(J1-Pad11)")
  (net 10 "Net-(J1-Pad10)")
  (net 11 "Net-(J1-Pad7)")
  (net 12 "Net-(J1-Pad5)")
  (net 13 "Net-(J1-Pad4)")
  (net 14 "Net-(J1-Pad3)")
  (net 15 "Net-(J1-Pad2)")
  (net 16 "Net-(J1-Pad1)")
  (net 17 "Net-(J2-Pad6)")
  (net 18 "Net-(J2-Pad5)")
  (net 19 "Net-(J2-Pad4)")
  (net 20 "Net-(J2-Pad3)")
  (net 21 "Net-(J2-Pad2)")
  (net 22 "Net-(J2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
  )
  (module Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 59.69 60.96 270)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D4 (at 5.08 -2.47 90) (layer F.SilkS))
    (fp_text value 1N4004 (at 5.08 2.47 90) (layer F.Fab))
    (fp_text user K (at 0 -2.1 90) (layer F.SilkS))
    (fp_text user K (at 0 -2.1 90) (layer F.Fab))
    (fp_text user %R (at 5.47 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relay_SMD:Relay_DPDT_Omron_G6K-2F-Y (layer F.Cu) (tedit 5A565DE2)
    (at 71.12 48.26 90)
    (descr "Omron G6K-2F-Y relay package http://omronfs.omron.com/en_US/ecb/products/pdf/en-g6k.pdf")
    (tags "Omron G6K-2F-Y relay")
    (attr smd)
    (fp_text reference K3 (at 0 -6 90) (layer F.SilkS))
    (fp_text value G6K-2 (at -0.04 6.3 90) (layer F.Fab))
    (fp_text user %R (at 0.01 0 90) (layer F.Fab))
    (pad 1 smd rect (at -3.5 -3.8 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at -3.5 -0.6 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J2-Pad5)"))
    (pad 3 smd rect (at -3.5 1.6 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J2-Pad5)"))
    (pad 4 smd rect (at -3.5 3.8 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad7)"))
    (pad 5 smd rect (at 3.5 3.8 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 6 smd rect (at 3.5 1.6 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J2-Pad6)"))
    (pad 7 smd rect (at 3.5 -0.6 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J2-Pad6)"))
    (pad 8 smd rect (at 3.5 -3.8 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Relay_SMD.3dshapes/Relay_DPDT_Omron_G6K-2F-Y.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relay_SMD:Relay_DPDT_Omron_G6K-2F-Y (layer F.Cu) (tedit 5A565DE2)
    (at 71.12 62.23 90)
    (descr "Omron G6K-2F-Y relay package http://omronfs.omron.com/en_US/ecb/products/pdf/en-g6k.pdf")
    (tags "Omron G6K-2F-Y relay")
    (attr smd)
    (fp_text reference K2 (at 0 -6 90) (layer F.SilkS))
    (fp_text value G6K-2 (at -0.04 6.3 90) (layer F.Fab))
    (fp_text user %R (at 0.01 0 90) (layer F.Fab))
    (pad 1 smd rect (at -3.5 -3.8 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -3.5 -0.6 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J2-Pad3)"))
    (pad 3 smd rect (at -3.5 1.6 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J2-Pad3)"))
    (pad 4 smd rect (at -3.5 3.8 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at 3.5 3.8 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at 3.5 1.6 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J2-Pad4)"))
    (pad 7 smd rect (at 3.5 -0.6 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J2-Pad4)"))
    (pad 8 smd rect (at 3.5 -3.8 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Relay_SMD.3dshapes/Relay_DPDT_Omron_G6K-2F-Y.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relay_SMD:Relay_DPDT_Omron_G6K-2F-Y (layer F.Cu) (tedit 5A565DE2)
    (at 71.12 76.2 90)
    (descr "Omron G6K-2F-Y relay package http://omronfs.omron.com/en_US/ecb/products/pdf/en-g6k.pdf")
    (tags "Omron G6K-2F-Y relay")
    (attr smd)
    (fp_text reference K1 (at 0 -6 90) (layer F.SilkS))
    (fp_text value G6K-2 (at -0.04 6.3 90) (layer F.Fab))
    (fp_text user %R (at 0.01 0 90) (layer F.Fab))
    (pad 1 smd rect (at -3.5 -3.8 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at -3.5 -0.6 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at -3.5 1.6 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J2-Pad1)"))
    (pad 4 smd rect (at -3.5 3.8 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J1-Pad2)"))
    (pad 5 smd rect (at 3.5 3.8 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J1-Pad3)"))
    (pad 6 smd rect (at 3.5 1.6 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J2-Pad2)"))
    (pad 7 smd rect (at 3.5 -0.6 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J2-Pad2)"))
    (pad 8 smd rect (at 3.5 -3.8 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Relay_SMD.3dshapes/Relay_DPDT_Omron_G6K-2F-Y.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 54.61 74.93 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 54.61 63.5 180)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x08 (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 0 8.89 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x14_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 81.28 78.74 180)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x14 (at 0 35.35) (layer F.Fab))
    (fp_text user %R (at 0 16.51 90) (layer F.Fab))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad14)"))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad13)"))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad12)"))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad11)"))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad7)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad5)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x14_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer B.Cu) (tedit 58645DC7)
    (at 67.31 48.26 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D3 (at 0 2 270) (layer B.SilkS))
    (fp_text value 1N4148W (at 0 -2.1 270) (layer B.Fab))
    (fp_text user %R (at 0 2 270) (layer B.Fab))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer B.Cu) (tedit 58645DC7)
    (at 67.31 62.23 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D2 (at 0 2 270) (layer B.SilkS))
    (fp_text value 1N4148W (at 0 -2.1 270) (layer B.Fab))
    (fp_text user %R (at 0 2 270) (layer B.Fab))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer B.Cu) (tedit 58645DC7)
    (at 67.31 76.2 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 0 2 270) (layer B.SilkS))
    (fp_text value 1N4148W (at 0 -2.1 270) (layer B.Fab))
    (fp_text user %R (at 0 2 270) (layer B.Fab))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P2.50mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 59.69 73.66 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm 5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm 5.00mm  length 7mm width 3.5mm Capacitor")
    (fp_text reference C4 (at 2.5 -3 90) (layer F.SilkS))
    (fp_text value C (at 2.5 3 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 3.75 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 1.25 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P2.50mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P2.50mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 63.5 50.8 90)
    (descr "C, Rect series, Radial, pin pitch=2.50mm 5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm 5.00mm  length 7mm width 3.5mm Capacitor")
    (fp_text reference C3 (at 2.5 -3 90) (layer F.SilkS))
    (fp_text value C (at 2.5 3 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 3.75 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (pad 1 thru_hole circle (at 1.25 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P2.50mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P2.50mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 63.5 59.69 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm 5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm 5.00mm  length 7mm width 3.5mm Capacitor")
    (fp_text reference C2 (at 2.5 -3 90) (layer F.SilkS))
    (fp_text value C (at 2.5 3 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 3.75 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 1.25 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P2.50mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P2.50mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 63.5 73.66 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm 5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm 5.00mm  length 7mm width 3.5mm Capacitor")
    (fp_text reference C1 (at 2.5 -3 90) (layer F.SilkS))
    (fp_text value C (at 2.5 3 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.25 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 3.75 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P2.50mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "KØTF © 2020" (at 63.5 41.91) (layer B.Cu))
  (gr_text "KØTF © 2020" (at 85.09 67.31 90) (layer F.Cu))
  (gr_text "K0TF (c) 2020" (at 59.69 81.28) (layer B.SilkS))
  (gr_line (start 49.53 39.37) (end 49.53 83.82) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 87.63 39.37) (end 49.53 39.37) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 87.63 83.82) (end 87.63 39.37) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 49.53 83.82) (end 87.63 83.82) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 52.07 41.91) (end 50.8 40.64) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 85.09 81.28) (end 86.36 80.01) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 52.07 81.28) (end 53.34 80.01) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 85.09 41.91) (end 83.82 40.64) (layer Edge.Cuts) (width 0.05))
  (gr_text "HL1.2KFX\n+15V PWR" (at 57.15 73.66 90) (layer B.SilkS))
  (gr_text "TO HL1.2 KFX BAND SWITCH" (at 57.15 54.61 90) (layer B.SilkS))
  (gr_text "TO BCD14 BAND DECODER" (at 78.74 63.5 90) (layer B.SilkS))
  (gr_text GND (at 54.61 69.85) (layer F.SilkS))
  (gr_text GND (at 57.15 72.39) (layer F.SilkS))
  (gr_text +15V (at 57.15 74.93) (layer F.SilkS))
  (gr_text "BAND SW\nGND" (at 58.42 48.26) (layer F.SilkS))
  (gr_text 24/28 (at 58.42 50.8) (layer F.SilkS))
  (gr_text 17/21 (at 58.42 53.34) (layer F.SilkS))
  (gr_text 10/14 (at 58.42 55.88) (layer F.SilkS))
  (gr_text 7.0 (at 57.15 58.42) (layer F.SilkS))
  (gr_text 3.5 (at 57.15 60.96) (layer F.SilkS))
  (gr_text 1.8 (at 57.15 63.5) (layer F.SilkS))
  (gr_text +15V (at 58.42 45.72) (layer F.SilkS))
  (gr_text AUX (at 78.74 45.72) (layer F.SilkS))
  (gr_text 440 (at 78.74 48.26) (layer F.SilkS))
  (gr_text 2 (at 78.74 50.8) (layer F.SilkS))
  (gr_text 6 (at 78.74 53.34) (layer F.SilkS))
  (gr_text 10 (at 78.74 55.88) (layer F.SilkS))
  (gr_text 12 (at 78.74 58.42) (layer F.SilkS))
  (gr_text 15 (at 78.74 60.96) (layer F.SilkS))
  (gr_text 17 (at 78.74 63.5) (layer F.SilkS))
  (gr_text 20 (at 78.74 66.04) (layer F.SilkS))
  (gr_text 30 (at 78.74 68.58) (layer F.SilkS))
  (gr_text 40 (at 78.74 71.12) (layer F.SilkS))
  (gr_text 80 (at 78.74 73.66) (layer F.SilkS))
  (gr_text 160 (at 78.74 76.2) (layer F.SilkS))
  (gr_text "AUX 0" (at 78.74 78.74) (layer F.SilkS))
)
