(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 58)
    (no_connects 3)
    (area 54.509999 74.829999 191.870001 90.270001)
    (thickness 1.6)
    (drawings 114)
    (tracks 293)
    (zones 0)
    (modules 35)
    (nets 46)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.3 5.6)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory share/))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 "Net-(JP1-Pad2)")
  (net 3 "Net-(JP2-Pad2)")
  (net 4 "Net-(JP3-Pad2)")
  (net 5 "Net-(P1-Pad3)")
  (net 6 "Net-(P1-Pad2)")
  (net 7 "Net-(P2-Pad3)")
  (net 8 "Net-(P2-Pad2)")
  (net 9 GND)
  (net 10 "Net-(P3-Pad3)")
  (net 11 "Net-(P4-Pad3)")
  (net 12 "Net-(P4-Pad2)")
  (net 13 "Net-(P5-Pad3)")
  (net 14 "Net-(P5-Pad2)")
  (net 15 "Net-(P5-Pad1)")
  (net 16 "Net-(P6-Pad1)")
  (net 17 "Net-(P6-Pad2)")
  (net 18 "Net-(P6-Pad3)")
  (net 19 "Net-(R1-Pad1)")
  (net 20 "Net-(R3-Pad1)")
  (net 21 "Net-(R5-Pad1)")
  (net 22 "Net-(R7-Pad1)")
  (net 23 "Net-(R10-Pad2)")
  (net 24 "Net-(R12-Pad2)")
  (net 25 "Net-(R14-Pad2)")
  (net 26 "Net-(R16-Pad2)")
  (net 27 "Net-(P3-Pad2)")
  (net 28 ~RST)
  (net 29 INTB)
  (net 30 INTA)
  (net 31 "Net-(P3-Pad1)")
  (net 32 ~CS)
  (net 33 SCK)
  (net 34 MOSI)
  (net 35 MISO)
  (net 36 "Net-(P2-Pad1)")
  (net 37 "Net-(R2-Pad1)")
  (net 38 "Net-(R4-Pad1)")
  (net 39 "Net-(R6-Pad1)")
  (net 40 "Net-(R8-Pad1)")
  (net 41 "Net-(R11-Pad2)")
  (net 42 "Net-(R13-Pad2)")
  (net 43 "Net-(R15-Pad2)")
  (net 44 "Net-(R17-Pad2)")
  (net 45 "Net-(JP4-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net INTA)
    (add_net INTB)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(JP3-Pad2)")
    (add_net "Net-(JP4-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad3)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(P5-Pad3)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P6-Pad2)")
    (add_net "Net-(P6-Pad3)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net SCK)
    (add_net VCC)
    (add_net ~CS)
    (add_net ~RST)
  )
  (module Housings_SOIC:SOIC-28_7.5x17.9mm_Pitch1.27mm (layer F.Cu) (tedit 54130A77)
    (at 80.391 82.296 270)
    (descr "28-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -8.255 270) (layer F.SilkS))
    (fp_text value MCP23S17 (at 0 10.05 270) (layer F.Fab) hide)
    (pad 28 smd rect (at 4.7 -8.255 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R10-Pad2)"))
    (pad 27 smd rect (at 4.7 -6.985 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R11-Pad2)"))
    (pad 26 smd rect (at 4.7 -5.715 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R12-Pad2)"))
    (pad 25 smd rect (at 4.7 -4.445 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R13-Pad2)"))
    (pad 24 smd rect (at 4.7 -3.175 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R14-Pad2)"))
    (pad 23 smd rect (at 4.7 -1.905 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R15-Pad2)"))
    (pad 22 smd rect (at 4.7 -0.635 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R16-Pad2)"))
    (pad 21 smd rect (at 4.7 0.635 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R17-Pad2)"))
    (pad 20 smd rect (at 4.7 1.905 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 INTA))
    (pad 19 smd rect (at 4.7 3.175 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 INTB))
    (pad 18 smd rect (at 4.7 4.445 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 ~RST))
    (pad 17 smd rect (at 4.7 5.715 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(JP1-Pad2)"))
    (pad 16 smd rect (at 4.7 6.985 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(JP2-Pad2)"))
    (pad 15 smd rect (at 4.7 8.255 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(JP3-Pad2)"))
    (pad 14 smd rect (at -4.7 8.255 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 MISO))
    (pad 13 smd rect (at -4.7 6.985 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 MOSI))
    (pad 12 smd rect (at -4.7 5.715 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 SCK))
    (pad 11 smd rect (at -4.7 4.445 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 ~CS))
    (pad 10 smd rect (at -4.7 3.175 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 GND))
    (pad 9 smd rect (at -4.7 1.905 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 8 smd rect (at -4.7 0.635 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R8-Pad1)"))
    (pad 7 smd rect (at -4.7 -0.635 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R7-Pad1)"))
    (pad 6 smd rect (at -4.7 -1.905 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R6-Pad1)"))
    (pad 5 smd rect (at -4.7 -3.175 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R5-Pad1)"))
    (pad 4 smd rect (at -4.7 -4.445 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R4-Pad1)"))
    (pad 3 smd rect (at -4.7 -5.715 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at -4.7 -6.985 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R2-Pad1)"))
    (pad 1 smd rect (at -4.7 -8.255 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R1-Pad1)"))
    (model Housings_SOIC.3dshapes/SOIC-28_7.5x17.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 164.145 83.439 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value R (at 0 2.1 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R14-Pad2)"))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(P5-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 96.393 82.296)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -3.048 0) (layer F.SilkS))
    (fp_text value R (at 0 2.1) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(P2-Pad1)"))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 96.393 77.724)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -3.048 0) (layer F.SilkS))
    (fp_text value R (at 0 2.1) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(P1-Pad2)"))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 96.393 80.01)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -3.048 0) (layer F.SilkS))
    (fp_text value R (at 0 2.1) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(P1-Pad3)"))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 123.19 83.185)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 2.032) (layer F.SilkS))
    (fp_text value R (at 0 2.1) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(P2-Pad2)"))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 128.524 83.439)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 1.905) (layer F.SilkS))
    (fp_text value R (at 0 2.1) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(P2-Pad3)"))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R5-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 133.604 83.439)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 1.905) (layer F.SilkS))
    (fp_text value R (at 0 2.1) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(P3-Pad1)"))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R6-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 138.43 83.439)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 1.905) (layer F.SilkS))
    (fp_text value R (at 0 2.1) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(P3-Pad2)"))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R7-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 143.83 83.439)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 1.905) (layer F.SilkS))
    (fp_text value R (at 0 2.1) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P3-Pad3)"))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R8-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 57.15 85.725 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 2.54 0 360) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 GND))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(JP3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 184.404 83.439 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value R (at 0 2.1 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R10-Pad2)"))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(P4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 179.3265 83.439 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0.0025 -1.905 180) (layer F.SilkS))
    (fp_text value R (at 0 2.1 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R11-Pad2)"))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(P4-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 173.99 83.439 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value R (at 0 2.1 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R12-Pad2)"))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(P5-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 168.59 83.439 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 0.061 -1.905 180) (layer F.SilkS))
    (fp_text value R (at 0 2.1 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R13-Pad2)"))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(P5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 159.004 83.439 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value R (at 0 2.1 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R15-Pad2)"))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(P6-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 153.67 83.439 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value R (at 0 2.1 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R16-Pad2)"))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(P6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 148.91 83.439 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value R (at 0 2.1 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R17-Pad2)"))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(P6-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 59.69 85.725 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at 2.54 0 360) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 GND))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(JP2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 62.23 85.725 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R19 (at 2.54 -0.254 360) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 GND))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(JP1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:card_edge_3_conductor (layer F.Cu) (tedit 56E1AE2E)
    (at 109.22 78.232)
    (fp_text reference P1 (at 0 4.191) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at -0.127 -5.08) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at -5.08 0) (size 2.25 6) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 9 GND))
    (pad 2 thru_hole rect (at 0 0) (size 2.25 6) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P1-Pad2)"))
    (pad 3 thru_hole rect (at 5.08 0) (size 2.25 6) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P1-Pad3)"))
  )
  (module .pretty:card_edge_3_conductor (layer F.Cu) (tedit 56E1AE2E)
    (at 124.46 78.232)
    (fp_text reference P2 (at 0 4.191) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at -0.127 -5.08) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at -5.08 0) (size 2.25 6) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(P2-Pad1)"))
    (pad 2 thru_hole rect (at 0 0) (size 2.25 6) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P2-Pad2)"))
    (pad 3 thru_hole rect (at 5.08 0) (size 2.25 6) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P2-Pad3)"))
  )
  (module .pretty:card_edge_3_conductor (layer F.Cu) (tedit 56E1AE2E)
    (at 185.42 78.232 180)
    (fp_text reference P4 (at 0 4.191 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at -0.127 -5.08 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at -5.08 0 180) (size 2.25 6) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 9 GND))
    (pad 2 thru_hole rect (at 0 0 180) (size 2.25 6) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P4-Pad2)"))
    (pad 3 thru_hole rect (at 5.08 0 180) (size 2.25 6) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P4-Pad3)"))
  )
  (module .pretty:card_edge_3_conductor (layer F.Cu) (tedit 56E1AE2E)
    (at 170.18 78.232 180)
    (fp_text reference P5 (at 0 4.191 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at -0.127 -5.08 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at -5.08 0 180) (size 2.25 6) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P5-Pad1)"))
    (pad 2 thru_hole rect (at 0 0 180) (size 2.25 6) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P5-Pad2)"))
    (pad 3 thru_hole rect (at 5.08 0 180) (size 2.25 6) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P5-Pad3)"))
  )
  (module .pretty:card_edge_3_conductor (layer F.Cu) (tedit 56E1AE2E)
    (at 154.94 78.232 180)
    (fp_text reference P6 (at 0 4.191 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at -0.127 -5.08 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at -5.08 0 180) (size 2.25 6) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P6-Pad1)"))
    (pad 2 thru_hole rect (at 0 0 180) (size 2.25 6) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P6-Pad2)"))
    (pad 3 thru_hole rect (at 5.08 0 180) (size 2.25 6) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P6-Pad3)"))
  )
  (module .pretty:card_edge_3_conductor (layer F.Cu) (tedit 56E1AE2E)
    (at 139.7 78.232)
    (fp_text reference P3 (at 0 4.191) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at -0.127 -5.08) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at -5.08 0) (size 2.25 6) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(P3-Pad1)"))
    (pad 2 thru_hole rect (at 0 0) (size 2.25 6) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(P3-Pad2)"))
    (pad 3 thru_hole rect (at 5.08 0) (size 2.25 6) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P3-Pad3)"))
  )
  (module .pretty:1814676 (layer B.Cu) (tedit 5A28493A)
    (at 65.178 84.114)
    (fp_text reference J1 (at 0 6.223) (layer B.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 7.747) (layer B.Fab) hide)
    (pad 1 smd rect (at -6.25 -3.85) (size 1.4 3.4) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at -3.75 -3.85) (size 1.4 3.4) (layers B.Cu B.Paste B.Mask)
      (net 9 GND))
    (pad 3 smd rect (at -1.25 -3.85) (size 1.4 3.4) (layers B.Cu B.Paste B.Mask)
      (net 32 ~CS))
    (pad 4 smd rect (at 1.25 -3.85) (size 1.4 3.4) (layers B.Cu B.Paste B.Mask)
      (net 33 SCK))
    (pad 5 smd rect (at 3.75 -3.85) (size 1.4 3.4) (layers B.Cu B.Paste B.Mask)
      (net 34 MOSI))
    (pad 6 smd rect (at 6.25 -3.85) (size 1.4 3.4) (layers B.Cu B.Paste B.Mask)
      (net 35 MISO))
    (pad 7 smd rect (at 8.85 2.75) (size 2.3 5.6) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at -8.85 2.75) (size 2.3 5.6) (layers B.Cu B.Paste B.Mask))
    (model "C:/Program Files/KiCad/3D lib/Junes.3dshapes/1814676_00.step"
      (at (xyz -0.3031496062992126 0.2519685039370079 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module .pretty:SOLDER-JUMPER_1-WAY (layer F.Cu) (tedit 59949359)
    (at 62.23 79.502 270)
    (fp_text reference JP1 (at 0 1.905 270) (layer F.SilkS) hide)
    (fp_text value Jumper_NO_Small (at 0 0 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.65 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(JP1-Pad2)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
  )
  (module .pretty:SOLDER-JUMPER_1-WAY (layer F.Cu) (tedit 59949359)
    (at 59.69 79.502 270)
    (fp_text reference JP2 (at 0 1.905 270) (layer F.SilkS) hide)
    (fp_text value Jumper_NO_Small (at 0 0 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.65 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(JP2-Pad2)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
  )
  (module .pretty:SOLDER-JUMPER_1-WAY (layer F.Cu) (tedit 59949359)
    (at 57.15 79.502 270)
    (fp_text reference JP3 (at 0 1.905 270) (layer F.SilkS) hide)
    (fp_text value Jumper_NO_Small (at 0 0 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.65 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(JP3-Pad2)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
  )
  (module .pretty:Wire_Pad5x2.5mm (layer B.Cu) (tedit 570699EE)
    (at 87.884 80.518 90)
    (fp_text reference J2 (at 0 -2.25 90) (layer B.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.25 90) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0 90) (size 5 2.5) (layers B.Cu B.Paste B.Mask)
      (net 30 INTA))
  )
  (module .pretty:Wire_Pad5x2.5mm (layer B.Cu) (tedit 570699EE)
    (at 84.328 80.518 90)
    (fp_text reference J3 (at 0 -2.25 90) (layer B.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.25 90) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0 90) (size 5 2.5) (layers B.Cu B.Paste B.Mask)
      (net 29 INTB))
  )
  (module .pretty:Wire_Pad5x2.5mm (layer B.Cu) (tedit 570699EE)
    (at 80.772 80.518 90)
    (fp_text reference J4 (at 0 -2.25 90) (layer B.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.25 90) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0 90) (size 5 2.5) (layers B.Cu B.Paste B.Mask)
      (net 28 ~RST))
  )
  (module .pretty:SOLDER-JUMPER_1-WAY (layer F.Cu) (tedit 5A8DDD87)
    (at 69.342 88.265)
    (fp_text reference JP4 (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Jumper_NO_Small (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.65 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(JP4-Pad1)"))
    (pad 2 smd rect (at 0.65 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 28 ~RST))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 65.659 88.265)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R20 (at 0 -1.905) (layer F.SilkS))
    (fp_text value R (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(JP4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text RST (at 69.215 86.233) (layer F.SilkS))
  (gr_text A7 (at 185.42 87.63 90) (layer B.SilkS))
  (gr_text GPIOA (at 167.64 87.63) (layer B.SilkS))
  (gr_text A0 (at 149.86 87.63 90) (layer B.SilkS))
  (gr_text "B7\n" (at 144.78 87.63 90) (layer B.SilkS))
  (gr_text GPIOB (at 127 87.63) (layer B.SilkS))
  (gr_text B0 (at 109.22 87.63 90) (layer B.SilkS))
  (gr_text MISO (at 58.928 76.708 270) (layer B.SilkS))
  (gr_text INTA (at 87.884 76.708) (layer B.SilkS))
  (gr_text 5V (at 71.374 76.708 270) (layer B.SilkS))
  (gr_text GND (at 68.834 76.708 270) (layer B.SilkS))
  (gr_text ~CS (at 66.294 76.708 270) (layer B.SilkS))
  (gr_text SCK (at 63.754 76.708 270) (layer B.SilkS))
  (gr_text MOSI (at 61.341 76.708 270) (layer B.SilkS))
  (gr_text A2 (at 62.23 81.788) (layer F.SilkS))
  (gr_text A7 (at 185.42 87.63 90) (layer F.SilkS))
  (gr_text GPIOA (at 167.64 87.63) (layer F.SilkS))
  (gr_text A0 (at 149.86 87.63 90) (layer F.SilkS))
  (gr_text GPIOB (at 127 87.63) (layer F.SilkS))
  (gr_text "B7\n" (at 144.78 87.63 90) (layer F.SilkS))
  (gr_text B0 (at 109.22 87.63 90) (layer F.SilkS))
  (gr_text 10K (at 59.7 88.35) (layer F.SilkS))
  (gr_line (start 105.41 74.93) (end 102.87 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 100.33 81.915) (end 100.33 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 102.87 81.915) (end 100.33 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 102.87 74.93) (end 102.87 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 54.61 74.93) (end 54.61 90.17) (layer Edge.Cuts) (width 0.2))
  (gr_text "INTB\n" (at 84.328 76.708) (layer B.SilkS))
  (gr_text "~RST\n" (at 80.518 76.708) (layer B.SilkS))
  (gr_text A1 (at 59.69 81.788) (layer F.SilkS))
  (gr_text A0 (at 57.15 81.788) (layer F.SilkS))
  (gr_line (start 191.77 74.93) (end 191.77 90.17) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 189.23 74.93) (end 191.77 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 100.33 74.93) (end 54.61 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 105.41 81.915) (end 105.41 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 107.95 81.915) (end 105.41 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 107.95 74.93) (end 107.95 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 110.49 74.93) (end 107.95 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 110.49 81.915) (end 110.49 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 113.03 81.915) (end 110.49 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 113.03 74.93) (end 113.03 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 115.57 74.93) (end 113.03 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 115.57 81.915) (end 115.57 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 118.11 81.915) (end 115.57 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 118.11 74.93) (end 118.11 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 120.65 74.93) (end 118.11 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 120.65 81.915) (end 120.65 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 123.19 81.915) (end 120.65 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 123.19 74.93) (end 123.19 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 125.73 74.93) (end 123.19 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 125.73 81.915) (end 125.73 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 128.27 81.915) (end 125.73 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 128.27 74.93) (end 128.27 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 130.81 74.93) (end 128.27 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 130.81 81.915) (end 130.81 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 133.35 81.915) (end 130.81 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 133.35 74.93) (end 133.35 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 135.89 74.93) (end 133.35 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 135.89 81.915) (end 135.89 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 138.43 81.915) (end 135.89 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 138.43 74.93) (end 138.43 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 140.97 74.93) (end 138.43 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 140.97 81.915) (end 140.97 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 143.51 81.915) (end 140.97 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 143.51 74.93) (end 143.51 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 146.05 74.93) (end 143.51 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 189.23 81.915) (end 189.23 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 186.69 81.915) (end 189.23 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 186.69 74.93) (end 186.69 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 184.15 74.93) (end 186.69 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 184.15 81.915) (end 184.15 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 181.61 81.915) (end 184.15 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 181.61 74.93) (end 181.61 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 179.07 74.93) (end 181.61 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 179.07 81.915) (end 179.07 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 176.53 81.915) (end 179.07 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 176.53 74.93) (end 176.53 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 173.99 74.93) (end 176.53 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 173.99 81.915) (end 173.99 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 171.45 81.915) (end 173.99 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 171.45 74.93) (end 171.45 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 168.91 74.93) (end 171.45 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 168.91 81.915) (end 168.91 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 166.37 81.915) (end 168.91 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 166.37 74.93) (end 166.37 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 163.83 74.93) (end 166.37 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 163.83 81.915) (end 163.83 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 161.29 81.915) (end 163.83 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 161.29 74.93) (end 161.29 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 158.75 74.93) (end 161.29 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 158.75 81.915) (end 158.75 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 156.21 81.915) (end 158.75 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 156.21 74.93) (end 156.21 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 153.67 74.93) (end 156.21 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 153.67 81.915) (end 153.67 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 151.13 81.915) (end 153.67 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 151.13 74.93) (end 151.13 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 148.59 74.93) (end 151.13 74.93) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 146.05 81.915) (end 148.59 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 146.05 74.93) (end 146.05 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 148.59 74.93) (end 148.59 81.915) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 54.61 90.17) (end 191.77 90.17) (layer Edge.Cuts) (width 0.2))
  (zone (net 9) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.61 74.93) (xy 191.77 74.93) (xy 191.77 90.17) (xy 54.61 90.17)
      )
    )
  )
)
