<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="30.48" x2="46.99" y2="30.48" width="0.2032" layer="20"/>
<wire x1="46.99" y1="30.48" x2="46.99" y2="0" width="0.2032" layer="20"/>
<wire x1="46.99" y1="0" x2="0" y2="0" width="0.2032" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="30.48" width="0.2032" layer="20"/>
<text>VCC</text>
<text>GND</text>
<text>MISO</text>
<text>MOSI</text>
<text>SCK</text>
<text>RST</text>
<text>Stat1</text>
<text>Stat2</text>
<text>Power</text>
<text>No</text>
<text>Target</text>
<text>Power</text>
<text>Power</text>
<text>JP1</text>
<text>Limor Fried</text>
<text>SMD Design/Layout: N. Seidle</text>
<text>Not ISP</text>
<text>ISP</text>
<text>D+</text>
<text>D-</text>
</plain>
<libraries>
<library name="avr">
<packages>
<package name="SO20L">
<description>&lt;B&gt;Small Outline Package&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="USB-MINIB">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="SO014">
</package>
<package name="AYZ0202">
<description>&lt;b&gt;DPDT Slide Switch SMD&lt;/b&gt;
www.SparkFun.com SKU : Comp-SMDS</description>
</package>
<package name="FIDUCIAL-1X2">
</package>
<package name="PTC-1206">
</package>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="LED-0603">
</package>
<package name="EIA3216">
</package>
<package name="1X02">
</package>
<package name="2X5-SHROUDED_LOCK">
</package>
<package name="2X3">
</package>
<package name="CRYSTAL-SMD-5X3">
</package>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="CREATIVE_COMMONS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X2" library="SparkFun" package="USB-MINIB" value="USBSMD"/>
<element name="U1" library="avr" package="SO20L" value="ATTINY2313-20S"/>
<element name="C2" library="SparkFun" package="0402-CAP" value="0.1uF"/>
<element name="R1" library="SparkFun" package="0402-RES" value="27"/>
<element name="R2" library="SparkFun" package="0402-RES" value="27"/>
<element name="C1" library="SparkFun" package="EIA3216" value="10uF"/>
<element name="R3" library="SparkFun" package="0402-RES" value="1.5K"/>
<element name="D2" library="SparkFun" package="LED-0603" value="Red"/>
<element name="D1" library="SparkFun" package="LED-0603" value="Blue"/>
<element name="R4" library="SparkFun" package="0402-RES" value="1K"/>
<element name="R5" library="SparkFun" package="0402-RES" value="1K"/>
<element name="JP1" library="SparkFun" package="1X02" value="Power Select"/>
<element name="R6" library="SparkFun" package="0402-RES" value="1K"/>
<element name="JP3" library="SparkFun" package="2X5-SHROUDED_LOCK" value="AVR_SPI_PROG2LOCK"/>
<element name="U2" library="SparkFun" package="SO014" value="74ACT125D"/>
<element name="JP2" library="SparkFun" package="2X3" value="AVR_SPI_PRG_6PTH"/>
<element name="R7" library="SparkFun" package="0402-RES" value="100"/>
<element name="R8" library="SparkFun" package="0402-RES" value="100"/>
<element name="S1" library="SparkFun" package="AYZ0202" value="Power Select"/>
<element name="U$1" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="U$3" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="U$4" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="U$5" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="U$6" library="SparkFun" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="U$7" library="SparkFun" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="D3" library="SparkFun" package="LED-0603" value="Blue"/>
<element name="R9" library="SparkFun" package="0402-RES" value="1K"/>
<element name="F1" library="SparkFun" package="PTC-1206" value="500mA"/>
<element name="LED1" library="SparkFun" package="LED-0603" value="Blue"/>
<element name="LED2" library="SparkFun" package="LED-0603" value="Blue"/>
<element name="Q1" library="SparkFun" package="CRYSTAL-SMD-5X3" value="12 MHz"/>
<element name="C3" library="SparkFun" package="0402-CAP" value="22pF"/>
<element name="C4" library="SparkFun" package="0402-CAP" value="22pF"/>
<element name="R10" library="SparkFun" package="0402-RES" value="22K"/>
<element name="U$9" library="SparkFun" package="CREATIVE_COMMONS" value="CREATIVE_COMMONS"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="A"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="U1" pad="20"/>
<contactref element="D3" pad="A"/>
<contactref element="F1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="X2" pad="GND"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="C"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="JP2" pad="6"/>
<contactref element="U2" pad="7"/>
<contactref element="JP3" pad="4"/>
<contactref element="JP3" pad="10"/>
<contactref element="JP3" pad="8"/>
<contactref element="JP3" pad="6"/>
<contactref element="U1" pad="10"/>
<contactref element="R9" pad="1"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="RST">
<contactref element="U1" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="RST'">
<contactref element="U1" pad="16"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="SCK'">
<contactref element="U1" pad="19"/>
<contactref element="JP2" pad="3"/>
<contactref element="U2" pad="12"/>
</signal>
<signal name="MOSI'">
<contactref element="U1" pad="17"/>
<contactref element="JP2" pad="4"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="MISO'">
<contactref element="U1" pad="18"/>
<contactref element="JP2" pad="1"/>
<contactref element="U2" pad="8"/>
</signal>
<signal name="D-">
<contactref element="X2" pad="D-"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="D+">
<contactref element="X2" pad="D+"/>
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="PD+">
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="PD-">
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="11"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="9"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$17">
<contactref element="U1" pad="12"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$18">
<contactref element="D1" pad="C"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="D2" pad="C"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="U1" pad="4"/>
<contactref element="Q1" pad="3"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="U1" pad="5"/>
<contactref element="Q1" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="CTL">
<contactref element="U1" pad="8"/>
<contactref element="U2" pad="13"/>
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="4"/>
<contactref element="U2" pad="10"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="U2" pad="6"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="U2" pad="11"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="TARGET-RST">
<contactref element="U2" pad="3"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="TARGET-MOSI">
<contactref element="R7" pad="2"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="TARGET-SCK">
<contactref element="R8" pad="2"/>
<contactref element="JP3" pad="7"/>
</signal>
<signal name="TARGET-MISO">
<contactref element="U2" pad="9"/>
<contactref element="JP3" pad="9"/>
</signal>
<signal name="TARGET-PWR">
<contactref element="JP3" pad="2"/>
<contactref element="U2" pad="14"/>
<contactref element="S1" pad="2"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="D3" pad="C"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="F1" pad="1"/>
<contactref element="X2" pad="VBUS"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
