(kicad_pcb (version 20171130) (host pcbnew "(5.1.7)-1")
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 54)
    (zones 0)
    (modules 7)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.4 0.39)
    (user_via 3.01 3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 139.35 79.87)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /EdgeNet)
  (net 2 /RFin)
  (net 3 /RFout)
  (net 4 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /EdgeNet)
    (add_net /RFin)
    (add_net /RFout)
    (add_net GND)
  )
  (module "KiCAD libraries:qlm logo mono" (layer B.Cu) (tedit 0)
    (at 148.3 80.8 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module "Edge detector circuit:BAS70-06" (layer F.Cu) (tedit 5F9959B1)
    (at 152.3 85 270)
    (fp_text reference D1 (at -2.1 -3.6 180) (layer F.SilkS))
    (fp_text value BAV70 (at 0 -0.5 270) (layer F.Fab))
    (fp_text user BAS70-05/-06 (at 2.87 -1.05) (layer F.SilkS))
    (pad 3 smd rect (at 0 -2.2 270) (size 0.8 0.9) (layers F.Cu F.Mask)
      (net 3 /RFout))
    (pad 2 smd rect (at 1 0 270) (size 0.8 0.9) (layers F.Cu F.Mask)
      (net 1 /EdgeNet))
    (pad 1 smd rect (at -1 0 270) (size 0.8 0.9) (layers F.Cu F.Mask)
      (net 4 GND))
    (model "C:/Users/Josh Rogers/Documents/SamacSys_PCB_Library/KiCad/3D_Models/infineon SOT23 diode.stp"
      (offset (xyz 0 1.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module "KiCAD libraries:qlm logo mono" (layer F.Cu) (tedit 0)
    (at 148.3 80)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module "Edge detector circuit:MurataCap" (layer F.Cu) (tedit 5F995587)
    (at 140.9 85.4)
    (fp_text reference C100p (at 0.25 2.2) (layer F.SilkS))
    (fp_text value GQM2195C2E101GB12D (at 0.2 -2.15) (layer F.Fab))
    (pad 2 smd rect (at 0.825 0) (size 0.95 1.45) (layers F.Cu F.Mask)
      (net 1 /EdgeNet))
    (pad 1 smd rect (at -0.825 0) (size 0.95 1.45) (layers F.Cu F.Mask)
      (net 2 /RFin))
    (model "C:/Users/Josh Rogers/Documents/SamacSys_PCB_Library/KiCad/3D_Models/GQM2195C2E101GB12D.step"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Edge detector circuit:VishayRFResistor" (layer F.Cu) (tedit 5F995B18)
    (at 146.8 84.2 90)
    (fp_text reference R50 (at 1 -2.6) (layer F.SilkS))
    (fp_text value 50 (at 0.45 -1.65 90) (layer F.Fab))
    (pad 2 smd rect (at 0.85 0 90) (size 0.75 0.95) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -0.85 0 90) (size 0.75 0.95) (layers F.Cu F.Mask)
      (net 1 /EdgeNet))
    (model "C:/Users/Josh Rogers/Documents/SamacSys_PCB_Library/KiCad/3D_Models/vishay RF resistor R50 0603 case.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Edge detector circuit:SMAEdgeMountLinxCONSMA021.062-G" (layer F.Cu) (tedit 5FA134C1)
    (at 160.879999 85.374999 180)
    (fp_text reference RFout1 (at -2.620001 -5.725001) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 3.23 -5.56) (layer F.Fab))
    (fp_text user "SMA RF" (at -2.470001 7.004999) (layer F.SilkS))
    (pad 2 smd rect (at -1.04 0 180) (size 3 5) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at -4.04 0 180) (size 3 7) (layers B.Cu B.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -0.7 -1.09 180) (size 0.5 0.5) (drill 0.41) (layers *.Cu F.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -1.7 -1.09 180) (size 0.5 0.5) (drill 0.41) (layers *.Cu F.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -2.7 -1.09 180) (size 0.5 0.5) (drill 0.41) (layers *.Cu F.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -3.7 -1.09 180) (size 0.5 0.5) (drill 0.41) (layers *.Cu F.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -4.7 -1.09 180) (size 0.5 0.5) (drill 0.41) (layers *.Cu F.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -0.7 1.09 180) (size 0.5 0.5) (drill 0.41) (layers *.Cu F.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -1.7 1.09 180) (size 0.5 0.5) (drill 0.41) (layers *.Cu F.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -2.7 1.09 180) (size 0.5 0.5) (drill 0.41) (layers *.Cu F.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -3.7 1.09 180) (size 0.5 0.5) (drill 0.41) (layers *.Cu F.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -4.7 1.09 180) (size 0.5 0.5) (drill 0.41) (layers *.Cu F.Mask)
      (net 4 GND))
    (pad 2 connect rect (at -2.77 2.3575 180) (size 5.54 3.415) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 2 connect rect (at -2.77 -2.3575 180) (size 5.54 3.415) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 1 connect rect (at -2.04 0 180) (size 7 1) (layers F.Cu)
      (net 3 /RFout))
    (model "C:/Users/Josh Rogers/Documents/SamacSys_PCB_Library/KiCad/3D_Models/Linx SMA Edge connector.stp"
      (offset (xyz -15.2 0 0.125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 90))
    )
  )
  (module "Edge detector circuit:SMAEdgeMountLinxCONSMA021.062-G" (layer F.Cu) (tedit 5FA134C1)
    (at 135.879999 85.374999)
    (fp_text reference RFin1 (at -2.779999 5.725001) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 3.23 -5.56) (layer F.Fab))
    (fp_text user "SMA RF" (at -2.529999 -7.004999) (layer F.SilkS))
    (pad 2 smd rect (at -1.04 0) (size 3 5) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at -4.04 0) (size 3 7) (layers B.Cu B.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -0.7 -1.09) (size 0.5 0.5) (drill 0.41) (layers *.Cu F.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -1.7 -1.09) (size 0.5 0.5) (drill 0.41) (layers *.Cu F.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -2.7 -1.09) (size 0.5 0.5) (drill 0.41) (layers *.Cu F.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -3.7 -1.09) (size 0.5 0.5) (drill 0.41) (layers *.Cu F.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -4.7 -1.09) (size 0.5 0.5) (drill 0.41) (layers *.Cu F.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -0.7 1.09) (size 0.5 0.5) (drill 0.41) (layers *.Cu F.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -1.7 1.09) (size 0.5 0.5) (drill 0.41) (layers *.Cu F.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -2.7 1.09) (size 0.5 0.5) (drill 0.41) (layers *.Cu F.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -3.7 1.09) (size 0.5 0.5) (drill 0.41) (layers *.Cu F.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -4.7 1.09) (size 0.5 0.5) (drill 0.41) (layers *.Cu F.Mask)
      (net 4 GND))
    (pad 2 connect rect (at -2.77 2.3575) (size 5.54 3.415) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 2 connect rect (at -2.77 -2.3575) (size 5.54 3.415) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 1 connect rect (at -2.04 0) (size 7 1) (layers F.Cu)
      (net 2 /RFin))
    (model "C:/Users/Josh Rogers/Documents/SamacSys_PCB_Library/KiCad/3D_Models/Linx SMA Edge connector.stp"
      (offset (xyz -15.2 0 0.125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 90))
    )
  )
  (gr_line (start 130.1 93.8) (end 130.1 90.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 166.6 90.8) (end 166.6 93.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 166.6 77) (end 166.6 80) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 130.1 80) (end 130.1 77) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 130.1 90.8) (end 130.1 80) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 166.6 93.8) (end 130.1 93.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 166.6 80) (end 166.6 90.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 130.1 77) (end 166.6 77) (layer Edge.Cuts) (width 0.05))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.2 86.4) (xy 140.575 86.4) (xy 140.575 84.4) (xy 141.2 84.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.45 84.6) (xy 146.15 84.6) (xy 146.15 83.75) (xy 147.45 83.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.55 84.45) (xy 153.95 84.45) (xy 153.95 85.425) (xy 154.55 86.025) (xy 154.55 86.5)
        (xy 152.875 86.5) (xy 152.875 85.525) (xy 151.85 84.5) (xy 152.85 84.5) (xy 152.85 83.55)
        (xy 154.55 83.55)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.6 90.8) (xy 130.1 90.8) (xy 130.1 80) (xy 166.6 80)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.6 90.8) (xy 130.1 90.8) (xy 130.1 80) (xy 166.6 80)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.6 93.8) (xy 130.1 93.8) (xy 130.1 77) (xy 166.6 77)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.6 93.8) (xy 130.1 93.8) (xy 130.1 77) (xy 166.6 77)
      )
    )
  )
)
