<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="1" y1="-0.6" x2="11.7" y2="-0.6" width="0" layer="20"/>
<wire x1="11.7" y1="-0.6" x2="11.7" y2="15" width="0" layer="20"/>
<wire x1="11.7" y1="15" x2="188.5" y2="15" width="0" layer="20"/>
<wire x1="188.5" y1="15" x2="188.5" y2="50" width="0" layer="20"/>
<wire x1="188.5" y1="50" x2="0" y2="50" width="0" layer="20"/>
<wire x1="0" y1="50" x2="0" y2="15" width="0" layer="20"/>
<wire x1="0" y1="15" x2="1" y2="15" width="0" layer="20"/>
<wire x1="1" y1="15" x2="1" y2="-0.6" width="0" layer="20"/>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="LED3535">
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="15-91-04">
<description>&lt;b&gt;2.54mm Pitch SL™ Wire-to-Board Header, Low Profile, Surface Mount, Single Row, Right Angle, 3.05mm Pocket, Shrouded, with Press-fit Plastic Peg, 4 Circuits, Tin (Sn) Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/015913044_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED1" library="adafruit" package="LED3535" value="WS2812B3535">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED10" library="adafruit" package="LED3535" value="WS2812B3535">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED11" library="adafruit" package="LED3535" value="WS2812B3535">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED12" library="adafruit" package="LED3535" value="WS2812B3535">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED13" library="adafruit" package="LED3535" value="WS2812B3535">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED14" library="adafruit" package="LED3535" value="WS2812B3535">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED15" library="adafruit" package="LED3535" value="WS2812B3535">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED16" library="adafruit" package="LED3535" value="WS2812B3535">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="LED3535" value="WS2812B3535">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="adafruit" package="LED3535" value="WS2812B3535">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="adafruit" package="LED3535" value="WS2812B3535">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED5" library="adafruit" package="LED3535" value="WS2812B3535">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED6" library="adafruit" package="LED3535" value="WS2812B3535">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED7" library="adafruit" package="LED3535" value="WS2812B3535">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED8" library="adafruit" package="LED3535" value="WS2812B3535">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED9" library="adafruit" package="LED3535" value="WS2812B3535">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CONN" library="con-molex" package="15-91-04" value="C-GRID-04-15-91">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="LED1" pad="3"/>
<contactref element="LED2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="LED2" pad="3"/>
<contactref element="LED3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="LED3" pad="3"/>
<contactref element="LED4" pad="1"/>
</signal>
<signal name="DATA">
<contactref element="CONN" pad="2"/>
<contactref element="LED1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="LED5" pad="3"/>
<contactref element="LED6" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="LED6" pad="3"/>
<contactref element="LED7" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="LED7" pad="3"/>
<contactref element="LED8" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="LED9" pad="3"/>
<contactref element="LED10" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="LED10" pad="3"/>
<contactref element="LED11" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="LED11" pad="3"/>
<contactref element="LED12" pad="1"/>
</signal>
<signal name="VDD">
<contactref element="LED9" pad="2"/>
<contactref element="LED10" pad="2"/>
<contactref element="LED11" pad="2"/>
<contactref element="LED12" pad="2"/>
<contactref element="LED5" pad="2"/>
<contactref element="LED6" pad="2"/>
<contactref element="LED7" pad="2"/>
<contactref element="LED8" pad="2"/>
<contactref element="LED13" pad="2"/>
<contactref element="LED14" pad="2"/>
<contactref element="LED15" pad="2"/>
<contactref element="LED16" pad="2"/>
<contactref element="CONN" pad="1"/>
<contactref element="LED1" pad="2"/>
<contactref element="LED2" pad="2"/>
<contactref element="LED3" pad="2"/>
<contactref element="LED4" pad="2"/>
</signal>
<signal name="GND">
<contactref element="LED12" pad="4"/>
<contactref element="LED11" pad="4"/>
<contactref element="LED10" pad="4"/>
<contactref element="LED9" pad="4"/>
<contactref element="LED8" pad="4"/>
<contactref element="LED7" pad="4"/>
<contactref element="LED6" pad="4"/>
<contactref element="LED5" pad="4"/>
<contactref element="LED4" pad="4"/>
<contactref element="LED3" pad="4"/>
<contactref element="LED2" pad="4"/>
<contactref element="LED1" pad="4"/>
<contactref element="CONN" pad="4"/>
<contactref element="LED16" pad="4"/>
<contactref element="LED15" pad="4"/>
<contactref element="LED14" pad="4"/>
<contactref element="LED13" pad="4"/>
</signal>
<signal name="N$17">
<contactref element="LED9" pad="1"/>
<contactref element="LED8" pad="3"/>
</signal>
<signal name="N$18">
<contactref element="LED13" pad="3"/>
<contactref element="LED14" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="LED14" pad="3"/>
<contactref element="LED15" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="LED15" pad="3"/>
<contactref element="LED16" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="LED13" pad="1"/>
<contactref element="LED12" pad="3"/>
</signal>
<signal name="N$24">
<contactref element="LED5" pad="1"/>
<contactref element="LED4" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
