<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.1">
<drawing>
<board>
<plain>
<wire x1="24.157940625" y1="27.3939" x2="24.157940625" y2="1.9939" width="0.1524" layer="20"/>
<wire x1="24.157940625" y1="1.9939" x2="22.887940625" y2="0.7239" width="0.1524" layer="20" curve="-90"/>
<wire x1="22.887940625" y1="0.7239" x2="2.567940625" y2="0.7239" width="0.1524" layer="20"/>
<wire x1="2.567940625" y1="0.7239" x2="1.297940625" y2="1.9939" width="0.1524" layer="20" curve="-90"/>
<wire x1="1.297940625" y1="1.9939" x2="1.297940625" y2="27.3939" width="0.1524" layer="20"/>
<wire x1="1.297940625" y1="27.3939" x2="2.567940625" y2="28.6639" width="0.1524" layer="20" curve="-90"/>
<wire x1="2.567940625" y1="28.6639" x2="22.887940625" y2="28.6639" width="0.1524" layer="20"/>
<wire x1="22.887940625" y1="28.6639" x2="24.157940625" y2="27.3939" width="0.1524" layer="20" curve="-90"/>
<text>Phantomic
Laboratories</text>
<text>sourDough
SOIC-20 N/W
Breakout</text>
<text>Phantomic
Laboratories</text>
<text>Phantomic
Laboratories</text>
<text>sourDough
SOIC-20 N/W
Breakout</text>
<text>Phantomic
Laboratories</text>
</plain>
<libraries>
<library name="dp_devices.v6">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="SOIC-20NW">
<description>&lt;B&gt;SSOP-20 Narrow - Wide&lt;/B&gt;
&lt;br&gt;Pad size: 0.6 x 3.56 mm
&lt;br&gt;Pad pitch: 1.27mm
&lt;br&gt;Pad pitch lateral: 7.56mm</description>
</package>
</packages>
</library>
<library name="Seeed-Connector">
<packages>
<package name="H10-2.54">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="dp_devices.v6" package="SOIC-20NW" value="IC_DIL20-SOIC-20NW"/>
<element name="J1" library="Seeed-Connector" package="H10-2.54" value="10p-2.54">
<attribute name="MPN" value="F185-1110A1BSYA1"/>
<attribute name="NAME"/>
</element>
<element name="J2" library="Seeed-Connector" package="H10-2.54" value="10p-2.54">
<attribute name="MPN" value="F185-1110A1BSYA1"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="J1" pad="1"/>
<contactref element="IC1" pad="P1"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="2"/>
<contactref element="IC1" pad="P2"/>
</signal>
<signal name="N$3">
<contactref element="J1" pad="3"/>
<contactref element="IC1" pad="P3"/>
</signal>
<signal name="N$4">
<contactref element="J1" pad="4"/>
<contactref element="IC1" pad="P4"/>
</signal>
<signal name="N$5">
<contactref element="J1" pad="5"/>
<contactref element="IC1" pad="P5"/>
</signal>
<signal name="N$6">
<contactref element="J1" pad="6"/>
<contactref element="IC1" pad="P6"/>
</signal>
<signal name="N$7">
<contactref element="J1" pad="7"/>
<contactref element="IC1" pad="P7"/>
</signal>
<signal name="N$8">
<contactref element="J1" pad="8"/>
<contactref element="IC1" pad="P8"/>
</signal>
<signal name="N$9">
<contactref element="J1" pad="9"/>
<contactref element="IC1" pad="P9"/>
</signal>
<signal name="N$10">
<contactref element="J1" pad="10"/>
<contactref element="IC1" pad="P10"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="P11"/>
<contactref element="J2" pad="10"/>
</signal>
<signal name="N$12">
<contactref element="J2" pad="9"/>
<contactref element="IC1" pad="P12"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="P13"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="N$14">
<contactref element="J2" pad="7"/>
<contactref element="IC1" pad="P14"/>
</signal>
<signal name="N$15">
<contactref element="IC1" pad="P15"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="N$16">
<contactref element="J2" pad="5"/>
<contactref element="IC1" pad="P16"/>
</signal>
<signal name="N$17">
<contactref element="IC1" pad="P17"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="N$18">
<contactref element="J2" pad="3"/>
<contactref element="IC1" pad="P18"/>
</signal>
<signal name="N$19">
<contactref element="IC1" pad="P19"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="J2" pad="1"/>
<contactref element="IC1" pad="P20"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
