(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 48)
    (zones 0)
    (modules 18)
    (nets 15)
  )
  (page A4)
  (title_block
    (title "Rpi Adaptor")
    (rev 2L_3)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.3048)
    (user_trace_width 0.6096)
    (user_trace_width 1.2192)
    (trace_clearance 0.1524)
    (zone_clearance 0.1016)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.762 0.762)
    (mod_text_width 0.127)
    (pad_size 0.6858 0.6858)
    (pad_drill 0.3302)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFDEF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.076200)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /3V3)
  (net 3 /UART0_Rx)
  (net 4 /UART0_Tx)
  (net 5 /5V)
  (net 6 "Net-(D1-Pad2)")
  (net 7 "Net-(D2-Pad2)")
  (net 8 "Net-(H1-Pad15)")
  (net 9 "Net-(H1-Pad13)")
  (net 10 /~RESET)
  (net 11 "Net-(JP1-Pad2)")
  (net 12 "Net-(JP2-Pad2)")
  (net 13 /GPIO_18)
  (net 14 "Net-(R1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /3V3)
    (add_net /5V)
    (add_net /GPIO_17)
    (add_net /GPIO_18)
    (add_net /GPIO_4)
    (add_net /I2C1_SCL)
    (add_net /I2C1_SDA)
    (add_net /UART0_Rx)
    (add_net /UART0_Tx)
    (add_net /~RESET)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(H1-Pad11)")
    (add_net "Net-(H1-Pad12)")
    (add_net "Net-(H1-Pad13)")
    (add_net "Net-(H1-Pad14)")
    (add_net "Net-(H1-Pad15)")
    (add_net "Net-(H1-Pad16)")
    (add_net "Net-(H1-Pad17)")
    (add_net "Net-(H1-Pad18)")
    (add_net "Net-(H1-Pad19)")
    (add_net "Net-(H1-Pad20)")
    (add_net "Net-(H1-Pad4)")
    (add_net "Net-(H1-Pad6)")
    (add_net "Net-(H1-Pad7)")
    (add_net "Net-(H1-Pad8)")
    (add_net "Net-(H1-Pad9)")
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(R1-Pad1)")
  )
  (module XBee-Adapter:MyBasic_rounded_50_1 (layer F.Cu) (tedit 0)
    (at 176.08042 45.57268 270)
    (fp_text reference Lg3 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value logo (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module "mech:Board Ref" (layer F.Cu) (tedit 6131D569)
    (at 166.116 45.974)
    (fp_text reference Brd1 (at 0 2.8) (layer Dwgs.User) hide)
    (fp_text value "XBee Board" (at 0 -2.9) (layer F.Fab))
    (model "${KIPRJMOD}/kicad_lib/lib/package3d/provided/User Library-XBee-Chip.STEP"
      (offset (xyz 0 0 5.334))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module "mech:Board Ref" (layer B.Cu) (tedit 6131D569)
    (at 178.308 36.068)
    (fp_text reference Brd2 (at 0 -2.8 180) (layer Dwgs.User) hide)
    (fp_text value "Raspberry Pi Zero" (at 0 2.9 180) (layer B.Fab))
    (model "${KIPRJMOD}/kicad_lib/lib/package3d/provided/Raspberry PI Zero W.step"
      (offset (xyz 0 0 11.00074))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module GoldCap-Check:SGM811B (layer F.Cu) (tedit 6131D01B)
    (at 166.88054 39.39724 180)
    (fp_text reference U1 (at -2.30448 1.12522 270) (layer F.SilkS))
    (fp_text value SGM811 (at 0 -5.25) (layer F.Fab))
    (pad 4 smd rect (at -0.95 -1.1 180) (size 0.55 1) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 3 smd rect (at 0.95 -1.1 180) (size 0.55 1) (layers F.Cu F.Paste F.Mask)
      (net 13 /GPIO_18))
    (pad 2 smd rect (at 0.95 1.1 180) (size 0.55 1) (layers F.Cu F.Paste F.Mask)
      (net 10 /~RESET))
    (pad 1 smd rect (at -0.75 1.1 180) (size 0.95 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/kicad_lib/lib/package3d/provided/TO-253AA.stp
      (offset (xyz -0.7874 -1.2192 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:KiCad-Logo2_6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 149.959096 45.50169 90)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference Lg2 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value KiCad (at 0.75 0 270) (layer B.Fab) hide)
  )
  (module XBee-Adapter:XBEE_S2C (layer F.Cu) (tedit 612E6092)
    (at 175.75 45.75 270)
    (fp_text reference H1 (at -8.6 1.1 180) (layer F.SilkS))
    (fp_text value DIGI_XBEE (at 0.4318 -3.683 90) (layer F.Fab))
    (fp_text user XBee (at -7.396 0.49 180) (layer F.SilkS))
    (pad 20 thru_hole circle (at 10.9982 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 19 thru_hole circle (at 10.9982 2.0066 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 18 thru_hole circle (at 10.9982 4.0132 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 17 thru_hole circle (at 10.9982 6.0198 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 16 thru_hole circle (at 10.9982 8.0264 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 15 thru_hole circle (at 10.9982 10.033 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(H1-Pad15)"))
    (pad 14 thru_hole circle (at 10.9982 12.0396 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole circle (at 10.9982 14.0462 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(H1-Pad13)"))
    (pad 12 thru_hole circle (at 10.9982 16.0528 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole circle (at 10.9982 18.0594 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole circle (at -10.9982 18.0594 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 9 thru_hole circle (at -10.9982 16.0528 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole circle (at -10.9982 14.0462 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole circle (at -10.9982 12.0396 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole circle (at -10.9982 10.033 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole circle (at -10.9982 8.0264 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 10 /~RESET))
    (pad 4 thru_hole circle (at -10.9982 6.0198 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at -10.9982 4.0132 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 4 /UART0_Tx))
    (pad 2 thru_hole circle (at -10.9982 2.0066 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 /UART0_Rx))
    (pad 1 thru_hole circle (at -10.9982 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 /3V3))
    (model :D:/pcbs/GoldCap/doc/3D/XBee-Chip_fc.wrl-
      (offset (xyz 0 -9.5 2))
      (scale (xyz 395 395 395))
      (rotate (xyz -90 0 0))
    )
    (model "${MYLIB}/package3d/provided/User Library-XBee-Chip.WRL-"
      (offset (xyz 0 -9.5 2))
      (scale (xyz 395 395 395))
      (rotate (xyz -90 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.00mm.3dshapes/PinSocket_1x10_P2.00mm_Vertical.wrl
      (offset (xyz -11 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.00mm.3dshapes/PinSocket_1x10_P2.00mm_Vertical.wrl
      (offset (xyz 11 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module XBee-Adapter:MyBasic_rounded_50_1 (layer B.Cu) (tedit 0)
    (at 176.09058 45.67936 90)
    (fp_text reference Lg1 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value logo (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 151.892 35.56)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference SW1 (at 0 -2.794) (layer F.SilkS))
    (fp_text value SW_Push (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /GPIO_18))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 174.752 32.258 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 2.794 0) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 159.258 44.45 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -2.794 0) (layer F.SilkS))
    (fp_text value 680Ω (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439004878048781)
      (net 7 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439004878048781)
      (net 11 "Net-(JP1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 159.258 50.546 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -2.794 0) (layer F.SilkS))
    (fp_text value 680Ω (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439004878048781)
      (net 6 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439004878048781)
      (net 12 "Net-(JP2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 163.22548 38.21938 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -0.00254 1.79324) (layer F.SilkS))
    (fp_text value 100kΩ (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439004878048781)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439004878048781)
      (net 10 /~RESET))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 157.9753 37.1348)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0.254 1.778) (layer F.SilkS))
    (fp_text value 100kΩ (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439004878048781)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439004878048781)
      (net 14 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5C745284)
    (at 159.258 47.244 180)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at -2.286 0 -90) (layer F.SilkS))
    (fp_text value ON (at 0 1.9) (layer F.Fab))
    (pad 1 smd custom (at -0.65 0 180) (size 1 0.5) (layers F.Cu F.Mask)
      (net 9 "Net-(H1-Pad13)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 180) (size 1 0.5) (layers F.Cu F.Mask)
      (net 12 "Net-(JP2-Pad2)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5C745284)
    (at 159.258 41.402 180)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at -2.286 0 270) (layer F.SilkS))
    (fp_text value ASSOCIATE (at 0 1.9) (layer F.Fab))
    (pad 1 smd custom (at -0.65 0 180) (size 1 0.5) (layers F.Cu F.Mask)
      (net 8 "Net-(H1-Pad15)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 180) (size 1 0.5) (layers F.Cu F.Mask)
      (net 11 "Net-(JP1-Pad2)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 152.908 44.45)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D2 (at 0 -1.65) (layer F.SilkS))
    (fp_text value LED (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 152.908 50.546)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D1 (at 0 -1.65) (layer F.SilkS))
    (fp_text value LED (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x06_Pitch2.54mm (layer B.Cu) (tedit 599349E3)
    (at 170.18 61.214 90)
    (descr "Through hole straight socket strip, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x06 2.54mm double row")
    (fp_text reference P1 (at 0.508 2.794 270) (layer B.SilkS))
    (fp_text value "Raspberry PI" (at -1.27 -15.03 270) (layer B.Fab))
    (fp_text user %R (at 3.006 -0.25 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /3V3))
    (pad 2 thru_hole oval (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /5V))
    (pad 3 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -2.54 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /5V))
    (pad 5 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at -2.54 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at -2.54 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /UART0_Tx))
    (pad 9 thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at -2.54 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /UART0_Rx))
    (pad 11 thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at -2.54 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /GPIO_18))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x06_Pitch2.54mm.wrl-
      (offset (xyz -1.269999980926514 -6.349999904632568 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x06_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "XBee Raspberry Pi \nAdapter R3" (at 172.49902 45.65904 270) (layer F.SilkS))
  (gr_text "XBee Raspberry Pi \nAdapter R3" (at 172.41012 45.62856 270) (layer B.SilkS))
  (gr_text ~RESET (at 148.3995 36.9951 -90) (layer F.SilkS))
  (gr_line (start 156.21 59.944) (end 156.21 66.04) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.2499 59.944) (end 156.21 59.944) (layer Edge.Cuts) (width 0.15))
  (gr_text PWR (at 156.718 41.656 90) (layer F.SilkS))
  (gr_text ASSC (at 156.464 47.244 90) (layer F.SilkS))
  (gr_text ASSC (at 152.908 52.578) (layer F.SilkS))
  (gr_text PWR (at 152.908 46.482) (layer F.SilkS))
  (gr_line (start 180.34 66.04) (end 180.34 30.48) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180.34 30.48) (end 145.25 30.48) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.21 66.04) (end 180.34 66.04) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.25 30.48) (end 145.25 59.944) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1016))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.1016) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180.34 66.04) (xy 156.21254 66.03492) (xy 156.1973 59.9567) (xy 145.2499 59.9313) (xy 145.2499 30.48)
        (xy 180.34254 30.47492)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1016))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.1016) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180.34 66.04) (xy 156.21254 66.03492) (xy 156.21 59.944) (xy 145.2499 59.944) (xy 145.2499 30.48)
        (xy 180.34508 30.47492)
      )
    )
  )
)
