(kicad_pcb (version 4) (host pcbnew 4.0.4+e1-6308~48~ubuntu16.04.1-stable)
  (general
    (links 106)
    (no_connects 0)
    (area 70.356667 68.24 177.690238 136.33)
    (thickness 1.6)
    (drawings 35)
    (tracks 264)
    (zones 0)
    (modules 54)
    (nets 42)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.381)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 RotA)
  (net 3 Button1)
  (net 4 RotB)
  (net 5 Button2)
  (net 6 Button4)
  (net 7 Button3)
  (net 8 VCC)
  (net 9 "Net-(D4-Pad2)")
  (net 10 "Net-(D5-Pad2)")
  (net 11 LED1)
  (net 12 LED2)
  (net 13 LED3)
  (net 14 LED4)
  (net 15 RAW)
  (net 16 RESET)
  (net 17 A2)
  (net 18 A1)
  (net 19 Set1)
  (net 20 LED5)
  (net 21 "Net-(R1-Pad1)")
  (net 22 "Net-(R3-Pad1)")
  (net 23 "Net-(R5-Pad1)")
  (net 24 "Net-(R6-Pad1)")
  (net 25 "Net-(R7-Pad1)")
  (net 26 "Net-(R10-Pad2)")
  (net 27 "Net-(R11-Pad1)")
  (net 28 "Net-(R13-Pad1)")
  (net 29 "Net-(R15-Pad1)")
  (net 30 D2)
  (net 31 A3)
  (net 32 "Net-(LED1-Pad4)")
  (net 33 "Net-(LED1-Pad2)")
  (net 34 "Net-(LED2-Pad4)")
  (net 35 "Net-(LED3-Pad4)")
  (net 36 "Net-(LED4-Pad4)")
  (net 37 "Net-(LED5-Pad4)")
  (net 38 "Net-(LED6-Pad4)")
  (net 39 "Net-(LED7-Pad4)")
  (net 40 LEDS)
  (net 41 Set2)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.381)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net A1)
    (add_net A2)
    (add_net A3)
    (add_net Button1)
    (add_net Button2)
    (add_net Button3)
    (add_net Button4)
    (add_net D2)
    (add_net LED1)
    (add_net LED2)
    (add_net LED3)
    (add_net LED4)
    (add_net LED5)
    (add_net LEDS)
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(LED1-Pad2)")
    (add_net "Net-(LED1-Pad4)")
    (add_net "Net-(LED2-Pad4)")
    (add_net "Net-(LED3-Pad4)")
    (add_net "Net-(LED4-Pad4)")
    (add_net "Net-(LED5-Pad4)")
    (add_net "Net-(LED6-Pad4)")
    (add_net "Net-(LED7-Pad4)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net RAW)
    (add_net RESET)
    (add_net RotA)
    (add_net RotB)
    (add_net Set1)
    (add_net Set2)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.635)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VCC)
  )
  (module Libraries:PlasticCaseOutline (layer F.Cu) (tedit 58322897)
    (at 76.2 132.08)
    (fp_text reference REF** (at 13.97 2.54) (layer F.SilkS))
    (fp_text value PlasticCaseOutline (at 13.335 1.905) (layer F.Fab))
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58328E19)
    (at 132.715 95.885)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at -0.635 -24.765) (layer F.SilkS))
    (fp_text value .1uF (at -1.27 -22.86) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 RotA))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5833DF7B)
    (at 88.9 118.11 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 0 -15.875 180) (layer F.SilkS))
    (fp_text value .1uF (at -0.635 -17.145 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 Button1))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58328DF1)
    (at 114.935 95.885 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 0 23.495 180) (layer F.SilkS))
    (fp_text value .1uF (at 0.635 24.13 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 RotB))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5833DF33)
    (at 114.3 118.11 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at 0.635 -15.875 180) (layer F.SilkS))
    (fp_text value .1uF (at 0.635 -15.24 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 Button2))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58328E0B)
    (at 123.825 92.71 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at 1.27 23.495 180) (layer F.SilkS))
    (fp_text value .1uF (at 1.905 22.225 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 Button4))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5833DF26)
    (at 139.7 118.11 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C6 (at 0 -15.875 180) (layer F.SilkS))
    (fp_text value .1uF (at 0.635 -15.875 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 Button3))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-3MM (layer B.Cu) (tedit 58328E05)
    (at 115.57 92.075 180)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D4 (at 0.635 20.955 180) (layer B.SilkS))
    (fp_text value Knob (at 0 20.32 180) (layer B.Fab))
    (fp_text user K (at 0 20.32 180) (layer B.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 9 "Net-(D4-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer B.Cu) (tedit 58328E2B)
    (at 132.08 92.075)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D5 (at 1.905 -20.32) (layer B.SilkS))
    (fp_text value Knob (at 0 -20.32) (layer B.Fab))
    (fp_text user K (at 0 -20.955) (layer B.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 10 "Net-(D5-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58328E29)
    (at 132.715 100.965)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at -0.635 -29.845) (layer F.SilkS))
    (fp_text value 10k (at -1.905 -29.21) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58328E21)
    (at 132.715 98.425 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 1.27 26.67 180) (layer F.SilkS))
    (fp_text value 10k (at 0.635 27.305 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 RotA))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5833DF6D)
    (at 88.922563 123.276385 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at -1.882437 -11.978615 180) (layer F.SilkS))
    (fp_text value 10k (at 0.022563 -11.978615 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5833DF75)
    (at 88.9 120.65)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 0.635 13.97) (layer F.SilkS))
    (fp_text value 10k (at 1.27 13.97) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 Button1))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5833DF6A)
    (at 88.9 115.57 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at -0.635 -19.685 180) (layer F.SilkS))
    (fp_text value 470 (at -1.27 -19.05 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 LED1))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5833DF01)
    (at 114.3 115.57 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at 0 -19.05 180) (layer F.SilkS))
    (fp_text value 470 (at 0.635 -18.415 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 LED2))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58328DF7)
    (at 114.935 100.965 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at 0 29.21 180) (layer F.SilkS))
    (fp_text value 10k (at -0.635 30.48 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R7-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58328E00)
    (at 114.935 98.425)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R8 (at 0.635 -26.67) (layer F.SilkS))
    (fp_text value 10k (at 0.635 -27.94) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 RotB))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R7-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5833DEFE)
    (at 114.3 123.19 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at -0.635 -10.795 180) (layer F.SilkS))
    (fp_text value 10k (at -0.635 -10.795 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R10-Pad2)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5833DF08)
    (at 114.3 120.65)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R10 (at 1.27 13.335) (layer F.SilkS))
    (fp_text value 10k (at 0 13.335) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 Button2))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R10-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5833DF17)
    (at 139.7 115.57 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R11 (at 0 -19.05 180) (layer F.SilkS))
    (fp_text value 470 (at -0.635 -18.415 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 LED3))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58328E02)
    (at 114.935 88.265)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R12 (at -0.635 -17.145) (layer F.SilkS))
    (fp_text value 470 (at 0 -17.78) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 14 LED4))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58328E0D)
    (at 123.825 87.63 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R13 (at 0.635 17.145 180) (layer F.SilkS))
    (fp_text value 10k (at 0.635 17.145 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R13-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58328E12)
    (at 123.825 90.17)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R14 (at -0.635 -19.685) (layer F.SilkS))
    (fp_text value 10k (at -0.635 -19.685) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 Button4))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R13-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5833DF1F)
    (at 139.7 123.19 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R15 (at -1.27 -10.795 180) (layer F.SilkS))
    (fp_text value 10k (at -3.175 -10.795 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R15-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5833DF11)
    (at 139.7 120.65)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R16 (at -0.635 13.335) (layer F.SilkS))
    (fp_text value 10k (at 1.27 13.335) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 Button3))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R15-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58328E25)
    (at 132.715 88.265 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R17 (at 0.635 17.145 180) (layer F.SilkS))
    (fp_text value 470 (at 0.635 15.875 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D5-Pad2)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 20 LED5))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_FSMSM (layer F.Cu) (tedit 583228EA)
    (at 167.005 117.475 270)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1437566-3&DocType=Customer+Drawing&DocLang=English)
    (tags "SPST button tactile switch")
    (attr smd)
    (fp_text reference SW5 (at 0 -7.62 270) (layer F.SilkS))
    (fp_text value Set0 (at 0 -6.985 270) (layer F.Fab))
    (pad 1 smd rect (at -4.60243 -0.00232 270) (size 2.18 1.6) (layers F.Cu F.Paste F.Mask)
      (net 19 Set1))
    (pad 2 smd rect (at 4.60243 0.00232 270) (size 2.18 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Buttons_Switches_SMD:SW_SPST_FSMSM (layer F.Cu) (tedit 583228F0)
    (at 167.005 104.14 270)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1437566-3&DocType=Customer+Drawing&DocLang=English)
    (tags "SPST button tactile switch")
    (attr smd)
    (fp_text reference SW6 (at 0 -6.35 270) (layer F.SilkS))
    (fp_text value Set1 (at 0 -6.985 270) (layer F.Fab))
    (pad 1 smd rect (at -4.60243 -0.00232 270) (size 2.18 1.6) (layers F.Cu F.Paste F.Mask)
      (net 41 Set2))
    (pad 2 smd rect (at 4.60243 0.00232 270) (size 2.18 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Buttons_Switches_SMD:SW_SPST_FSMSM (layer F.Cu) (tedit 583228F6)
    (at 167.005 90.805 270)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1437566-3&DocType=Customer+Drawing&DocLang=English)
    (tags "SPST button tactile switch")
    (attr smd)
    (fp_text reference SW7 (at 0 -6.35 270) (layer F.SilkS))
    (fp_text value Reset (at 0.635 -6.35 270) (layer F.Fab))
    (pad 1 smd rect (at -4.60243 -0.00232 270) (size 2.18 1.6) (layers F.Cu F.Paste F.Mask)
      (net 16 RESET))
    (pad 2 smd rect (at 4.60243 0.00232 270) (size 2.18 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 58322875)
    (at 80.01 128.27)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 6.35) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 1.27 6.35) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5832287D)
    (at 167.64 128.27)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at -1.27 6.35) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at -1.27 5.715) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 58322900)
    (at 167.64 80.01)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -5.715) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at -1.905 -5.715) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5832285F)
    (at 80.01 80.01)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -5.08) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 6.35 -5.715) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Libraries:CherryMX (layer B.Cu) (tedit 5833DF58)
    (at 149.225 120.65)
    (fp_text reference SW3 (at 0 13.97) (layer B.SilkS))
    (fp_text value Forward (at 0 13.335) (layer B.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.4986 1.4986) (drill 1.4986) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.4986 1.4986) (drill 1.4986) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -3.81 2.54) (size 2.54 2.54) (drill 1.4986) (layers *.Cu *.Mask)
      (net 29 "Net-(R15-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 5.08) (size 2.54 2.54) (drill 1.4986) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -1.27 -5.08) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask)
      (net 27 "Net-(R11-Pad1)"))
    (pad 3 thru_hole circle (at 1.27 -5.08) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Libraries:CherryMX (layer B.Cu) (tedit 5833DF61)
    (at 98.447563 120.736385)
    (fp_text reference SW1 (at 1.247437 13.248615) (layer B.SilkS))
    (fp_text value Back (at -0.657563 13.883615) (layer B.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.4986 1.4986) (drill 1.4986) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.4986 1.4986) (drill 1.4986) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -3.81 2.54) (size 2.54 2.54) (drill 1.4986) (layers *.Cu *.Mask)
      (net 22 "Net-(R3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 5.08) (size 2.54 2.54) (drill 1.4986) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -1.27 -5.08) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask)
      (net 23 "Net-(R5-Pad1)"))
    (pad 3 thru_hole circle (at 1.27 -5.08) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Libraries:CherryMX (layer B.Cu) (tedit 5833DEF5)
    (at 123.825 120.65)
    (fp_text reference SW2 (at 0 13.335) (layer B.SilkS))
    (fp_text value Pause (at -3.175 13.335) (layer B.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.4986 1.4986) (drill 1.4986) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.4986 1.4986) (drill 1.4986) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -3.81 2.54) (size 2.54 2.54) (drill 1.4986) (layers *.Cu *.Mask)
      (net 26 "Net-(R10-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 5.08) (size 2.54 2.54) (drill 1.4986) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -1.27 -5.08) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask)
      (net 24 "Net-(R6-Pad1)"))
    (pad 3 thru_hole circle (at 1.27 -5.08) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Libraries:DIP-24_W15.24mm_SMT (layer F.Cu) (tedit 58328C8F)
    (at 144.145 80.645)
    (descr "24-lead dip package, row spacing 15.24 mm (600 mils), SMT for gull wings")
    (tags "dil dip 2.54 600 smt")
    (fp_text reference U1 (at 0 -5.22) (layer F.SilkS))
    (fp_text value Leonardo_Pro_Micro (at 0 -6.35) (layer F.Fab))
    (pad 1 smd rect (at -1.27 0) (size 5.08 1.524) (layers F.Cu F.Paste F.Mask)
      (net 4 RotB))
    (pad 2 smd oval (at -1.27 2.54) (size 5.08 1.524) (layers F.Cu F.Paste F.Mask)
      (net 6 Button4))
    (pad 3 smd oval (at -1.27 5.08) (size 5.08 1.524) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd oval (at -1.27 7.62) (size 5.08 1.524) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd oval (at -1.27 10.16) (size 5.08 1.524) (layers F.Cu F.Paste F.Mask)
      (net 30 D2))
    (pad 6 smd oval (at -1.27 12.7) (size 5.08 1.524) (layers F.Cu F.Paste F.Mask)
      (net 20 LED5))
    (pad 7 smd oval (at -1.27 15.24) (size 5.08 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 RotA))
    (pad 8 smd oval (at -1.27 17.78) (size 5.08 1.524) (layers F.Cu F.Paste F.Mask)
      (net 14 LED4))
    (pad 9 smd oval (at -1.27 20.32) (size 5.08 1.524) (layers F.Cu F.Paste F.Mask)
      (net 11 LED1))
    (pad 10 smd oval (at -1.27 22.86) (size 5.08 1.524) (layers F.Cu F.Paste F.Mask)
      (net 3 Button1))
    (pad 11 smd oval (at -1.27 25.4) (size 5.08 1.524) (layers F.Cu F.Paste F.Mask)
      (net 5 Button2))
    (pad 12 smd oval (at -1.27 27.94) (size 5.08 1.524) (layers F.Cu F.Paste F.Mask)
      (net 12 LED2))
    (pad 13 smd oval (at 16.51 27.94) (size 5.08 1.524) (layers F.Cu F.Paste F.Mask)
      (net 13 LED3))
    (pad 14 smd oval (at 16.51 25.4) (size 5.08 1.524) (layers F.Cu F.Paste F.Mask)
      (net 7 Button3))
    (pad 15 smd oval (at 16.51 22.86) (size 5.08 1.524) (layers F.Cu F.Paste F.Mask)
      (net 40 LEDS))
    (pad 16 smd oval (at 16.51 20.32) (size 5.08 1.524) (layers F.Cu F.Paste F.Mask)
      (net 19 Set1))
    (pad 17 smd oval (at 16.51 17.78) (size 5.08 1.524) (layers F.Cu F.Paste F.Mask)
      (net 41 Set2))
    (pad 18 smd oval (at 16.51 15.24) (size 5.08 1.524) (layers F.Cu F.Paste F.Mask)
      (net 18 A1))
    (pad 19 smd oval (at 16.51 12.7) (size 5.08 1.524) (layers F.Cu F.Paste F.Mask)
      (net 17 A2))
    (pad 20 smd oval (at 16.51 10.16) (size 5.08 1.524) (layers F.Cu F.Paste F.Mask)
      (net 31 A3))
    (pad 21 smd oval (at 16.51 7.62) (size 5.08 1.524) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (pad 22 smd oval (at 16.51 5.08) (size 5.08 1.524) (layers F.Cu F.Paste F.Mask)
      (net 16 RESET))
    (pad 23 smd oval (at 16.51 2.54) (size 5.08 1.524) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd oval (at 16.51 0) (size 5.08 1.524) (layers F.Cu F.Paste F.Mask)
      (net 15 RAW))
    (model Housings_DIP.3dshapes/DIP-24_W15.24mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:RotaryEncoder (layer B.Cu) (tedit 5833DF46)
    (at 123.825 92.075 180)
    (fp_text reference SW4 (at 0.635 22.225 180) (layer B.SilkS))
    (fp_text value RotaryEncoder (at 0 20.32 180) (layer B.Fab))
    (pad 1 thru_hole oval (at -2.5 -7.5 180) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(R1-Pad1)"))
    (pad 2 thru_hole oval (at 0 -7.5 180) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 2.5 -7.5 180) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(R7-Pad1)"))
    (pad 4 thru_hole oval (at -2.5 7 180) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(R13-Pad1)"))
    (pad 5 thru_hole oval (at 2.5 7 180) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at -5.5 0 180) (size 2.7 2.7) (drill 2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 5.5 0 180) (size 2.7 2.7) (drill 2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58329DDF)
    (at 101.6 106.045 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C7 (at 27.94 1.905 180) (layer B.SilkS))
    (fp_text value .1uF (at 28.575 -0.635 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 8 VCC))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58329DDC)
    (at 88.9 106.045 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C8 (at 15.875 1.905 180) (layer B.SilkS))
    (fp_text value .1uF (at 15.875 -1.905 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 8 VCC))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58329DE2)
    (at 88.9 93.345 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C9 (at 15.875 -1.905 180) (layer B.SilkS))
    (fp_text value .1uF (at 15.875 -5.08 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 8 VCC))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58329DFA)
    (at 146.05 93.345 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C10 (at -28.575 5.715 180) (layer B.SilkS))
    (fp_text value .1uF (at -28.575 1.27 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 8 VCC))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58329DE5)
    (at 101.6 93.345 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C11 (at 27.94 -1.27 180) (layer B.SilkS))
    (fp_text value .1uF (at 28.575 -3.175 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 8 VCC))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58329E09)
    (at 146.05 106.045 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C12 (at -29.21 1.905 180) (layer B.SilkS))
    (fp_text value .1uF (at -28.575 -0.635 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 8 VCC))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58329E02)
    (at 158.75 106.045 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C13 (at -15.875 5.08 180) (layer B.SilkS))
    (fp_text value .1uF (at -17.145 3.175 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 8 VCC))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58329DFC)
    (at 158.75 93.345 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C14 (at -15.875 3.81 180) (layer B.SilkS))
    (fp_text value .1uF (at -15.875 0.635 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 8 VCC))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer B.Cu) (tedit 58329BF4)
    (at 101.6 101.6)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED1 (at -28.575 0.635) (layer B.SilkS))
    (fp_text value WS2812B-5050-SMD (at 1.27 -27.305) (layer B.Fab))
    (pad 3 smd rect (at 2.5 -1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 2.5 1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(LED1-Pad4)"))
    (pad 2 smd rect (at -2.5 -1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(LED1-Pad2)"))
    (pad 1 smd rect (at -2.5 1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 8 VCC))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0.004))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer B.Cu) (tedit 58329FEA)
    (at 88.9 101.6)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED2 (at -15.875 8.89) (layer B.SilkS))
    (fp_text value WS2812B-5050-SMD (at -0.635 -27.94) (layer B.Fab))
    (pad 3 smd rect (at 2.5 -1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 2.5 1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(LED2-Pad4)"))
    (pad 2 smd rect (at -2.5 -1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(LED1-Pad4)"))
    (pad 1 smd rect (at -2.5 1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 8 VCC))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0.004))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer B.Cu) (tedit 58329FD7)
    (at 88.9 88.9)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED3 (at -16.51 3.81) (layer B.SilkS))
    (fp_text value WS2812B-5050-SMD (at -1.27 -15.875) (layer B.Fab))
    (pad 3 smd rect (at 2.5 -1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 2.5 1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(LED3-Pad4)"))
    (pad 2 smd rect (at -2.5 -1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(LED2-Pad4)"))
    (pad 1 smd rect (at -2.5 1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 8 VCC))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0.004))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer B.Cu) (tedit 58329FD9)
    (at 101.6 88.9)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED4 (at -29.21 2.54) (layer B.SilkS))
    (fp_text value WS2812B-5050-SMD (at 1.905 -15.24) (layer B.Fab))
    (pad 3 smd rect (at 2.5 -1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 2.5 1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(LED4-Pad4)"))
    (pad 2 smd rect (at -2.5 -1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(LED3-Pad4)"))
    (pad 1 smd rect (at -2.5 1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 8 VCC))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0.004))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer B.Cu) (tedit 58329979)
    (at 158.75 88.9)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED5 (at 15.24 5.715) (layer B.SilkS))
    (fp_text value WS2812B-5050-SMD (at -0.635 -14.605) (layer B.Fab))
    (pad 3 smd rect (at 2.5 -1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 2.5 1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(LED5-Pad4)"))
    (pad 2 smd rect (at -2.5 -1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(LED4-Pad4)"))
    (pad 1 smd rect (at -2.5 1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 8 VCC))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0.004))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer B.Cu) (tedit 5832997C)
    (at 146.05 88.9)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED6 (at 27.94 7.62) (layer B.SilkS))
    (fp_text value WS2812B-5050-SMD (at -1.27 -14.605) (layer B.Fab))
    (pad 3 smd rect (at 2.5 -1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 2.5 1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(LED6-Pad4)"))
    (pad 2 smd rect (at -2.5 -1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(LED5-Pad4)"))
    (pad 1 smd rect (at -2.5 1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 8 VCC))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0.004))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer B.Cu) (tedit 58329976)
    (at 146.05 101.6)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED7 (at 28.575 0.635) (layer B.SilkS))
    (fp_text value WS2812B-5050-SMD (at 0.635 -27.305) (layer B.Fab))
    (pad 3 smd rect (at 2.5 -1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 2.5 1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(LED7-Pad4)"))
    (pad 2 smd rect (at -2.5 -1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(LED6-Pad4)"))
    (pad 1 smd rect (at -2.5 1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 8 VCC))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0.004))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer B.Cu) (tedit 58329973)
    (at 158.75 101.6)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED8 (at 16.51 -0.635) (layer B.SilkS))
    (fp_text value WS2812B-5050-SMD (at -0.635 -26.67) (layer B.Fab))
    (pad 3 smd rect (at 2.5 -1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 2.5 1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 40 LEDS))
    (pad 2 smd rect (at -2.5 -1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(LED7-Pad4)"))
    (pad 1 smd rect (at -2.5 1.6) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 8 VCC))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0.004))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_text "Arduino Pro Micro" (at 151.765 94.615 90) (layer F.SilkS))
  (gr_text 470 (at 135.89 115.57) (layer F.SilkS))
  (gr_text .1uF (at 135.89 118.11) (layer F.SilkS))
  (gr_text 10k (at 135.89 120.65) (layer F.SilkS))
  (gr_text 10k (at 135.89 123.19) (layer F.SilkS))
  (gr_text .1uF (at 85.09 118.11) (layer F.SilkS))
  (gr_text 10k (at 85.09 123.19) (layer F.SilkS))
  (gr_text 10k (at 110.49 120.65) (layer F.SilkS))
  (gr_text 470 (at 110.49 115.57) (layer F.SilkS))
  (gr_line (start 76.2 132.08) (end 76.2 76.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.45 132.08) (end 76.2 132.08) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.45 76.2) (end 171.45 132.08) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 76.2 76.2) (end 171.45 76.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text mark@halibut.com (at 78.74 93.345) (layer F.SilkS))
  (gr_text @SmittyHalibut (at 78.74 90.805) (layer F.SilkS))
  (gr_text "BY-NC-SA 2016" (at 78.74 88.265) (layer F.SilkS))
  (gr_text "Halibut Transport v1.0a" (at 78.74 85.725) (layer F.SilkS))
  (gr_text Reset (at 170.18 90.805 90) (layer F.SilkS))
  (gr_text "Set 2" (at 170.18 104.14 90) (layer F.SilkS))
  (gr_text "Set 1" (at 170.18 117.475 90) (layer F.SilkS))
  (gr_text 470 (at 85.09 115.57) (layer F.SilkS))
  (gr_text 10k (at 85.09 120.65) (layer F.SilkS))
  (gr_text 10k (at 110.49 123.19) (layer F.SilkS))
  (gr_text .1uF (at 110.49 118.11) (layer F.SilkS))
  (gr_text .1uF (at 123.825 97.155) (layer F.SilkS))
  (gr_text 10k (at 123.825 95.885) (layer F.SilkS))
  (gr_text 10k (at 123.825 94.615) (layer F.SilkS))
  (gr_text 470 (at 136.525 88.265) (layer F.SilkS))
  (gr_text .1uF (at 136.525 95.885) (layer F.SilkS))
  (gr_text 10k (at 136.525 98.425) (layer F.SilkS))
  (gr_text 10k (at 136.525 100.965) (layer F.SilkS))
  (gr_text 10k (at 111.125 100.965) (layer F.SilkS))
  (gr_text 10k (at 111.125 98.425) (layer F.SilkS))
  (gr_text .1uF (at 111.125 95.885) (layer F.SilkS))
  (gr_text 470 (at 111.125 88.265) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.2 76.2) (xy 171.45 76.2) (xy 171.45 132.08) (xy 76.2 132.08)
      )
    )
  )
  (zone (net 8) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.2 76.2) (xy 171.45 76.2) (xy 171.45 132.08) (xy 76.2 132.08)
      )
    )
  )
)
