(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 0.8)
    (drawings 16)
    (tracks 609)
    (zones 0)
    (modules 23)
    (nets 49)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.2)
    (zone_clearance 0.4)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.2)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.5 2)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "MicroGerbers/"))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 /XIN)
  (net 3 "Net-(C6-Pad1)")
  (net 4 "Net-(IC3-Pad15)")
  (net 5 /A7)
  (net 6 /A6)
  (net 7 /A5)
  (net 8 /RESET)
  (net 9 "Net-(LED1-Pad1)")
  (net 10 "Net-(LED2-Pad1)")
  (net 11 "Net-(LED3-Pad2)")
  (net 12 "Net-(LED4-Pad1)")
  (net 13 "Net-(C4-Pad2)")
  (net 14 "Net-(IC1-Pad5)")
  (net 15 /TXLED)
  (net 16 /RXLED)
  (net 17 "Net-(IC1-Pad7)")
  (net 18 /A9)
  (net 19 /WR)
  (net 20 /RD)
  (net 21 /CS)
  (net 22 /A0)
  (net 23 /A1)
  (net 24 /A2)
  (net 25 /A3)
  (net 26 /A4)
  (net 27 /A8)
  (net 28 /A10)
  (net 29 /A11)
  (net 30 /A12)
  (net 31 /A13)
  (net 32 /A14)
  (net 33 /A15)
  (net 34 /D0)
  (net 35 /D1)
  (net 36 /D2)
  (net 37 /D3)
  (net 38 /D4)
  (net 39 /D5)
  (net 40 /D6)
  (net 41 /D7)
  (net 42 /RST)
  (net 43 /RWLED)
  (net 44 GND)
  (net 45 /SNDAIN)
  (net 46 "Net-(IC3-Pad16)")
  (net 47 "Net-(J2-Pad2)")
  (net 48 "Net-(J1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /CS)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /RD)
    (add_net /RESET)
    (add_net /RST)
    (add_net /RWLED)
    (add_net /RXLED)
    (add_net /SNDAIN)
    (add_net /TXLED)
    (add_net /WR)
    (add_net /XIN)
    (add_net GND)
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC3-Pad15)")
    (add_net "Net-(IC3-Pad16)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(LED1-Pad1)")
    (add_net "Net-(LED2-Pad1)")
    (add_net "Net-(LED3-Pad2)")
    (add_net "Net-(LED4-Pad1)")
  )
  (module Symbol:OSHW-Logo2_7.3x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 144.3 53.6)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Custom:FQ1045A-6.000 (layer B.Cu) (tedit 5CFBF0E0)
    (at 127.218 67.7418 180)
    (fp_text reference X1 (at 0.10922 -1.89738 180) (layer B.SilkS))
    (fp_text value 6MHz (at 0 0.5 180) (layer B.Fab))
    (pad 1 smd rect (at 4.28244 -1.96596 180) (size 2.5 3) (layers B.Cu B.Paste B.Mask)
      (net 2 /XIN))
    (pad 2 smd rect (at -4.22402 -1.97358 180) (size 2.5 3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C6-Pad1)"))
  )
  (module Custom:DSL_Cartridge_Reader_Micro (layer F.Cu) (tedit 5CF930D9)
    (at 144.323 64.8208)
    (descr "GBA DS Lite slots commonly found on aliexpress")
    (tags "gameboy cartridge slot")
    (attr smd)
    (fp_text reference J2 (at 0 1.7272 180) (layer F.SilkS) hide)
    (fp_text value CartBus (at 0 -11) (layer F.Fab))
    (fp_text user %R (at 0 -1) (layer F.Fab))
    (pad "" np_thru_hole circle (at -12.93204 -2.04724) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 12.93204 -2.04724) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad GND smd rect (at 12.68204 -12.9208) (size 4.5 2) (layers F.Cu F.Paste F.Mask)
      (net 44 GND))
    (pad GND smd rect (at -12.68204 -12.9208) (size 4.5 2) (layers F.Cu F.Paste F.Mask)
      (net 44 GND))
    (pad 1 smd rect (at -23.25 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 15 smd rect (at -2.25 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /A9))
    (pad 2 smd rect (at -21.75 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(J2-Pad2)"))
    (pad 3 smd rect (at -20.25 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 19 /WR))
    (pad 4 smd rect (at -18.75 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 20 /RD))
    (pad 5 smd rect (at -17.25 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 21 /CS))
    (pad 6 smd rect (at -15.75 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 22 /A0))
    (pad 7 smd rect (at -14.25 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 23 /A1))
    (pad 8 smd rect (at -12.75 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 24 /A2))
    (pad 9 smd rect (at -11.25 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 25 /A3))
    (pad 10 smd rect (at -9.75 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 26 /A4))
    (pad 11 smd rect (at -8.25 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 /A5))
    (pad 12 smd rect (at -6.75 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 6 /A6))
    (pad 13 smd rect (at -5.25 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 /A7))
    (pad 14 smd rect (at -3.75 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 27 /A8))
    (pad 16 smd rect (at -0.75 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 28 /A10))
    (pad 17 smd rect (at 0.75 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 29 /A11))
    (pad 18 smd rect (at 2.25 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 30 /A12))
    (pad 19 smd rect (at 3.75 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 31 /A13))
    (pad 20 smd rect (at 5.25 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 32 /A14))
    (pad 21 smd rect (at 6.75 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 33 /A15))
    (pad 22 smd rect (at 8.25 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 34 /D0))
    (pad 23 smd rect (at 9.75 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 35 /D1))
    (pad 24 smd rect (at 11.25 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 36 /D2))
    (pad 25 smd rect (at 12.75 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 37 /D3))
    (pad 26 smd rect (at 14.25 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 38 /D4))
    (pad 27 smd rect (at 15.75 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 39 /D5))
    (pad 28 smd rect (at 17.25 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 40 /D6))
    (pad 29 smd rect (at 18.75 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 41 /D7))
    (pad 30 smd rect (at 20.25 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 42 /RST))
    (pad 31 smd rect (at 21.75 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 45 /SNDAIN))
    (pad 32 smd rect (at 23.25 5.75) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 44 GND))
  )
  (module Custom:0480372100 (layer B.Cu) (tedit 5CF80A64)
    (at 100.217 61.3562 90)
    (descr 0480372100)
    (tags Connector)
    (fp_text reference J1 (at 0.0254 21.2672 90) (layer B.SilkS) hide)
    (fp_text value USB_B_Micro (at -0.321 5.702 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at 3.5 20.4 90) (size 1.2 2) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 1 20.4 90) (size 1.2 2) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(IC3-Pad16)"))
    (pad 3 smd rect (at -1 20.4 90) (size 1.2 2) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(IC3-Pad15)"))
    (pad 4 smd rect (at -3.5 20.4 90) (size 1.2 2) (layers B.Cu B.Paste B.Mask)
      (net 44 GND))
    (pad 5 thru_hole circle (at -5.85 17.8 90) (size 3.5 3.5) (drill 2.4042) (layers *.Cu *.Mask)
      (net 44 GND))
    (pad 6 thru_hole circle (at 5.85 17.8 90) (size 3.5 3.5) (drill 2.4042) (layers *.Cu *.Mask)
      (net 44 GND))
    (pad 7 thru_hole circle (at 2.25 17.8 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 44 GND))
    (pad 8 thru_hole circle (at -2.25 17.8 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 44 GND))
  )
  (module Custom:Pin_Header_Angled_2x03_Pitch2.54mm (layer B.Cu) (tedit 5C375F91)
    (at 161.201 60.0423 270)
    (descr "Through hole angled pin header, 2x03, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x03 2.54mm double row")
    (fp_text reference JP1 (at 0.762 2.794 270) (layer B.SilkS) hide)
    (fp_text value Conn_02x03_Odd_Even (at 7.3604 -6.1035 270) (layer B.Fab))
    (pad 6 thru_hole oval (at 2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 GND))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /RESET))
    (pad 4 thru_hole oval (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /A5))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /A7))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /A6))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5C796B98)
    (at 130.4 54.3)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.3335) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0.114999 -0.027999) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 44 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 127 53.086)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 1.4224 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 44 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 154 60.1 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 1.27 90) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 44 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 163.614 67.3702 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0.012 1.2065 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 44 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 165.577 53.5814 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 1.2192 180) (layer B.SilkS))
    (fp_text value 22pF (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 44 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 /XIN))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 161.767 53.5814)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0 -1.1684) (layer B.SilkS))
    (fp_text value 22pF (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 44 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer B.Cu) (tedit 5C376399)
    (at 135.607 51.5379 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LED1 (at 0 1.25 180) (layer B.SilkS) hide)
    (fp_text value R/W (at 3.207 0.0379 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(LED1-Pad1)"))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer B.Cu) (tedit 5C37639E)
    (at 141.576 51.5379 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LED2 (at 0 1.25 180) (layer B.SilkS) hide)
    (fp_text value LED (at 0 -1.35 180) (layer B.Fab))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(LED2-Pad1)"))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer B.Cu) (tedit 5C3763A3)
    (at 147.418 51.5379 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LED3 (at 0 1.25 180) (layer B.SilkS) hide)
    (fp_text value LED (at 0 -1.35 180) (layer B.Fab))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(LED3-Pad2)"))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 43 /RWLED))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer B.Cu) (tedit 5CA97E91)
    (at 153.26 51.5379 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LED4 (at 0 1.25 180) (layer B.SilkS) hide)
    (fp_text value PWR (at -2.94 -0.0621 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(LED4-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 134.845 53.8874 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 1.45 90) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 15 /TXLED))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(LED1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 140.814 53.8874 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 1.45 90) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(LED2-Pad1)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 16 /RXLED))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 146.656 53.8874 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.524 270) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(LED3-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 152.498 53.8874 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 1.45 90) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 1 0 90) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(LED4-Pad1)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 44 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 157.366 57.8579 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 1.397 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0.1778 -0.2286 90) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 /RESET))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-44_10x10mm_Pitch0.8mm (layer B.Cu) (tedit 5CF80A6D)
    (at 144.204 62.7411 270)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U1 (at 0 0 270) (layer B.SilkS))
    (fp_text value ATmega8515L-8AU (at 0 -7.45 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -5.7 4 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 7 /A5))
    (pad 2 smd rect (at -5.7 3.2 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 6 /A6))
    (pad 3 smd rect (at -5.7 2.4 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 5 /A7))
    (pad 4 smd rect (at -5.7 1.6 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 8 /RESET))
    (pad 5 smd rect (at -5.7 0.8 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(IC1-Pad5)"))
    (pad 6 smd rect (at -5.7 0 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at -5.7 -0.8 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at -5.7 -1.6 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 43 /RWLED))
    (pad 9 smd rect (at -5.7 -2.4 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 19 /WR))
    (pad 10 smd rect (at -5.7 -3.2 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 20 /RD))
    (pad 11 smd rect (at -5.7 -4 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 21 /CS))
    (pad 12 smd rect (at -4 -5.7 180) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 42 /RST))
    (pad 13 smd rect (at -3.2 -5.7 180) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 45 /SNDAIN))
    (pad 14 smd rect (at -2.4 -5.7 180) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C6-Pad1)"))
    (pad 15 smd rect (at -1.6 -5.7 180) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 /XIN))
    (pad 16 smd rect (at -0.8 -5.7 180) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 44 GND))
    (pad 17 smd rect (at 0 -5.7 180) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 18 smd rect (at 0.8 -5.7 180) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 34 /D0))
    (pad 19 smd rect (at 1.6 -5.7 180) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 35 /D1))
    (pad 20 smd rect (at 2.4 -5.7 180) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 36 /D2))
    (pad 21 smd rect (at 3.2 -5.7 180) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 37 /D3))
    (pad 22 smd rect (at 4 -5.7 180) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 38 /D4))
    (pad 23 smd rect (at 5.7 -4 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 39 /D5))
    (pad 24 smd rect (at 5.7 -3.2 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 40 /D6))
    (pad 25 smd rect (at 5.7 -2.4 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 41 /D7))
    (pad 26 smd rect (at 5.7 -1.6 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 27 smd rect (at 5.7 -0.8 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 28 smd rect (at 5.7 0 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 29 smd rect (at 5.7 0.8 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 30 smd rect (at 5.7 1.6 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 33 /A15))
    (pad 31 smd rect (at 5.7 2.4 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 32 /A14))
    (pad 32 smd rect (at 5.7 3.2 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 31 /A13))
    (pad 33 smd rect (at 5.7 4 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 30 /A12))
    (pad 34 smd rect (at 4 5.7 180) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 29 /A11))
    (pad 35 smd rect (at 3.2 5.7 180) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 28 /A10))
    (pad 36 smd rect (at 2.4 5.7 180) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 18 /A9))
    (pad 37 smd rect (at 1.6 5.7 180) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 27 /A8))
    (pad 38 smd rect (at 0.8 5.7 180) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 39 smd rect (at 0 5.7 180) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 40 smd rect (at -0.8 5.7 180) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 22 /A0))
    (pad 41 smd rect (at -1.6 5.7 180) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 23 /A1))
    (pad 42 smd rect (at -2.4 5.7 180) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 24 /A2))
    (pad 43 smd rect (at -3.2 5.7 180) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 25 /A3))
    (pad 44 smd rect (at -4 5.7 180) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 26 /A4))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/TQFP-44_10x10mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_0603 (layer B.Cu) (tedit 590CE922)
    (at 123.698 53.848 270)
    (descr "Diode SMD in 0603 package http://datasheets.avx.com/schottky.pdf")
    (tags "smd diode")
    (attr smd)
    (fp_text reference PTC1 (at 0 1.397 270) (layer B.SilkS))
    (fp_text value 500mA (at 0 -1.4 270) (layer B.Fab))
    (fp_text user %R (at 0 1.4 270) (layer B.Fab))
    (pad 1 smd rect (at -0.85 0 270) (size 0.6 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.85 0 270) (size 0.6 0.8) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:SSOP-28_5.3x10.2mm_Pitch0.65mm (layer B.Cu) (tedit 5CF80A68)
    (at 130.256 61.4885)
    (descr "28-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U2 (at 0 0 -90) (layer B.SilkS))
    (fp_text value FT232RL (at 0 -6.25) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -3.6 4.225) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(IC1-Pad5)"))
    (pad 2 smd rect (at -3.6 3.575) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at -3.6 2.925) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at -3.6 2.275) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -3.6 1.625) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(IC1-Pad7)"))
    (pad 6 smd rect (at -3.6 0.975) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at -3.6 0.325) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 44 GND))
    (pad 8 smd rect (at -3.6 -0.325) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at -3.6 -0.975) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd rect (at -3.6 -1.625) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd rect (at -3.6 -2.275) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 12 smd rect (at -3.6 -2.925) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 13 smd rect (at -3.6 -3.575) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 14 smd rect (at -3.6 -4.225) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 15 smd rect (at 3.6 -4.225) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(IC3-Pad15)"))
    (pad 16 smd rect (at 3.6 -3.575) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(IC3-Pad16)"))
    (pad 17 smd rect (at 3.6 -2.925) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C4-Pad2)"))
    (pad 18 smd rect (at 3.6 -2.275) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 44 GND))
    (pad 19 smd rect (at 3.6 -1.625) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 20 smd rect (at 3.6 -0.975) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 21 smd rect (at 3.6 -0.325) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 44 GND))
    (pad 22 smd rect (at 3.6 0.325) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 16 /RXLED))
    (pad 23 smd rect (at 3.6 0.975) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 15 /TXLED))
    (pad 24 smd rect (at 3.6 1.625) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 25 smd rect (at 3.6 2.275) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 44 GND))
    (pad 26 smd rect (at 3.6 2.925) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 44 GND))
    (pad 27 smd rect (at 3.6 3.575) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 2 /XIN))
    (pad 28 smd rect (at 3.6 4.225) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/SSOP-28_5.3x10.2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text HDR (at 117.983 70.8) (layer F.SilkS))
  (gr_text 16.08.19 (at 144.6 64.7) (layer F.SilkS))
  (gr_text 6 (at 166.3192 64.8556) (layer B.SilkS))
  (gr_text 1 (at 161.1884 58.0484) (layer B.SilkS))
  (gr_text "Martin Refseth" (at 144.2 62.5) (layer F.SilkS))
  (gr_text "GBFlasher Plug 1.3" (at 157.2768 70.6374) (layer B.SilkS))
  (gr_line (start 115.5294 72) (end 115.5294 50.675) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.35 50.675) (end 115.5294 50.675) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.35 72) (end 115.5294 72) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.35 72) (end 168.35 50.675) (layer Edge.Cuts) (width 0.15))
  (zone (net 44) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.4))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.5192 50.673) (xy 168.3512 50.673) (xy 168.3512 72.009) (xy 115.57 72.009)
      )
    )
  )
  (zone (net 44) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.4))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.5192 50.673) (xy 168.3512 50.673) (xy 168.3512 72.009) (xy 115.57 72.009)
      )
    )
  )
)
