(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 136.398 83.312)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "5V")
  (net 3 "3V3")
  (net 4 "1V8")
  (net 5 "DRV")
  (net 6 "Net-(R1-Pad2)")
  (net 7 "Net-(R3-Pad2)")
  (net 8 "Net-(R4-Pad2)")
  (net 9 "Net-(R5-Pad2)")
  (net 10 "LED2")
  (net 11 "LED1")
  (net 12 "D4-")
  (net 13 "D4+")
  (net 14 "D3-")
  (net 15 "D3+")
  (net 16 "D2-")
  (net 17 "D2+")
  (net 18 "D1-")
  (net 19 "D1+")
  (net 20 "DU-")
  (net 21 "DU+")
  (net 22 "unconnected-(U1-Pad25)")
  (net 23 "unconnected-(U1-Pad27)")
  (net 24 "Net-(U1-Pad2)")
  (net 25 "Net-(U1-Pad3)")
  (footprint "Connector_PinHeader_2.54mm:2.54mm 1x4 header edge" (layer "F.Cu")
    (tedit 0)
    (at 120.65 93.98 90)
    (property "Sheetfile" "simple_fe1.1s_hub.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at 4.318 0.762 unlocked) (layer "F.SilkS"))
    (fp_text value "Conn_01x04" (at 1.651 12.7 90 unlocked) (layer "F.Fab"))
    (fp_text user "Pins out this way" (at -2.159 4.445 180 unlocked) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 1.651 11.43 90 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 1.651 1.27 90) (size 3.1 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.651 3.81 90) (size 3.1 1.524) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "D1-") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at 1.651 6.35 90) (size 3.1 1.524) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "D1+") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at 1.651 8.89 90) (size 3.1 1.524) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 127.508 89.408 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "simple_fe1.1s_hub.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at -2.413 0) (layer "F.SilkS"))
    (fp_text value "2.7K 1%" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 9 "Net-(R5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 132.588 78.994 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "simple_fe1.1s_hub.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 0) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 4 "1V8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 138.303 71.882)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (property "Sheetfile" "simple_fe1.1s_hub.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -5.08) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Package_SO:SSOP-28_3.9x9.9mm_P0.635mm" (layer "F.Cu")
    (tedit 5A02F25C)
    (at 126.492 83.058)
    (descr "SSOP28: plastic shrink small outline package; 28 leads; body width 3.9 mm; lead pitch 0.635; (see http://cds.linear.com/docs/en/datasheet/38901fb.pdf)")
    (tags "SSOP 0.635")
    (property "Sheetfile" "simple_fe1.1s_hub.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -1.778) (layer "F.SilkS"))
    (fp_text value "FE1.1s" (at -0.1 6.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.6 -4.1275) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "2" smd rect (at -2.6 -3.4925) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(U1-Pad2)") (pinfunction "XOUT") (pintype "output"))
    (pad "3" smd rect (at -2.6 -2.8575) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(U1-Pad3)") (pinfunction "XIN") (pintype "input"))
    (pad "4" smd rect (at -2.6 -2.2225) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "D4-") (pinfunction "DM4") (pintype "bidirectional"))
    (pad "5" smd rect (at -2.6 -1.5875) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "D4+") (pinfunction "DP4") (pintype "bidirectional"))
    (pad "6" smd rect (at -2.6 -0.9525) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "D3-") (pinfunction "DM3") (pintype "bidirectional"))
    (pad "7" smd rect (at -2.6 -0.3175) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "D3+") (pinfunction "DP3") (pintype "bidirectional"))
    (pad "8" smd rect (at -2.6 0.3175) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "D2-") (pinfunction "DM2") (pintype "bidirectional"))
    (pad "9" smd rect (at -2.6 0.9525) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "D2+") (pinfunction "DP2") (pintype "bidirectional"))
    (pad "10" smd rect (at -2.6 1.5875) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "D1-") (pinfunction "DM1") (pintype "bidirectional"))
    (pad "11" smd rect (at -2.6 2.2225) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "D1+") (pinfunction "DP1") (pintype "bidirectional"))
    (pad "12" smd rect (at -2.6 2.8575) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "1V8") (pinfunction "VD18_O") (pintype "power_out"))
    (pad "13" smd rect (at -2.6 3.4925) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "3V3") (pinfunction "VD33") (pintype "power_in"))
    (pad "14" smd rect (at -2.6 4.1275) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(R5-Pad2)") (pinfunction "REXT") (pintype "passive"))
    (pad "15" smd rect (at 2.6 4.1275) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "DU-") (pinfunction "DMU") (pintype "bidirectional"))
    (pad "16" smd rect (at 2.6 3.4925) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "DU+") (pinfunction "DPU") (pintype "bidirectional"))
    (pad "17" smd rect (at 2.6 2.8575) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(R4-Pad2)") (pinfunction "~{XRSTJ}") (pintype "input"))
    (pad "18" smd rect (at 2.6 2.2225) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(R1-Pad2)") (pinfunction "VBUSM") (pintype "input"))
    (pad "19" smd rect (at 2.6 1.5875) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(R3-Pad2)") (pinfunction "BUSJ") (pintype "input"))
    (pad "20" smd rect (at 2.6 0.9525) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "5V") (pinfunction "VDD5") (pintype "power_in"))
    (pad "21" smd rect (at 2.6 0.3175) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "3V3") (pinfunction "VD33_O") (pintype "power_out"))
    (pad "22" smd rect (at 2.6 -0.3175) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "DRV") (pinfunction "DRV") (pintype "bidirectional"))
    (pad "23" smd rect (at 2.6 -0.9525) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "LED1") (pinfunction "LED1/EESCL") (pintype "bidirectional"))
    (pad "24" smd rect (at 2.6 -1.5875) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "LED2") (pinfunction "LED2") (pintype "bidirectional"))
    (pad "25" smd rect (at 2.6 -2.2225) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "unconnected-(U1-Pad25)") (pinfunction "PWRJ") (pintype "output+no_connect"))
    (pad "26" smd rect (at 2.6 -2.8575) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "3V3") (pinfunction "OVCJ") (pintype "input"))
    (pad "27" smd rect (at 2.6 -3.4925) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "unconnected-(U1-Pad27)") (pinfunction "TESTJ/EESDA") (pintype "bidirectional+no_connect"))
    (pad "28" smd rect (at 2.6 -4.1275) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "1V8") (pinfunction "VD18") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SSOP-28_3.9x9.9mm_P0.635mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_HC49-U_Vertical" (layer "F.Cu")
    (tedit 5A1AD3B8)
    (at 125.603 74.93)
    (descr "Crystal THT HC-49/U http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49/U")
    (property "Sheetfile" "simple_fe1.1s_hub.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Y1" (at 2.44 0) (layer "F.SilkS"))
    (fp_text value "Crystal" (at 2.44 3.525) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.44 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(U1-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 4.88 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(U1-Pad3)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_HC49-U_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:2.54mm 1x4 header edge" (layer "F.Cu")
    (tedit 0)
    (at 116.205 82.55)
    (property "Sheetfile" "simple_fe1.1s_hub.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J2" (at 2.921 -0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "Conn_01x04" (at 1.651 12.7 unlocked) (layer "F.Fab"))
    (fp_text user "Pins out this way" (at -2.159 4.445 90 unlocked) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 1.651 11.43 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 1.651 1.27) (size 3.1 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.651 3.81) (size 3.1 1.524) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "D2-") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at 1.651 6.35) (size 3.1 1.524) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "D2+") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at 1.651 8.89) (size 3.1 1.524) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive"))
  )
  (footprint "Connector_PinHeader_2.54mm:2.54mm 1x4 header edge" (layer "F.Cu")
    (tedit 0)
    (at 116.205 69.85)
    (property "Sheetfile" "simple_fe1.1s_hub.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J3" (at 2.921 -0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "Conn_01x04" (at 1.651 12.7 unlocked) (layer "F.Fab"))
    (fp_text user "Pins out this way" (at -2.159 4.445 90 unlocked) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 1.651 11.43 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 1.651 1.27) (size 3.1 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.651 3.81) (size 3.1 1.524) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "D3-") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at 1.651 6.35) (size 3.1 1.524) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "D3+") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at 1.651 8.89) (size 3.1 1.524) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive"))
  )
  (footprint "Connector_PinHeader_2.54mm:2.54mm 1x4 header edge" (layer "F.Cu")
    (tedit 0)
    (at 130.556 68.58 -90)
    (property "Sheetfile" "simple_fe1.1s_hub.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J4" (at 2.921 -0.635 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "Conn_01x04" (at 1.651 12.7 -90 unlocked) (layer "F.Fab"))
    (fp_text user "Pins out this way" (at -2.159 4.445 unlocked) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 1.651 11.43 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 1.651 1.27 270) (size 3.1 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.651 3.81 270) (size 3.1 1.524) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "D4-") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at 1.651 6.35 270) (size 3.1 1.524) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "D4+") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at 1.651 8.89 270) (size 3.1 1.524) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive"))
  )
  (footprint "Connector_PinHeader_2.54mm:2.54mm 1x4 header edge" (layer "F.Cu")
    (tedit 0)
    (at 141.383 92.202 180)
    (property "Sheetfile" "simple_fe1.1s_hub.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J5" (at 2.921 -0.635 unlocked) (layer "F.SilkS"))
    (fp_text value "Conn_01x04" (at 1.651 12.7 180 unlocked) (layer "F.Fab"))
    (fp_text user "Pins out this way" (at -2.159 4.445 270 unlocked) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 1.651 11.43 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 1.651 1.27 180) (size 3.1 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.651 3.81 180) (size 3.1 1.524) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "DU-") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at 1.651 6.35 180) (size 3.1 1.524) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "DU+") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at 1.651 8.89 180) (size 3.1 1.524) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 131.826 84.582 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "simple_fe1.1s_hub.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 2.54 0 90) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 3 "3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 7 "Net-(R3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 134.112 84.582 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "simple_fe1.1s_hub.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 2.54 0 90) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 3 "3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 8 "Net-(R4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 136.398 82.804 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "simple_fe1.1s_hub.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 0 90) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 132.842 69.85)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "simple_fe1.1s_hub.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 0 0) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 132.588 81.534 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "simple_fe1.1s_hub.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 0) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 3 "3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 136.144 90.678 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "simple_fe1.1s_hub.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.524 90) (layer "F.SilkS"))
    (fp_text value "47K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 2 "5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 6 "Net-(R1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 132.842 90.678 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "simple_fe1.1s_hub.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.524 90) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 6 "Net-(R1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 140.434186 68.58) (end 117.375814 68.58) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 116.205 69.750814) (end 116.205 92.809186) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 117.375814 93.98) (mid 116.547923 93.637077) (end 116.205 92.809186) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 117.375814 93.98) (end 140.434186 93.98) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 140.434186 68.58) (mid 141.262077 68.922923) (end 141.605 69.750814) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 141.605 92.809186) (end 141.605 69.750814) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 141.605 92.809186) (mid 141.262077 93.637077) (end 140.434186 93.98) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 116.205 69.750814) (mid 116.547923 68.922923) (end 117.375814 68.58) (layer "Edge.Cuts") (width 0.1))
  (gr_text "One Square Inch of Love\nfrom\ngithub.com/xunker" (at 128.778 80.772) (layer "B.SilkS"))
  (gr_text "D-" (at 140.97 88.392 180) (layer "B.SilkS"))
  (gr_text "UPLINK\nPORT 0" (at 136.906 87.122 90) (layer "B.SilkS"))
  (gr_text "GND" (at 121.158 69.088 270) (layer "B.SilkS"))
  (gr_text "5V" (at 140.97 90.932 180) (layer "B.SilkS"))
  (gr_text "D-" (at 116.586 73.66) (layer "B.SilkS"))
  (gr_text "5V" (at 116.586 83.82) (layer "B.SilkS"))
  (gr_text "D+" (at 140.97 85.852 180) (layer "B.SilkS"))
  (gr_text "GND" (at 129.794 93.472 90) (layer "B.SilkS"))
  (gr_text "D+" (at 123.698 69.088 270) (layer "B.SilkS"))
  (gr_text "5V" (at 122.174 93.472 90) (layer "B.SilkS"))
  (gr_text "5V" (at 128.778 69.088 270) (layer "B.SilkS"))
  (gr_text "D+" (at 127.254 93.472 90) (layer "B.SilkS"))
  (gr_text "GND" (at 140.97 83.312 180) (layer "B.SilkS"))
  (gr_text "D+" (at 116.586 88.9) (layer "B.SilkS"))
  (gr_text "PORT 3" (at 119.634 74.93 270) (layer "B.SilkS"))
  (gr_text "GND" (at 116.586 91.44) (layer "B.SilkS"))
  (gr_text "PORT 4" (at 125.476 72.136 180) (layer "B.SilkS"))
  (gr_text "D-" (at 126.238 69.088 270) (layer "B.SilkS"))
  (gr_text "PORT 2" (at 119.634 87.63 270) (layer "B.SilkS"))
  (gr_text "5V" (at 116.586 71.12) (layer "B.SilkS"))
  (gr_text "D+" (at 116.586 76.2) (layer "B.SilkS"))
  (gr_text "PORT 1" (at 125.73 90.678) (layer "B.SilkS"))
  (gr_text "D-" (at 124.714 93.472 90) (layer "B.SilkS"))
  (gr_text "GND" (at 116.586 78.74) (layer "B.SilkS"))
  (gr_text "FE1.1S\nUSB HUB" (at 137.668 75.692) (layer "B.SilkS"))
  (gr_text "D-" (at 116.586 86.36) (layer "B.SilkS"))
  (gr_text "UPLINK" (at 137.414 89.408 90) (layer "F.SilkS"))
  (gr_text "FE1.1S\nUSB HUB" (at 137.668 75.692) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 116.205 93.98) (xy 141.605 93.98))
    (height 3.81)
    (gr_text "25.4000 mm" (at 128.905 96.64) (layer "Cmts.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 118.11 68.58) (xy 118.11 93.98))
    (height 3.81)
    (gr_text "25.4000 mm" (at 113.15 81.28 90) (layer "Cmts.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 1) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162.56 116.84)
        (xy 111.76 116.84)
        (xy 111.76 63.5)
        (xy 162.56 63.5)
      )
    )
  )
)
