<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.1">
<drawing>
<board>
<plain>
<wire x1="34.8674125" y1="5.61841875" x2="50.090853125" y2="6.12786875" width="0" layer="20"/>
<wire x1="50.090853125" y1="6.12786875" x2="50.9674125" y2="7.034253125" width="0" layer="20" curve="88.084705"/>
<wire x1="50.9674125" y1="7.034253125" x2="50.9674125" y2="10.375540625" width="0" layer="20"/>
<wire x1="50.9674125" y1="10.375540625" x2="49.092953125" y2="12" width="0" layer="20" curve="90"/>
<wire x1="49.092953125" y1="12" x2="17.346090625" y2="12" width="0" layer="20"/>
<wire x1="17.346090625" y1="12" x2="15.4174125" y2="10.321321875" width="0" layer="20" curve="90"/>
<wire x1="15.4174125" y1="10.321321875" x2="15.4174125" y2="7.05413125" width="0" layer="20"/>
<wire x1="15.4174125" y1="7.05413125" x2="16.306146875" y2="6.133928125" width="0" layer="20" curve="88.006597"/>
<wire x1="16.306146875" y1="6.133928125" x2="31.1174125" y2="5.61841875" width="0" layer="20"/>
<wire x1="31.1174125" y1="5.61841875" x2="31.1174125" y2="6.764975" width="0" layer="20"/>
<wire x1="31.1174125" y1="6.764975" x2="32.67085625" y2="8.66841875" width="0" layer="20" curve="-90"/>
<wire x1="32.67085625" y1="8.66841875" x2="33.23493125" y2="8.66841875" width="0" layer="20"/>
<wire x1="33.23493125" y1="8.66841875" x2="34.8674125" y2="6.6359375" width="0" layer="20" curve="-90"/>
<wire x1="34.8674125" y1="6.6359375" x2="34.8674125" y2="5.61841875" width="0" layer="20"/>
<text>C:/My Downloads/gbabattery/pics/002-2.bmp</text>
<text>insideGadgets</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="R0805_2">
</package>
<package name="CHIPLED_1206_SLIM">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="1X01_SMD_SM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED2" library="adafruit" package="CHIPLED_1206_SLIM" value="Red">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="SparkFun" package="1X01_SMD_SM" value="M01"/>
<element name="LED3" library="adafruit" package="CHIPLED_1206_SLIM" value="Red">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="adafruit" package="CHIPLED_1206_SLIM" value="Blue">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED5" library="adafruit" package="CHIPLED_1206_SLIM" value="Blue">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R0805_2" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="R0805_2" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="R0805_2" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="adafruit" package="R0805_2" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED6" library="adafruit" package="CHIPLED_1206_SLIM" value="Blue">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED8" library="adafruit" package="CHIPLED_1206_SLIM" value="Green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED7" library="adafruit" package="CHIPLED_1206_SLIM" value="Blue">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="adafruit" package="R0805_2" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="adafruit" package="R0805_2" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="adafruit" package="R0805_2" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED9" library="adafruit" package="CHIPLED_1206_SLIM" value="Green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="adafruit" package="R0805_2" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun" package="1X01_SMD_SM" value="M01"/>
<element name="JP2" library="SparkFun" package="1X01_SMD_SM" value="M01"/>
<element name="JP3" library="SparkFun" package="1X01_SMD_SM" value="M01"/>
<element name="JP4" library="SparkFun" package="1X01_SMD_SM" value="M01"/>
<element name="JP5" library="SparkFun" package="1X01_SMD_SM" value="M01"/>
<element name="JP6" library="SparkFun" package="1X01_SMD_SM" value="M01"/>
<element name="JP7" library="SparkFun" package="1X01_SMD_SM" value="M01"/>
<element name="JP8" library="SparkFun" package="1X01_SMD_SM" value="M01"/>
<element name="LED1" library="adafruit" package="CHIPLED_1206_SLIM" value="Red">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="R0805_2" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP9" library="SparkFun" package="1X01_SMD_SM" value="M01"/>
<element name="LED10" library="adafruit" package="CHIPLED_1206_SLIM" value="Green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="adafruit" package="R0805_2" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP10" library="SparkFun" package="1X01_SMD_SM" value="M01"/>
</elements>
<signals>
<signal name="GND">
<contactref element="LED5" pad="C"/>
<contactref element="LED4" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED7" pad="C"/>
<contactref element="LED8" pad="C"/>
<contactref element="LED6" pad="C"/>
<contactref element="LED9" pad="C"/>
<contactref element="GND" pad="P$1"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED10" pad="C"/>
</signal>
<signal name="N$1">
<contactref element="LED2" pad="A"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="LED3" pad="A"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="LED4" pad="A"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="LED5" pad="A"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="LED6" pad="A"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="LED8" pad="A"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="LED7" pad="A"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="LED9" pad="A"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R12" pad="1"/>
<contactref element="JP1" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="R9" pad="1"/>
<contactref element="JP2" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="R10" pad="1"/>
<contactref element="JP3" pad="P$1"/>
</signal>
<signal name="N$12">
<contactref element="R11" pad="1"/>
<contactref element="JP4" pad="P$1"/>
</signal>
<signal name="N$13">
<contactref element="R1" pad="1"/>
<contactref element="JP5" pad="P$1"/>
</signal>
<signal name="N$14">
<contactref element="R3" pad="1"/>
<contactref element="JP6" pad="P$1"/>
</signal>
<signal name="N$15">
<contactref element="R4" pad="1"/>
<contactref element="JP7" pad="P$1"/>
</signal>
<signal name="N$16">
<contactref element="R5" pad="1"/>
<contactref element="JP8" pad="P$1"/>
</signal>
<signal name="N$18">
<contactref element="LED1" pad="A"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="R2" pad="1"/>
<contactref element="JP9" pad="P$1"/>
</signal>
<signal name="N$20">
<contactref element="LED10" pad="A"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="R6" pad="1"/>
<contactref element="JP10" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
