(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "USLetter")
  (title_block
    (rev "1")
  )
  (layers
    (0 "F.Cu" signal "Front")
    (31 "B.Cu" signal "Back")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./gerbers")
    )
  )
  (net 0 "")
  (net 1 "unconnected-(CC1-PadD4)")
  (net 2 "unconnected-(CC1-Pad5V2)")
  (net 3 "unconnected-(CC1-PadAREF)")
  (net 4 "unconnected-(CC1-PadGND4)")
  (net 5 "unconnected-(CC1-PadIORF)")
  (net 6 "unconnected-(CC1-PadMISO)")
  (net 7 "unconnected-(CC1-PadMOSI)")
  (net 8 "Net-(CC1-PadRST1)")
  (net 9 "unconnected-(CC1-PadRST2)")
  (net 10 "unconnected-(CC1-PadSCK)")
  (net 11 "GND")
  (net 12 "unconnected-(CC1-PadD5)")
  (net 13 "unconnected-(CC1-PadD10)")
  (net 14 "unconnected-(CC1-PadD13)")
  (net 15 "unconnected-(CC1-Pad5V1)")
  (net 16 "/12v")
  (net 17 "+3.3V")
  (net 18 "/chain_top_ctl")
  (net 19 "/chain_middle_ctl")
  (net 20 "/chain_bottom_ctl")
  (net 21 "/center_drawer_rtn")
  (net 22 "/chain_top_rtn")
  (net 23 "/chain_middle_rtn")
  (net 24 "/chain_bottom_rtn")
  (net 25 "/chain_top_left_sense")
  (net 26 "/chain_top_right_sense")
  (net 27 "/chain_middle_left_sense")
  (net 28 "/chain_middle_right_sense")
  (net 29 "/chain_bottom_left_sense")
  (net 30 "/chain_bottom_right_sense")
  (net 31 "/center_drawer_sense")
  (net 32 "/pen_sense")
  (net 33 "/arithmo_0")
  (net 34 "/arithmo_1")
  (net 35 "/arithmo_2")
  (net 36 "/arithmo_3")
  (net 37 "/arithmo_4")
  (net 38 "/arithmo_5")
  (net 39 "/center_drawer_ctl")
  (footprint "digikey-footprints:PinHeader_1x3_P2.5mm_Drill1.1mm" (layer "F.Cu")
    (tedit 5A4D0CA0)
    (at 120.65 83.82)
    (descr "http://www.jst-mfg.com/product/pdf/eng/eXH.pdf")
    (property "Category" "Connectors, Interconnects")
    (property "DK_Datasheet_Link" "http://www.jst-mfg.com/product/pdf/eng/eXH.pdf")
    (property "DK_Detail_Page" "/product-detail/en/jst-sales-america-inc/B3B-XH-A(LF)(SN)/455-2248-ND/1651046")
    (property "Description" "CONN HEADER VERT 3POS 2.5MM")
    (property "Digi-Key_PN" "455-2248-ND")
    (property "Family" "Rectangular Connectors - Headers, Male Pins")
    (property "MPN" "B3B-XH-A(LF)(SN)")
    (property "Manufacturer" "JST Sales America Inc.")
    (property "Sheetfile" "desk_bottom_controller_shield.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (attr through_hole)
    (fp_text reference "J4" (at 2.8 -4) (layer "F.SilkS"))
    (fp_text value "Pen" (at 1.48 4.41) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.4 -0.1) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 "GND") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 5 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 32 "/pen_sense") (pintype "passive"))
  )
  (footprint "B8B_XH_A_LF__SN_:JST_B8B-XH-A(LF)(SN)" (layer "F.Cu")
    (tedit 648A17A1)
    (at 137.795 96.52)
    (property "MANUFACTURER" "JST Sales America Inc.")
    (property "MAXIMUM_PACKAGE_HEIGHT" "7 mm")
    (property "PARTREV" "N/A")
    (property "SNAPEDA_PN" "B8B-XH-A(LF)(SN)")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "desk_bottom_controller_shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at -8.275 -4.76) (layer "F.SilkS"))
    (fp_text value "Arithmometer" (at 1.25 4.76) (layer "F.SilkS"))
    (pad "1" thru_hole rect locked (at -8.75 0.525) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 11 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -6.25 0.525) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 17 "+3.3V") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -3.75 0.525) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 33 "/arithmo_0") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at -1.25 0.525) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 34 "/arithmo_1") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 1.25 0.525) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 35 "/arithmo_2") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 3.75 0.525) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 36 "/arithmo_3") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle locked (at 6.25 0.525) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 37 "/arithmo_4") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle locked (at 8.75 0.525) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 38 "/arithmo_5") (pinfunction "8") (pintype "passive"))
  )
  (footprint "G3VM-41AY1:A-DIP4_THD_OMR" (layer "F.Cu")
    (tedit 0)
    (at 144.78 77.47 -90)
    (tags "G3VM-41AY1 ")
    (property "Sheetfile" "desk_bottom_controller_shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "K1" (at 3.81 1.27 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "CH_TP" (at 3.81 1.27 -90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -1.4224 -90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -1.4224 90) (layer "F.SilkS"))
    (fp_text user "*" (at 0.864 0 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 1.27 -90 unlocked) (layer "F.Fab") hide)
    (fp_text user "*" (at 0.864 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 18 "/chain_top_ctl") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 0 2.54 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 "GND") (pinfunction "2") (pintype "unspecified"))
    (pad "3" thru_hole circle (at 7.62 2.54 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 "GND") (pinfunction "3") (pintype "unspecified"))
    (pad "4" thru_hole circle (at 7.62 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 22 "/chain_top_rtn") (pinfunction "4") (pintype "unspecified"))
  )
  (footprint "digikey-footprints:PinHeader_1x4_P2.5mm_Drill1.1mm" (layer "F.Cu")
    (tedit 5A4D1100)
    (at 155.575 96.52)
    (descr "http://www.jst-mfg.com/product/pdf/eng/eXH.pdf")
    (property "Category" "Connectors, Interconnects")
    (property "DK_Datasheet_Link" "http://www.jst-mfg.com/product/pdf/eng/eXH.pdf")
    (property "DK_Detail_Page" "/product-detail/en/jst-sales-america-inc/B4B-XH-A(LF)(SN)/455-2249-ND/1651047")
    (property "Description" "CONN HEADER VERT 4POS 2.5MM")
    (property "Digi-Key_PN" "455-2249-ND")
    (property "Family" "Rectangular Connectors - Headers, Male Pins")
    (property "MPN" "B4B-XH-A(LF)(SN)")
    (property "Manufacturer" "JST Sales America Inc.")
    (property "Sheetfile" "desk_bottom_controller_shield.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (attr through_hole)
    (fp_text reference "J1" (at 3.4 -3.9) (layer "F.SilkS"))
    (fp_text value "Locks" (at 3.3 4.3) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.8 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 "/chain_top_rtn") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 23 "/chain_middle_rtn") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 5 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 24 "/chain_bottom_rtn") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 7.5 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 21 "/center_drawer_rtn") (pintype "passive"))
  )
  (footprint "orange_switch:SW_B3F-1000_OMR" (layer "F.Cu")
    (tedit 0)
    (at 109.855 100.33)
    (tags "B3F-1002 ")
    (property "Sheetfile" "desk_bottom_controller_shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW1" (at 3.250001 2.250001 unlocked) (layer "F.SilkS"))
    (fp_text value "Reset" (at 3.250001 6.35 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.250001 2.250001 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.507998 1.507998) (drill 0.999998) (layers *.Cu *.Mask)
      (net 8 "Net-(CC1-PadRST1)") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 6.500002 0) (size 1.507998 1.507998) (drill 0.999998) (layers *.Cu *.Mask))
    (pad "3" thru_hole circle (at 0 4.500001) (size 1.507998 1.507998) (drill 0.999998) (layers *.Cu *.Mask))
    (pad "4" thru_hole circle (at 6.500002 4.500001) (size 1.507998 1.507998) (drill 0.999998) (layers *.Cu *.Mask)
      (net 11 "GND") (pinfunction "4") (pintype "unspecified"))
  )
  (footprint "B7B_XH_A_LF__SN_:B7B-XH-A_LF__SN_" (layer "F.Cu")
    (tedit 6489E0FC)
    (at 128.27 73.025)
    (property "MANUFACTURER" "JST Sales America Inc.")
    (property "MAXIMUM_PACKAGE_HEIGHT" "7 mm")
    (property "PARTREV" "N/A")
    (property "SNAPEDA_PN" "B7B-XH-A(LF)(SN)")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "desk_bottom_controller_shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -7.025 -4.76) (layer "F.SilkS"))
    (fp_text value "Lock Sense" (at 0 4.445) (layer "F.SilkS"))
    (pad "1" thru_hole rect locked (at -7.5 0.525) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 25 "/chain_top_left_sense") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -5 0.525) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 26 "/chain_top_right_sense") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -2.5 0.525) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 27 "/chain_middle_left_sense") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 0 0.525) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 28 "/chain_middle_right_sense") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 2.5 0.525) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 29 "/chain_bottom_left_sense") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 5 0.525) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 30 "/chain_bottom_right_sense") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle locked (at 7.5 0.525) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 31 "/center_drawer_sense") (pinfunction "7") (pintype "passive"))
  )
  (footprint "G3VM-41AY1:A-DIP4_THD_OMR" (layer "F.Cu")
    (tedit 0)
    (at 163.83 77.47 -90)
    (tags "G3VM-41AY1 ")
    (property "Sheetfile" "desk_bottom_controller_shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "K3" (at 3.81 1.27 -90 unlocked) (layer "F.Fab") hide)
    (fp_text value "DRWR" (at 3.81 1.27 -90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -1.4224 -90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -1.4224 90) (layer "F.SilkS"))
    (fp_text user "*" (at 0.864 0 -90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0.864 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 1.27 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 39 "/center_drawer_ctl") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 0 2.54 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 "GND") (pinfunction "2") (pintype "unspecified"))
    (pad "3" thru_hole circle (at 7.62 2.54 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 "GND") (pinfunction "3") (pintype "unspecified"))
    (pad "4" thru_hole circle (at 7.62 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 21 "/center_drawer_rtn") (pinfunction "4") (pintype "unspecified"))
  )
  (footprint "G3VM-41AY1:A-DIP4_THD_OMR" (layer "F.Cu")
    (tedit 0)
    (at 157.48 77.47 -90)
    (tags "G3VM-41AY1 ")
    (property "Sheetfile" "desk_bottom_controller_shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "K4" (at 3.81 1.27 -90 unlocked) (layer "F.Fab") hide)
    (fp_text value "CH_BT" (at 3.81 1.27 -90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -1.4224 -90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -1.4224 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 1.27 -90 unlocked) (layer "F.Fab") hide)
    (fp_text user "*" (at 0.864 0 90) (layer "F.Fab"))
    (fp_text user "*" (at 0.864 0 -90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 20 "/chain_bottom_ctl") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 0 2.54 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 "GND") (pinfunction "2") (pintype "unspecified"))
    (pad "3" thru_hole circle (at 7.62 2.54 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 "GND") (pinfunction "3") (pintype "unspecified"))
    (pad "4" thru_hole circle (at 7.62 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 24 "/chain_bottom_rtn") (pinfunction "4") (pintype "unspecified"))
  )
  (footprint "Arduino:Arduino_Uno_Shield" locked (layer "F.Cu")
    (tedit 5A8605EC)
    (at 104.514 113.084237)
    (descr "https://docs.arduino.cc/hardware/uno-rev3")
    (property "Sheetfile" "desk_bottom_controller_shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "CC1" (at -2.914 -52.124237) (layer "F.Fab") hide)
    (fp_text value "Desk Bottom Control Shield" (at 27.305 -54.356) (layer "B.Fab") hide)
    (fp_text user "Barrel Jack" (at 5.065 -7.7981) (layer "B.Fab") hide)
    (fp_text user "USB" (at 1.535 -38.0986) (layer "B.Fab") hide)
    (pad "" thru_hole oval locked (at 27.94 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 13.97 -2.54) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 66.04 -7.62) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 66.04 -35.56) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 15.24 -50.8) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "3V3" thru_hole oval locked (at 35.56 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "+3.3V") (pinfunction "3.3V") (pintype "power_out"))
    (pad "5V1" thru_hole oval locked (at 38.1 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "unconnected-(CC1-Pad5V1)") (pinfunction "5V") (pintype "power_in"))
    (pad "5V2" thru_hole oval locked (at 66.167 -30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "unconnected-(CC1-Pad5V2)") (pinfunction "SPI_5V") (pintype "power_in"))
    (pad "A0" thru_hole oval locked (at 50.8 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 "/arithmo_0") (pinfunction "A0") (pintype "bidirectional"))
    (pad "A1" thru_hole oval locked (at 53.34 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 "/arithmo_1") (pinfunction "A1") (pintype "bidirectional"))
    (pad "A2" thru_hole oval locked (at 55.88 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 "/arithmo_2") (pinfunction "A2") (pintype "bidirectional"))
    (pad "A3" thru_hole oval locked (at 58.42 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 "/arithmo_3") (pinfunction "A3") (pintype "bidirectional"))
    (pad "A4" thru_hole oval locked (at 60.96 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 "/arithmo_4") (pinfunction "A4") (pintype "bidirectional"))
    (pad "A5" thru_hole oval locked (at 63.5 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 "/arithmo_5") (pinfunction "A5") (pintype "bidirectional"))
    (pad "AREF" thru_hole oval locked (at 23.876 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "unconnected-(CC1-PadAREF)") (pinfunction "AREF") (pintype "input"))
    (pad "D0" thru_hole oval locked (at 63.5 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 "/center_drawer_ctl") (pinfunction "D0_RX0") (pintype "bidirectional"))
    (pad "D1" thru_hole oval locked (at 60.96 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "/chain_bottom_ctl") (pinfunction "D1_TX0") (pintype "bidirectional"))
    (pad "D2" thru_hole oval locked (at 58.42 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "/chain_middle_ctl") (pinfunction "D2_INT0") (pintype "bidirectional"))
    (pad "D3" thru_hole oval locked (at 55.88 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "/chain_top_ctl") (pinfunction "D3_INT1") (pintype "bidirectional"))
    (pad "D4" thru_hole oval locked (at 53.34 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "unconnected-(CC1-PadD4)") (pinfunction "D4") (pintype "bidirectional"))
    (pad "D5" thru_hole oval locked (at 50.8 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "unconnected-(CC1-PadD5)") (pinfunction "D5") (pintype "bidirectional"))
    (pad "D6" thru_hole oval locked (at 48.26 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 "/center_drawer_sense") (pinfunction "D6") (pintype "bidirectional"))
    (pad "D7" thru_hole oval locked (at 45.72 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "/chain_bottom_right_sense") (pinfunction "D7") (pintype "bidirectional"))
    (pad "D8" thru_hole oval locked (at 41.656 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "/chain_bottom_left_sense") (pinfunction "D8") (pintype "bidirectional"))
    (pad "D9" thru_hole oval locked (at 39.116 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "/chain_middle_right_sense") (pinfunction "D9") (pintype "bidirectional"))
    (pad "D10" thru_hole oval locked (at 36.576 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "unconnected-(CC1-PadD10)") (pinfunction "D10_CS") (pintype "bidirectional"))
    (pad "D11" thru_hole oval locked (at 34.036 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "/chain_middle_left_sense") (pinfunction "D11") (pintype "bidirectional"))
    (pad "D12" thru_hole oval locked (at 31.496 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "/chain_top_right_sense") (pinfunction "D12") (pintype "bidirectional"))
    (pad "D13" thru_hole oval locked (at 28.956 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "unconnected-(CC1-PadD13)") (pinfunction "D13") (pintype "bidirectional"))
    (pad "GND1" thru_hole rect locked (at 26.416 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "GND2" thru_hole rect locked (at 40.64 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "GND3" thru_hole rect locked (at 43.18 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "GND4" thru_hole rect locked (at 66.167 -25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "unconnected-(CC1-PadGND4)") (pinfunction "SPI_GND") (pintype "power_in"))
    (pad "IORF" thru_hole oval locked (at 30.48 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "unconnected-(CC1-PadIORF)") (pinfunction "IOREF") (pintype "output"))
    (pad "MISO" thru_hole oval locked (at 63.627 -30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "unconnected-(CC1-PadMISO)") (pinfunction "SPI_MISO") (pintype "input"))
    (pad "MOSI" thru_hole oval locked (at 66.167 -27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "unconnected-(CC1-PadMOSI)") (pinfunction "SPI_MOSI") (pintype "output"))
    (pad "RST1" thru_hole oval locked (at 33.02 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(CC1-PadRST1)") (pinfunction "RESET") (pintype "open_collector"))
    (pad "RST2" thru_hole oval locked (at 63.627 -25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "unconnected-(CC1-PadRST2)") (pinfunction "SPI_RESET") (pintype "open_collector"))
    (pad "SCK" thru_hole oval locked (at 63.627 -27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "unconnected-(CC1-PadSCK)") (pinfunction "SPI_SCK") (pintype "output"))
    (pad "SCL" thru_hole oval locked (at 18.796 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 "/pen_sense") (pinfunction "SCL") (pintype "bidirectional"))
    (pad "SDA" thru_hole oval locked (at 21.336 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "/chain_top_left_sense") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "VIN" thru_hole oval locked (at 45.72 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "/12v") (pinfunction "VIN") (pintype "power_in"))
  )
  (footprint "G3VM-41AY1:A-DIP4_THD_OMR" (layer "F.Cu")
    (tedit 0)
    (at 151.13 77.47 -90)
    (tags "G3VM-41AY1 ")
    (property "Sheetfile" "desk_bottom_controller_shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "K2" (at 3.81 1.27 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "CH_MD" (at 3.81 1.27 -90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -1.4224 90) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -1.4224 -90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at 0.864 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 1.27 -90 unlocked) (layer "F.Fab") hide)
    (fp_text user "*" (at 0.864 0 -90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 19 "/chain_middle_ctl") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 0 2.54 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 "GND") (pinfunction "2") (pintype "unspecified"))
    (pad "3" thru_hole circle (at 7.62 2.54 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 "GND") (pinfunction "3") (pintype "unspecified"))
    (pad "4" thru_hole circle (at 7.62 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 23 "/chain_middle_rtn") (pinfunction "4") (pintype "unspecified"))
  )
  (gr_rect (start 104.14 59.69) (end 173.355 113.03) (layer "Edge.Cuts") (width 0.0381) (fill none))
  (gr_text "Fantastic Experience LLC" (at 146 71.755) (layer "F.SilkS"))
  (gr_text "Desk Bottom V3" (at 145 70) (layer "F.SilkS"))
  (zone (net 11) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.72 112.395)
        (xy 106.68 112.395)
        (xy 106.68 60.325)
        (xy 172.72 60.325)
      )
    )
  )
)
