<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="5.08" y1="3.4925" x2="39.04" y2="3.4925" width="0" layer="20"/>
<wire x1="39.04" y1="3.4925" x2="39.04" y2="40.9475" width="0" layer="20"/>
<wire x1="39.04" y1="40.9475" x2="5.08" y2="40.9475" width="0" layer="20"/>
<wire x1="5.08" y1="40.9475" x2="5.08" y2="3.4925" width="0" layer="20"/>
<hole x="7.62" y="6.35" drill="3.2"/>
<hole x="7.62" y="38.1" drill="3.2"/>
<text>RV-Builders Products 2013</text>
<text>Power Feed &amp; Sensor input</text>
</plain>
<libraries>
<library name="wifi_WX">
<packages>
<package name="RJ45_VERT">
</package>
<package name="32005-301">
<description>&lt;b&gt;MINI USB-B R/A SMT W/O REAR&lt;/b&gt;&lt;p&gt;
Source: http://www.cypressindustries.com/pdf/32005-301.pdf</description>
</package>
<package name="1X3_MOLEX_KK">
<description>Molex KK series pin header with frictiuon lock</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="wifi_WX" package="RJ45_VERT" value="RJ45-8VERT"/>
<element name="J2" library="wifi_WX" package="RJ45_VERT" value="RJ45-8VERT"/>
<element name="USB" library="wifi_WX" package="32005-301" value="MINI-USB-32005-301"/>
<element name="RAIN" library="wifi_WX" package="1X3_MOLEX_KK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SUN" library="wifi_WX" package="1X3_MOLEX_KK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J1" pad="P$1"/>
<contactref element="J1" pad="P$2"/>
<contactref element="J2" pad="P$2"/>
<contactref element="J2" pad="P$1"/>
<contactref element="USB" pad="5_USB_GND"/>
<contactref element="USB" pad="M4"/>
<contactref element="USB" pad="M2"/>
<contactref element="USB" pad="M3"/>
<contactref element="USB" pad="M1"/>
<contactref element="RAIN" pad="3"/>
<contactref element="SUN" pad="3"/>
</signal>
<signal name="+5V">
<contactref element="J1" pad="P$3"/>
<contactref element="J1" pad="P$6"/>
<contactref element="J2" pad="P$6"/>
<contactref element="J2" pad="P$3"/>
<contactref element="USB" pad="1_VBUS"/>
<contactref element="RAIN" pad="1"/>
<contactref element="SUN" pad="1"/>
</signal>
<signal name="WIN_DIR_IN">
<contactref element="J1" pad="P$4"/>
<contactref element="J2" pad="P$4"/>
</signal>
<signal name="SUN_IN">
<contactref element="J1" pad="P$5"/>
<contactref element="J2" pad="P$5"/>
<contactref element="SUN" pad="2"/>
</signal>
<signal name="RAIN_CNT_IN">
<contactref element="J1" pad="P$7"/>
<contactref element="J2" pad="P$7"/>
<contactref element="RAIN" pad="2"/>
</signal>
<signal name="WIND_COUNT">
<contactref element="J1" pad="P$8"/>
<contactref element="J2" pad="P$8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
