(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu16.04.1)
  (general
    (thickness 1.6)
    (drawings 33)
    (tracks 428)
    (zones 0)
    (modules 38)
    (nets 56)
  )
  (page USLetter)
  (title_block
    (title "Car Scanner")
    (rev 1.0)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.762)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.3)
    (via_min_size 0.508)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.4 1.4)
    (pad_drill 0.7)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x3f2f3_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 2)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(MCU1-Pad1)")
  (net 2 "Net-(MCU1-Pad3)")
  (net 3 "Net-(MCU1-Pad6)")
  (net 4 "Net-(MCU1-Pad7)")
  (net 5 "Net-(MCU1-Pad8)")
  (net 6 "Net-(MCU1-Pad9)")
  (net 7 "Net-(MCU1-Pad10)")
  (net 8 "Net-(MCU1-Pad11)")
  (net 9 "Net-(MCU1-Pad12)")
  (net 10 "Net-(MCU1-Pad13)")
  (net 11 "Net-(TCA_A1-Pad5)")
  (net 12 "Net-(TCA_A1-Pad6)")
  (net 13 "Net-(TCA_A1-Pad7)")
  (net 14 "Net-(TCA_A1-Pad8)")
  (net 15 +3V3)
  (net 16 GND)
  (net 17 "Net-(MCU2-Pad1)")
  (net 18 "Net-(MCU2-Pad2)")
  (net 19 +5V)
  (net 20 "Net-(MCU1-Pad16)")
  (net 21 /USB)
  (net 22 "Net-(MCU2-Pad4)")
  (net 23 +7.5V)
  (net 24 "Net-(J10-Pad4)")
  (net 25 /ENable_5v)
  (net 26 "Net-(J13-Pad5)")
  (net 27 "Net-(J13-Pad6)")
  (net 28 /SDA)
  (net 29 /SCL)
  (net 30 /3V3)
  (net 31 /SD0)
  (net 32 /SC0)
  (net 33 /SD1)
  (net 34 /SC1)
  (net 35 /SD3)
  (net 36 /SC2)
  (net 37 /SD2)
  (net 38 /SC3)
  (net 39 /SD4)
  (net 40 /SC4)
  (net 41 /SD5)
  (net 42 /SC5)
  (net 43 /SC7)
  (net 44 /SD7)
  (net 45 /SC6)
  (net 46 /SD6)
  (net 47 /TcaReset)
  (net 48 /IRQ0)
  (net 49 /IRQ1)
  (net 50 /IRQ7)
  (net 51 /IRQ6)
  (net 52 /IRQ5)
  (net 53 /IRQ4)
  (net 54 /IRQ3)
  (net 55 /IRQ2)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net +7.5V)
    (add_net /3V3)
    (add_net /ENable_5v)
    (add_net /IRQ0)
    (add_net /IRQ1)
    (add_net /IRQ2)
    (add_net /IRQ3)
    (add_net /IRQ4)
    (add_net /IRQ5)
    (add_net /IRQ6)
    (add_net /IRQ7)
    (add_net /SC0)
    (add_net /SC1)
    (add_net /SC2)
    (add_net /SC3)
    (add_net /SC4)
    (add_net /SC5)
    (add_net /SC6)
    (add_net /SC7)
    (add_net /SCL)
    (add_net /SD0)
    (add_net /SD1)
    (add_net /SD2)
    (add_net /SD3)
    (add_net /SD4)
    (add_net /SD5)
    (add_net /SD6)
    (add_net /SD7)
    (add_net /SDA)
    (add_net /TcaReset)
    (add_net /USB)
    (add_net GND)
    (add_net "Net-(J10-Pad4)")
    (add_net "Net-(J13-Pad5)")
    (add_net "Net-(J13-Pad6)")
    (add_net "Net-(MCU1-Pad1)")
    (add_net "Net-(MCU1-Pad10)")
    (add_net "Net-(MCU1-Pad11)")
    (add_net "Net-(MCU1-Pad12)")
    (add_net "Net-(MCU1-Pad13)")
    (add_net "Net-(MCU1-Pad16)")
    (add_net "Net-(MCU1-Pad3)")
    (add_net "Net-(MCU1-Pad6)")
    (add_net "Net-(MCU1-Pad7)")
    (add_net "Net-(MCU1-Pad8)")
    (add_net "Net-(MCU1-Pad9)")
    (add_net "Net-(MCU2-Pad1)")
    (add_net "Net-(MCU2-Pad2)")
    (add_net "Net-(MCU2-Pad4)")
    (add_net "Net-(TCA_A1-Pad5)")
    (add_net "Net-(TCA_A1-Pad6)")
    (add_net "Net-(TCA_A1-Pad7)")
    (add_net "Net-(TCA_A1-Pad8)")
  )
  (module Connector_JST:JST_XH_B02B-XH-A_1x02_P2.50mm_Vertical (layer F.Cu) (tedit 5B7754C5)
    (at 36.83 70.612 270)
    (descr "JST XH series connector, B02B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry")
    (fp_text reference J9 (at 1.25 -3.55 270) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 1.25 4.6 270) (layer F.Fab))
    (fp_text user %R (at 1.25 2.7 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 23 +7.5V))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B02B-XH-A_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5C2BA524)
    (at 134.62 28.448 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R15 (at -1.651 0 270) (layer F.SilkS))
    (fp_text value 1.5k (at 3.81 1.92 270) (layer F.Fab))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 +3V3))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 34 /SC1))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XHP_B06B-XH-A_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 5C28336D)
    (at 104.14 28.448 270)
    (descr "JST XH series connector, B06B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry")
    (fp_text reference J5 (at 6.25 -3.55 270) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 6.25 4.6 270) (layer F.Fab))
    (fp_text user %R (at 6.25 2.7 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 15 +3V3))
    (pad 2 thru_hole oval (at 2.54064 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 16 GND))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 47 /TcaReset))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 54 /IRQ3))
    (pad 5 thru_hole oval (at 10.16 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 35 /SD3))
    (pad 6 thru_hole oval (at 12.7 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 38 /SC3))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B06B-XH-A_1x06_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XHP_B06B-XH-A_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 5C2A843D)
    (at 53.34 28.448 270)
    (descr "JST XH series connector, B06B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry")
    (fp_text reference J1 (at 6.25 -3.55 270) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 6.25 4.6 270) (layer F.Fab))
    (fp_text user %R (at 6.25 2.7 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 15 +3V3))
    (pad 2 thru_hole oval (at 2.54064 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 16 GND))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 47 /TcaReset))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 51 /IRQ6))
    (pad 5 thru_hole oval (at 10.16 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 46 /SD6))
    (pad 6 thru_hole oval (at 12.7 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 45 /SC6))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B06B-XH-A_1x06_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XHP_B06B-XH-A_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 5C2A8424)
    (at 66.04 28.448 270)
    (descr "JST XH series connector, B06B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry")
    (fp_text reference J2 (at 6.25 -3.55 270) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 6.25 4.6 270) (layer F.Fab))
    (fp_text user %R (at 6.25 2.7 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 15 +3V3))
    (pad 2 thru_hole oval (at 2.54064 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 16 GND))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 47 /TcaReset))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 50 /IRQ7))
    (pad 5 thru_hole oval (at 10.16 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 44 /SD7))
    (pad 6 thru_hole oval (at 12.7 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 43 /SC7))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B06B-XH-A_1x06_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XHP_B06B-XH-A_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 5C28336D)
    (at 142.24 55.372 270)
    (descr "JST XH series connector, B06B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry")
    (fp_text reference J13 (at 6.25 5.08 270) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 6.25 4.6 270) (layer F.Fab))
    (fp_text user %R (at 6.25 2.7 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 15 +3V3))
    (pad 2 thru_hole oval (at 2.54064 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 16 GND))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 28 /SDA))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 29 /SCL))
    (pad 5 thru_hole oval (at 10.16 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 26 "Net-(J13-Pad5)"))
    (pad 6 thru_hole oval (at 12.7 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 27 "Net-(J13-Pad6)"))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B06B-XH-A_1x06_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XHP_B06B-XH-A_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 5C28336D)
    (at 91.44 28.448 270)
    (descr "JST XH series connector, B06B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry")
    (fp_text reference J4 (at 6.25 -3.55 270) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 6.25 4.6 270) (layer F.Fab))
    (fp_text user %R (at 6.25 2.7 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 15 +3V3))
    (pad 2 thru_hole oval (at 2.54064 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 16 GND))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 47 /TcaReset))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 53 /IRQ4))
    (pad 5 thru_hole oval (at 10.16 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 39 /SD4))
    (pad 6 thru_hole oval (at 12.7 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 40 /SC4))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B06B-XH-A_1x06_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XHP_B06B-XH-A_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 5C2A8850)
    (at 142.24 28.448 270)
    (descr "JST XH series connector, B06B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry")
    (fp_text reference J8 (at 6.25 -3.55 270) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 6.25 4.6 270) (layer F.Fab))
    (fp_text user %R (at 6.25 2.7 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 15 +3V3))
    (pad 2 thru_hole oval (at 2.54064 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 16 GND))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 47 /TcaReset))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 49 /IRQ1))
    (pad 5 thru_hole oval (at 10.16 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 33 /SD1))
    (pad 6 thru_hole oval (at 12.7 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 34 /SC1))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B06B-XH-A_1x06_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XHP_B06B-XH-A_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 5C28336D)
    (at 116.84 28.448 270)
    (descr "JST XH series connector, B06B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry")
    (fp_text reference J6 (at 6.25 -3.55 270) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 6.25 4.6 270) (layer F.Fab))
    (fp_text user %R (at 6.25 2.7 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 15 +3V3))
    (pad 2 thru_hole oval (at 2.54064 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 16 GND))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 47 /TcaReset))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 55 /IRQ2))
    (pad 5 thru_hole oval (at 10.16 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 37 /SD2))
    (pad 6 thru_hole oval (at 12.7 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 36 /SC2))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B06B-XH-A_1x06_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XHP_B06B-XH-A_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 5C2A882A)
    (at 129.54 28.448 270)
    (descr "JST XH series connector, B06B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry")
    (fp_text reference J7 (at 6.25 -3.55 270) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 6.25 4.6 270) (layer F.Fab))
    (fp_text user %R (at 6.25 2.7 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 15 +3V3))
    (pad 2 thru_hole oval (at 2.54064 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 16 GND))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 47 /TcaReset))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 48 /IRQ0))
    (pad 5 thru_hole oval (at 10.16 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 31 /SD0))
    (pad 6 thru_hole oval (at 12.7 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 32 /SC0))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B06B-XH-A_1x06_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XHP_B06B-XH-A_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 5C28336D)
    (at 78.74 28.448 270)
    (descr "JST XH series connector, B06B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry")
    (fp_text reference J3 (at 6.25 -3.55 270) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 6.25 4.6 270) (layer F.Fab))
    (fp_text user %R (at 6.25 2.7 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 15 +3V3))
    (pad 2 thru_hole oval (at 2.54064 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 16 GND))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 47 /TcaReset))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 52 /IRQ5))
    (pad 5 thru_hole oval (at 10.16 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 41 /SD5))
    (pad 6 thru_hole oval (at 12.7 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 42 /SC5))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B06B-XH-A_1x06_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5C2A8918)
    (at 137.16 28.448 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R16 (at -1.651 0 270) (layer F.SilkS))
    (fp_text value 1.5k (at 3.81 1.92 270) (layer F.Fab))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 +3V3))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 33 /SD1))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 42.672 43.688)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J14 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /ENable_5v))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 40.64 60.198)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J12 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /USB))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C2580CF)
    (at 148.844 28.956)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H4 (at 0 4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 -4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C2580C7)
    (at 28.956 72.644)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C2580BB)
    (at 28.956 28.956)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H2 (at 0 4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 -4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C2580D9)
    (at 148.844 72.644)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x16_P2.54mm_Vertical (layer F.Cu) (tedit 5C295453)
    (at 50.8 71.628 90)
    (descr "Through hole straight socket strip, 1x16, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x16 2.54mm single row")
    (fp_text reference MCU1 (at 0 -2.77 90) (layer F.SilkS))
    (fp_text value Conn_01x16 (at 0 40.87 90) (layer F.Fab))
    (fp_text user %R (at 0 19.05 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(MCU1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /3V3))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(MCU1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 GND))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /TcaReset))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(MCU1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(MCU1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(MCU1-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(MCU1-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(MCU1-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(MCU1-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(MCU1-Pad12)"))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(MCU1-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 /IRQ1))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 /IRQ0))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(MCU1-Pad16)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x16_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x12_P2.54mm_Vertical (layer F.Cu) (tedit 5C2A7EAD)
    (at 60.96 51.308 90)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference MCU2 (at 0 -2.77 90) (layer F.SilkS))
    (fp_text value Conn_01x12 (at 0 30.71 90) (layer F.Fab))
    (fp_text user %R (at 0 13.97 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(MCU2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(MCU2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /USB))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(MCU2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 /IRQ6))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 /IRQ7))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 /IRQ5))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 /IRQ4))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 /IRQ3))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 /IRQ2))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /SCL))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /SDA))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x12_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5C2440A9)
    (at 38.1 41.148)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference J11 (at 0 10.16) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 0 10.39) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /ENable_5v))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 +7.5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 +5V))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5C279C59)
    (at 109.22 28.448 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R11 (at -1.651 0 270) (layer F.SilkS))
    (fp_text value 1.5k (at 3.81 1.92 270) (layer F.Fab))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 +3V3))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 36 /SC2))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5C279CA4)
    (at 96.52 28.448 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R9 (at -1.651 0 270) (layer F.SilkS))
    (fp_text value 1.5k (at 3.81 1.92 270) (layer F.Fab))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 38 /SC3))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 +3V3))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5C2694AB)
    (at 38.1 28.448)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference J10 (at 0 9.906) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 0 10.39) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 +3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 +7.5V))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J10-Pad4)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5C2A88F6)
    (at 121.92 28.448 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R13 (at -1.651 0 270) (layer F.SilkS))
    (fp_text value 1.5k (at 3.81 1.92 270) (layer F.Fab))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 32 /SC0))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 +3V3))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5C2A8903)
    (at 124.46 28.448 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R14 (at -1.651 0 270) (layer F.SilkS))
    (fp_text value 1.5k (at 3.81 1.92 270) (layer F.Fab))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 +3V3))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 31 /SD0))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5C279CBC)
    (at 86.36 28.448 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R8 (at -1.651 0 270) (layer F.SilkS))
    (fp_text value 1.5k (at 3.81 1.92 270) (layer F.Fab))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 39 /SD4))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 +3V3))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5C279C3D)
    (at 111.76 28.448 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R12 (at -1.651 0 270) (layer F.SilkS))
    (fp_text value 1.5k (at 3.81 1.92 270) (layer F.Fab))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 +3V3))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 37 /SD2))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5C279C79)
    (at 99.06 28.448 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R10 (at -1.651 0 270) (layer F.SilkS))
    (fp_text value 1.5k (at 3.81 1.92 270) (layer F.Fab))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 +3V3))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 35 /SD3))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5C279CDE)
    (at 83.82 28.448 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R7 (at -1.651 0 270) (layer F.SilkS))
    (fp_text value 1.5k (at 3.81 1.92 270) (layer F.Fab))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 +3V3))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 40 /SC4))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5C279CF9)
    (at 73.66 28.448 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R6 (at -1.651 0 270) (layer F.SilkS))
    (fp_text value 1.5k (at 3.81 1.92 270) (layer F.Fab))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 41 /SD5))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 +3V3))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5C2A84D8)
    (at 45.72 28.448 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at -1.651 0 270) (layer F.SilkS))
    (fp_text value 1.5k (at 3.81 1.92 270) (layer F.Fab))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 +3V3))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 45 /SC6))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5C2A84D1)
    (at 48.26 28.448 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at -1.651 0 270) (layer F.SilkS))
    (fp_text value 1.5k (at 3.81 1.92 270) (layer F.Fab))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 46 /SD6))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 +3V3))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5C279D12)
    (at 71.12 28.448 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R5 (at -1.651 0 270) (layer F.SilkS))
    (fp_text value 1.5k (at 3.81 1.92 270) (layer F.Fab))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 +3V3))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 42 /SC5))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5C2A84CA)
    (at 58.42 28.448 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at -1.651 0 270) (layer F.SilkS))
    (fp_text value 1.5k (at 3.81 1.92 270) (layer F.Fab))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 +3V3))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 43 /SC7))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5C2A84C2)
    (at 60.96 28.448 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R4 (at -1.651 0 270) (layer F.SilkS))
    (fp_text value 1.5k (at 3.81 1.92 270) (layer F.Fab))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 +3V3))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 44 /SD7))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x12_P2.54mm_Vertical (layer F.Cu) (tedit 5C2A835D)
    (at 101.6 53.848 90)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference TCA_B1 (at 0 -2.77 90) (layer F.SilkS))
    (fp_text value Conn_01x12 (at 0 30.71 90) (layer F.Fab))
    (fp_text user %R (at 0 13.97 180) (layer F.Fab))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /SD2))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /SC2))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /SD3))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /SC3))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /SD4))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /SC4))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /SD5))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /SC5))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /SD6))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /SC6))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /SD7))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /SC7))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x12_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x12_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A41D)
    (at 101.6 69.088 90)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference TCA_A1 (at 0 -2.77 90) (layer F.SilkS))
    (fp_text value Conn_01x12 (at 0 30.71 90) (layer F.Fab))
    (fp_text user %R (at 0 13.97 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /3V3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /SDA))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /SCL))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(TCA_A1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(TCA_A1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(TCA_A1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(TCA_A1-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /SD0))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /SC0))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /SD1))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /SC1))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x12_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Yard Master" (at 115.57 73.66) (layer F.SilkS))
  (gr_text "Version 1.0 12/30/2018" (at 150.495 49.53 90) (layer F.SilkS))
  (gr_text TCA9548A (at 115.57 60.96) (layer F.SilkS))
  (gr_text "Feather MØ WiFi" (at 71.12 60.96) (layer F.SilkS))
  (gr_text "3.3v reg." (at 35.306 31.75 90) (layer F.SilkS))
  (gr_text "5v reg." (at 35.306 43.942 90) (layer F.SilkS))
  (gr_text "5v disable" (at 44.704 44.45 90) (layer F.SilkS))
  (gr_text "5v to USB" (at 38.227 60.96 90) (layer F.SilkS))
  (gr_text 6.5-12v (at 32.004 65.278 90) (layer F.SilkS))
  (gr_text 3.3v (at 147.193 55.372) (layer F.SilkS))
  (gr_text GND (at 147.066 58.039) (layer F.SilkS))
  (gr_text SDA (at 146.939 60.579) (layer F.SilkS))
  (gr_text SCL (at 146.939 62.992) (layer F.SilkS))
  (gr_text 8 (at 139.7 44.45 90) (layer F.SilkS))
  (gr_text 7 (at 127 44.45 90) (layer F.SilkS))
  (gr_text 6 (at 114.3 44.45 90) (layer F.SilkS))
  (gr_text 5 (at 101.6 44.45 90) (layer F.SilkS))
  (gr_text 4 (at 88.9 44.45 90) (layer F.SilkS))
  (gr_text 3 (at 76.2 44.45 90) (layer F.SilkS))
  (gr_text 2 (at 63.5 44.45 90) (layer F.SilkS))
  (gr_text 1 (at 50.8 44.45 90) (layer F.SilkS))
  (gr_line (start 25.4762 25.4762) (end 152.3238 25.4762) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.3238 76.1238) (end 152.3238 25.4762) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 25.4762 76.1238) (end 152.3238 76.1238) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 25.4762 25.4762) (end 25.4762 76.1238) (layer Edge.Cuts) (width 0.15))
  (zone (net 16) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 25.4 25.4) (xy 25.4 76.2) (xy 152.4 76.2) (xy 152.4 25.4)
      )
    )
  )
  (zone (net 16) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 25.4 25.4) (xy 25.4 76.2) (xy 152.4 76.2) (xy 152.4 25.4)
      )
    )
  )
)
