(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 142)
    (no_connects 0)
    (area 29.114287 35.4 184.35 131.650001)
    (thickness 1.6)
    (drawings 35)
    (tracks 793)
    (zones 0)
    (modules 59)
    (nets 87)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 +3V3)
  (net 5 +24V)
  (net 6 "Net-(D1-Pad1)")
  (net 7 "Net-(D1-Pad3)")
  (net 8 "Net-(D2-Pad1)")
  (net 9 "Net-(D2-Pad2)")
  (net 10 "Net-(J2-Pad9)")
  (net 11 /ETH0_TX+)
  (net 12 /ETH0_TX-)
  (net 13 /ETH0_RX+)
  (net 14 /ETH0_RX-)
  (net 15 /ETH0_LED)
  (net 16 /WLAN_LED)
  (net 17 /Omega_RX)
  (net 18 /Omega_TX)
  (net 19 "Net-(R1-Pad1)")
  (net 20 "Net-(R2-Pad1)")
  (net 21 /USB+)
  (net 22 /USB-)
  (net 23 +5V)
  (net 24 "Net-(R9-Pad2)")
  (net 25 "Net-(C8-Pad1)")
  (net 26 "Net-(J2-Pad12)")
  (net 27 /LED_DATA1)
  (net 28 /LED_FET_5V)
  (net 29 /LED_FET_3V)
  (net 30 /LED_DATA1_3V)
  (net 31 /LED_DATA2_3V)
  (net 32 /LED_DATA3_3V)
  (net 33 /LED_DATA2)
  (net 34 "Net-(J6-Pad2)")
  (net 35 "Net-(J6-Pad3)")
  (net 36 /SPI_MOSI)
  (net 37 /SPI_MISO)
  (net 38 /SPI_CLK)
  (net 39 /SPI_CS1)
  (net 40 /LED_DATA3)
  (net 41 /CHS_GND)
  (net 42 /FET_PWR)
  (net 43 /SENS_PWR)
  (net 44 "Net-(MH1-Pad1)")
  (net 45 "Net-(MH2-Pad1)")
  (net 46 "Net-(MH3-Pad1)")
  (net 47 "Net-(MH4-Pad1)")
  (net 48 "Net-(P1-Pad2)")
  (net 49 "Net-(P1-Pad3)")
  (net 50 "Net-(P1-Pad6)")
  (net 51 "Net-(U1-PadA13)")
  (net 52 "Net-(U1-PadA12)")
  (net 53 "Net-(U1-PadA11)")
  (net 54 "Net-(U1-PadA10)")
  (net 55 "Net-(U1-PadA9)")
  (net 56 "Net-(U1-PadA8)")
  (net 57 "Net-(U1-PadA6)")
  (net 58 "Net-(U1-PadA5)")
  (net 59 "Net-(U1-PadB7)")
  (net 60 "Net-(U1-PadB8)")
  (net 61 "Net-(U1-PadB9)")
  (net 62 "Net-(U1-PadB10)")
  (net 63 "Net-(U1-PadB11)")
  (net 64 "Net-(U1-PadB12)")
  (net 65 "Net-(U1-PadB15)")
  (net 66 "Net-(U1-PadB16)")
  (net 67 "Net-(U1-PadB17)")
  (net 68 "Net-(U1-PadB18)")
  (net 69 "Net-(U1-PadB19)")
  (net 70 "Net-(U1-PadB20)")
  (net 71 "Net-(U1-PadB21)")
  (net 72 "Net-(U1-PadB22)")
  (net 73 "Net-(U1-PadC2)")
  (net 74 "Net-(U1-PadC9)")
  (net 75 "Net-(U1-PadC10)")
  (net 76 "Net-(U1-PadC11)")
  (net 77 "Net-(U1-PadC12)")
  (net 78 "Net-(U1-PadC13)")
  (net 79 "Net-(U1-PadC14)")
  (net 80 "Net-(U1-PadC15)")
  (net 81 "Net-(U1-PadC16)")
  (net 82 "Net-(U1-PadC19)")
  (net 83 "Net-(U1-PadC20)")
  (net 84 "Net-(U1-PadC21)")
  (net 85 /V_REG_IN)
  (net 86 "Net-(P7-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ETH0_LED)
    (add_net /ETH0_RX+)
    (add_net /ETH0_RX-)
    (add_net /ETH0_TX+)
    (add_net /ETH0_TX-)
    (add_net /LED_DATA1)
    (add_net /LED_DATA1_3V)
    (add_net /LED_DATA2)
    (add_net /LED_DATA2_3V)
    (add_net /LED_DATA3)
    (add_net /LED_DATA3_3V)
    (add_net /LED_FET_3V)
    (add_net /LED_FET_5V)
    (add_net /Omega_RX)
    (add_net /Omega_TX)
    (add_net /SPI_CLK)
    (add_net /SPI_CS1)
    (add_net /SPI_MISO)
    (add_net /SPI_MOSI)
    (add_net /USB+)
    (add_net /USB-)
    (add_net /WLAN_LED)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(MH1-Pad1)")
    (add_net "Net-(MH2-Pad1)")
    (add_net "Net-(MH3-Pad1)")
    (add_net "Net-(MH4-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P7-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(U1-PadA10)")
    (add_net "Net-(U1-PadA11)")
    (add_net "Net-(U1-PadA12)")
    (add_net "Net-(U1-PadA13)")
    (add_net "Net-(U1-PadA5)")
    (add_net "Net-(U1-PadA6)")
    (add_net "Net-(U1-PadA8)")
    (add_net "Net-(U1-PadA9)")
    (add_net "Net-(U1-PadB10)")
    (add_net "Net-(U1-PadB11)")
    (add_net "Net-(U1-PadB12)")
    (add_net "Net-(U1-PadB15)")
    (add_net "Net-(U1-PadB16)")
    (add_net "Net-(U1-PadB17)")
    (add_net "Net-(U1-PadB18)")
    (add_net "Net-(U1-PadB19)")
    (add_net "Net-(U1-PadB20)")
    (add_net "Net-(U1-PadB21)")
    (add_net "Net-(U1-PadB22)")
    (add_net "Net-(U1-PadB7)")
    (add_net "Net-(U1-PadB8)")
    (add_net "Net-(U1-PadB9)")
    (add_net "Net-(U1-PadC10)")
    (add_net "Net-(U1-PadC11)")
    (add_net "Net-(U1-PadC12)")
    (add_net "Net-(U1-PadC13)")
    (add_net "Net-(U1-PadC14)")
    (add_net "Net-(U1-PadC15)")
    (add_net "Net-(U1-PadC16)")
    (add_net "Net-(U1-PadC19)")
    (add_net "Net-(U1-PadC2)")
    (add_net "Net-(U1-PadC20)")
    (add_net "Net-(U1-PadC21)")
    (add_net "Net-(U1-PadC9)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 1)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +24V)
    (add_net +3V3)
    (add_net +5V)
    (add_net /CHS_GND)
    (add_net /V_REG_IN)
    (add_net GND)
  )
  (net_class PowerFET ""
    (clearance 0.2)
    (trace_width 5)
    (via_dia 1)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /FET_PWR)
  )
  (net_class PowerSmall ""
    (clearance 0.15)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /SENS_PWR)
  )
  (module plan44:PULSE-J0026D21B (layer F.Cu) (tedit 5B44C41D)
    (at 110.75 106.5 180)
    (fp_text reference J2 (at -4.312 5.408 360) (layer F.SilkS))
    (fp_text value Pulse-J0026D21B (at -4.318 -15.748 180) (layer F.Fab))
    (pad 9 thru_hole circle (at 1.905 -11.1506 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad9)"))
    (pad 10 thru_hole circle (at -0.635 -9.6266 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 /ETH0_LED))
    (pad 11 thru_hole circle (at -8.2042 -11.1252 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 /WLAN_LED))
    (pad 12 thru_hole circle (at -10.7442 -9.6012 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad12)"))
    (pad S2 thru_hole circle (at -12.319 -3.302 180) (size 3.048 3.048) (drill 1.6002) (layers *.Cu *.Mask)
      (net 41 /CHS_GND))
    (pad S1 thru_hole circle (at 3.429 -3.302 180) (size 3.048 3.048) (drill 1.6002) (layers *.Cu *.Mask)
      (net 41 /CHS_GND))
    (pad "" np_thru_hole circle (at -10.16 -6.35 180) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 /ETH0_TX+))
    (pad 2 thru_hole circle (at -1.27 2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 /ETH0_TX-))
    (pad 3 thru_hole circle (at -2.54 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 "Net-(C8-Pad1)"))
    (pad 4 thru_hole circle (at -3.81 2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at -5.08 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at -6.35 2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 "Net-(C8-Pad1)"))
    (pad 7 thru_hole circle (at -7.62 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 /ETH0_RX+))
    (pad 8 thru_hole circle (at -8.89 2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 /ETH0_RX-))
    (pad "" np_thru_hole circle (at 1.27 -6.35 180) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5B44C2FC)
    (at 139.25 105.25)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 4.006 -0.094 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5B44C2F5)
    (at 139.25 102.75)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 4.006 0.12 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5B44C37C)
    (at 141.75 74)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 0.05 1.3 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5B44C382)
    (at 131.75 74)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C6 (at 0.05 1.3 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58AA84D1)
    (at 110 99.75)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C8 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 1uF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5B44C3ED)
    (at 109.75 84.5 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C10 (at 3.982 0.232 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58AA84D1)
    (at 86.5 87.5)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C12 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 100nF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 85 /V_REG_IN))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D7.5mm_P2.50mm (layer F.Cu) (tedit 5B44C252)
    (at 77 101.25 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=7.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 7.5mm Electrolytic Capacitor")
    (fp_text reference C13 (at 5.938 2.324 360) (layer F.SilkS))
    (fp_text value "10uF 50VDC" (at 1.25 4.81 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 /V_REG_IN))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/CP_Radial_D7.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm-3 (layer B.Cu) (tedit 591A2DFE)
    (at 96.75 94.5 90)
    (descr "LED, diameter 5.0mm, 2 pins, diameter 5.0mm, 3 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-59EGC(Ver.17A).pdf")
    (tags "LED diameter 5.0mm 2 pins diameter 5.0mm 3 pins")
    (fp_text reference D1 (at 2.706 -4.06 90) (layer B.SilkS))
    (fp_text value "Everlight 339-1SURSYGW/S530-A3" (at 2.54 -3.96 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D1-Pad3)"))
    (model LEDs.3dshapes/LED_D5.0mm-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMB_Handsoldering (layer F.Cu) (tedit 5B44C410)
    (at 99.75 97.75 180)
    (descr "Diode SMB Handsoldering")
    (tags "Diode SMB Handsoldering")
    (attr smd)
    (fp_text reference D2 (at -5.66 -0.04 270) (layer F.SilkS))
    (fp_text value DO-214AA (at 0 3 180) (layer F.Fab))
    (fp_text user %R (at 0 -3 180) (layer F.Fab))
    (pad 1 smd rect (at -2.7 0 180) (size 3.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 2.7 0 180) (size 3.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMB_Handsoldering (layer F.Cu) (tedit 5B44C423)
    (at 99.75 101.75 180)
    (descr "Diode SMB Handsoldering")
    (tags "Diode SMB Handsoldering")
    (attr smd)
    (fp_text reference D3 (at -5.66 -0.104 270) (layer F.SilkS))
    (fp_text value DO-214AA (at 0 3 180) (layer F.Fab))
    (fp_text user %R (at 0 -3 180) (layer F.Fab))
    (pad 1 smd rect (at -2.7 0 180) (size 3.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 2.7 0 180) (size 3.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMB_Handsoldering (layer F.Cu) (tedit 5B44C40B)
    (at 99.75 106.5 180)
    (descr "Diode SMB Handsoldering")
    (tags "Diode SMB Handsoldering")
    (attr smd)
    (fp_text reference D4 (at -5.66 0.074 270) (layer F.SilkS))
    (fp_text value DO-214AA (at 0 3 180) (layer F.Fab))
    (fp_text user %R (at 0 -3 180) (layer F.Fab))
    (pad 1 smd rect (at -2.7 0 180) (size 3.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 2.7 0 180) (size 3.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad locked (layer F.Cu) (tedit 591A2AD3)
    (at 78.5 73.75)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference MH1 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 44 "Net-(MH1-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad locked (layer F.Cu) (tedit 591A2AB0)
    (at 156 73.75)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference MH2 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 45 "Net-(MH2-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad locked (layer F.Cu) (tedit 591A2AC4)
    (at 78.75 110.25)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference MH3 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 46 "Net-(MH3-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad locked (layer F.Cu) (tedit 591A2ABA)
    (at 156 110.25)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference MH4 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 47 "Net-(MH4-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5B44C325)
    (at 127.75 109 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference P1 (at 0.6 14.85 90) (layer F.SilkS))
    (fp_text value FDI_Cable (at 0 15.03 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /Omega_RX))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /Omega_TX))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(P1-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B44C3E0)
    (at 104.25 84.5 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at -3.982 -0.144 360) (layer F.SilkS))
    (fp_text value 470 (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B44C3F4)
    (at 101.5 84.5 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at -3.982 -0.1 360) (layer F.SilkS))
    (fp_text value 1k2 (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B44C31D)
    (at 126.25 104 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 3.162 -0.012 180) (layer F.SilkS))
    (fp_text value 49.9_1% (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /ETH0_TX+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B44C319)
    (at 129 104 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 3.162 0.286 180) (layer F.SilkS))
    (fp_text value 49.9_1% (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 /ETH0_TX-))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B44C3E7)
    (at 107 84.5 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at -3.982 0.066 360) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R9-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B44C27D)
    (at 104.75 115.75 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R10 (at 5.006 -0.102 90) (layer F.SilkS))
    (fp_text value 1k (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad9)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_6mm_h4.3mm (layer B.Cu) (tedit 591A2E06)
    (at 108.75 89.75 180)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=4.3mm")
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at -2.536 -2.348 270) (layer B.SilkS))
    (fp_text value "Omron PB" (at 3.75 -6.7 180) (layer B.Fab))
    (pad 2 thru_hole circle (at 0 -4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 24 "Net-(R9-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at 6.5 -4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 24 "Net-(R9-Pad2)"))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (model Buttons_Switches_THT.3dshapes/SW_PUSH_6mm_h4.3mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module plan44:Recom-R78Cxx (layer F.Cu) (tedit 5B44C438)
    (at 79.25 89.5 270)
    (descr "Recom R-78HBxx.0.5")
    (tags "Recom DCDC R-78")
    (fp_text reference U3 (at -2.378 -3.046 270) (layer F.SilkS))
    (fp_text value Recom_R783.3-0.5 (at 2.4 -3.2 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole oval (at 5.08 0 270) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 85 /V_REG_IN))
    (pad 3 thru_hole oval (at 0 0 270) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3V3))
  )
  (module plan44:ONION-OMEGA2S (layer F.Cu) (tedit 5B44C46E)
    (at 133.75 85.75 90)
    (clearance 0.25)
    (fp_text reference U1 (at -2.134 15.348 360) (layer F.SilkS))
    (fp_text value ONION-OMEGA2S (at 4.4 -3.9 180) (layer F.Fab))
    (pad A13 smd rect (at -9.8155 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U1-PadA13)"))
    (pad A12 smd rect (at -8.5455 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U1-PadA12)"))
    (pad A11 smd rect (at -7.2755 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U1-PadA11)"))
    (pad A10 smd rect (at -6.0055 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U1-PadA10)"))
    (pad A9 smd rect (at -4.7355 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U1-PadA9)"))
    (pad A8 smd rect (at -3.4655 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U1-PadA8)"))
    (pad A7 smd rect (at -2.1955 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad A6 smd rect (at -0.9255 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U1-PadA6)"))
    (pad A5 smd rect (at 0.3445 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U1-PadA5)"))
    (pad A4 smd rect (at 1.6145 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 37 /SPI_MISO))
    (pad A3 smd rect (at 2.8845 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 36 /SPI_MOSI))
    (pad A2 smd rect (at 4.1545 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 38 /SPI_CLK))
    (pad B1 smd rect (at -13.0125 -17.78 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 18 /Omega_TX))
    (pad B2 smd rect (at -13.0125 -16.51 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 17 /Omega_RX))
    (pad B3 smd rect (at -13.0125 -15.24 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 13 /ETH0_RX+))
    (pad B4 smd rect (at -13.0125 -13.97 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 14 /ETH0_RX-))
    (pad B5 smd rect (at -13.0125 -12.7 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 11 /ETH0_TX+))
    (pad B6 smd rect (at -13.0125 -11.43 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 12 /ETH0_TX-))
    (pad B7 smd rect (at -13.0125 -10.16 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U1-PadB7)"))
    (pad B8 smd rect (at -13.0125 -8.89 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(U1-PadB8)"))
    (pad B9 smd rect (at -13.0125 -7.62 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(U1-PadB9)"))
    (pad B10 smd rect (at -13.0125 -6.35 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(U1-PadB10)"))
    (pad B11 smd rect (at -13.0125 -5.08 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U1-PadB11)"))
    (pad B12 smd rect (at -13.0125 -3.81 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(U1-PadB12)"))
    (pad B13 smd rect (at -13.0125 -2.54 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 31 /LED_DATA2_3V))
    (pad B14 smd rect (at -13.0125 -1.27 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 32 /LED_DATA3_3V))
    (pad B15 smd rect (at -13.0125 0 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(U1-PadB15)"))
    (pad B16 smd rect (at -13.0125 1.27 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(U1-PadB16)"))
    (pad B17 smd rect (at -13.0125 2.54 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(U1-PadB17)"))
    (pad B18 smd rect (at -13.0125 3.81 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(U1-PadB18)"))
    (pad B19 smd rect (at -13.0125 5.08 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(U1-PadB19)"))
    (pad B20 smd rect (at -13.0125 6.35 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U1-PadB20)"))
    (pad B21 smd rect (at -13.0125 7.62 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(U1-PadB21)"))
    (pad B22 smd rect (at -13.0125 8.89 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U1-PadB22)"))
    (pad B23 smd rect (at -13.0125 10.16 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 21 /USB+))
    (pad B24 smd rect (at -13.0125 11.43 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 22 /USB-))
    (pad B25 smd rect (at -13.0125 12.7 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad C1 smd rect (at 8.5675 -17.78 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad C2 smd rect (at 8.5675 -16.51 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U1-PadC2)"))
    (pad C3 smd rect (at 8.5675 -15.24 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad C4 smd rect (at 8.5675 -13.97 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad C5 smd rect (at 8.5675 -12.7 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 30 /LED_DATA1_3V))
    (pad C6 smd rect (at 8.5675 -11.43 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 29 /LED_FET_3V))
    (pad C7 smd rect (at 8.5675 -10.16 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 16 /WLAN_LED))
    (pad C8 smd rect (at 8.5675 -8.89 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 15 /ETH0_LED))
    (pad C9 smd rect (at 8.5675 -7.62 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U1-PadC9)"))
    (pad C10 smd rect (at 8.5675 -6.35 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(U1-PadC10)"))
    (pad C11 smd rect (at 8.5675 -5.08 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U1-PadC11)"))
    (pad C12 smd rect (at 8.5675 -3.81 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U1-PadC12)"))
    (pad C13 smd rect (at 8.5675 -2.54 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U1-PadC13)"))
    (pad C14 smd rect (at 8.5675 -1.27 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(U1-PadC14)"))
    (pad C15 smd rect (at 8.5675 0 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U1-PadC15)"))
    (pad C16 smd rect (at 8.5675 1.27 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(U1-PadC16)"))
    (pad C17 smd rect (at 8.5675 2.54 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad C18 smd rect (at 8.5675 3.81 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad C19 smd rect (at 8.5675 5.08 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(U1-PadC19)"))
    (pad C20 smd rect (at 8.5675 6.35 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(U1-PadC20)"))
    (pad C21 smd rect (at 8.5675 7.62 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(U1-PadC21)"))
    (pad C22 smd rect (at 8.5675 8.89 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R9-Pad2)"))
    (pad C23 smd rect (at 8.5675 10.16 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R2-Pad1)"))
    (pad C24 smd rect (at 8.5675 11.43 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R1-Pad1)"))
    (pad C25 smd rect (at 8.5675 12.7 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad A1 smd rect (at 5.4245 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 39 /SPI_CS1))
    (pad "" thru_hole rect (at -5.65 -6.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad 3 smd rect (at -3.15 -3.55 90) (size 10 15) (layers B.Cu B.Paste B.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -4.65 -6.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -3.65 -6.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -2.65 -6.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -1.65 -6.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -0.65 -6.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -5.65 -5.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -4.65 -5.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -3.65 -5.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -2.65 -5.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -1.65 -5.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -0.65 -5.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -5.65 -4.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -4.65 -4.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -1.65 -4.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -0.65 -4.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -5.65 -3.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -4.65 -3.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -1.65 -3.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -0.65 -3.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -5.65 -2.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -4.65 -2.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -3.65 -2.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -2.65 -2.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -1.65 -2.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -0.65 -2.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -5.65 -1.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -4.65 -1.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -3.65 -1.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -2.65 -1.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -1.65 -1.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -0.65 -1.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
  )
  (module Connect:USB_A (layer F.Cu) (tedit 5B44C269)
    (at 88.25 110.5)
    (descr "USB A connector")
    (tags "USB USB_A")
    (fp_text reference J1 (at -5.954 7.61) (layer F.SilkS))
    (fp_text value USB_A (at 3.84 7.44) (layer F.Fab))
    (pad 4 thru_hole circle (at 7.11 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 4.57 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 23 +5V))
    (pad 5 thru_hole circle (at 10.16 2.67 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at -3.56 2.67 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connectors.3dshapes/USB_A.wrl
      (at (xyz 0.14 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:TO-252-2 (layer F.Cu) (tedit 590079C0)
    (at 92.75 79.25 270)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference Q1 (at 0 -4.5 270) (layer F.SilkS))
    (fp_text value IRLR2905PBF (at 0 4.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -4.2 -2.28 270) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 /LED_FET_5V))
    (pad 3 smd rect (at -4.2 2.28 270) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2.1 0 270) (size 6.4 5.8) (layers F.Cu F.Mask)
      (net 42 /FET_PWR))
    (pad 2 smd rect (at 3.775 1.525 270) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 42 /FET_PWR))
    (pad 2 smd rect (at 0.425 -1.525 270) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 42 /FET_PWR))
    (pad 2 smd rect (at 3.775 -1.525 270) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 42 /FET_PWR))
    (pad 2 smd rect (at 0.425 1.525 270) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 42 /FET_PWR))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B44C2C8)
    (at 154.75 97.25 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at -4.508 0.222 180) (layer F.SilkS))
    (fp_text value 47R (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 21 /USB+))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B44C2D3)
    (at 149.75 97 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 4.036 0.11 180) (layer F.SilkS))
    (fp_text value 47R (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 22 /USB-))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B44C310)
    (at 131.75 104 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 3.162 0.076 180) (layer F.SilkS))
    (fp_text value 49.9_1% (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 /ETH0_RX+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B44C306)
    (at 134.5 104 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 3.162 0.12 180) (layer F.SilkS))
    (fp_text value 49.9_1% (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /ETH0_RX-))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B44C2A7)
    (at 125.75 115.75 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R11 (at 3.99 0.742 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J2-Pad12)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B44C34C)
    (at 149.75 81.25 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R12 (at 4.796 -0.144 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 /LED_FET_3V))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B44C353)
    (at 153 81.25 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R13 (at 4.796 -0.6 90) (layer F.SilkS))
    (fp_text value 100k (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 30 /LED_DATA1_3V))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B44C361)
    (at 156.5 81.25 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R14 (at -4.094 -0.29 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 31 /LED_DATA2_3V))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module plan44:Recom-R78Cxx (layer F.Cu) (tedit 5B44C430)
    (at 90.5 105 180)
    (descr "Recom R-78HBxx.0.5")
    (tags "Recom DCDC R-78")
    (fp_text reference U2 (at -2.718 7.464 180) (layer F.SilkS))
    (fp_text value Recom_R785.0-0.5 (at 2.4 -3.2 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole oval (at 5.08 0 180) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 85 /V_REG_IN))
    (pad 3 thru_hole oval (at 0 0 180) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 23 +5V))
  )
  (module Capacitors_ThroughHole:CP_Radial_D7.5mm_P2.50mm (layer F.Cu) (tedit 5B44C2EB)
    (at 148.25 107.25 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=7.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 7.5mm Electrolytic Capacitor")
    (fp_text reference C7 (at 4.888 3.134 180) (layer F.SilkS))
    (fp_text value "22uF 25V" (at 1.25 5.06 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 +5V))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D7.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5B44C282)
    (at 102 115.75 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C9 (at -5.006 -0.108 270) (layer F.SilkS))
    (fp_text value 1nF/2kV (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 41 /CHS_GND))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58AA84D1)
    (at 112.25 69.75 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C11 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5B44C23B)
    (at 82.75 81.75 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C14 (at -0.038 2.086 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D7.5mm_P2.50mm (layer F.Cu) (tedit 5B44C43D)
    (at 77 82.5 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=7.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 7.5mm Electrolytic Capacitor")
    (fp_text reference C15 (at 5.538 -2.578 180) (layer F.SilkS))
    (fp_text value "22uF 25V" (at 1.25 5.06 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D7.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D7.5mm_P2.50mm (layer F.Cu) (tedit 5B44C2C0)
    (at 158 102.75 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=7.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 7.5mm Electrolytic Capacitor")
    (fp_text reference C16 (at -2.274 3.69 180) (layer F.SilkS))
    (fp_text value 10uF (at 1.25 5.06 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D7.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5B44C369)
    (at 159.25 90.25 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C17 (at 4.238 -0.262 360) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module plan44:CONFIG-PAD-2P (layer F.Cu) (tedit 5B44C45B)
    (at 112.25 75.5 90)
    (fp_text reference P2 (at -1.9 0.05 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -1.55 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.55 0 90) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 28 /LED_FET_5V))
    (pad 1 smd rect (at -0.55 0 90) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 29 /LED_FET_3V))
  )
  (module plan44:CONFIG-PAD-2P (layer F.Cu) (tedit 5B44C25A)
    (at 79.5 115.5)
    (fp_text reference P3 (at 0.002 1.8) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -1.55) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.55 0) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 1 smd rect (at -0.55 0) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 85 /V_REG_IN))
  )
  (module plan44:CONFIG-PAD-2P (layer F.Cu) (tedit 5B44C2B3)
    (at 157.5 116.5 270)
    (fp_text reference P4 (at 1.864 0.02 360) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -1.55 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.55 0 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 43 /SENS_PWR))
    (pad 1 smd rect (at -0.55 0 270) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module plan44:CONFIG-PAD-2P (layer F.Cu) (tedit 5B44C2B7)
    (at 154 116.5 90)
    (fp_text reference P5 (at -1.864 0.178 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -1.55 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.55 0 90) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 1 smd rect (at -0.55 0 90) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 43 /SENS_PWR))
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5B44C35B)
    (at 159.75 81.25 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R15 (at 4.796 0.524 90) (layer F.SilkS))
    (fp_text value 100k (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 32 /LED_DATA3_3V))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-14_N (layer F.Cu) (tedit 5B44C39F)
    (at 119.25 70 180)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U4 (at -5.972 1.674 450) (layer F.SilkS))
    (fp_text value 74AHCT125 (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -3.81 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.54 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 29 /LED_FET_3V))
    (pad 3 smd rect (at -1.27 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(P7-Pad2)"))
    (pad 4 smd rect (at 0 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.27 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 30 /LED_DATA1_3V))
    (pad 6 smd rect (at 2.54 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 27 /LED_DATA1))
    (pad 7 smd rect (at 3.81 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 3.81 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 33 /LED_DATA2))
    (pad 9 smd rect (at 2.54 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 31 /LED_DATA2_3V))
    (pad 11 smd rect (at 0 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 40 /LED_DATA3))
    (pad 12 smd rect (at -1.27 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 32 /LED_DATA3_3V))
    (pad 13 smd rect (at -2.54 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at -3.81 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 10 smd rect (at 1.27 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 5B44C47C)
    (at 154.5 90.25)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U5 (at -3.624 0.174 180) (layer F.SilkS))
    (fp_text value MCP3002 (at 0 1.27) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 7 smd rect (at -0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 38 /SPI_CLK))
    (pad 6 smd rect (at 0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 37 /SPI_MISO))
    (pad 5 smd rect (at 1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 36 /SPI_MOSI))
    (pad 4 smd rect (at 1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J6-Pad3)"))
    (pad 2 smd rect (at -0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J6-Pad2)"))
    (pad 1 smd rect (at -1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 39 /SPI_CS1))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D7.5mm_P2.50mm (layer F.Cu) (tedit 5B44C245)
    (at 85.25 93.5)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=7.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 7.5mm Electrolytic Capacitor")
    (fp_text reference C4 (at 4.92 -3.33) (layer F.SilkS))
    (fp_text value "10uF 50VDC" (at 1.25 5.06) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 /V_REG_IN))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D7.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module plan44:CONFIG-PAD-2P (layer F.Cu) (tedit 57FF90FF)
    (at 82.85 76.6 180)
    (fp_text reference P6 (at -2.05 -0.1 360) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -1.55 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.55 0 180) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 5 +24V))
    (pad 1 smd rect (at -0.55 0 180) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 85 /V_REG_IN))
  )
  (module plan44:CONFIG-PAD-2P (layer F.Cu) (tedit 57FF90FF)
    (at 109.5 75.5 90)
    (fp_text reference P7 (at -1.9 0 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -1.55 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.55 0 90) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(P7-Pad2)"))
    (pad 1 smd rect (at -0.55 0 90) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 28 /LED_FET_5V))
  )
  (module plan44:STELVIO-5P-508 (layer F.Cu) (tedit 5B6069A3)
    (at 149.25 70.5)
    (attr virtual)
    (fp_text reference J5 (at 4.25 -4.3 90) (layer F.SilkS))
    (fp_text value STELVIO-5P-508 (at -7.62 -11.43) (layer F.Fab))
    (pad 5 thru_hole circle (at -20.32 0) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 23 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 27 /LED_DATA1))
    (pad 2 thru_hole circle (at -5.08 0) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 33 /LED_DATA2))
    (pad 3 thru_hole circle (at -10.16 0) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 40 /LED_DATA3))
    (pad 4 thru_hole circle (at -15.24 0) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
  )
  (module plan44:STELVIO-2P-508 (layer F.Cu) (tedit 5B6068C4)
    (at 90.5 70.3)
    (attr virtual)
    (fp_text reference J3 (at 4.2 -4.1 90) (layer F.SilkS))
    (fp_text value STELVIO-2P-508 (at -2.54 -11.43) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 5 +24V))
    (pad 2 thru_hole circle (at -5.08 0) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
  )
  (module plan44:STELVIO-2P-508 (layer F.Cu) (tedit 5B6068C4)
    (at 105 70.3)
    (attr virtual)
    (fp_text reference J4 (at 4.2 -4.1 90) (layer F.SilkS))
    (fp_text value STELVIO-2P-508 (at -2.54 -11.43) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 5 +24V))
    (pad 2 thru_hole circle (at -5.08 0) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 42 /FET_PWR))
  )
  (module plan44:STELVIO-4P-508 (layer F.Cu) (tedit 5B60695C)
    (at 132.25 113.45 180)
    (attr virtual)
    (fp_text reference J6 (at 4.05 -4.15 270) (layer F.SilkS))
    (fp_text value STELVIO-4P-508 (at -7.62 -11.43 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 43 /SENS_PWR))
    (pad 2 thru_hole circle (at -5.08 0 180) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 34 "Net-(J6-Pad2)"))
    (pad 3 thru_hole circle (at -10.16 0 180) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 35 "Net-(J6-Pad3)"))
    (pad 4 thru_hole circle (at -15.24 0 180) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
  )
  (gr_text VCC (at 132.3 110.9) (layer F.SilkS))
  (gr_text GND (at 147.6 110.9) (layer F.SilkS))
  (gr_text CH1 (at 142.4 110.9) (layer F.SilkS))
  (gr_text CH0 (at 137.3 110.9) (layer F.SilkS))
  (gr_text L1 (at 149.3 73.5 90) (layer F.SilkS))
  (gr_text L2 (at 146 73.5 90) (layer F.SilkS))
  (gr_text L3 (at 137.9 73.5 90) (layer F.SilkS))
  (gr_text GND (at 135.7 74.2 90) (layer F.SilkS))
  (gr_text +5V (at 127.7 74.2 90) (layer F.SilkS))
  (gr_text LED- (at 99.7 73.2) (layer F.SilkS))
  (gr_text LED+ (at 105.7 73.2) (layer F.SilkS))
  (gr_text GND (at 90.6 73.2) (layer F.SilkS))
  (gr_text 24V (at 85.5 73.2) (layer F.SilkS))
  (dimension 56 (width 0.3) (layer Dwgs.User)
    (gr_text "56.000 mm" (at 177.85 92 90) (layer Dwgs.User))
    (feature1 (pts (xy 162.5 64) (xy 179.2 64)))
    (feature2 (pts (xy 162.5 120) (xy 179.2 120)))
    (crossbar (pts (xy 176.5 120) (xy 176.5 64)))
    (arrow1a (pts (xy 176.5 64) (xy 177.086421 65.126504)))
    (arrow1b (pts (xy 176.5 64) (xy 175.913579 65.126504)))
    (arrow2a (pts (xy 176.5 120) (xy 177.086421 118.873496)))
    (arrow2b (pts (xy 176.5 120) (xy 175.913579 118.873496)))
  )
  (dimension 90.5 (width 0.3) (layer Dwgs.User)
    (gr_text "90.500 mm" (at 117.25 128.85) (layer Dwgs.User))
    (feature1 (pts (xy 162.5 120) (xy 162.5 130.2)))
    (feature2 (pts (xy 72 120) (xy 72 130.2)))
    (crossbar (pts (xy 72 127.5) (xy 162.5 127.5)))
    (arrow1a (pts (xy 162.5 127.5) (xy 161.373496 128.086421)))
    (arrow1b (pts (xy 162.5 127.5) (xy 161.373496 126.913579)))
    (arrow2a (pts (xy 72 127.5) (xy 73.126504 128.086421)))
    (arrow2b (pts (xy 72 127.5) (xy 73.126504 126.913579)))
  )
  (dimension 6 (width 0.3) (layer Dwgs.User)
    (gr_text "0.2362 in" (at 93 55.65) (layer Dwgs.User))
    (feature1 (pts (xy 96 79) (xy 96 54.3)))
    (feature2 (pts (xy 90 79) (xy 90 54.3)))
    (crossbar (pts (xy 90 57) (xy 96 57)))
    (arrow1a (pts (xy 96 57) (xy 94.873496 57.586421)))
    (arrow1b (pts (xy 96 57) (xy 94.873496 56.413579)))
    (arrow2a (pts (xy 90 57) (xy 91.126504 57.586421)))
    (arrow2b (pts (xy 90 57) (xy 91.126504 56.413579)))
  )
  (dimension 2.9 (width 0.3) (layer Dwgs.User)
    (gr_text "2.900 mm" (at 39 130.3 270) (layer Dwgs.User))
    (feature1 (pts (xy 67.8 123.6) (xy 36.4 123.6)))
    (feature2 (pts (xy 67.8 120.7) (xy 36.4 120.7)))
    (crossbar (pts (xy 39.1 120.7) (xy 39.1 123.6)))
    (arrow1a (pts (xy 39.1 123.6) (xy 38.513579 122.473496)))
    (arrow1b (pts (xy 39.1 123.6) (xy 39.686421 122.473496)))
    (arrow2a (pts (xy 39.1 120.7) (xy 38.513579 121.826504)))
    (arrow2b (pts (xy 39.1 120.7) (xy 39.686421 121.826504)))
  )
  (dimension 2.9 (width 0.3) (layer Dwgs.User)
    (gr_text "2.900 mm" (at 34.9 53.7 90) (layer Dwgs.User))
    (feature1 (pts (xy 67.8 60.3) (xy 32 60.3)))
    (feature2 (pts (xy 67.8 63.2) (xy 32 63.2)))
    (crossbar (pts (xy 34.7 63.2) (xy 34.7 60.3)))
    (arrow1a (pts (xy 34.7 60.3) (xy 35.286421 61.426504)))
    (arrow1b (pts (xy 34.7 60.3) (xy 34.113579 61.426504)))
    (arrow2a (pts (xy 34.7 63.2) (xy 35.286421 62.073496)))
    (arrow2b (pts (xy 34.7 63.2) (xy 34.113579 62.073496)))
  )
  (gr_line (start 72 120) (end 72 64) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.5 120) (end 72 120) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.5 64) (end 162.5 120) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72 64) (end 162.5 64) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 108 (width 0.3) (layer Dwgs.User)
    (gr_text "108.000 mm" (at 117.25 36.75) (layer Dwgs.User))
    (feature1 (pts (xy 171.25 73.8) (xy 171.25 35.4)))
    (feature2 (pts (xy 63.25 73.8) (xy 63.25 35.4)))
    (crossbar (pts (xy 63.25 38.1) (xy 171.25 38.1)))
    (arrow1a (pts (xy 171.25 38.1) (xy 170.123496 38.686421)))
    (arrow1b (pts (xy 171.25 38.1) (xy 170.123496 37.513579)))
    (arrow2a (pts (xy 63.25 38.1) (xy 64.376504 38.686421)))
    (arrow2b (pts (xy 63.25 38.1) (xy 64.376504 37.513579)))
  )
  (dimension 8 (width 0.3) (layer Dwgs.User)
    (gr_text "8.000 mm" (at 57 47.5) (layer Dwgs.User))
    (feature1 (pts (xy 63.25 73.8) (xy 63.25 45.05)))
    (feature2 (pts (xy 71.25 73.8) (xy 71.25 45.05)))
    (crossbar (pts (xy 71.25 47.75) (xy 63.25 47.75)))
    (arrow1a (pts (xy 63.25 47.75) (xy 64.376504 47.163579)))
    (arrow1b (pts (xy 63.25 47.75) (xy 64.376504 48.336421)))
    (arrow2a (pts (xy 71.25 47.75) (xy 70.123496 47.163579)))
    (arrow2b (pts (xy 71.25 47.75) (xy 70.123496 48.336421)))
  )
  (dimension 8 (width 0.3) (layer Dwgs.User)
    (gr_text "8.000 mm" (at 34.9 69.8 90) (layer Dwgs.User))
    (feature1 (pts (xy 67.8 63.3) (xy 36.3 63.3)))
    (feature2 (pts (xy 67.8 71.3) (xy 36.3 71.3)))
    (crossbar (pts (xy 39 71.3) (xy 39 63.3)))
    (arrow1a (pts (xy 39 63.3) (xy 39.586421 64.426504)))
    (arrow1b (pts (xy 39 63.3) (xy 38.413579 64.426504)))
    (arrow2a (pts (xy 39 71.3) (xy 39.586421 70.173496)))
    (arrow2b (pts (xy 39 71.3) (xy 38.413579 70.173496)))
  )
  (dimension 49.5 (width 0.3) (layer Dwgs.User)
    (gr_text "49.500 mm" (at 37.7 96.05 270) (layer Dwgs.User))
    (feature1 (pts (xy 67.8 120.8) (xy 36.35 120.8)))
    (feature2 (pts (xy 67.8 71.3) (xy 36.35 71.3)))
    (crossbar (pts (xy 39.05 71.3) (xy 39.05 120.8)))
    (arrow1a (pts (xy 39.05 120.8) (xy 38.463579 119.673496)))
    (arrow1b (pts (xy 39.05 120.8) (xy 39.636421 119.673496)))
    (arrow2a (pts (xy 39.05 71.3) (xy 38.463579 72.426504)))
    (arrow2b (pts (xy 39.05 71.3) (xy 39.636421 72.426504)))
  )
  (dimension 41.5 (width 0.3) (layer Dwgs.User)
    (gr_text "41.500 mm" (at 43.35 92.05 270) (layer Dwgs.User))
    (feature1 (pts (xy 67.8 112.8) (xy 42 112.8)))
    (feature2 (pts (xy 67.8 71.3) (xy 42 71.3)))
    (crossbar (pts (xy 44.7 71.3) (xy 44.7 112.8)))
    (arrow1a (pts (xy 44.7 112.8) (xy 44.113579 111.673496)))
    (arrow1b (pts (xy 44.7 112.8) (xy 45.286421 111.673496)))
    (arrow2a (pts (xy 44.7 71.3) (xy 44.113579 72.426504)))
    (arrow2b (pts (xy 44.7 71.3) (xy 45.286421 72.426504)))
  )
  (dimension 2.5 (width 0.3) (layer Dwgs.User)
    (gr_text "2.500 mm" (at 58.4 80 90) (layer Dwgs.User))
    (feature1 (pts (xy 67.8 71.3) (xy 55.8 71.3)))
    (feature2 (pts (xy 67.8 73.8) (xy 55.8 73.8)))
    (crossbar (pts (xy 58.5 73.8) (xy 58.5 71.3)))
    (arrow1a (pts (xy 58.5 71.3) (xy 59.086421 72.426504)))
    (arrow1b (pts (xy 58.5 71.3) (xy 57.913579 72.426504)))
    (arrow2a (pts (xy 58.5 73.8) (xy 59.086421 72.673496)))
    (arrow2b (pts (xy 58.5 73.8) (xy 57.913579 72.673496)))
  )
  (dimension 92 (width 0.3) (layer Dwgs.User)
    (gr_text "92.000 mm" (at 117.25 46.4) (layer Dwgs.User))
    (feature1 (pts (xy 163.25 70.5) (xy 163.25 45.05)))
    (feature2 (pts (xy 71.25 70.5) (xy 71.25 45.05)))
    (crossbar (pts (xy 71.25 47.75) (xy 163.25 47.75)))
    (arrow1a (pts (xy 163.25 47.75) (xy 162.123496 48.336421)))
    (arrow1b (pts (xy 163.25 47.75) (xy 162.123496 47.163579)))
    (arrow2a (pts (xy 71.25 47.75) (xy 72.376504 48.336421)))
    (arrow2b (pts (xy 71.25 47.75) (xy 72.376504 47.163579)))
  )
  (dimension 7.25 (width 0.3) (layer Dwgs.User)
    (gr_text "7.250 mm" (at 84.8 43.5) (layer Dwgs.User))
    (feature1 (pts (xy 71.25 73.8) (xy 71.25 40.9)))
    (feature2 (pts (xy 78.5 73.8) (xy 78.5 40.9)))
    (crossbar (pts (xy 78.5 43.6) (xy 71.25 43.6)))
    (arrow1a (pts (xy 71.25 43.6) (xy 72.376504 43.013579)))
    (arrow1b (pts (xy 71.25 43.6) (xy 72.376504 44.186421)))
    (arrow2a (pts (xy 78.5 43.6) (xy 77.373496 43.013579)))
    (arrow2b (pts (xy 78.5 43.6) (xy 77.373496 44.186421)))
  )
  (dimension 77.5 (width 0.3) (layer Dwgs.User)
    (gr_text "77.500 mm" (at 117.25 51.75) (layer Dwgs.User))
    (feature1 (pts (xy 156 77) (xy 156 50.4)))
    (feature2 (pts (xy 78.5 77) (xy 78.5 50.4)))
    (crossbar (pts (xy 78.5 53.1) (xy 156 53.1)))
    (arrow1a (pts (xy 156 53.1) (xy 154.873496 53.686421)))
    (arrow1b (pts (xy 156 53.1) (xy 154.873496 52.513579)))
    (arrow2a (pts (xy 78.5 53.1) (xy 79.626504 53.686421)))
    (arrow2b (pts (xy 78.5 53.1) (xy 79.626504 52.513579)))
  )
  (dimension 36.5 (width 0.3) (layer Dwgs.User)
    (gr_text "36.500 mm" (at 61.45 92.05 270) (layer Dwgs.User))
    (feature1 (pts (xy 85.6 110.3) (xy 60.1 110.3)))
    (feature2 (pts (xy 85.6 73.8) (xy 60.1 73.8)))
    (crossbar (pts (xy 62.8 73.8) (xy 62.8 110.3)))
    (arrow1a (pts (xy 62.8 110.3) (xy 62.213579 109.173496)))
    (arrow1b (pts (xy 62.8 110.3) (xy 63.386421 109.173496)))
    (arrow2a (pts (xy 62.8 73.8) (xy 62.213579 74.926504)))
    (arrow2b (pts (xy 62.8 73.8) (xy 63.386421 74.926504)))
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162 119) (xy 73 119) (xy 73 65) (xy 162 65)
      )
    )
  )
  (zone (net 5) (net_name +24V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107 73) (xy 88 73) (xy 88 65) (xy 107 65)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87 74) (xy 108 74) (xy 108 65) (xy 162 65) (xy 162 119)
        (xy 73 119) (xy 73 65) (xy 87 65)
      )
    )
  )
)
