(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 76)
    (zones 0)
    (modules 13)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1.78)
    (user_trace_width 0.5)
    (user_trace_width 1.78)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.99898 1.99898)
    (pad_drill 1.2)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 114.3 105.41)
    (grid_origin 114.3 105.41)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(Blue1-Pad1)")
  (net 2 "Net-(Green1-Pad1)")
  (net 3 GND)
  (net 4 "Net-(R1-Pad2)")
  (net 5 +12V)
  (net 6 "Net-(Blue1-Pad3)")
  (net 7 "Net-(Output1-Pad3)")
  (net 8 "Net-(Blue1-Pad2)")
  (net 9 "Net-(Green1-Pad2)")
  (net 10 "Net-(Pololu1-Pad4)")
  (net 11 "Net-(PowerMosfet1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net GND)
    (add_net "Net-(Blue1-Pad1)")
    (add_net "Net-(Blue1-Pad2)")
    (add_net "Net-(Blue1-Pad3)")
    (add_net "Net-(Green1-Pad1)")
    (add_net "Net-(Green1-Pad2)")
    (add_net "Net-(Output1-Pad3)")
    (add_net "Net-(Pololu1-Pad4)")
    (add_net "Net-(PowerMosfet1-Pad1)")
    (add_net "Net-(R1-Pad2)")
  )
  (module fossil:fossil (layer B.Cu) (tedit 5D3263A9)
    (at 156.21 95.25 180)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Connector_Wire:SolderWirePad_1x02_P3.81mm_Drill0.8mm (layer F.Cu) (tedit 5D37A739)
    (at 156.21 76.2)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference 12v_In1 (at 1.905 2.54) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 1.905 2.54) (layer F.Fab) hide)
    (fp_text user %R (at 1.905 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.99898 1.99898) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.99898 1.99898) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 +12V))
  )
  (module EndConnectors:Pololu_4Pin_Power (layer F.Cu) (tedit 5D3254CE)
    (at 125.73 92.71 270)
    (descr "JST EH series connector, B4B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (fp_text reference Pololu (at 3.75 -2.8 90) (layer F.SilkS))
    (fp_text value "Pololu 4 Pin" (at 3.75 3.4 90) (layer F.Fab))
    (fp_text user %R (at 3.75 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 0.95) (layers *.Cu *.Mask))
    (pad 2 thru_hole rect (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 5 +12V))
    (pad 3 thru_hole circle (at 5 0 270) (size 1.7 1.7) (drill 0.95) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 4 thru_hole roundrect (at 7.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(Pololu1-Pad4)"))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B4B-EH-A_1x04_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire:SolderWirePad_1x04_P3.175mm_Drill0.8mm (layer F.Cu) (tedit 5D37A72D)
    (at 125.73 76.2 270)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference Output1 (at 3.81 2.54 90) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 4.7625 3.175 90) (layer F.Fab))
    (fp_text user %R (at 3.81 -0.762 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 9.525 0 270) (size 1.99898 1.99898) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(Blue1-Pad2)"))
    (pad 3 thru_hole circle (at 6.35 0 270) (size 1.99898 1.99898) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(Output1-Pad3)"))
    (pad 2 thru_hole circle (at 3.175 0 270) (size 1.99898 1.99898) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 "Net-(Green1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.99898 1.99898) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 +12V))
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 144.78 78.74)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference PowerMosfet (at 2.54 2.54) (layer F.SilkS))
    (fp_text value FQP30N06L (at 2.54 2.54) (layer F.Fab) hide)
    (fp_text user %R (at 2.54 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(Blue1-Pad3)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 "Net-(PowerMosfet1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 130.81 101.6 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value R (at 3.81 2.37 90) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(Blue1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 123.19 106.68)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 3.81 0) (layer F.SilkS))
    (fp_text value R (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(Green1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 130.81 90.17 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value R (at 3.81 2.37 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(R1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 135.89 93.98 90)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Blue (at 2.54 -4.27 90) (layer F.SilkS))
    (fp_text value FQP30N06L (at 2.54 2.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.54 -4.27 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(Blue1-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 "Net-(Blue1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(Blue1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 135.89 82.55 90)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Red (at 2.54 -4.27 90) (layer F.SilkS))
    (fp_text value FQP30N06L (at 2.54 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.27 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(Blue1-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "Net-(Output1-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Module:WEMOS_D1_mini_light (layer F.Cu) (tedit 5BBFB1CE)
    (at 165.1 83.82 270)
    (descr "16-pin module, column spacing 22.86 mm (900 mils), https://wiki.wemos.cc/products:d1:d1_mini, https://c1.staticflickr.com/1/734/31400410271_f278b087db_z.jpg")
    (tags "ESP8266 WiFi microcontroller")
    (fp_text reference U1 (at 22 27 90) (layer F.SilkS))
    (fp_text value WeMos_D1_mini (at 11.7 0 90) (layer F.Fab))
    (fp_text user "No copper" (at 11.43 -3.81 90) (layer Cmts.User))
    (fp_text user "KEEP OUT" (at 11.43 -6.35 90) (layer Cmts.User))
    (fp_text user %R (at 11.43 10 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 22.86 0 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 22.86 2.54 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 22.86 5.08 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 22.86 7.62 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(PowerMosfet1-Pad1)"))
    (pad 12 thru_hole oval (at 22.86 10.16 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 22.86 12.7 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 22.86 15.24 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 9 thru_hole oval (at 22.86 17.78 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(Pololu1-Pad4)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(R1-Pad2)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(Green1-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(Blue1-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Module.3dshapes/WEMOS_D1_mini_light.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (offset (xyz 0 0 9.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -180 0))
    )
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (offset (xyz 22.86 0 9.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -180 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl
      (offset (xyz 22.86 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 135.89 105.41 90)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Green (at 2.54 -4.27 90) (layer F.SilkS))
    (fp_text value FQP30N06L (at 2.54 2.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.54 -4.27 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(Blue1-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 "Net-(Green1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(Green1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fossil:fossil (layer F.Cu) (tedit 5D3263A9)
    (at 151.13 95.25)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (gr_text "Wemos Mini D1 lite SMD 5050 RGB LED Strip Controller" (at 146.05 73.66) (layer F.SilkS))
  (gr_text 2.2 (at 163.83 77.47) (layer F.SilkS))
  (gr_line (start 168.91 110.49) (end 168.91 72.39) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.65 110.49) (end 168.91 110.49) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.65 72.39) (end 120.65 110.49) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 168.91 72.39) (end 120.65 72.39) (layer Edge.Cuts) (width 0.1))
  (gr_text 2.2 (at 163.83 77.47) (layer B.SilkS))
  (gr_text "Wemos Mini D1 lite SMD 5050 RGB LED Strip Controller" (at 146.05 73.66) (layer B.SilkS))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.37 73.66) (xy 121.92 73.66) (xy 121.92 109.22) (xy 166.37 109.22)
      )
    )
  )
)
