(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 36)
    (no_connects 0)
    (area 118.034999 91.3667 189.035 132.155001)
    (thickness 1.6)
    (drawings 28)
    (tracks 101)
    (zones 0)
    (modules 32)
    (nets 25)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 SCART_Red)
  (net 5 "Net-(C3-Pad1)")
  (net 6 SCART_Green)
  (net 7 "Net-(C5-Pad1)")
  (net 8 SCART_Sync)
  (net 9 "Net-(R1-Pad1)")
  (net 10 Jamma_Red)
  (net 11 "Net-(R2-Pad1)")
  (net 12 Jamma_Blue)
  (net 13 "Net-(R3-Pad1)")
  (net 14 Jamma_Green)
  (net 15 "Net-(R4-Pad1)")
  (net 16 Jamma_Sync)
  (net 17 "Net-(R9-Pad2)")
  (net 18 "Net-(R10-Pad2)")
  (net 19 "Net-(C4-Pad1)")
  (net 20 "Net-(R11-Pad2)")
  (net 21 "Net-(R12-Pad2)")
  (net 22 "Net-(U1-Pad7)")
  (net 23 "Net-(U1-Pad8)")
  (net 24 SCART_Blue)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net Jamma_Blue)
    (add_net Jamma_Green)
    (add_net Jamma_Red)
    (add_net Jamma_Sync)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net SCART_Blue)
    (add_net SCART_Green)
    (add_net SCART_Red)
    (add_net SCART_Sync)
  )
  (net_class +5V ""
    (clearance 0.2)
    (trace_width 0.45)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
  )
  (net_class GND ""
    (clearance 0.2)
    (trace_width 0.45)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5AD0419A)
    (at 153.67 114.3)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -1.27 1.27) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_8x10 (layer F.Cu) (tedit 5AD04136)
    (at 167.64 97.79)
    (descr "SMT capacitor, aluminium electrolytic, 8x10")
    (attr smd)
    (fp_text reference C2 (at -6.35 -2.54) (layer F.SilkS))
    (fp_text value 220uF (at 0 -5.4483) (layer F.Fab))
    (fp_text user + (at -2.3114 -0.0762) (layer F.Fab))
    (fp_text user + (at -4.7752 3.8989) (layer F.SilkS))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 4 SCART_Red))
    (model Capacitors_SMD.3dshapes/c_elec_8x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:c_elec_8x10 (layer F.Cu) (tedit 5AD04142)
    (at 167.64 106.68)
    (descr "SMT capacitor, aluminium electrolytic, 8x10")
    (attr smd)
    (fp_text reference C3 (at -6.35 -2.54) (layer F.SilkS))
    (fp_text value 220uF (at 0 -5.4483) (layer F.Fab))
    (fp_text user + (at -2.3114 -0.0762) (layer F.Fab))
    (fp_text user + (at -4.7752 3.8989) (layer F.SilkS))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 6 SCART_Green))
    (model Capacitors_SMD.3dshapes/c_elec_8x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:c_elec_8x10 (layer F.Cu) (tedit 5AD04149)
    (at 167.64 115.57)
    (descr "SMT capacitor, aluminium electrolytic, 8x10")
    (attr smd)
    (fp_text reference C4 (at -6.35 -2.54) (layer F.SilkS))
    (fp_text value 220uF (at 0 -5.4483) (layer F.Fab))
    (fp_text user + (at -2.3114 -0.0762) (layer F.Fab))
    (fp_text user + (at -4.7752 3.8989) (layer F.SilkS))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 24 SCART_Blue))
    (model Capacitors_SMD.3dshapes/c_elec_8x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:c_elec_8x10 (layer F.Cu) (tedit 5AD0414E)
    (at 167.64 124.46)
    (descr "SMT capacitor, aluminium electrolytic, 8x10")
    (attr smd)
    (fp_text reference C5 (at -6.35 -3.81) (layer F.SilkS))
    (fp_text value 220uF (at 0 -5.4483) (layer F.Fab))
    (fp_text user + (at -2.3114 -0.0762) (layer F.Fab))
    (fp_text user + (at -4.7752 3.8989) (layer F.SilkS))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 SCART_Sync))
    (model Capacitors_SMD.3dshapes/c_elec_8x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5AD04157)
    (at 134.62 95.25 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value 6k8 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 Jamma_Red))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5AD04163)
    (at 134.62 101.6 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value 6k8 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 Jamma_Blue))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5AD0416E)
    (at 134.62 107.95 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value 6k8 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 Jamma_Green))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5AD04176)
    (at 134.62 114.3 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value 6k8 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 Jamma_Sync))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5AD0417A)
    (at 134.62 116.84 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value 1k1 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5AD04172)
    (at 134.62 110.49 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value 1k4 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5AD04168)
    (at 134.62 104.14 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value 1k4 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5AD0415E)
    (at 134.62 97.79 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value 1k4 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5AD04183)
    (at 157.48 105.41 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 75R (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R9-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5AD04189)
    (at 157.48 107.95 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 75R (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R10-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5AD0418D)
    (at 157.48 110.49 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 75R (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R11-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5AD04192)
    (at 157.48 113.03 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 75R (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R12-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:SSOP-14_5.3x6.2mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 147.32 110.49)
    (descr "SSOP14: plastic shrink small outline package; 14 leads; body width 5.3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot337-1_po.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 -4.2) (layer F.SilkS))
    (fp_text value THS7374 (at 0 4.2) (layer F.Fab))
    (pad 1 smd rect (at -3.45 -1.95) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at -3.45 -1.3) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R2-Pad1)"))
    (pad 3 smd rect (at -3.45 -0.65) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R3-Pad1)"))
    (pad 4 smd rect (at -3.45 0) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R4-Pad1)"))
    (pad 5 smd rect (at -3.45 0.65) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -3.45 1.3) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -3.45 1.95) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U1-Pad7)"))
    (pad 8 smd rect (at 3.45 1.95) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U1-Pad8)"))
    (pad 9 smd rect (at 3.45 1.3) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 3.45 0.65) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 11 smd rect (at 3.45 0) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R12-Pad2)"))
    (pad 12 smd rect (at 3.45 -0.65) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R11-Pad2)"))
    (pad 13 smd rect (at 3.45 -1.3) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R10-Pad2)"))
    (pad 14 smd rect (at 3.45 -1.95) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R9-Pad2)"))
    (model Housings_SSOP.3dshapes/SSOP-14_5.3x6.2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 5AD042F1)
    (at 124.46 96.52 90)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference W1 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value Jamma_Red (at 0 6.35 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 5 10) (layers F.Cu F.Paste F.Mask)
      (net 10 Jamma_Red))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 5AD042F9)
    (at 124.46 102.87 90)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference W2 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value Jamma_Blue (at 0 6.35 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 5 10) (layers F.Cu F.Paste F.Mask)
      (net 12 Jamma_Blue))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 5AD042FE)
    (at 124.46 109.22 90)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference W3 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value Jamma_Green (at 0 6.35 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 5 10) (layers F.Cu F.Paste F.Mask)
      (net 14 Jamma_Green))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 5AD04306)
    (at 124.46 115.57 90)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference W4 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value "Jamma Sync" (at 0 6.35 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 5 10) (layers F.Cu F.Paste F.Mask)
      (net 16 Jamma_Sync))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 5AD0433A)
    (at 181.61 96.52 90)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference W5 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value SCART_Red (at 0 6.35 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 5 10) (layers F.Cu F.Paste F.Mask)
      (net 4 SCART_Red))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 5AD0433D)
    (at 181.61 102.87 90)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference W6 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value SCART_Blue (at 0 6.35 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 5 10) (layers F.Cu F.Paste F.Mask)
      (net 6 SCART_Green))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 5AD04341)
    (at 181.61 109.22 90)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference W7 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value SCART_Green (at 0 6.35 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 5 10) (layers F.Cu F.Paste F.Mask)
      (net 24 SCART_Blue))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 5AD04346)
    (at 181.61 115.57 90)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference W8 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value SCART_Sync (at 0 6.35 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 5 10) (layers F.Cu F.Paste F.Mask)
      (net 8 SCART_Sync))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 5AD091B0)
    (at 124.46 121.92 90)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference W9 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value GND_IN (at 0 6.35 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 5 10) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 5AD0434C)
    (at 181.61 121.92 90)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference W10 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value GND_OUT (at 0 6.35 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 5 10) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 5AD0430E)
    (at 124.46 128.27 90)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference W11 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value +5V_IN (at 0 6.35 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 5 10) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 5AD04352)
    (at 181.61 128.27 90)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference W12 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value +5V_OUT (at 0 6.35 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 5 10) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module Symbols:OSHW-Logo2_7.3x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 158.75 124.46)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module cmvs-rgb:logo (layer B.Cu) (tedit 0)
    (at 170.18 119.38 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_text NEO⋅GEO (at 149.86 96.52) (layer F.SilkS))
  (gr_text "MAX 7374 MEGA\nPRO SCART SPEC" (at 149.86 101.6) (layer F.SilkS))
  (gr_text "Value:\nTHS7374\n6k8\n1k1\n1k4\n0.1uF\n220uF\n" (at 157.48 104.14) (layer B.SilkS))
  (gr_text "Footprint:\nSSOP14\n0603\n0603\n0603\n0603\n8x10" (at 144.78 104.14) (layer B.SilkS))
  (gr_text "philenotfound <phil@zankapfel.net>" (at 153.67 125.73) (layer B.SilkS))
  (gr_text "SCART Output" (at 181.61 111.76 90) (layer B.SilkS))
  (gr_text "JAMMA Input" (at 124.46 111.76 270) (layer B.SilkS))
  (gr_text " ." (at 144.78 107.95) (layer F.SilkS))
  (gr_text "Part:\nU1\nR1,R2,R3,R4\nR5\nR6,R7,R8\nC1\nC2,C3,C4\n" (at 173.99 104.14) (layer B.SilkS))
  (gr_text "CMVS-RGB\nV1" (at 154.94 124.46) (layer F.SilkS))
  (gr_text S (at 175.26 115.57) (layer F.SilkS))
  (gr_text B (at 175.26 109.22) (layer F.SilkS))
  (gr_text G (at 175.26 102.87) (layer F.SilkS))
  (gr_text R (at 175.26 96.52) (layer F.SilkS))
  (gr_text +5V (at 173.99 127) (layer F.SilkS))
  (gr_text Gnd (at 173.99 120.65) (layer F.SilkS))
  (gr_text +5V (at 132.08 127) (layer F.SilkS))
  (gr_text Gnd (at 132.08 120.65) (layer F.SilkS))
  (gr_text S (at 130.81 115.57) (layer F.SilkS))
  (gr_text B (at 130.81 109.22) (layer F.SilkS))
  (gr_text G (at 130.81 102.87) (layer F.SilkS))
  (gr_text R (at 130.81 96.52) (layer F.SilkS))
  (gr_line (start 187.96 92.71) (end 118.11 92.71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 187.96 132.08) (end 187.96 92.71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.11 132.08) (end 187.96 132.08) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.11 92.71) (end 118.11 132.08) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.38 93.98) (xy 186.69 93.98) (xy 186.69 130.81) (xy 119.38 130.81)
      )
    )
  )
)
