(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 0)
    (no_connects 23)
    (area 0 0 0 0)
    (thickness 1.6)
    (drawings 4)
    (tracks 378)
    (zones 0)
    (modules 17)
    (nets 88)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.305)
    (user_trace_width 0.178)
    (user_trace_width 0.305)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.178)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFE1)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /D0OUT)
  (net 2 /D1OUT)
  (net 3 /D2OUT)
  (net 4 /D3OUT)
  (net 5 /D4OUT)
  (net 6 /D5OUT)
  (net 7 /D6OUT)
  (net 8 /D7OUT)
  (net 9 /D8OUT)
  (net 10 /D9OUT)
  (net 11 /D10OUT)
  (net 12 /D11OUT)
  (net 13 /D12OUT)
  (net 14 /D13OUT)
  (net 15 /D14OUT)
  (net 16 /D15OUT)
  (net 17 /D16OUT)
  (net 18 /D17OUT)
  (net 19 /D18OUT)
  (net 20 /D19OUT)
  (net 21 /D20OUT)
  (net 22 /D21OUT)
  (net 23 /D22OUT)
  (net 24 /D23OUT)
  (net 25 /D24OUT)
  (net 26 /D25OUT)
  (net 27 /D26OUT)
  (net 28 /D27OUT)
  (net 29 /D28OUT)
  (net 30 /D29OUT)
  (net 31 /D30OUT)
  (net 32 /D31OUT)
  (net 33 /D32OUT)
  (net 34 /D33OUT)
  (net 35 /D34OUT)
  (net 36 /D35OUT)
  (net 37 /D0IN)
  (net 38 /D1IN)
  (net 39 /D2IN)
  (net 40 /D3IN)
  (net 41 /D4IN)
  (net 42 /D5IN)
  (net 43 /D6IN)
  (net 44 /D7IN)
  (net 45 /D8IN)
  (net 46 /D9IN)
  (net 47 /D10IN)
  (net 48 /D11IN)
  (net 49 /D12IN)
  (net 50 /D13IN)
  (net 51 /D14IN)
  (net 52 /D15IN)
  (net 53 /D16IN)
  (net 54 /D17IN)
  (net 55 /D18IN)
  (net 56 /D19IN)
  (net 57 /D20IN)
  (net 58 /D21IN)
  (net 59 /D22IN)
  (net 60 /D23IN)
  (net 61 /D24IN)
  (net 62 /D25IN)
  (net 63 /D26IN)
  (net 64 /D27IN)
  (net 65 /D28IN)
  (net 66 /D29IN)
  (net 67 /D30IN)
  (net 68 /D31IN)
  (net 69 /D32IN)
  (net 70 /D33IN)
  (net 71 /D34IN)
  (net 72 /D35IN)
  (net 73 "Net-(U1-Pad1)")
  (net 74 +5)
  (net 75 GND)
  (net 76 "Net-(U2-Pad1)")
  (net 77 "Net-(U3-Pad1)")
  (net 78 "Net-(U4-Pad1)")
  (net 79 "Net-(U4-Pad2)")
  (net 80 "Net-(U4-Pad3)")
  (net 81 "Net-(U4-Pad21)")
  (net 82 "Net-(U4-Pad22)")
  (net 83 +3)
  (net 84 "Net-(U4-Pad10)")
  (net 85 "Net-(U4-Pad11)")
  (net 86 "Net-(U4-Pad13)")
  (net 87 "Net-(U4-Pad14)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.178)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3)
    (add_net +5)
    (add_net /D0IN)
    (add_net /D0OUT)
    (add_net /D10IN)
    (add_net /D10OUT)
    (add_net /D11IN)
    (add_net /D11OUT)
    (add_net /D12IN)
    (add_net /D12OUT)
    (add_net /D13IN)
    (add_net /D13OUT)
    (add_net /D14IN)
    (add_net /D14OUT)
    (add_net /D15IN)
    (add_net /D15OUT)
    (add_net /D16IN)
    (add_net /D16OUT)
    (add_net /D17IN)
    (add_net /D17OUT)
    (add_net /D18IN)
    (add_net /D18OUT)
    (add_net /D19IN)
    (add_net /D19OUT)
    (add_net /D1IN)
    (add_net /D1OUT)
    (add_net /D20IN)
    (add_net /D20OUT)
    (add_net /D21IN)
    (add_net /D21OUT)
    (add_net /D22IN)
    (add_net /D22OUT)
    (add_net /D23IN)
    (add_net /D23OUT)
    (add_net /D24IN)
    (add_net /D24OUT)
    (add_net /D25IN)
    (add_net /D25OUT)
    (add_net /D26IN)
    (add_net /D26OUT)
    (add_net /D27IN)
    (add_net /D27OUT)
    (add_net /D28IN)
    (add_net /D28OUT)
    (add_net /D29IN)
    (add_net /D29OUT)
    (add_net /D2IN)
    (add_net /D2OUT)
    (add_net /D30IN)
    (add_net /D30OUT)
    (add_net /D31IN)
    (add_net /D31OUT)
    (add_net /D32IN)
    (add_net /D32OUT)
    (add_net /D33IN)
    (add_net /D33OUT)
    (add_net /D34IN)
    (add_net /D34OUT)
    (add_net /D35IN)
    (add_net /D35OUT)
    (add_net /D3IN)
    (add_net /D3OUT)
    (add_net /D4IN)
    (add_net /D4OUT)
    (add_net /D5IN)
    (add_net /D5OUT)
    (add_net /D6IN)
    (add_net /D6OUT)
    (add_net /D7IN)
    (add_net /D7OUT)
    (add_net /D8IN)
    (add_net /D8OUT)
    (add_net /D9IN)
    (add_net /D9OUT)
    (add_net GND)
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U4-Pad1)")
    (add_net "Net-(U4-Pad10)")
    (add_net "Net-(U4-Pad11)")
    (add_net "Net-(U4-Pad13)")
    (add_net "Net-(U4-Pad14)")
    (add_net "Net-(U4-Pad2)")
    (add_net "Net-(U4-Pad21)")
    (add_net "Net-(U4-Pad22)")
    (add_net "Net-(U4-Pad3)")
  )
  (module pads:via-3mm (layer F.Cu) (tedit 5B50AD61)
    (at 180.25 143.25)
    (zone_connect 2)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND) (zone_connect 2))
  )
  (module pads:via-3mm (layer F.Cu) (tedit 5B50AD61)
    (at 180 137.25)
    (zone_connect 2)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND) (zone_connect 2))
  )
  (module pads:via-3mm (layer F.Cu) (tedit 5B50AD61)
    (at 152 144.25)
    (zone_connect 2)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND) (zone_connect 2))
  )
  (module pads:via-3mm (layer F.Cu) (tedit 5B50AD61)
    (at 155.25 137.25)
    (zone_connect 2)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND) (zone_connect 2))
  )
  (module pads:via-3mm (layer F.Cu) (tedit 5B50AD61)
    (at 155 144.25)
    (zone_connect 2)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND) (zone_connect 2))
  )
  (module pads:via-3mm (layer F.Cu) (tedit 5B50AD61)
    (at 167.5 144.25)
    (zone_connect 2)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND) (zone_connect 2))
  )
  (module de10_lvl:DE10_40PIN (layer F.Cu) (tedit 5B50A3D1)
    (at 142.24 149.86 180)
    (fp_text reference CON1 (at -0.762 4.572 180) (layer B.SilkS))
    (fp_text value DE10_OUTPUT (at -0.01 3.92 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 /D0OUT))
    (pad 2 thru_hole circle (at 0 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 /D1OUT))
    (pad 3 thru_hole circle (at -2.54 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 /D2OUT))
    (pad 4 thru_hole circle (at -2.54 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 /D3OUT))
    (pad 5 thru_hole circle (at -5.08 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 /D4OUT))
    (pad 6 thru_hole circle (at -5.08 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 /D5OUT))
    (pad 7 thru_hole circle (at -7.62 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 /D6OUT))
    (pad 8 thru_hole circle (at -7.62 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 /D7OUT))
    (pad 9 thru_hole circle (at -10.16 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 /D8OUT))
    (pad 10 thru_hole circle (at -10.16 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 /D9OUT))
    (pad 11 thru_hole circle (at -12.7 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 74 +5))
    (pad 12 thru_hole circle (at -12.7 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 75 GND))
    (pad 13 thru_hole circle (at -15.24 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 /D10OUT))
    (pad 14 thru_hole circle (at -15.24 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 /D11OUT))
    (pad 15 thru_hole circle (at -17.78 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 /D12OUT))
    (pad 16 thru_hole circle (at -17.78 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 /D13OUT))
    (pad 17 thru_hole circle (at -20.32 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 /D14OUT))
    (pad 18 thru_hole circle (at -20.32 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 /D15OUT))
    (pad 19 thru_hole circle (at -22.86 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 /D16OUT))
    (pad 20 thru_hole circle (at -22.86 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 18 /D17OUT))
    (pad 21 thru_hole circle (at -25.4 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 /D18OUT))
    (pad 22 thru_hole circle (at -25.4 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 20 /D19OUT))
    (pad 23 thru_hole circle (at -27.94 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 21 /D20OUT))
    (pad 24 thru_hole circle (at -27.94 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 /D21OUT))
    (pad 25 thru_hole circle (at -30.48 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 23 /D22OUT))
    (pad 26 thru_hole circle (at -30.48 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 24 /D23OUT))
    (pad 27 thru_hole circle (at -33.02 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 /D24OUT))
    (pad 28 thru_hole circle (at -33.02 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 26 /D25OUT))
    (pad 29 thru_hole circle (at -35.56 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 83 +3))
    (pad 30 thru_hole circle (at -35.56 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 75 GND))
    (pad 31 thru_hole circle (at -38.1 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 27 /D26OUT))
    (pad 32 thru_hole circle (at -38.1 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 28 /D27OUT))
    (pad 33 thru_hole circle (at -40.64 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 29 /D28OUT))
    (pad 34 thru_hole circle (at -40.64 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 30 /D29OUT))
    (pad 35 thru_hole circle (at -43.18 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 31 /D30OUT))
    (pad 36 thru_hole circle (at -43.18 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 32 /D31OUT))
    (pad 37 thru_hole circle (at -45.72 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 /D32OUT))
    (pad 38 thru_hole circle (at -45.72 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 34 /D33OUT))
    (pad 39 thru_hole circle (at -48.26 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 35 /D34OUT))
    (pad 40 thru_hole circle (at -48.26 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 36 /D35OUT))
  )
  (module de10_lvl:DE10_40PIN (layer F.Cu) (tedit 5B50A3CA)
    (at 142.24 132.08 180)
    (fp_text reference CON5 (at -1.016 -2.54 180) (layer F.SilkS))
    (fp_text value DE10_INPUT (at 0.02 -1.37 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 37 /D0IN))
    (pad 2 thru_hole circle (at 0 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 38 /D1IN))
    (pad 3 thru_hole circle (at -2.54 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 39 /D2IN))
    (pad 4 thru_hole circle (at -2.54 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 40 /D3IN))
    (pad 5 thru_hole circle (at -5.08 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 41 /D4IN))
    (pad 6 thru_hole circle (at -5.08 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 42 /D5IN))
    (pad 7 thru_hole circle (at -7.62 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 43 /D6IN))
    (pad 8 thru_hole circle (at -7.62 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 44 /D7IN))
    (pad 9 thru_hole circle (at -10.16 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 45 /D8IN))
    (pad 10 thru_hole circle (at -10.16 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 46 /D9IN))
    (pad 11 thru_hole circle (at -12.7 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 74 +5))
    (pad 12 thru_hole circle (at -12.7 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 75 GND))
    (pad 13 thru_hole circle (at -15.24 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 47 /D10IN))
    (pad 14 thru_hole circle (at -15.24 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 48 /D11IN))
    (pad 15 thru_hole circle (at -17.78 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 49 /D12IN))
    (pad 16 thru_hole circle (at -17.78 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 50 /D13IN))
    (pad 17 thru_hole circle (at -20.32 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 51 /D14IN))
    (pad 18 thru_hole circle (at -20.32 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 52 /D15IN))
    (pad 19 thru_hole circle (at -22.86 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 53 /D16IN))
    (pad 20 thru_hole circle (at -22.86 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 54 /D17IN))
    (pad 21 thru_hole circle (at -25.4 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 55 /D18IN))
    (pad 22 thru_hole circle (at -25.4 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 56 /D19IN))
    (pad 23 thru_hole circle (at -27.94 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 57 /D20IN))
    (pad 24 thru_hole circle (at -27.94 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 58 /D21IN))
    (pad 25 thru_hole circle (at -30.48 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 59 /D22IN))
    (pad 26 thru_hole circle (at -30.48 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 60 /D23IN))
    (pad 27 thru_hole circle (at -33.02 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 61 /D24IN))
    (pad 28 thru_hole circle (at -33.02 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 62 /D25IN))
    (pad 29 thru_hole circle (at -35.56 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 83 +3))
    (pad 30 thru_hole circle (at -35.56 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 75 GND))
    (pad 31 thru_hole circle (at -38.1 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 63 /D26IN))
    (pad 32 thru_hole circle (at -38.1 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 64 /D27IN))
    (pad 33 thru_hole circle (at -40.64 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 65 /D28IN))
    (pad 34 thru_hole circle (at -40.64 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 66 /D29IN))
    (pad 35 thru_hole circle (at -43.18 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 67 /D30IN))
    (pad 36 thru_hole circle (at -43.18 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 68 /D31IN))
    (pad 37 thru_hole circle (at -45.72 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 69 /D32IN))
    (pad 38 thru_hole circle (at -45.72 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 70 /D33IN))
    (pad 39 thru_hole circle (at -48.26 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 71 /D34IN))
    (pad 40 thru_hole circle (at -48.26 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 72 /D35IN))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B50A82E)
    (at 190.5 139.954 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 3.048 0 90) (layer F.SilkS))
    (fp_text value .1u (at 0 0 180) (layer F.Fab))
    (fp_text user %R (at 3.048 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 74 +5))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 75 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B50A846)
    (at 178.562 140 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 2.982 0 90) (layer F.SilkS))
    (fp_text value .1u (at 0 0 180) (layer F.Fab))
    (fp_text user %R (at 2.982 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 74 +5))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 75 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B50A88E)
    (at 165.608 140 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 2.86 0 90) (layer F.SilkS))
    (fp_text value .1u (at 0 0 180) (layer F.Fab))
    (fp_text user %R (at 2.86 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 74 +5))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 75 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B50A90A)
    (at 152.146 139.954 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 2.794 0 90) (layer F.SilkS))
    (fp_text value .1u (at 0 0 180) (layer F.Fab))
    (fp_text user %R (at 2.794 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 74 +5))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 75 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:TSSOP-24_W4.40mm (layer F.Cu) (tedit 5B50A3C3)
    (at 146.875 139.96 180)
    (descr http://www.ti.com/lit/ds/symlink/tca9548a.pdf)
    (fp_text reference U1 (at -5.295 -3.09 180) (layer F.SilkS))
    (fp_text value SN74CBTD3861PWR (at -2.555 1.55 180) (layer F.Fab) hide)
    (fp_text user %R (at -5.275 -3.09 180) (layer F.Fab))
    (pad 1 smd rect (at -3.575 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U1-Pad1)") (solder_mask_margin 0.07))
    (pad 2 smd rect (at -2.925 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 46 /D9IN) (solder_mask_margin 0.07))
    (pad 3 smd rect (at -2.275 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 45 /D8IN) (solder_mask_margin 0.07))
    (pad 4 smd rect (at -1.625 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 44 /D7IN) (solder_mask_margin 0.07))
    (pad 5 smd rect (at -0.975 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 43 /D6IN) (solder_mask_margin 0.07))
    (pad 6 smd rect (at -0.325 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 42 /D5IN) (solder_mask_margin 0.07))
    (pad 7 smd rect (at 0.325 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 41 /D4IN) (solder_mask_margin 0.07))
    (pad 8 smd rect (at 0.975 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 40 /D3IN) (solder_mask_margin 0.07))
    (pad 9 smd rect (at 1.625 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 39 /D2IN) (solder_mask_margin 0.07))
    (pad 10 smd rect (at 2.275 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 /D1IN) (solder_mask_margin 0.07))
    (pad 11 smd rect (at 2.925 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 37 /D0IN) (solder_mask_margin 0.07))
    (pad 12 smd rect (at 3.575 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 75 GND) (solder_mask_margin 0.07))
    (pad 13 smd rect (at 3.575 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 /D0OUT) (solder_mask_margin 0.07))
    (pad 14 smd rect (at 2.925 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /D1OUT) (solder_mask_margin 0.07))
    (pad 15 smd rect (at 2.275 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /D2OUT) (solder_mask_margin 0.07))
    (pad 16 smd rect (at 1.625 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /D3OUT) (solder_mask_margin 0.07))
    (pad 17 smd rect (at 0.975 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /D4OUT) (solder_mask_margin 0.07))
    (pad 18 smd rect (at 0.325 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /D5OUT) (solder_mask_margin 0.07))
    (pad 19 smd rect (at -0.325 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /D6OUT) (solder_mask_margin 0.07))
    (pad 20 smd rect (at -0.975 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /D7OUT) (solder_mask_margin 0.07))
    (pad 21 smd rect (at -1.625 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /D8OUT) (solder_mask_margin 0.07))
    (pad 22 smd rect (at -2.275 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /D9OUT) (solder_mask_margin 0.07))
    (pad 23 smd rect (at -2.925 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 75 GND) (solder_mask_margin 0.07))
    (pad 24 smd rect (at -3.575 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 74 +5) (solder_mask_margin 0.07))
  )
  (module digikey-footprints:TSSOP-24_W4.40mm (layer F.Cu) (tedit 5B50A3FA)
    (at 160.225 139.96 180)
    (descr http://www.ti.com/lit/ds/symlink/tca9548a.pdf)
    (fp_text reference U2 (at -5.129 -3.042 180) (layer F.SilkS))
    (fp_text value SN74CBTD3861PWR (at -2.595 1.53 180) (layer F.Fab) hide)
    (fp_text user %R (at -5.129 -3.042 180) (layer F.Fab))
    (pad 1 smd rect (at -3.575 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U2-Pad1)") (solder_mask_margin 0.07))
    (pad 2 smd rect (at -2.925 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 56 /D19IN) (solder_mask_margin 0.07))
    (pad 3 smd rect (at -2.275 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 55 /D18IN) (solder_mask_margin 0.07))
    (pad 4 smd rect (at -1.625 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 54 /D17IN) (solder_mask_margin 0.07))
    (pad 5 smd rect (at -0.975 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 53 /D16IN) (solder_mask_margin 0.07))
    (pad 6 smd rect (at -0.325 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 52 /D15IN) (solder_mask_margin 0.07))
    (pad 7 smd rect (at 0.325 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 51 /D14IN) (solder_mask_margin 0.07))
    (pad 8 smd rect (at 0.975 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 50 /D13IN) (solder_mask_margin 0.07))
    (pad 9 smd rect (at 1.625 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 49 /D12IN) (solder_mask_margin 0.07))
    (pad 10 smd rect (at 2.275 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 48 /D11IN) (solder_mask_margin 0.07))
    (pad 11 smd rect (at 2.925 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 47 /D10IN) (solder_mask_margin 0.07))
    (pad 12 smd rect (at 3.575 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 75 GND) (solder_mask_margin 0.07))
    (pad 13 smd rect (at 3.575 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /D10OUT) (solder_mask_margin 0.07))
    (pad 14 smd rect (at 2.925 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 /D11OUT) (solder_mask_margin 0.07))
    (pad 15 smd rect (at 2.275 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /D12OUT) (solder_mask_margin 0.07))
    (pad 16 smd rect (at 1.625 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /D13OUT) (solder_mask_margin 0.07))
    (pad 17 smd rect (at 0.975 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /D14OUT) (solder_mask_margin 0.07))
    (pad 18 smd rect (at 0.325 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /D15OUT) (solder_mask_margin 0.07))
    (pad 19 smd rect (at -0.325 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /D16OUT) (solder_mask_margin 0.07))
    (pad 20 smd rect (at -0.975 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 /D17OUT) (solder_mask_margin 0.07))
    (pad 21 smd rect (at -1.625 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 19 /D18OUT) (solder_mask_margin 0.07))
    (pad 22 smd rect (at -2.275 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /D19OUT) (solder_mask_margin 0.07))
    (pad 23 smd rect (at -2.925 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 75 GND) (solder_mask_margin 0.07))
    (pad 24 smd rect (at -3.575 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 74 +5) (solder_mask_margin 0.07))
  )
  (module digikey-footprints:TSSOP-24_W4.40mm (layer F.Cu) (tedit 5B50A410)
    (at 173.105 139.96 180)
    (descr http://www.ti.com/lit/ds/symlink/tca9548a.pdf)
    (fp_text reference U3 (at -5.215 -3.1 180) (layer F.SilkS))
    (fp_text value SN74CBTD3861PWR (at -2.585 1.6 180) (layer F.Fab) hide)
    (fp_text user %R (at -5.195 -3.1 180) (layer F.Fab))
    (pad 1 smd rect (at -3.575 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U3-Pad1)") (solder_mask_margin 0.07))
    (pad 2 smd rect (at -2.925 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 66 /D29IN) (solder_mask_margin 0.07))
    (pad 3 smd rect (at -2.275 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 65 /D28IN) (solder_mask_margin 0.07))
    (pad 4 smd rect (at -1.625 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 64 /D27IN) (solder_mask_margin 0.07))
    (pad 5 smd rect (at -0.975 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 63 /D26IN) (solder_mask_margin 0.07))
    (pad 6 smd rect (at -0.325 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 62 /D25IN) (solder_mask_margin 0.07))
    (pad 7 smd rect (at 0.325 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 61 /D24IN) (solder_mask_margin 0.07))
    (pad 8 smd rect (at 0.975 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 60 /D23IN) (solder_mask_margin 0.07))
    (pad 9 smd rect (at 1.625 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 59 /D22IN) (solder_mask_margin 0.07))
    (pad 10 smd rect (at 2.275 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 58 /D21IN) (solder_mask_margin 0.07))
    (pad 11 smd rect (at 2.925 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 57 /D20IN) (solder_mask_margin 0.07))
    (pad 12 smd rect (at 3.575 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 75 GND) (solder_mask_margin 0.07))
    (pad 13 smd rect (at 3.575 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 21 /D20OUT) (solder_mask_margin 0.07))
    (pad 14 smd rect (at 2.925 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /D21OUT) (solder_mask_margin 0.07))
    (pad 15 smd rect (at 2.275 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 23 /D22OUT) (solder_mask_margin 0.07))
    (pad 16 smd rect (at 1.625 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 24 /D23OUT) (solder_mask_margin 0.07))
    (pad 17 smd rect (at 0.975 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 25 /D24OUT) (solder_mask_margin 0.07))
    (pad 18 smd rect (at 0.325 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 26 /D25OUT) (solder_mask_margin 0.07))
    (pad 19 smd rect (at -0.325 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /D26OUT) (solder_mask_margin 0.07))
    (pad 20 smd rect (at -0.975 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /D27OUT) (solder_mask_margin 0.07))
    (pad 21 smd rect (at -1.625 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 29 /D28OUT) (solder_mask_margin 0.07))
    (pad 22 smd rect (at -2.275 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 30 /D29OUT) (solder_mask_margin 0.07))
    (pad 23 smd rect (at -2.925 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 75 GND) (solder_mask_margin 0.07))
    (pad 24 smd rect (at -3.575 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 74 +5) (solder_mask_margin 0.07))
  )
  (module digikey-footprints:TSSOP-24_W4.40mm (layer F.Cu) (tedit 5B50A431)
    (at 185.147 139.96 180)
    (descr http://www.ti.com/lit/ds/symlink/tca9548a.pdf)
    (fp_text reference U4 (at -5.099 -3.042 180) (layer F.SilkS))
    (fp_text value SN74CBTD3861PWR (at -2.685 1.49 180) (layer F.Fab) hide)
    (fp_text user %R (at -5.099 -3.042 180) (layer F.Fab))
    (pad 1 smd rect (at -3.575 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U4-Pad1)") (solder_mask_margin 0.07))
    (pad 2 smd rect (at -2.925 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(U4-Pad2)") (solder_mask_margin 0.07))
    (pad 3 smd rect (at -2.275 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U4-Pad3)") (solder_mask_margin 0.07))
    (pad 4 smd rect (at -1.625 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 72 /D35IN) (solder_mask_margin 0.07))
    (pad 5 smd rect (at -0.975 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 71 /D34IN) (solder_mask_margin 0.07))
    (pad 6 smd rect (at -0.325 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 70 /D33IN) (solder_mask_margin 0.07))
    (pad 7 smd rect (at 0.325 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 69 /D32IN) (solder_mask_margin 0.07))
    (pad 8 smd rect (at 0.975 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 68 /D31IN) (solder_mask_margin 0.07))
    (pad 9 smd rect (at 1.625 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 67 /D30IN) (solder_mask_margin 0.07))
    (pad 10 smd rect (at 2.275 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(U4-Pad10)") (solder_mask_margin 0.07))
    (pad 11 smd rect (at 2.925 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(U4-Pad11)") (solder_mask_margin 0.07))
    (pad 12 smd rect (at 3.575 2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 75 GND) (solder_mask_margin 0.07))
    (pad 13 smd rect (at 3.575 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(U4-Pad13)") (solder_mask_margin 0.07))
    (pad 14 smd rect (at 2.925 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(U4-Pad14)") (solder_mask_margin 0.07))
    (pad 15 smd rect (at 2.275 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 31 /D30OUT) (solder_mask_margin 0.07))
    (pad 16 smd rect (at 1.625 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 32 /D31OUT) (solder_mask_margin 0.07))
    (pad 17 smd rect (at 0.975 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 33 /D32OUT) (solder_mask_margin 0.07))
    (pad 18 smd rect (at 0.325 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 34 /D33OUT) (solder_mask_margin 0.07))
    (pad 19 smd rect (at -0.325 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 35 /D34OUT) (solder_mask_margin 0.07))
    (pad 20 smd rect (at -0.975 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 36 /D35OUT) (solder_mask_margin 0.07))
    (pad 21 smd rect (at -1.625 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(U4-Pad21)") (solder_mask_margin 0.07))
    (pad 22 smd rect (at -2.275 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(U4-Pad22)") (solder_mask_margin 0.07))
    (pad 23 smd rect (at -2.925 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 75 GND) (solder_mask_margin 0.07))
    (pad 24 smd rect (at -3.575 -2.8 180) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 74 +5) (solder_mask_margin 0.07))
  )
  (module pads:via-3mm (layer F.Cu) (tedit 5B50AD61)
    (at 167 136.75)
    (zone_connect 2)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 75 GND) (zone_connect 2))
  )
  (gr_line (start 192.5 151.9) (end 140 151.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140 127.5) (end 192.5 127.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 192.5 151.9) (end 192.5 127.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140 127.5) (end 140 151.9) (layer Edge.Cuts) (width 0.15))
  (zone (net 75) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140 127.5) (xy 192.5 127.5) (xy 192.5 152) (xy 140 152)
      )
    )
  )
  (zone (net 75) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140 127.5) (xy 192.5 127.5) (xy 192.5 152) (xy 140 152)
      )
    )
  )
)
