(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 76)
    (no_connects 0)
    (area 129.083999 61.5212 155.726551 83.3604)
    (thickness 1.6)
    (drawings 21)
    (tracks 304)
    (zones 0)
    (modules 36)
    (nets 22)
  )
  (page A4)
  (title_block
    (title pwrup1000)
    (date 2017-05-31)
    (rev 0.01)
    (company "1rel interactive")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (trace_clearance 0.15)
    (zone_clearance 0.3)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.1)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory OUT/svg/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3.3V)
  (net 3 "Net-(D1-Pad1)")
  (net 4 "Net-(D2-Pad1)")
  (net 5 "Net-(D3-Pad1)")
  (net 6 "Net-(D4-Pad1)")
  (net 7 "Net-(L1-Pad2)")
  (net 8 "Net-(L1-Pad1)")
  (net 9 /VBAT)
  (net 10 /CHG_OUT)
  (net 11 /CHG_IN)
  (net 12 /~PGOOD)
  (net 13 /STAT2)
  (net 14 /STAT1)
  (net 15 /BOOST_ENABLE)
  (net 16 /VPCC)
  (net 17 /PROG1)
  (net 18 /PROG3)
  (net 19 /THERM)
  (net 20 /VINA)
  (net 21 /BOOST_PS/SYNC)
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /BOOST_ENABLE)
    (add_net /BOOST_PS/SYNC)
    (add_net /PROG1)
    (add_net /PROG3)
    (add_net /STAT1)
    (add_net /STAT2)
    (add_net /THERM)
    (add_net /VPCC)
    (add_net /~PGOOD)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(L1-Pad2)")
  )
  (net_class PWR ""
    (clearance 0.15)
    (trace_width 0.7)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3.3V)
    (add_net /CHG_IN)
    (add_net /CHG_OUT)
    (add_net /VBAT)
    (add_net /VINA)
    (add_net GND)
  )
  (module mylib:jmp3 (layer F.Cu) (tedit 599185F6)
    (at 152.8445 73.279 90)
    (fp_text reference P11 (at -0.0254 1.1176 90) (layer F.SilkS) hide)
    (fp_text value jmp3 (at -0.1524 -1.3716 90) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.508 0 90) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask)
      (net 20 /VINA))
    (pad 2 smd rect (at 0 0 90) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 /BOOST_PS/SYNC))
    (pad 1 smd rect (at -0.508 0 90) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 5991870C)
    (at 151.765 76.581 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R11 (at -1.5875 0.127 270) (layer F.SilkS))
    (fp_text value 100k (at 0 0.7 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 20 /VINA))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 15 /BOOST_ENABLE))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 59918C22)
    (at 153.416 68.2752)
    (descr "SMT resistor, 0402")
    (fp_text reference R10 (at 1.524 -0.0762 90) (layer F.SilkS))
    (fp_text value 1k5 (at 0 0.7) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 +3.3V))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:pin_socket_1m (layer F.Cu) (tedit 58441945)
    (at 132.08 66.04)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P10 (at 0 -2.159) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module mylib:pin_socket_1m (layer F.Cu) (tedit 58441945)
    (at 149.86 78.74)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P9 (at 0 -2.159) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module mylib:pin_socket_1m (layer F.Cu) (tedit 58441945)
    (at 152.4 78.74)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P8 (at 0 -2.159) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 15 /BOOST_ENABLE))
  )
  (module mylib:pin_socket_1m (layer F.Cu) (tedit 58441945)
    (at 149.86 66.04 180)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P7 (at 0 -2.159 180) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module mylib:pin_socket_1m (layer F.Cu) (tedit 58441945)
    (at 152.4 66.04 180)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P6 (at 0 -2.159 180) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 +3.3V))
  )
  (module mylib:1pin (layer F.Cu) (tedit 592EF84A)
    (at 139.8905 69.6595 90)
    (fp_text reference P5 (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 12 /~PGOOD))
  )
  (module mylib:1pin (layer F.Cu) (tedit 592EF84A)
    (at 138.43 69.6595 90)
    (fp_text reference P4 (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 13 /STAT2))
  )
  (module mylib:MCP73871 (layer F.Cu) (tedit 5990E93E)
    (at 137.801 73.703 180)
    (fp_text reference U2 (at -2.915 -1.989 270) (layer F.SilkS))
    (fp_text value MCP73871 (at 0.25 0.25 180) (layer F.Fab) hide)
    (pad 21 thru_hole rect (at 0.55 0.55 180) (size 1.1 1.1) (drill 0.3) (layers *.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 21 thru_hole rect (at 0.55 -0.55 180) (size 1.1 1.1) (drill 0.3) (layers *.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 21 thru_hole rect (at -0.55 -0.55 180) (size 1.1 1.1) (drill 0.3) (layers *.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 20 smd rect (at -1 -2 180) (size 0.28 0.73) (layers F.Cu F.Paste F.Mask)
      (net 10 /CHG_OUT))
    (pad 19 smd rect (at -0.5 -2 180) (size 0.28 0.73) (layers F.Cu F.Paste F.Mask)
      (net 11 /CHG_IN))
    (pad 17 smd rect (at 0.5 -2 180) (size 0.28 0.73) (layers F.Cu F.Paste F.Mask)
      (net 11 /CHG_IN))
    (pad 18 smd rect (at 0 -2 180) (size 0.28 0.73) (layers F.Cu F.Paste F.Mask)
      (net 11 /CHG_IN))
    (pad 16 smd rect (at 1 -2 180) (size 0.28 0.73) (layers F.Cu F.Paste F.Mask)
      (net 9 /VBAT))
    (pad 15 smd rect (at 2 -1 270) (size 0.28 0.73) (layers F.Cu F.Paste F.Mask)
      (net 9 /VBAT))
    (pad 13 smd rect (at 2 0 270) (size 0.28 0.73) (layers F.Cu F.Paste F.Mask)
      (net 17 /PROG1))
    (pad 14 smd rect (at 2 -0.5 270) (size 0.28 0.73) (layers F.Cu F.Paste F.Mask)
      (net 9 /VBAT))
    (pad 12 smd rect (at 2 0.5 270) (size 0.28 0.73) (layers F.Cu F.Paste F.Mask)
      (net 18 /PROG3))
    (pad 11 smd rect (at 2 1 270) (size 0.28 0.73) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -2 1 270) (size 0.28 0.73) (layers F.Cu F.Paste F.Mask)
      (net 19 /THERM))
    (pad 4 smd rect (at -2 0.5 270) (size 0.28 0.73) (layers F.Cu F.Paste F.Mask)
      (net 11 /CHG_IN))
    (pad 2 smd rect (at -2 -0.5 270) (size 0.28 0.73) (layers F.Cu F.Paste F.Mask)
      (net 16 /VPCC))
    (pad 3 smd rect (at -2 0 270) (size 0.28 0.73) (layers F.Cu F.Paste F.Mask)
      (net 11 /CHG_IN))
    (pad 1 smd rect (at -2 -1 270) (size 0.28 0.73) (layers F.Cu F.Paste F.Mask)
      (net 10 /CHG_OUT))
    (pad 10 smd rect (at 1 2 180) (size 0.28 0.73) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 0 2 180) (size 0.28 0.73) (layers F.Cu F.Paste F.Mask)
      (net 14 /STAT1))
    (pad 9 smd rect (at 0.5 2 180) (size 0.28 0.73) (layers F.Cu F.Paste F.Mask)
      (net 11 /CHG_IN))
    (pad 7 smd rect (at -0.5 2 180) (size 0.28 0.73) (layers F.Cu F.Paste F.Mask)
      (net 13 /STAT2))
    (pad 6 smd rect (at -1 2 180) (size 0.28 0.73) (layers F.Cu F.Paste F.Mask)
      (net 12 /~PGOOD))
    (pad 21 thru_hole rect (at -0.55 0.55 180) (size 1.1 1.1) (drill 0.3) (layers *.Cu F.Paste F.Mask)
      (net 1 GND))
    (model 1rel/MCP73871.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:1pin (layer F.Cu) (tedit 592EF84A)
    (at 136.9695 69.6595)
    (fp_text reference P3 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 14 /STAT1))
  )
  (module mylib:c_0603_mod0 (layer F.Cu) (tedit 59918C26)
    (at 150.495 68.326)
    (descr "SMT capacitor, 0603")
    (fp_text reference C6 (at -1.905 0 90) (layer F.SilkS))
    (fp_text value 10u (at 0 0.85) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 2 +3.3V))
    (pad 2 smd rect (at -0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0402_mod0 (layer F.Cu) (tedit 59918C45)
    (at 153.797 72.517 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference C2 (at 0 -1.143 450) (layer F.SilkS))
    (fp_text value 100n (at 0 0.6 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 20 /VINA))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0603_mod0 (layer F.Cu) (tedit 59918710)
    (at 147.447 76.962 90)
    (descr "SMT capacitor, 0603")
    (fp_text reference C1 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 10u (at 0 0.85 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 90) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 10 /CHG_OUT))
    (pad 2 smd rect (at -0.75184 0 90) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 5990E60A)
    (at 142.24 72.263)
    (descr "SMT resistor, 0402")
    (fp_text reference R9 (at 0 -1.143) (layer F.SilkS))
    (fp_text value 10k (at 0 0.7) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 19 /THERM))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 59918C54)
    (at 143.383 74.168 90)
    (descr "SMT resistor, 0402")
    (fp_text reference R8 (at -1.651 0 180) (layer F.SilkS))
    (fp_text value 100k (at 0 0.7 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 16 /VPCC))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 59918C5C)
    (at 133.985 72.771 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R7 (at 1.778 0 180) (layer F.SilkS))
    (fp_text value 100k (at 0 0.7 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 18 /PROG3))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 59918C5E)
    (at 133.985 74.041 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R6 (at 1.778 0 360) (layer F.SilkS))
    (fp_text value 1k (at 0 0.7 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 17 /PROG1))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 5991874A)
    (at 139.827 65.659 270)
    (descr "SMT resistor, 0402")
    (fp_text reference R2 (at -0.127 -2.9845 450) (layer F.SilkS))
    (fp_text value 1k5 (at 0 0.7 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 11 /CHG_IN))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 59918C56)
    (at 142.24 74.168 270)
    (descr "SMT resistor, 0402")
    (fp_text reference R5 (at 1.651 0 360) (layer F.SilkS))
    (fp_text value 270k (at 0 0.7 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 16 /VPCC))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 11 /CHG_IN))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 59918732)
    (at 137.033 65.659 270)
    (descr "SMT resistor, 0402")
    (fp_text reference R4 (at -0.127 -4.2545 450) (layer F.SilkS))
    (fp_text value 1k5 (at 0 0.7 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 11 /CHG_IN))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 5991873C)
    (at 138.43 65.659 270)
    (descr "SMT resistor, 0402")
    (fp_text reference R3 (at -0.127 -3.6195 450) (layer F.SilkS))
    (fp_text value 1k5 (at 0 0.7 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 11 /CHG_IN))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 59918708)
    (at 150.622 75.184 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R1 (at 1.524 0 450) (layer F.SilkS))
    (fp_text value 100R (at 0 0.7 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 10 /CHG_OUT))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 20 /VINA))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0603_mod0 (layer F.Cu) (tedit 59918C27)
    (at 150.495 69.596)
    (descr "SMT capacitor, 0603")
    (fp_text reference C5 (at -1.905 0 90) (layer F.SilkS))
    (fp_text value 10u (at 0 0.85) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 2 +3.3V))
    (pad 2 smd rect (at -0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0603_mod0 (layer F.Cu) (tedit 5990E678)
    (at 136.144 76.835)
    (descr "SMT capacitor, 0603")
    (fp_text reference C3 (at -1.524 -1.016 180) (layer F.SilkS))
    (fp_text value 10u (at 0 0.85) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 11 /CHG_IN))
    (pad 2 smd rect (at -0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:pin_socket_1m (layer F.Cu) (tedit 58441945)
    (at 142.24 78.74 180)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P2 (at 0 -2.159 180) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module mylib:pin_socket_1m (layer F.Cu) (tedit 58441945)
    (at 139.7 78.74 180)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P1 (at 0 -2.159 180) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 11 /CHG_IN))
  )
  (module mylib:pin_socket_2m (layer F.Cu) (tedit 58441928)
    (at 133.35 78.74 180)
    (descr "Pin socket 2pin")
    (tags "CONN DEV")
    (fp_text reference BT1 (at 0 -2.159 180) (layer F.SilkS) hide)
    (fp_text value BATTERYm0 (at 0.254 -3.556 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 0 180) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 9 /VBAT))
  )
  (module mylib:c_0603_mod0 (layer F.Cu) (tedit 59910439)
    (at 133.35 76.835 180)
    (descr "SMT capacitor, 0603")
    (fp_text reference C4 (at 1.778 0.127 270) (layer F.SilkS))
    (fp_text value 10u (at 0 0.85 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 9 /VBAT))
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:TPS63001 (layer F.Cu) (tedit 5990E342)
    (at 150.495 72.771)
    (fp_text reference U1 (at 1.397 -1.905 180) (layer F.SilkS))
    (fp_text value TPS63001 (at 0.2 1.8) (layer F.Fab) hide)
    (pad 11 thru_hole rect (at 0.3875 0.55 90) (size 1.1 0.775) (drill 0.3) (layers *.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 thru_hole rect (at 0.3875 -0.55 90) (size 1.1 0.775) (drill 0.3) (layers *.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 thru_hole rect (at -0.3875 -0.55 90) (size 1.1 0.775) (drill 0.3) (layers *.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.379 0 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -1.379 0.5 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(L1-Pad1)"))
    (pad 2 smd rect (at -1.379 -0.5 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(L1-Pad2)"))
    (pad 5 smd rect (at -1.379 1 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 10 /CHG_OUT))
    (pad 1 smd rect (at -1.379 -1 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 2 +3.3V))
    (pad 10 smd rect (at 1.371 -1 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 2 +3.3V))
    (pad 6 smd rect (at 1.371 1 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 15 /BOOST_ENABLE))
    (pad 9 smd rect (at 1.371 -0.5 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 1.371 0.5 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 21 /BOOST_PS/SYNC))
    (pad 8 smd rect (at 1.371 0 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 20 /VINA))
    (pad 11 thru_hole rect (at -0.3875 0.545 90) (size 1.1 0.775) (drill 0.3) (layers *.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_qfn/dfn10_3x3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:Led_0603_mod0 (layer F.Cu) (tedit 59918747)
    (at 139.827 67.945 270)
    (descr "SMD LED, 0603")
    (fp_text reference D1 (at 0.635 -2.9845 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.19888 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 12 /~PGOOD))
    (model walter/smd_leds/led_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:Led_0603_mod0 (layer F.Cu) (tedit 59918742)
    (at 138.43 67.945 270)
    (descr "SMD LED, 0603")
    (fp_text reference D2 (at 0.635 -3.6195 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.19888 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 13 /STAT2))
    (model walter/smd_leds/led_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:Led_0603_mod0 (layer F.Cu) (tedit 59918C48)
    (at 153.797 69.723 180)
    (descr "SMD LED, 0603")
    (fp_text reference D4 (at 0 -1.143 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.19888 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_leds/led_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:Led_0603_mod0 (layer F.Cu) (tedit 59918751)
    (at 137.033 67.945 270)
    (descr "SMD LED, 0603")
    (fp_text reference D3 (at 0.635 -4.191 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.19888 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 14 /STAT1))
    (model walter/smd_leds/led_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:inductor_smd_NR3015 (layer F.Cu) (tedit 59918B53)
    (at 146.558 72.771 90)
    (descr "Inductor SMD, 1008")
    (fp_text reference L1 (at -2.54 -1.143 180) (layer F.SilkS))
    (fp_text value 2u2 (at 2.375 0.375 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.2 0 90) (size 1.3 2.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(L1-Pad1)"))
    (pad 2 smd rect (at 1.2 0 90) (size 1.3 2.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(L1-Pad2)"))
    (model walter/smd_inductors/inductor_smd_1008.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 153.3398 81.407) (end 131.4704 81.407) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.6512 65.6844) (end 155.6512 79.0956) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.4704 63.373) (end 153.3398 63.373) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.159 65.6844) (end 129.159 79.0956) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 153.34015 79.0956) (end 155.65155 79.0956) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text GND (at 130.556 66.04 90) (layer F.SilkS))
  (gr_text GND (at 148.463 78.74 90) (layer F.SilkS))
  (gr_text "pwrup1000\nrev0.01\nrel/2017-08" (at 144.8816 76.6572 270) (layer B.SilkS))
  (gr_text 3V3 (at 154.051 66.04 90) (layer F.SilkS))
  (gr_arc (start 131.4704 79.0956) (end 131.4704 81.407) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 153.34015 65.6844) (end 153.34015 63.373) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 131.4704 65.6844) (end 129.159 65.6844) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text STAT2 (at 138.43 68.58 180) (layer B.SilkS))
  (gr_text STAT1 (at 137.033 70.866 180) (layer B.SilkS))
  (gr_text VBAT (at 130.556 78.74 90) (layer F.SilkS))
  (gr_text GND (at 143.891 78.74 90) (layer F.SilkS))
  (gr_text GND (at 148.336 66.04 90) (layer F.SilkS))
  (gr_text EN (at 154.051 78.74 90) (layer F.SilkS))
  (gr_text PGOOD (at 139.827 70.866) (layer B.SilkS))
  (gr_text VIN (at 136.271 78.74 90) (layer F.SilkS))
  (gr_text CHG (at 138.049 78.74 90) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.4)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.8))
    (polygon
      (pts
        (xy 155.6639 81.412) (xy 129.159 81.412) (xy 129.159 63.373) (xy 155.6639 63.373)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.4)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.8))
    (polygon
      (pts
        (xy 155.6639 81.412) (xy 129.159 81.412) (xy 129.159 63.373) (xy 155.6639 63.373)
      )
    )
  )
)
