(kicad_pcb (version 20171130) (host pcbnew 5.1.10-88a1d61d58~88~ubuntu20.04.1)
  (general
    (thickness 1.6002)
    (drawings 11)
    (tracks 334)
    (zones 0)
    (modules 13)
    (nets 10)
  )
  (page USLetter)
  (title_block
    (rev 1)
  )
  (layers
    (0 Front signal)
    (1 In1.Cu signal hide)
    (2 In2.Cu signal hide)
    (31 Back signal hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (44 Edge.Cuts user hide)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.508)
    (user_trace_width 0.127)
    (user_trace_width 0.254)
    (user_trace_width 0.3429)
    (user_trace_width 0.508)
    (user_trace_width 1.016)
    (trace_clearance 0.127)
    (zone_clearance 0.15)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.4572)
    (via_drill 0.254)
    (via_min_size 0.4572)
    (via_min_drill 0.254)
    (user_via 0.4572 0.254)
    (user_via 0.889 0.381)
    (uvia_size 0.4572)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.0381)
    (segment_width 0.254)
    (pcb_text_width 0.3048)
    (pcb_text_size 1.524 1.524)
    (mod_edge_width 0.127)
    (mod_text_size 0.762 0.762)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0381)
    (aux_axis_origin 0 0)
    (visible_elements FEFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.152400)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./gerbers"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /v3p3)
  (net 3 "Net-(C4-Pad1)")
  (net 4 /EN)
  (net 5 /LO_ac)
  (net 6 /LO)
  (net 7 /VIN)
  (net 8 /RF)
  (net 9 /IF)
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.4572)
    (uvia_drill 0.254)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
    (add_net /EN)
    (add_net /IF)
    (add_net /LO)
    (add_net /LO_ac)
    (add_net /RF)
    (add_net /VIN)
    (add_net /v3p3)
    (add_net GND)
    (add_net "Net-(C4-Pad1)")
  )
  (module rz:sma_psf-s01_oshpark4layer locked (layer Front) (tedit 60E49AFD)
    (at 34.5 5.875 180)
    (descr "Connector SMA, 0Hz to 20GHz, 50Ohm, Edge Mount (http://suddendocs.samtec.com/prints/sma-j-p-x-st-em1-mkt.pdf)")
    (tags "SMA Straight Samtec Edge Mount")
    (attr smd)
    (fp_text reference J3 (at 3.225 -1.85 180) (layer F.SilkS) hide)
    (fp_text value sma_psf-s01 (at -10.968 0 270) (layer F.Fab))
    (fp_text user "PCB Edge" (at -0.568 0 270) (layer Dwgs.User))
    (fp_text user %R (at -2.758 0 90) (layer F.Fab))
    (pad 1 smd trapezoid (at 1 0 90) (size 0.4 1) (rect_delta 0 0.05 ) (layers Front)
      (net 9 /IF))
    (pad 2 smd rect (at 2 3.5 90) (size 3 4) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 -3.5 90) (size 3 4) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 3.5 90) (size 3 4) (layers Back B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 -3.5 90) (size 3 4) (layers Back B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Samtec_SMA-J-P-X-ST-EM1_EdgeMount.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module rz:sma_psf-s01_oshpark4layer locked (layer Front) (tedit 60E49AFD)
    (at 25 11.5 90)
    (descr "Connector SMA, 0Hz to 20GHz, 50Ohm, Edge Mount (http://suddendocs.samtec.com/prints/sma-j-p-x-st-em1-mkt.pdf)")
    (tags "SMA Straight Samtec Edge Mount")
    (attr smd)
    (fp_text reference J2 (at 2.9 -1.75) (layer F.SilkS) hide)
    (fp_text value sma_psf-s01 (at -10.968 0 180) (layer F.Fab))
    (fp_text user "PCB Edge" (at -0.568 0 180) (layer Dwgs.User))
    (fp_text user %R (at -2.758 0) (layer F.Fab))
    (pad 1 smd trapezoid (at 1 0) (size 0.4 1) (rect_delta 0 0.05 ) (layers Front)
      (net 5 /LO_ac))
    (pad 2 smd rect (at 2 3.5) (size 3 4) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 -3.5) (size 3 4) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 3.5) (size 3 4) (layers Back B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 -3.5) (size 3 4) (layers Back B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Samtec_SMA-J-P-X-ST-EM1_EdgeMount.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module rz:sma_psf-s01_oshpark4layer locked (layer Front) (tedit 60E49AFD)
    (at 25 0.5 270)
    (descr "Connector SMA, 0Hz to 20GHz, 50Ohm, Edge Mount (http://suddendocs.samtec.com/prints/sma-j-p-x-st-em1-mkt.pdf)")
    (tags "SMA Straight Samtec Edge Mount")
    (attr smd)
    (fp_text reference J1 (at 3.075 -1.625 270) (layer F.SilkS) hide)
    (fp_text value sma_psf-s01 (at -10.968 0 180) (layer F.Fab))
    (fp_text user "PCB Edge" (at -0.568 0 180) (layer Dwgs.User))
    (fp_text user %R (at -2.758 0) (layer F.Fab))
    (pad 1 smd trapezoid (at 1 0 180) (size 0.4 1) (rect_delta 0 0.05 ) (layers Front)
      (net 8 /RF))
    (pad 2 smd rect (at 2 3.5 180) (size 3 4) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 -3.5 180) (size 3 4) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 3.5 180) (size 3 4) (layers Back B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 -3.5 180) (size 3 4) (layers Back B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Samtec_SMA-J-P-X-ST-EM1_EdgeMount.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module rz:LTC5553IUDB-TRMPBF locked (layer Front) (tedit 60E485FD)
    (at 25 5.875 180)
    (fp_text reference U1 (at 2.2 2.15) (layer F.SilkS) hide)
    (fp_text value LTC5553IUDB-TRMPBF (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (fp_text user * (at -2.45 -1.425) (layer F.SilkS))
    (fp_text user * (at -2.45 -1.425) (layer F.SilkS))
    (pad 13 smd rect (at 0 -0.127 270) (size 0.3 0.85) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd oval (at -1.4478 -0.499999 270) (size 0.254 0.8128) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd oval (at -1.4478 0 270) (size 0.254 0.8128) (layers Front F.Paste F.Mask)
      (net 9 /IF))
    (pad 3 smd oval (at -1.4478 0.499999 270) (size 0.254 0.8128) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd oval (at -0.499999 0.9525 180) (size 0.254 0.8128) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd oval (at 0 0.9525 180) (size 0.254 0.8128) (layers Front F.Paste F.Mask)
      (net 8 /RF))
    (pad 6 smd oval (at 0.499999 0.9525 180) (size 0.254 0.8128) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd oval (at 1.4478 0.499999 270) (size 0.254 0.8128) (layers Front F.Paste F.Mask)
      (net 4 /EN))
    (pad 8 smd oval (at 1.4478 0 270) (size 0.254 0.8128) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd oval (at 1.4478 -0.499999 270) (size 0.254 0.8128) (layers Front F.Paste F.Mask)
      (net 2 /v3p3))
    (pad 10 smd oval (at 0.499999 -0.9525 180) (size 0.254 0.8128) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd oval (at 0 -0.9525 180) (size 0.254 0.8128) (layers Front F.Paste F.Mask)
      (net 6 /LO))
    (pad 12 smd oval (at -0.499999 -0.9525 180) (size 0.254 0.8128) (layers Front F.Paste F.Mask)
      (net 1 GND))
  )
  (module Package_TO_SOT_SMD:SOT-223-3_TabPin2 (layer Front) (tedit 5A02FF57)
    (at 11.725 6.025 270)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 3.3 -2.9 90) (layer F.SilkS))
    (fp_text value LD1117S33TR_SOT223 (at 0 4.5 90) (layer F.Fab))
    (fp_text user %R (at 0.381 0) (layer F.Fab))
    (pad 1 smd rect (at -3.15 -2.3 270) (size 2 1.5) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -3.15 2.3 270) (size 2 1.5) (layers Front F.Paste F.Mask)
      (net 3 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at -3.15 0 270) (size 2 1.5) (layers Front F.Paste F.Mask)
      (net 2 /v3p3))
    (pad 2 smd rect (at 3.15 0 270) (size 2 3.8) (layers Front F.Paste F.Mask)
      (net 2 /v3p3))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder locked (layer Front) (tedit 5F68FEEE)
    (at 16.7005 9.398 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 1.527 2.5005 180) (layer F.SilkS))
    (fp_text value "jumper 0805" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0.13 -0.351 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 4 /EN))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 2 /v3p3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical locked (layer Front) (tedit 59FED5CC)
    (at 2.05 2.175)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J4 (at 3.1 8.8 180) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /EN))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /v3p3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VIN))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 locked (layer Front) (tedit 58645DC7)
    (at 6.075 8 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 0 -2 90) (layer F.SilkS))
    (fp_text value MBR0520 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers Front F.Paste F.Mask)
      (net 7 /VIN))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers Front F.Paste F.Mask)
      (net 3 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-3528-12_Kemet-T_Pad1.50x2.35mm_HandSolder locked (layer Front) (tedit 5EBA9318)
    (at 17.399 4.445 90)
    (descr "Tantalum Capacitor SMD Kemet-T (3528-12 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C5 (at 3.27 -1.374 180) (layer F.SilkS))
    (fp_text value cap_tant_10uF_16V_1411_ECST1CX106R (at 0 2.35 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.625 0 90) (size 1.5 2.35) (layers Front F.Paste F.Mask) (roundrect_rratio 0.166667)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.625 0 90) (size 1.5 2.35) (layers Front F.Paste F.Mask) (roundrect_rratio 0.166667)
      (net 2 /v3p3))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3528-12_Kemet-T.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-3528-12_Kemet-T_Pad1.50x2.35mm_HandSolder locked (layer Front) (tedit 5EBA9318)
    (at 6.1 3 90)
    (descr "Tantalum Capacitor SMD Kemet-T (3528-12 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C4 (at 1.8 2.575) (layer F.SilkS))
    (fp_text value cap_tant_10uF_16V_1411_ECST1CX106R (at 0 2.35 90) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.625 0 90) (size 1.5 2.35) (layers Front F.Paste F.Mask) (roundrect_rratio 0.166667)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.625 0 90) (size 1.5 2.35) (layers Front F.Paste F.Mask) (roundrect_rratio 0.166667)
      (net 3 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3528-12_Kemet-T.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder locked (layer Front) (tedit 5F68FEEE)
    (at 19 9.3 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference C3 (at -2.8845 -1.1655 270) (layer F.SilkS))
    (fp_text value cap_1uf_x7r_16v_0603_CL10B105MO8NNWC‎ (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /v3p3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder locked (layer Front) (tedit 5F6BB9E0)
    (at 22.5 7.225 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference C2 (at -1.125 1.2 90) (layer F.SilkS))
    (fp_text value cap_18pf_c0g_50v_0402_GJM1555C1H180FB01 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5975 0 270) (size 0.715 0.64) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5975 0 270) (size 0.715 0.64) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /v3p3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module rz:C_0201_oshpark4layer_gcpw locked (layer Front) (tedit 60E44304)
    (at 25 8.6 270)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -0.05 -1.8 180) (layer F.SilkS) hide)
    (fp_text value cap_33pf_c0g_25v_250R05L330GV4T (at 0 1.05 90) (layer F.Fab))
    (fp_text user %R (at 0 -0.68 90) (layer F.Fab))
    (pad 2 smd rect (at 0.32 0 270) (size 0.46 0.35) (layers Front F.Mask)
      (net 5 /LO_ac))
    (pad 1 smd rect (at -0.32 0 270) (size 0.46 0.35) (layers Front F.Mask)
      (net 6 /LO))
    (pad "" smd roundrect (at 0.345 0 270) (size 0.318 0.31) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 270) (size 0.318 0.31) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "EN  3v3  5v GND" (at 3.875 6.075 270) (layer B.SilkS))
  (gr_text "EN  3v3  5v GND" (at 3.95 6.075 90) (layer F.SilkS))
  (gr_text "LTC5553 Mixer 3G-20G -6-+6dbm" (at 16.275 5.95) (layer B.SilkS))
  (gr_text RF (at 19 1.175) (layer F.SilkS))
  (gr_line (start 0 12) (end 0 0) (layer Edge.Cuts) (width 0.0381))
  (gr_line (start 35 12) (end 0 12) (layer Edge.Cuts) (width 0.0381))
  (gr_line (start 35 0) (end 35 12) (layer Edge.Cuts) (width 0.0381))
  (gr_line (start 0 0) (end 35 0) (layer Edge.Cuts) (width 0.0381))
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.254))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 34.5 11.5) (xy 0.5 11.5) (xy 0.5 0.5) (xy 34.5 0.5)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Back) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.254))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 34.5 11.5) (xy 0.5 11.5) (xy 0.5 0.5) (xy 34.5 0.5)
      )
    )
  )
  (zone (net 2) (net_name /v3p3) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.254))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 34.5 11.5) (xy 0.5 11.5) (xy 0.5 0.5) (xy 34.5 0.5)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.15))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 34.5 11.5) (xy 3.4 11.5) (xy 3.4 3.65) (xy 0.5 3.65) (xy 0.5 0.5)
        (xy 34.5 0.5)
      )
    )
  )
  (zone (net 2) (net_name /v3p3) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads thru_hole_only (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.425 3.85) (xy 12.8 4.625) (xy 18.65 4.625) (xy 18.6 7.325) (xy 18.025 7.925)
        (xy 18 9.125) (xy 13.65 10.175) (xy 9.8 10.175) (xy 9.775 5.275) (xy 11 3.825)
      )
    )
  )
  (zone (net 2) (net_name /v3p3) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads thru_hole_only (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23.175 6.35) (xy 23.175 6.725) (xy 23.2875 7.15) (xy 21.6 7.15) (xy 21.6 6.15)
        (xy 22.7875 6.15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.518588 11.5) (xy 23.468588 11.5) (xy 23.45 7.45) (xy 26.5 7.45)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23.481412 0.5) (xy 26.531412 0.5) (xy 26.55 4.325) (xy 23.5 4.325)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34.5 4.356412) (xy 34.5 7.406412) (xy 30.375 6.825) (xy 30.4 4.875)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.425 4.875) (xy 30.425 6.8125) (xy 27.075 6.8) (xy 27.075 4.875)
      )
    )
  )
)
