<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="54.59" y2="0" width="0" layer="20"/>
<wire x1="54.59" y1="0" x2="54.59" y2="59.36" width="0" layer="20"/>
<wire x1="54.59" y1="59.36" x2="0" y2="59.36" width="0" layer="20"/>
<wire x1="0" y1="59.36" x2="0" y2="0" width="0" layer="20"/>
<text>Joystick Module - V 1.1
CARRT/Ramy</text>
<hole x="52.07" y="2.54" drill="2.54"/>
<hole x="48.26" y="57.15" drill="2.54"/>
<hole x="1.27" y="1.27" drill="2.54"/>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="DCJACK_2MM_PTH">
<description>DJ Jack 2.0mm PTH Right-Angle</description>
</package>
<package name="0309/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 10mm</description>
</package>
<package name="C050-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.4 x 4.4 mm</description>
</package>
</packages>
</library>
<library name="con-lsta">
<description>&lt;b&gt;Female Headers etc.&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
FE = female&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="FE06">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-IC-Microcontroller">
<description>&lt;h3&gt;SparkFun Microcontrollers&lt;/h3&gt;
This library contains microcontrollers.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIP28">
<description>Standard 28-pin DIP package.&lt;br&gt;
IC needs to have legs bent before insertion.</description>
</package>
</packages>
</library>
<library name="SparkFun-Clocks">
<description>&lt;h3&gt;SparkFun Clocks, Oscillators and Resonators&lt;/h3&gt;
This library contains the real-time clocks, oscillators, resonators, and crystals we use. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="HC49US">
<description>&lt;h3&gt;HC49/US 11.6x4.6mm PTH Crystal&lt;/h3&gt;
&lt;p&gt;&lt;a href="https://www.digikey.com/Web%20Export/Supplier%20Content/Citizen_300/PDF/Citizen_HC49US.pdf?redirected=1"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SamacSys_Parts">
<description>&lt;b&gt;https://componentsearchengine.com&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="G5V-2">
<description>&lt;b&gt;G5V-2&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA04-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="MA05-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C6" library="adafruit" package="C025-024X044" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="adafruit" package="C025-024X044" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="adafruit" package="C025-024X044" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="adafruit" package="C025-024X044" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN1" library="adafruit" package="DCJACK_2MM_PTH" value="">
<attribute name="VALUE"/>
</element>
<element name="SV1" library="con-lsta" package="FE06" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="transistor" package="TO92" value="2N3904">
<attribute name="NAME"/>
</element>
<element name="U1" library="SparkFun-IC-Microcontroller" package="DIP28" value="328P">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-09136"/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="SparkFun-Clocks" package="HC49US" value="16MHz">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="XTAL-08181"/>
<attribute name="SF_ID" value="COM-00536"/>
<attribute name="VALUE"/>
</element>
<element name="K1" library="SamacSys_Parts" package="G5V-2" value="G5V-2-DC5">
<attribute name="DESCRIPTION" value="Low Signal Relays - PCB ThruHole Sealed DPDT 5VDC 500mW"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_NAME" value="Omron Electronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="G5V-2-DC5"/>
<attribute name="MOUSER_PART_NUMBER" value="653-G5V-2-DC5"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="K2" library="SamacSys_Parts" package="G5V-2" value="G5V-2-DC5">
<attribute name="DESCRIPTION" value="Low Signal Relays - PCB ThruHole Sealed DPDT 5VDC 500mW"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_NAME" value="Omron Electronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="G5V-2-DC5"/>
<attribute name="MOUSER_PART_NUMBER" value="653-G5V-2-DC5"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="0309/10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="0309/10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="0309/10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="0309/10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="adafruit" package="0309/10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="adafruit" package="0309/10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="adafruit" package="0309/10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="C050-024X044" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="C050-024X044" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="adafruit" package="C050-024X044" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SV3" library="con-lstb" package="MA04-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SV4" library="con-lstb" package="MA05-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GNDBREAK">
<contactref element="CN1" pad="GNDBREAK"/>
</signal>
<signal name="N$2">
<contactref element="Y1" pad="2"/>
<contactref element="U1" pad="10"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="CN1" pad="GND"/>
<contactref element="U1" pad="8"/>
<contactref element="C7" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="SV1" pad="4"/>
<contactref element="T1" pad="3"/>
<contactref element="K1" pad="8"/>
<contactref element="K2" pad="8"/>
<contactref element="R5" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="SV4" pad="5"/>
</signal>
<signal name="VCC">
<contactref element="CN1" pad="PWR"/>
<contactref element="U1" pad="7"/>
<contactref element="SV1" pad="5"/>
<contactref element="K1" pad="1"/>
<contactref element="K2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="C6" pad="1"/>
<contactref element="K2" pad="4"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="17"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="C5" pad="1"/>
<contactref element="K1" pad="5"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="C4" pad="1"/>
<contactref element="K1" pad="4"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="C7" pad="1"/>
<contactref element="K2" pad="5"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="K1" pad="3"/>
<contactref element="U1" pad="23"/>
<contactref element="SV4" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="K1" pad="6"/>
<contactref element="U1" pad="24"/>
<contactref element="SV4" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="U1" pad="25"/>
<contactref element="K2" pad="3"/>
<contactref element="SV4" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="U1" pad="26"/>
<contactref element="K2" pad="6"/>
<contactref element="SV4" pad="4"/>
</signal>
<signal name="N$15">
<contactref element="SV1" pad="3"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="SV1" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="U1" pad="3"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="U1" pad="1"/>
<contactref element="T1" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="SV1" pad="1"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="Y1" pad="1"/>
<contactref element="U1" pad="9"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="K1" pad="2"/>
<contactref element="SV3" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="K1" pad="7"/>
<contactref element="SV3" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="K2" pad="2"/>
<contactref element="SV3" pad="3"/>
</signal>
<signal name="N$26">
<contactref element="K2" pad="7"/>
<contactref element="SV3" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="15"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="16"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="5"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="R5" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="T1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
