(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 130)
    (zones 0)
    (modules 8)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.2)
    (user_trace_width 0.508)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /L_FIRE)
  (net 2 GND)
  (net 3 "Net-(J1-Pad7)")
  (net 4 /Vcc)
  (net 5 /R_FIRE)
  (net 6 /RIGHT)
  (net 7 /LEFT)
  (net 8 /DOWN)
  (net 9 /UP)
  (net 10 /FIRE2)
  (net 11 "Net-(J2-Pad7)")
  (net 12 /FIRE1)
  (net 13 "Net-(Q1-Pad2)")
  (net 14 "Net-(Q2-Pad2)")
  (net 15 "Net-(Q1-Pad3)")
  (net 16 "Net-(Q2-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.508)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /Vcc)
    (add_net GND)
  )
  (net_class Signal ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /DOWN)
    (add_net /FIRE1)
    (add_net /FIRE2)
    (add_net /LEFT)
    (add_net /L_FIRE)
    (add_net /RIGHT)
    (add_net /R_FIRE)
    (add_net /UP)
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(Q2-Pad3)")
  )
  (module digikey-footprints:TO-92-3 (layer F.Cu) (tedit 5AF9CDD1)
    (at 114.3 74.295 270)
    (descr http://www.ti.com/lit/ds/symlink/tl431a.pdf)
    (fp_text reference Q2 (at 1.27 -3.35 90) (layer F.SilkS))
    (fp_text value 2N4401 (at 1.27 2.5 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -1.25 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1.5) (drill 0.55) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 1 1.5) (drill 0.55) (layers *.Cu *.Mask)
      (net 16 "Net-(Q2-Pad3)"))
    (pad 2 thru_hole oval (at 1.27 0 90) (size 1 1.5) (drill 0.55) (layers *.Cu *.Mask)
      (net 14 "Net-(Q2-Pad2)"))
  )
  (module digikey-footprints:TO-92-3 (layer F.Cu) (tedit 5AF9CDD1)
    (at 114.3 67.945 270)
    (descr http://www.ti.com/lit/ds/symlink/tl431a.pdf)
    (fp_text reference Q1 (at 1.27 -3.35 90) (layer F.SilkS))
    (fp_text value 2N4401 (at 1.27 2.5 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -1.25 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1.5) (drill 0.55) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 1 1.5) (drill 0.55) (layers *.Cu *.Mask)
      (net 15 "Net-(Q1-Pad3)"))
    (pad 2 thru_hole oval (at 1.27 0 90) (size 1 1.5) (drill 0.55) (layers *.Cu *.Mask)
      (net 13 "Net-(Q1-Pad2)"))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering_RevA_Date25Jun2010 (layer F.Cu) (tedit 0)
    (at 125.73 72.39 270)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering, Rev A, Date 25 Jun 2010,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering, Rev A, Date 25 Jun 2010,")
    (fp_text reference R4 (at 0.09906 -1.905 90) (layer F.SilkS))
    (fp_text value 270 (at -0.39878 4.20116 90) (layer F.Fab))
    (pad 1 smd trapezoid (at -1.99898 0 270) (size 2.79908 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 10 /FIRE2))
    (pad 2 smd trapezoid (at 1.99898 0 90) (size 2.79908 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(Q2-Pad3)"))
    (pad 1 thru_hole rect (at -5.00126 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 10 /FIRE2))
    (pad 2 thru_hole rect (at 5.00126 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 16 "Net-(Q2-Pad3)"))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering_RevA_Date25Jun2010 (layer F.Cu) (tedit 0)
    (at 120.65 72.39 270)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering, Rev A, Date 25 Jun 2010,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering, Rev A, Date 25 Jun 2010,")
    (fp_text reference R3 (at 0.09906 -1.905 90) (layer F.SilkS))
    (fp_text value 270 (at -0.39878 4.20116 90) (layer F.Fab))
    (pad 1 smd trapezoid (at -1.99898 0 270) (size 2.79908 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 12 /FIRE1))
    (pad 2 smd trapezoid (at 1.99898 0 90) (size 2.79908 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(Q1-Pad3)"))
    (pad 1 thru_hole rect (at -5.00126 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 12 /FIRE1))
    (pad 2 thru_hole rect (at 5.00126 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 15 "Net-(Q1-Pad3)"))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering_RevA_Date25Jun2010 (layer F.Cu) (tedit 0)
    (at 107.95 72.39 90)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering, Rev A, Date 25 Jun 2010,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering, Rev A, Date 25 Jun 2010,")
    (fp_text reference R2 (at 0 1.905 90) (layer F.SilkS))
    (fp_text value 1.8K (at -0.39878 4.20116 90) (layer F.Fab))
    (pad 1 smd trapezoid (at -1.99898 0 90) (size 2.79908 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(Q2-Pad2)"))
    (pad 2 smd trapezoid (at 1.99898 0 270) (size 2.79908 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 5 /R_FIRE))
    (pad 1 thru_hole rect (at -5.00126 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 14 "Net-(Q2-Pad2)"))
    (pad 2 thru_hole rect (at 5.00126 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 5 /R_FIRE))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering_RevA_Date25Jun2010 (layer F.Cu) (tedit 0)
    (at 102.87 72.39 90)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering, Rev A, Date 25 Jun 2010,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering, Rev A, Date 25 Jun 2010,")
    (fp_text reference R1 (at 0 1.905 90) (layer F.SilkS))
    (fp_text value 1.8K (at -0.39878 4.20116 90) (layer F.Fab))
    (pad 1 smd trapezoid (at -1.99898 0 90) (size 2.79908 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(Q1-Pad2)"))
    (pad 2 smd trapezoid (at 1.99898 0 270) (size 2.79908 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 1 /L_FIRE))
    (pad 1 thru_hole rect (at -5.00126 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 13 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole rect (at 5.00126 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 /L_FIRE))
  )
  (module Connector_Dsub:DSUB-9_Female_EdgeMount_P2.77mm (layer F.Cu) (tedit 59FEDEE2)
    (at 132.08 72.517 90)
    (descr "9-pin D-Sub connector, solder-cups edge-mounted, female, x-pin-pitch 2.77mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "9-pin D-Sub connector edge mount solder cup female x-pin-pitch 2.77mm mounting holes distance 25mm")
    (attr smd)
    (fp_text reference J2 (at 5.842 -3.175 90) (layer F.SilkS))
    (fp_text value DB9_Female (at 0 16.86 90) (layer F.Fab))
    (fp_text user "PCB edge" (at -10.425 1.323333 90) (layer Dwgs.User))
    (fp_text user %R (at 0 3.39 90) (layer F.Fab))
    (pad 9 smd rect (at -4.155 0 90) (size 1.846667 3.48) (layers B.Cu B.Paste B.Mask)
      (net 10 /FIRE2))
    (pad 8 smd rect (at -1.385 0 90) (size 1.846667 3.48) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 1.385 0 90) (size 1.846667 3.48) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(J2-Pad7)"))
    (pad 6 smd rect (at 4.155 0 90) (size 1.846667 3.48) (layers B.Cu B.Paste B.Mask)
      (net 12 /FIRE1))
    (pad 5 smd rect (at -5.54 0 90) (size 1.846667 3.48) (layers F.Cu F.Paste F.Mask)
      (net 4 /Vcc))
    (pad 4 smd rect (at -2.77 0 90) (size 1.846667 3.48) (layers F.Cu F.Paste F.Mask)
      (net 6 /RIGHT))
    (pad 3 smd rect (at 0 0 90) (size 1.846667 3.48) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEFT))
    (pad 2 smd rect (at 2.77 0 90) (size 1.846667 3.48) (layers F.Cu F.Paste F.Mask)
      (net 8 /DOWN))
    (pad 1 smd rect (at 5.54 0 90) (size 1.846667 3.48) (layers F.Cu F.Paste F.Mask)
      (net 9 /UP))
    (model ${KISYS3DMOD}/Connector_Dsub.3dshapes/DSUB-9_Female_EdgeMount_P2.77mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Dsub:DSUB-9_Male_EdgeMount_P2.77mm (layer F.Cu) (tedit 59FEDEE2)
    (at 96.901 72.517 270)
    (descr "9-pin D-Sub connector, solder-cups edge-mounted, male, x-pin-pitch 2.77mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "9-pin D-Sub connector edge mount solder cup male x-pin-pitch 2.77mm mounting holes distance 25mm")
    (attr smd)
    (fp_text reference J1 (at -5.842 -3.048 90) (layer F.SilkS))
    (fp_text value DB9_Male (at 0 16.69 90) (layer F.Fab))
    (fp_text user "PCB edge" (at -10.425 1.323333 90) (layer Dwgs.User))
    (fp_text user %R (at 0 3.39 90) (layer F.Fab))
    (pad 9 smd rect (at 4.155 0 270) (size 1.846667 3.48) (layers B.Cu B.Paste B.Mask)
      (net 1 /L_FIRE))
    (pad 8 smd rect (at 1.385 0 270) (size 1.846667 3.48) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -1.385 0 270) (size 1.846667 3.48) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad7)"))
    (pad 6 smd rect (at -4.155 0 270) (size 1.846667 3.48) (layers B.Cu B.Paste B.Mask)
      (net 4 /Vcc))
    (pad 5 smd rect (at 5.54 0 270) (size 1.846667 3.48) (layers F.Cu F.Paste F.Mask)
      (net 5 /R_FIRE))
    (pad 4 smd rect (at 2.77 0 270) (size 1.846667 3.48) (layers F.Cu F.Paste F.Mask)
      (net 6 /RIGHT))
    (pad 3 smd rect (at 0 0 270) (size 1.846667 3.48) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEFT))
    (pad 2 smd rect (at -2.77 0 270) (size 1.846667 3.48) (layers F.Cu F.Paste F.Mask)
      (net 8 /DOWN))
    (pad 1 smd rect (at -5.54 0 270) (size 1.846667 3.48) (layers F.Cu F.Paste F.Mask)
      (net 9 /UP))
    (model ${KISYS3DMOD}/Connector_Dsub.3dshapes/DSUB-9_Male_EdgeMount_P2.77mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Atari 7800 Joystick to SMS Adapter" (at 114.173 72.39) (layer B.SilkS))
  (gr_text FEMALE (at 128.651 72.39 270) (layer B.SilkS))
  (gr_text MALE (at 100.203 72.39 90) (layer B.SilkS))
  (gr_line (start 134 65) (end 134 80) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95 65) (end 134 65) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95 80) (end 95 65) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 134 80) (end 95 80) (layer Edge.Cuts) (width 0.1))
)
