(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 23)
    (no_connects 0)
    (area 140.259999 99.619999 155.650001 122.630001)
    (thickness 1.6)
    (drawings 11)
    (tracks 103)
    (zones 0)
    (modules 10)
    (nets 29)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 /CE)
  (net 4 /CS)
  (net 5 /SCK)
  (net 6 /MOSI)
  (net 7 /MISO)
  (net 8 /IRQ)
  (net 9 /RST)
  (net 10 /TEST)
  (net 11 "Net-(U1-Pad2)")
  (net 12 "Net-(U1-Pad3)")
  (net 13 "Net-(U1-Pad5)")
  (net 14 "Net-(U1-Pad6)")
  (net 15 "Net-(U1-Pad7)")
  (net 16 "Net-(U1-Pad8)")
  (net 17 "Net-(U1-Pad9)")
  (net 18 "Net-(U1-Pad13)")
  (net 19 "Net-(U1-Pad14)")
  (net 20 "Net-(U1-Pad15)")
  (net 21 "Net-(U1-Pad16)")
  (net 22 "Net-(U1-Pad19)")
  (net 23 "Net-(U1-Pad20)")
  (net 24 "Net-(U1-Pad21)")
  (net 25 "Net-(U1-Pad23)")
  (net 26 "Net-(U1-Pad26)")
  (net 27 "Net-(U1-Pad27)")
  (net 28 /TX)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CE)
    (add_net /CS)
    (add_net /IRQ)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RST)
    (add_net /SCK)
    (add_net /TEST)
    (add_net /TX)
    (add_net GND)
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
    (add_net VCC)
  )
  (module MSP430-Part-Library-for-Kicad-master:nrf24_smd (layer B.Cu) (tedit 5AA5F6F1)
    (at 152.4 119.38 180)
    (fp_text reference J1 (at 4.572 -1.778 180) (layer B.SilkS) hide)
    (fp_text value NRF24L01+ (at 4.572 -1.778 180) (layer B.SilkS))
    (pad 1 smd rect (at 0 0 180) (size 0.85 1.524) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.27 0 180) (size 0.85 1.524) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 3 smd rect (at 2.54 0 180) (size 0.85 1.524) (layers B.Cu B.Paste B.Mask)
      (net 3 /CE))
    (pad 4 smd rect (at 3.81 0 180) (size 0.85 1.524) (layers B.Cu B.Paste B.Mask)
      (net 4 /CS))
    (pad 5 smd rect (at 5.08 0 180) (size 0.85 1.524) (layers B.Cu B.Paste B.Mask)
      (net 5 /SCK))
    (pad 6 smd rect (at 6.35 0 180) (size 0.85 1.524) (layers B.Cu B.Paste B.Mask)
      (net 6 /MOSI))
    (pad 7 smd rect (at 7.62 0 180) (size 0.85 1.524) (layers B.Cu B.Paste B.Mask)
      (net 7 /MISO))
    (pad 8 smd rect (at 8.89 0 180) (size 0.85 1.524) (layers B.Cu B.Paste B.Mask)
      (net 8 /IRQ))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch1.00mm_SMD_Pin1Left (layer F.Cu) (tedit 5AA5F0CB)
    (at 152.146 115.57)
    (descr "surface-mounted straight pin header, 1x04, 1.00mm pitch, single row, style 1 (pin 1 left)")
    (tags "Surface mounted pin header SMD 1x04 1.00mm single row style1 pin1 left")
    (attr smd)
    (fp_text reference SWD1 (at 0 -3.06) (layer F.SilkS) hide)
    (fp_text value SWD (at -0.508 -3.048) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.875 -1.5) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 3 smd rect (at -0.875 0.5) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /TEST))
    (pad 2 smd rect (at 0.875 -0.5) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /RST))
    (pad 4 smd rect (at 0.875 1.5) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch1.00mm_SMD_Pin1Left.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 144.78 116.84 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 2.794 0 180) (layer F.SilkS))
    (fp_text value 10uf (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at -3.048 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 144.78 114.3 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 2.794 0 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at -3.048 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSP430-Part-Library-for-Kicad-master:TSSOP28 (layer F.Cu) (tedit 5AA5E26B)
    (at 147.828 105.156 180)
    (fp_text reference U1 (at 4.09956 1.00076 180) (layer F.SilkS))
    (fp_text value MSP430G2553_TSSOP28 (at -0.508 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -4.22402 2.79908) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at -3.57378 2.79908) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -2.92354 2.79908) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -2.2733 2.79908) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 28 /TX))
    (pad 5 smd rect (at -1.62306 2.79908) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at -0.97282 2.79908) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at -0.32258 2.79908) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad7)"))
    (pad 8 smd rect (at 0.32258 2.79908) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad8)"))
    (pad 9 smd rect (at 0.97282 2.79908) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad9)"))
    (pad 10 smd rect (at 1.62306 2.79908) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 6 /MOSI))
    (pad 11 smd rect (at 2.2733 2.79908) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 5 /SCK))
    (pad 12 smd rect (at 2.92354 2.79908) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 7 /MISO))
    (pad 13 smd rect (at 3.57378 2.79908) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U1-Pad13)"))
    (pad 14 smd rect (at 4.22402 2.79908) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at 4.22402 -2.79908 180) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U1-Pad15)"))
    (pad 16 smd rect (at 3.57378 -2.79908 180) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U1-Pad16)"))
    (pad 17 smd rect (at 2.92354 -2.79908 180) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 4 /CS))
    (pad 18 smd rect (at 2.2733 -2.79908 180) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 8 /IRQ))
    (pad 19 smd rect (at 1.62306 -2.79908 180) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U1-Pad19)"))
    (pad 20 smd rect (at 0.97282 -2.79908 180) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U1-Pad20)"))
    (pad 21 smd rect (at 0.32258 -2.79908 180) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U1-Pad21)"))
    (pad 22 smd rect (at -0.32258 -2.79908 180) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 3 /CE))
    (pad 23 smd rect (at -0.97282 -2.79908 180) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U1-Pad23)"))
    (pad 24 smd rect (at -1.62306 -2.79908 180) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 9 /RST))
    (pad 25 smd rect (at -2.2733 -2.79908 180) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 10 /TEST))
    (pad 26 smd rect (at -2.92354 -2.79908 180) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U1-Pad26)"))
    (pad 27 smd rect (at -3.57378 -2.79908 180) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U1-Pad27)"))
    (pad 28 smd rect (at -4.22402 -2.79908 180) (size 0.24892 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 5AA5F752)
    (at 147.828 119.888)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference V1 (at 0 1.778) (layer F.SilkS) hide)
    (fp_text value V (at 0 1.778) (layer F.SilkS))
    (pad 2 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 2 VCC))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 5AA5EF67)
    (at 150.368 119.888)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference G1 (at 0 1.778) (layer F.SilkS) hide)
    (fp_text value G (at 0 1.778) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 5AA5F746)
    (at 145.288 119.888)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference S1 (at 0 1.778) (layer F.SilkS) hide)
    (fp_text value S1 (at 0 1.778) (layer F.SilkS))
    (pad 3 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 28 /TX))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 153.924 102.092 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -1.508 1.778 360) (layer F.SilkS))
    (fp_text value 100nf (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at -0.238 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 148.729 116.967)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -0.012 -1.27) (layer F.SilkS))
    (fp_text value 47k (at -0.508 -1.524) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 /TEST))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "MSPr v0.1" (at 141.732 105.156 90) (layer F.SilkS))
  (gr_line (start 140.335 122.555) (end 140.335 120.65) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.575 122.555) (end 140.335 122.555) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.575 120.65) (end 155.575 122.555) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.335 99.695) (end 140.335 120.65) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.575 99.695) (end 140.335 99.695) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.575 120.65) (end 155.575 99.695) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.575 120.65) (xy 140.335 120.65) (xy 140.335 99.695) (xy 155.575 99.695)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 140.335 99.695) (xy 140.335 122.555) (xy 155.575 122.555) (xy 155.575 99.695)
      )
    )
  )
)
