(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.646)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(material "Liquid Photo")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Purple")
				(thickness 0.0254)
				(material "SMOBC")
				(epsilon_r 3.3)
				(loss_tangent 0)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.0356)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.524)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.0356)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Purple")
				(thickness 0.0254)
				(material "SMOBC")
				(epsilon_r 3.3)
				(loss_tangent 0)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(material "Liquid Photo")
			)
			(copper_finish "ENIG")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0.0762)
		(solder_mask_min_width 0.1016)
		(allow_soldermask_bridges_in_footprints yes)
		(tenting front back)
		(aux_axis_origin 127.20111 115.16359)
		(grid_origin 127.20111 115.16359)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "+3.3V")
	(net 3 "EN")
	(net 4 "/MCU/HSPI_MOSI")
	(net 5 "/MCU/VSPI_MISO")
	(net 6 "/MCU/VSPI_CS")
	(net 7 "/MCU/HSPI_CS")
	(net 8 "/MCU/VSPI_SCLK")
	(net 9 "/MCU/VSPI_GDO2")
	(net 10 "/MCU/HSPI_SCLK")
	(net 11 "/MCU/VSPI_MOSI")
	(net 12 "/MCU/HSPI_DC")
	(net 13 "/MCU/VSPI_GDO0")
	(net 14 "Net-(U1-IO0)")
	(net 15 "unconnected-(X9-Pad6)")
	(net 16 "Net-(C4-Pad2)")
	(net 17 "unconnected-(X9-Pad2)")
	(net 18 "unconnected-(X9-Pad16)")
	(net 19 "unconnected-(X9-Pad8)")
	(net 20 "unconnected-(U1-NC-Pad22)")
	(net 21 "unconnected-(U1-NC-Pad17)")
	(net 22 "unconnected-(U1-NC-Pad18)")
	(net 23 "unconnected-(U1-NC-Pad27)")
	(net 24 "unconnected-(U1-NC-Pad19)")
	(net 25 "unconnected-(U2-P6-Pad10)")
	(net 26 "unconnected-(U1-NC-Pad20)")
	(net 27 "unconnected-(U1-NC-Pad32)")
	(net 28 "unconnected-(X8-Pad4)")
	(net 29 "unconnected-(X8-Pad5)")
	(net 30 "unconnected-(X8-Pad6)")
	(net 31 "unconnected-(U1-NC-Pad21)")
	(net 32 "unconnected-(X8-Pad8)")
	(net 33 "unconnected-(X8-Pad9)")
	(net 34 "unconnected-(U1-NC-Pad28)")
	(net 35 "unconnected-(X9-Pad4)")
	(net 36 "unconnected-(X9-Pad5)")
	(net 37 "unconnected-(X9-Pad7)")
	(net 38 "unconnected-(X9-Pad9)")
	(net 39 "unconnected-(X7-Pad6)")
	(net 40 "unconnected-(U2-P14-Pad17)")
	(net 41 "unconnected-(X7-Pad10)")
	(net 42 "unconnected-(X7-Pad11)")
	(net 43 "unconnected-(X7-Pad12)")
	(net 44 "unconnected-(X7-Pad16)")
	(net 45 "unconnected-(X7-Pad17)")
	(net 46 "unconnected-(U2-P17-Pad20)")
	(net 47 "unconnected-(U2-P12-Pad15)")
	(net 48 "unconnected-(U2-P7-Pad11)")
	(net 49 "unconnected-(U2-P15-Pad18)")
	(net 50 "unconnected-(U2-P13-Pad16)")
	(net 51 "unconnected-(U2-P16-Pad19)")
	(net 52 "unconnected-(U2-P11-Pad14)")
	(net 53 "unconnected-(U2-P10-Pad13)")
	(net 54 "/MCU/X_INT")
	(net 55 "/MCU/DIN")
	(net 56 "/MCU/DOUT")
	(net 57 "SCL")
	(net 58 "SDA")
	(net 59 "/MCU/BCLK")
	(net 60 "/MCU/LRCLK")
	(net 61 "/MCU/BMS_INT")
	(net 62 "/MCU/AUDIO_INT")
	(net 63 "/MCU/TX0")
	(net 64 "/MCU/HMI_INT")
	(net 65 "/MCU/RF_INT")
	(net 66 "/MCU/RX0")
	(net 67 "/TFT_BL_EN")
	(net 68 "/TFT_RST")
	(net 69 "/CC1200_RST")
	(net 70 "/AMP_SD")
	(net 71 "/FUEL_GUAGE_ALERT")
	(net 72 "/PD_ALERT{slash}INT")
	(net 73 "unconnected-(X6-Pad11)")
	(net 74 "unconnected-(X6-Pad10)")
	(net 75 "unconnected-(X6-Pad12)")
	(net 76 "unconnected-(X7-Pad15)")
	(footprint "Package_SO:SSOP-24_5.3x8.2mm_P0.65mm"
		(layer "F.Cu")
		(at 211.892 75.203)
		(descr "SSOP, 24 Pin (JEDEC MO-150 variation AG, 1.75mm body thickness, https://www.jedec.org/document_search?search_api_views_fulltext=MO-150, https://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=398, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-ssop/ssop_24_05-08-1640.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SSOP SO")
		(property "Reference" "U2"
			(at 0 -5.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "PCF8575DBR"
			(at 0 5.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/pcf8575.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "16 Bits Port/Expander to I2C Bus, SSOP-24"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP*5.3x8.2mm*P0.65mm*")
		(sheetname "/")
		(sheetfile "testbed-mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.5 -3.575)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "/MCU/X_INT")
			(pinfunction "~{INT}")
			(pintype "open_collector")
		)
		(pad "2" smd roundrect
			(at -3.5 -2.925)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -3.5 -2.275)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -3.5 -1.625)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "/AMP_SD")
			(pinfunction "P0")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -3.5 -0.975)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 68 "/TFT_RST")
			(pinfunction "P1")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -3.5 -0.325)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "/TFT_BL_EN")
			(pinfunction "P2")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -3.5 0.325)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 69 "/CC1200_RST")
			(pinfunction "P3")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -3.5 0.975)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "/PD_ALERT{slash}INT")
			(pinfunction "P4")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -3.5 1.625)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "/FUEL_GUAGE_ALERT")
			(pinfunction "P5")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -3.5 2.275)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "unconnected-(U2-P6-Pad10)")
			(pinfunction "P6")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at -3.5 2.925)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "unconnected-(U2-P7-Pad11)")
			(pinfunction "P7")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at -3.5 3.575)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" smd roundrect
			(at 3.5 3.575)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "unconnected-(U2-P10-Pad13)")
			(pinfunction "P10")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at 3.5 2.925)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "unconnected-(U2-P11-Pad14)")
			(pinfunction "P11")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at 3.5 2.275)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "unconnected-(U2-P12-Pad15)")
			(pinfunction "P12")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at 3.5 1.625)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "unconnected-(U2-P13-Pad16)")
			(pinfunction "P13")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at 3.5 0.975)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "unconnected-(U2-P14-Pad17)")
			(pinfunction "P14")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at 3.5 0.325)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "unconnected-(U2-P15-Pad18)")
			(pinfunction "P15")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at 3.5 -0.325)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "unconnected-(U2-P16-Pad19)")
			(pinfunction "P16")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at 3.5 -0.975)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "unconnected-(U2-P17-Pad20)")
			(pinfunction "P17")
			(pintype "bidirectional")
		)
		(pad "21" smd roundrect
			(at 3.5 -1.625)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at 3.5 -2.275)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 3.5 -2.925)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 58 "SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "24" smd roundrect
			(at 3.5 -3.575)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SSOP-24_5.3x8.2mm_P0.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 181.864 40.64 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 1.989067 0.120429 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/MCU/")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 223.52 84.836 90)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH horizontal")
		(property "Reference" "J1"
			(at 0 1.31646 270)
			(layer "F.SilkS")
		)
		(property "Value" "Stemma QT"
			(at 0 3.98 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4208/4208_Kaweei_C13396_diagram.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic shielded connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1SH*")
		(sheetname "/")
		(sheetfile "testbed-mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.3V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 58 "SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "SCL")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875 90)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875 90)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
		)
		(embedded_fonts no)
		(model "/Users/adriannequick/seniorProject/capstone repo/capstone-project/Hardware/KiCAD/system-testbed/capstone-project.pretty/3dmodels/SM04B-SRSS-TB.step"
			(offset
				(xyz 0 1 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_SPST_EVQP2_MiddlePushTravel_H2.5mm"
		(layer "F.Cu")
		(at 197.647 74.51)
		(descr "Tactile switch, 4.7 x 3.5 mm, middle push travel, H2.5mm, https://industry.panasonic.com/ac/cdn/e/control/switch/light-touch/catalog/sw_lt_eng_4735s.pdf")
		(tags "SMD SMT SPST EVQP2")
		(property "Reference" "SW2"
			(at 0 -2.75 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push"
			(at 0 3 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/MCU/")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.575 -0.85)
			(size 1.45 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Net-(C4-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" smd roundrect
			(at 2.575 -0.85)
			(size 1.45 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Net-(C4-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -2.575 0.85)
			(size 1.45 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.575 0.85)
			(size 1.45 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_EVQP2_MiddlePushTravel_H2.5mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 215.9 85.535 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at -2.5245 0.06184 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "testbed-mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "SCL")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 213.043 51.816)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/MCU/")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/MCU/VSPI_CS")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:Adafruit EYESPI FPC Connector"
		(layer "F.Cu")
		(at 212.852 42.304645 180)
		(descr "WR-FPC SMT ZIF Horizontal Hinge Type")
		(tags "EYESPI, FPC")
		(property "Reference" "X8"
			(at -4.85 2.172645 0)
			(layer "F.SilkS")
		)
		(property "Value" "EYESPI"
			(at 7.582896 -4.066008 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/687118149022.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "WR-FPC SMT ZIF Horizontal Hinge Type"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Assignment" "PSU_I2C+INT"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "testbed-mcu.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -4.25 -3.35 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at -3.75 -3.35 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at -3.25 -3.35 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at -2.75 -3.35 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "unconnected-(X8-Pad4)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd rect
			(at -2.25 -3.35 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "unconnected-(X8-Pad5)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd rect
			(at -1.75 -3.35 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "unconnected-(X8-Pad6)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd rect
			(at -1.25 -3.35 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd rect
			(at -0.75 -3.35 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "unconnected-(X8-Pad8)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd rect
			(at -0.25 -3.35 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "unconnected-(X8-Pad9)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd rect
			(at 0.25 -3.35 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd rect
			(at 0.75 -3.35 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd rect
			(at 1.25 -3.35 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd rect
			(at 1.75 -3.35 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "SDA")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd rect
			(at 2.25 -3.35 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "SCL")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "15" smd rect
			(at 2.75 -3.35 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "/MCU/BMS_INT")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "16" smd rect
			(at 3.25 -3.35 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "17" smd rect
			(at 3.75 -3.35 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 63 "/MCU/TX0")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "18" smd rect
			(at 4.25 -3.35 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "/MCU/RX0")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "Z1" smd rect
			(at -6.05 -0.6 180)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "Z2" smd rect
			(at 6.05 -0.6 180)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "/Users/adriannequick/seniorProject/capstone repo/capstone-project/Hardware/KiCAD/system-testbed/capstone-project.pretty/3dmodels/687118149022+(rev1).step"
			(offset
				(xyz 0 1 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 178.308 49.276)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at -0.107996 1.317687 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/MCU/")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "EN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "EN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 179.324 52.324 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 -1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/MCU/")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.14 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "EN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO14580_Pad"
		(layer "F.Cu")
		(at 173.30994 89.815863 90)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO14580")
		(property "Reference" "H17"
			(at -2.132137 -4.65394 180)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 3.7 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "testbed-mcu.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 5.5 5.5)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO14580_Pad"
		(layer "F.Cu")
		(at 224.091417 74.622927 90)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO14580")
		(property "Reference" "H19"
			(at 4.010927 0.952583 180)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 3.7 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "testbed-mcu.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 5.5 5.5)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO14580_Pad"
		(layer "F.Cu")
		(at 224.089514 46.676936 90)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO14580")
		(property "Reference" "H20"
			(at 4.004936 -0.061514 180)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 3.7 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "testbed-mcu.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 5.5 5.5)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "capstone-project:Adafruit EYESPI FPC Connector"
		(layer "F.Cu")
		(at 223.52 58.928 90)
		(descr "WR-FPC SMT ZIF Horizontal Hinge Type")
		(tags "EYESPI, FPC")
		(property "Reference" "X6"
			(at -6.096 2.032 180)
			(layer "F.SilkS")
		)
		(property "Value" "EYESPI"
			(at -7.62 -4.064 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/687118149022.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "WR-FPC SMT ZIF Horizontal Hinge Type"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Assignment" "CC1200_VSPI"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "testbed-mcu.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -4.25 -3.35 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at -3.75 -3.35 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at -3.25 -3.35 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at -2.75 -3.35 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "/MCU/VSPI_SCLK")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd rect
			(at -2.25 -3.35 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "/MCU/VSPI_MOSI")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd rect
			(at -1.75 -3.35 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/MCU/VSPI_MISO")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd rect
			(at -1.25 -3.35 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd rect
			(at -0.75 -3.35 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 69 "/CC1200_RST")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd rect
			(at -0.25 -3.35 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/MCU/VSPI_CS")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd rect
			(at 0.25 -3.35 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 74 "unconnected-(X6-Pad10)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd rect
			(at 0.75 -3.35 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 73 "unconnected-(X6-Pad11)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd rect
			(at 1.25 -3.35 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 75 "unconnected-(X6-Pad12)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd rect
			(at 1.75 -3.35 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "SDA")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd rect
			(at 2.25 -3.35 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "SCL")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "15" smd rect
			(at 2.75 -3.35 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "/MCU/RF_INT")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "16" smd rect
			(at 3.25 -3.35 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "17" smd rect
			(at 3.75 -3.35 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "/MCU/VSPI_GDO0")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "18" smd rect
			(at 4.25 -3.35 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "/MCU/VSPI_GDO2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "Z1" smd rect
			(at -6.05 -0.6 90)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "Z2" smd rect
			(at 6.05 -0.6 90)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "/Users/adriannequick/seniorProject/capstone repo/capstone-project/Hardware/KiCAD/system-testbed/capstone-project.pretty/3dmodels/687118149022+(rev1).step"
			(offset
				(xyz 0 1 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 177.8 44.196 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/MCU/")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "EN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO14580_Pad"
		(layer "F.Cu")
		(at 172.066268 41.429316 90)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO14580")
		(property "Reference" "H18"
			(at 1.805316 -4.426268 180)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 3.7 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "testbed-mcu.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 5.5 5.5)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 201.168 68.58 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/MCU/")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/MCU/HSPI_CS")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 173.228 73.66)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Button_Switch_SMD:SW_SPST_EVQP2_MiddlePushTravel_H2.5mm"
		(layer "F.Cu")
		(at 172.212 48.26)
		(descr "Tactile switch, 4.7 x 3.5 mm, middle push travel, H2.5mm, https://industry.panasonic.com/ac/cdn/e/control/switch/light-touch/catalog/sw_lt_eng_4735s.pdf")
		(tags "SMD SMT SPST EVQP2")
		(property "Reference" "SW1"
			(at 0 -2.75 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push"
			(at 0 3 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/MCU/")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.575 -0.85)
			(size 1.45 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" smd roundrect
			(at 2.575 -0.85)
			(size 1.45 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -2.575 0.85)
			(size 1.45 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "EN")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.575 0.85)
			(size 1.45 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "EN")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_EVQP2_MiddlePushTravel_H2.5mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:Adafruit EYESPI FPC Connector"
		(layer "F.Cu")
		(at 192.532 89.407998)
		(descr "WR-FPC SMT ZIF Horizontal Hinge Type")
		(tags "EYESPI, FPC")
		(property "Reference" "X7"
			(at 5.627237 2.229219 0)
			(layer "F.SilkS")
		)
		(property "Value" "EYESPI"
			(at -10.16 -2.54 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/687118149022.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "WR-FPC SMT ZIF Horizontal Hinge Type"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Assignment" "DISPLAY_HSPI"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "testbed-mcu.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -4.25 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at -3.75 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "/TFT_BL_EN")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at -3.25 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at -2.75 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/MCU/HSPI_SCLK")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd rect
			(at -2.25 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/MCU/HSPI_MOSI")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd rect
			(at -1.75 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "unconnected-(X7-Pad6)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd rect
			(at -1.25 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "/MCU/HSPI_DC")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd rect
			(at -0.75 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "EN")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd rect
			(at -0.25 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/MCU/HSPI_CS")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd rect
			(at 0.25 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "unconnected-(X7-Pad10)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd rect
			(at 0.75 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "unconnected-(X7-Pad11)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd rect
			(at 1.25 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "unconnected-(X7-Pad12)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd rect
			(at 1.75 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "SDA")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd rect
			(at 2.25 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "SCL")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "15" smd rect
			(at 2.75 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 76 "unconnected-(X7-Pad15)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "16" smd rect
			(at 3.25 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "unconnected-(X7-Pad16)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "17" smd rect
			(at 3.75 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "unconnected-(X7-Pad17)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "18" smd rect
			(at 4.25 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "/MCU/HMI_INT")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "Z1" smd rect
			(at -6.05 -0.6)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "Z2" smd rect
			(at 6.05 -0.6)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "/Users/adriannequick/seniorProject/capstone repo/capstone-project/Hardware/KiCAD/system-testbed/capstone-project.pretty/3dmodels/687118149022+(rev1).step"
			(offset
				(xyz 0 1 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "capstone-project:ESP32-WROVER-IE"
		(layer "F.Cu")
		(at 193.04 51.308)
		(property "Reference" "U1"
			(at 0 2.54 180)
			(layer "F.SilkS")
		)
		(property "Value" "ESP32-WROVER-E"
			(at 0 10.668 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "kicad-embed://esp32-wrover-e_esp32-wrover-ie_datasheet_en.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "WROVER-E & WROVER-IE Footprint"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/MCU/")
		(sheetfile "MCU.kicad_sch")
		(attr through_hole)
		(fp_text user "Keep Out Area"
			(at 0 -16.256 180)
			(layer "F.SilkS")
		)
		(fp_text user "Keep Out Area"
			(at 0 -16.256 180)
			(layer "Dwgs.User")
		)
		(pad "1" smd rect
			(at -8.75 -11.43)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -8.75 -10.16)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.3V")
			(pinfunction "3V3")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at -8.75 -8.89)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "EN")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -8.75 -7.62)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "/MCU/BMS_INT")
			(pinfunction "GPIO36")
			(pintype "output")
		)
		(pad "5" smd rect
			(at -8.75 -6.35)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "/MCU/RF_INT")
			(pinfunction "GPIO39")
			(pintype "output")
		)
		(pad "6" smd rect
			(at -8.75 -5.08)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "/MCU/DIN")
			(pinfunction "GPIO34")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -8.75 -3.81)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "/MCU/HMI_INT")
			(pinfunction "GPIO35")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at -8.75 -2.54)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "/MCU/VSPI_GDO0")
			(pinfunction "GPIO32")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at -8.75 -1.27)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "/MCU/VSPI_GDO2")
			(pinfunction "GPIO33")
			(pintype "input")
		)
		(pad "10" smd rect
			(at -8.75 0)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "/MCU/LRCLK")
			(pinfunction "GPIO25")
			(pintype "output")
		)
		(pad "11" smd rect
			(at -8.75 1.27)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "/MCU/BCLK")
			(pinfunction "GPIO26")
			(pintype "bidirectional")
		)
		(pad "12" smd rect
			(at -8.75 2.54)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "/MCU/DOUT")
			(pinfunction "GPIO27")
			(pintype "output")
		)
		(pad "13" smd rect
			(at -8.75 3.81)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/MCU/HSPI_SCLK")
			(pinfunction "GPIO14")
			(pintype "bidirectional")
		)
		(pad "14" smd rect
			(at -8.75 5.08)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "/MCU/X_INT")
			(pinfunction "IO12")
			(pintype "bidirectional")
		)
		(pad "15" smd rect
			(at -8.75 6.35)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "16" smd rect
			(at -8.75 7.62)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/MCU/HSPI_MOSI")
			(pinfunction "GPIO13")
			(pintype "bidirectional")
		)
		(pad "17" smd rect
			(at -8.75 8.89)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "unconnected-(U1-NC-Pad17)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "18" smd rect
			(at -8.75 10.16)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "unconnected-(U1-NC-Pad18)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "19" smd rect
			(at -8.75 11.43)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "unconnected-(U1-NC-Pad19)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "20" smd rect
			(at 8.75 11.43)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "unconnected-(U1-NC-Pad20)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "21" smd rect
			(at 8.75 10.16)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "unconnected-(U1-NC-Pad21)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "22" smd rect
			(at 8.75 8.89)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "unconnected-(U1-NC-Pad22)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "23" smd rect
			(at 8.75 7.62)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/MCU/HSPI_CS")
			(pinfunction "IO15")
			(pintype "bidirectional")
		)
		(pad "24" smd rect
			(at 8.75 6.35)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "/MCU/AUDIO_INT")
			(pinfunction "IO2")
			(pintype "bidirectional")
		)
		(pad "25" smd rect
			(at 8.75 5.08)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(U1-IO0)")
			(pinfunction "IO0")
			(pintype "bidirectional")
		)
		(pad "26" smd rect
			(at 8.75 3.81)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "/MCU/HSPI_DC")
			(pinfunction "GPIO4")
			(pintype "bidirectional")
		)
		(pad "27" smd rect
			(at 8.75 2.54)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "unconnected-(U1-NC-Pad27)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "28" smd rect
			(at 8.75 1.27)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "unconnected-(U1-NC-Pad28)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "29" smd rect
			(at 8.75 0)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/MCU/VSPI_CS")
			(pinfunction "IO5")
			(pintype "bidirectional")
		)
		(pad "30" smd rect
			(at 8.75 -1.27)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "/MCU/VSPI_SCLK")
			(pinfunction "GPIO18")
			(pintype "bidirectional")
		)
		(pad "31" smd rect
			(at 8.75 -2.54)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/MCU/VSPI_MISO")
			(pinfunction "GPIO19")
			(pintype "bidirectional")
		)
		(pad "32" smd rect
			(at 8.75 -3.81)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "unconnected-(U1-NC-Pad32)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "33" smd rect
			(at 8.75 -5.08)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "SDA")
			(pinfunction "GPIO21")
			(pintype "bidirectional")
		)
		(pad "34" smd rect
			(at 8.75 -6.35)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "/MCU/RX0")
			(pinfunction "RXD0")
			(pintype "output")
		)
		(pad "35" smd rect
			(at 8.75 -7.62)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 63 "/MCU/TX0")
			(pinfunction "TXD0")
			(pintype "output")
		)
		(pad "36" smd rect
			(at 8.75 -8.89)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "SCL")
			(pinfunction "GPIO22")
			(pintype "bidirectional")
		)
		(pad "37" smd rect
			(at 8.75 -10.16)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "/MCU/VSPI_MOSI")
			(pinfunction "GPIO23")
			(pintype "bidirectional")
		)
		(pad "38" smd rect
			(at 8.75 -11.43)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "39" smd rect
			(at -2.9 -4.42)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "39" smd rect
			(at -2.9 -3.02)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "39" smd rect
			(at -2.9 -1.62)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "39" smd rect
			(at -1.5 -4.42)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "39" smd rect
			(at -1.5 -3.02)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "39" smd rect
			(at -1.5 -1.62)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "39" smd rect
			(at -0.1 -4.42)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "39" smd rect
			(at -0.1 -3.02)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "39" smd rect
			(at -0.1 -1.62)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(embedded_fonts no)
		(model "/Users/adriannequick/seniorProject/capstone repo/capstone-project/Hardware/KiCAD/system-testbed/capstone-project.pretty/3dmodels/ESP32-WROVER-E.step"
			(offset
				(xyz -9 -12.5 0.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 192.441105 68.58 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/MCU/")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.14058 0.51 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "Net-(U1-IO0)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Net-(C4-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 217.932 85.535 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at -2.5245 0.06184 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "testbed-mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.191 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 58 "SDA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 180.34 40.64 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 2.001929 0.114091 180)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/MCU/")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:Adafruit EYESPI FPC Connector"
		(layer "F.Cu")
		(at 161.96 53.894 -90)
		(descr "WR-FPC SMT ZIF Horizontal Hinge Type")
		(tags "EYESPI, FPC")
		(property "Reference" "X9"
			(at 5.542 1.94 0)
			(layer "F.SilkS")
		)
		(property "Value" "EYESPI"
			(at 9.846897 1.077763 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/687118149022.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "WR-FPC SMT ZIF Horizontal Hinge Type"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Assignment" "AUDIO_I2S"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "testbed-mcu.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -4.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at -3.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "unconnected-(X9-Pad2)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at -3.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at -2.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "unconnected-(X9-Pad4)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd rect
			(at -2.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "unconnected-(X9-Pad5)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd rect
			(at -1.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "unconnected-(X9-Pad6)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd rect
			(at -1.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "unconnected-(X9-Pad7)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd rect
			(at -0.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "unconnected-(X9-Pad8)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd rect
			(at -0.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "unconnected-(X9-Pad9)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd rect
			(at 0.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 70 "/AMP_SD")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd rect
			(at 0.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "/MCU/DOUT")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd rect
			(at 1.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "/MCU/DIN")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd rect
			(at 1.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "SDA")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd rect
			(at 2.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "SCL")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "15" smd rect
			(at 2.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "/MCU/AUDIO_INT")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "16" smd rect
			(at 3.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "unconnected-(X9-Pad16)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "17" smd rect
			(at 3.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "/MCU/BCLK")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "18" smd rect
			(at 4.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "/MCU/LRCLK")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "Z1" smd rect
			(at -6.05 -0.6 270)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "Z2" smd rect
			(at 6.05 -0.6 270)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "/Users/adriannequick/seniorProject/capstone repo/capstone-project/Hardware/KiCAD/system-testbed/capstone-project.pretty/3dmodels/687118149022+(rev1).step"
			(offset
				(xyz 0 1 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(gr_rect
		(start 157.988 38.1)
		(end 227.584 93.98)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "I2C"
		(at 221.735 89.916 0)
		(layer "F.SilkS")
	)
	(gr_text "Audio Connector"
		(at 159.512 71.12 90)
		(layer "F.SilkS")
	)
	(gr_text "Power\nConnector"
		(at 220.89635 41.109603 0)
		(layer "F.SilkS")
	)
	(gr_text "HMI Connector\n"
		(at 176.5465 92.990961 0)
		(layer "F.SilkS")
	)
	(gr_text "RF \nConnector"
		(at 216.870134 63.367076 270)
		(layer "F.SilkS")
	)
	(gr_text "ESP32 Modulino"
		(at 14.82746 15.119573 0)
		(layer "Cmts.User")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 156.972 37.592) (xy 228.092 37.592) (xy 228.6 94.996) (xy 156.972 94.488)
			)
		)
	)
	(embedded_fonts no)
)
