(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A5")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "VCC")
  (net 3 "Net-(D1-K)")
  (net 4 "/P1")
  (net 5 "/P4")
  (net 6 "/P7")
  (net 7 "/KB_{Rx}")
  (net 8 "/KB_{Tx}")
  (net 9 "/SIO1")
  (net 10 "/CS")
  (net 11 "/SIO3")
  (net 12 "/SIO2")
  (net 13 "/SCLK")
  (net 14 "/SIO0")
  (net 15 "/Half")
  (net 16 "unconnected-(J4-Pin_2-Pad2)")
  (net 17 "unconnected-(J4-Pin_3-Pad3)")
  (net 18 "/Rst")
  (net 19 "unconnected-(J4-Pin_11-Pad11)")
  (net 20 "unconnected-(J4-Pin_12-Pad12)")
  (net 21 "/~{StartFrame}")
  (net 22 "/DO+")
  (net 23 "/DO-")
  (net 24 "/D7")
  (net 25 "/D6")
  (net 26 "/D5")
  (net 27 "/D4")
  (net 28 "/D3")
  (net 29 "/D2")
  (net 30 "/D1")
  (net 31 "/D0")
  (net 32 "/Clk")
  (net 33 "/Vis")
  (net 34 "/Q7")
  (net 35 "/Q6")
  (net 36 "/Q5")
  (net 37 "/Q4")
  (net 38 "/Q3")
  (net 39 "/Q2")
  (net 40 "/Q1")
  (net 41 "/Q0")
  (net 42 "/Empty")
  (net 43 "/HalfFull")
  (net 44 "/Full")
  (net 45 "/P6")
  (net 46 "/P5")
  (net 47 "/P3")
  (net 48 "/P2")
  (net 49 "/P0")
  (net 50 "/Clk_{pixel}")
  (net 51 "/L4")
  (net 52 "/L5")
  (net 53 "/L6")
  (net 54 "/L7")
  (net 55 "/L3")
  (net 56 "/L2")
  (net 57 "/L1")
  (net 58 "/L0")
  (net 59 "unconnected-(U3-NC_1-Pad1)")
  (net 60 "unconnected-(U3-NC_2-Pad12)")
  (net 61 "unconnected-(U3-Q8-Pad15)")
  (net 62 "unconnected-(U3-NC_3-Pad17)")
  (net 63 "unconnected-(U3-NC_4-Pad27)")
  (net 64 "/U0Rxd")
  (net 65 "/U0Txd")
  (net 66 "/U-")
  (net 67 "/U+")
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (at 141 58)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (property "Sheetfile" "vgaterm-schematics.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 1.524 2.032) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (at 138.438999 73.152 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "vgaterm-schematics.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D1" (at -3.293001 0) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 3 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "VCC") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 138.43 64.008)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (property "Sheetfile" "vgaterm-schematics.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J9" (at 2.54 0) (layer "F.SilkS"))
    (fp_text value "Conn_01x03_Socket" (at 0 7.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 42 "/Empty") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 43 "/HalfFull") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 44 "/Full") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 92.71 80.518)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "vgaterm-schematics.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 2.778 0) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 18 "/Rst") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 2 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x15_P2.54mm_Vertical" (layer "F.Cu")
    (at 102.955 74.422 -90)
    (descr "Through hole straight socket strip, 1x15, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x15 2.54mm single row")
    (property "Sheetfile" "vgaterm-schematics.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x15, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J5" (at 0 -2.77 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x15_Socket" (at 0 38.33 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 17.78) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "/KB_{Tx}") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "/KB_{Rx}") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "/SIO1") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "/~{StartFrame}") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "/CS") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 64 "/U0Rxd") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 65 "/U0Txd") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 66 "/U-") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 67 "/U+") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_15") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x15_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x05_P2.54mm_Horizontal" (layer "F.Cu")
    (at 121.158 80.264 90)
    (descr "Through hole angled socket strip, 2x05, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole angled socket strip THT 2x05 2.54mm double row")
    (property "Sheetfile" "vgaterm-schematics.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J6" (at 2.286 11.176 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x10" (at -5.65 12.93 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -8.315 5.08 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "/DO+") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "/DO-") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at -2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 65 "/U0Txd") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 64 "/U0Rxd") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at -2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at -2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 67 "/U+") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at -2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 66 "/U-") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x05_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 86.36 80.01 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "vgaterm-schematics.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33 -270) (layer "B.SilkS"))
    (fp_text value "Rst" (at 1.016 5.334 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "/Rst") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 138.446 75.692 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "vgaterm-schematics.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at -3.032 0) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 3 "Net-(D1-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm" (layer "F.Cu")
    (at 107.273 62.406 90)
    (descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "vgaterm-schematics.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "8-bit Register, 3-state outputs")
    (property "ki_keywords" "TTL REG DFF DFF8 3State")
    (attr smd)
    (fp_text reference "U4" (at -0.586 -7.747 90) (layer "F.SilkS"))
    (fp_text value "74HCT574" (at 0 7.35 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -4.65 -5.715 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "OE") (pintype "input"))
    (pad "2" smd roundrect (at -4.65 -4.445 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/Q0") (pinfunction "D0") (pintype "input"))
    (pad "3" smd roundrect (at -4.65 -3.175 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/Q1") (pinfunction "D1") (pintype "input"))
    (pad "4" smd roundrect (at -4.65 -1.905 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/Q2") (pinfunction "D2") (pintype "input"))
    (pad "5" smd roundrect (at -4.65 -0.635 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/Q3") (pinfunction "D3") (pintype "input"))
    (pad "6" smd roundrect (at -4.65 0.635 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "/Q4") (pinfunction "D4") (pintype "input"))
    (pad "7" smd roundrect (at -4.65 1.905 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/Q5") (pinfunction "D5") (pintype "input"))
    (pad "8" smd roundrect (at -4.65 3.175 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/Q6") (pinfunction "D6") (pintype "input"))
    (pad "9" smd roundrect (at -4.65 4.445 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/Q7") (pinfunction "D7") (pintype "input"))
    (pad "10" smd roundrect (at -4.65 5.715 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "11" smd roundrect (at 4.65 5.715 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "/Clk_{pixel}") (pinfunction "Cp") (pintype "input"))
    (pad "12" smd roundrect (at 4.65 4.445 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/P7") (pinfunction "Q7") (pintype "tri_state"))
    (pad "13" smd roundrect (at 4.65 3.175 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "/P6") (pinfunction "Q6") (pintype "tri_state"))
    (pad "14" smd roundrect (at 4.65 1.905 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "/P5") (pinfunction "Q5") (pintype "tri_state"))
    (pad "15" smd roundrect (at 4.65 0.635 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/P4") (pinfunction "Q4") (pintype "tri_state"))
    (pad "16" smd roundrect (at 4.65 -0.635 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "/P3") (pinfunction "Q3") (pintype "tri_state"))
    (pad "17" smd roundrect (at 4.65 -1.905 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "/P2") (pinfunction "Q2") (pintype "tri_state"))
    (pad "18" smd roundrect (at 4.65 -3.175 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/P1") (pinfunction "Q1") (pintype "tri_state"))
    (pad "19" smd roundrect (at 4.65 -4.445 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "/P0") (pinfunction "Q0") (pintype "tri_state"))
    (pad "20" smd roundrect (at 4.65 -5.715 90) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x15_P2.54mm_Horizontal" (layer "F.Cu")
    (at 142.24 52.832 -90)
    (descr "Through hole angled socket strip, 1x15, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole angled socket strip THT 1x15 2.54mm single row")
    (property "Sheetfile" "vgaterm-schematics.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x15, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J7" (at -2.794 0 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x15" (at -4.38 38.33 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -5.775 17.78) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "/~{StartFrame}") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 33 "/Vis") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 32 "/Clk") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "/KB_{Tx}") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "/KB_{Rx}") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "/P7") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 45 "/P6") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 46 "/P5") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "/P4") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 47 "/P3") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 48 "/P2") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "/P1") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 49 "/P0") (pinfunction "Pin_15") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x15_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 72.644 78.486)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (property "Sheetfile" "vgaterm-schematics.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at -2.286 -0.508) (layer "F.SilkS"))
    (fp_text value "Conn_01x04" (at 1.27 4.87) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "/DO+") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "/DO-") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 75.9245 54.61 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Product" "https://www.mouser.com/ProductDetail/Samsung-Electro-Mechanics/CL21B106KPQNNNG?qs=yOVawPpwOwmi1gAJqK4H6Q%3D%3D")
    (property "Sheetfile" "vgaterm-schematics.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C2" (at -2.8155 0) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 75.946 57.404 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Product" "https://www.mouser.com/ProductDetail/Samsung-Electro-Mechanics/CL21B106KPQNNNG?qs=yOVawPpwOwmi1gAJqK4H6Q%3D%3D")
    (property "Sheetfile" "vgaterm-schematics.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C4" (at 2.8155 0) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (at 68 56)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (property "Sheetfile" "vgaterm-schematics.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 3.048 -1.524) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm" (layer "F.Cu")
    (at 111.337 75.438 90)
    (descr "TSSOP, 20 Pin (JEDEC MO-153 Var AC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Field5" "")
    (property "Product" "https://www.mouser.com/ProductDetail/Toshiba/74VHCT244AFT?qs=j%252B1pi9TdxUZ3ko%252BkOnpcOg%3D%3D")
    (property "Sheetfile" "vgaterm-schematics.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "8-bit Buffer/Line Driver 3-state")
    (property "ki_keywords" "AHCTMOS BUFFER 3State")
    (attr smd)
    (fp_text reference "U2" (at 0 -4.2 90) (layer "F.SilkS"))
    (fp_text value "74AHCT244" (at 0 4.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.925 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "1OE") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/D0") (pinfunction "1A0") (pintype "input"))
    (pad "3" smd roundrect (at -2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "/L4") (pinfunction "2Y0") (pintype "tri_state"))
    (pad "4" smd roundrect (at -2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/D1") (pinfunction "1A1") (pintype "input"))
    (pad "5" smd roundrect (at -2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "/L5") (pinfunction "2Y1") (pintype "tri_state"))
    (pad "6" smd roundrect (at -2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/D2") (pinfunction "1A2") (pintype "input"))
    (pad "7" smd roundrect (at -2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "/L6") (pinfunction "2Y2") (pintype "tri_state"))
    (pad "8" smd roundrect (at -2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/D3") (pinfunction "1A3") (pintype "input"))
    (pad "9" smd roundrect (at -2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "/L7") (pinfunction "2Y3") (pintype "tri_state"))
    (pad "10" smd roundrect (at -2.8625 2.925 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "11" smd roundrect (at 2.8625 2.925 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/D7") (pinfunction "2A3") (pintype "input"))
    (pad "12" smd roundrect (at 2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "/L3") (pinfunction "1Y3") (pintype "tri_state"))
    (pad "13" smd roundrect (at 2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "/D6") (pinfunction "2A2") (pintype "input"))
    (pad "14" smd roundrect (at 2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "/L2") (pinfunction "1Y2") (pintype "tri_state"))
    (pad "15" smd roundrect (at 2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/D5") (pinfunction "2A1") (pintype "input"))
    (pad "16" smd roundrect (at 2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "/L1") (pinfunction "1Y1") (pintype "tri_state"))
    (pad "17" smd roundrect (at 2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/D4") (pinfunction "2A0") (pintype "input"))
    (pad "18" smd roundrect (at 2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "/L0") (pinfunction "1Y0") (pintype "tri_state"))
    (pad "19" smd roundrect (at 2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "2OE") (pintype "input"))
    (pad "20" smd roundrect (at 2.8625 -2.925 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "plcc32:plcc32-socket" (layer "F.Cu")
    (at 126.3483 65.801)
    (property "Arrow Part Number" "")
    (property "Arrow Price/Stock" "")
    (property "Datasheet_1" "https://www.idt.com/document/dst/7203-7208-datasheet")
    (property "Footprint_1" "PLCC127P1245X1499X356-32N")
    (property "Height" "3.556")
    (property "Manufacturer_Name" "IDT")
    (property "Manufacturer_Part_Number" "IDT7205L12JG")
    (property "Mouser Part Number" "")
    (property "Mouser Price/Stock" "")
    (property "Product" "https://www.jameco.com/z/69802-032-Amphenol-Socket-PLCC-32-Pin-Surface-Mount_71811.html")
    (property "Reference_1" "IC")
    (property "Sheetfile" "vgaterm-schematics.kicad_sch")
    (property "Sheetname" "")
    (property "Value_1" "IDT7205L12JG")
    (property "ki_description" "IDT IDT7205L12JG, FIFO Memory, Dual 72kbit, 8K x 9 bit, Bi-Directional 12ns, 4.5  5.5 V, 32-Pin PLCC")
    (attr smd)
    (fp_text reference "U3" (at -0.4858 -1.855 unlocked) (layer "F.SilkS"))
    (fp_text value "IDT7205L12JG" (at -0.4858 -0.355 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.037502 -6.8375) (size 0.65 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "unconnected-(U3-NC_1-Pad1)") (pinfunction "NC_1") (pintype "passive+no_connect"))
    (pad "2" smd roundrect (at -1.316668 -6.8375) (size 0.65 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/Half") (pinfunction "~{W}") (pintype "passive"))
    (pad "3" smd roundrect (at -2.595834 -6.8375) (size 0.65 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "D8") (pintype "passive"))
    (pad "4" smd roundrect (at -3.875 -6.8375) (size 0.65 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "/L3") (pinfunction "D3") (pintype "passive"))
    (pad "5" smd roundrect (at -5.6133 -5.18) (size 2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "/L2") (pinfunction "D2") (pintype "passive"))
    (pad "6" smd roundrect (at -5.6133 -3.88875) (size 2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "/L1") (pinfunction "D1") (pintype "passive"))
    (pad "7" smd roundrect (at -5.6133 -2.5975) (size 2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "/L0") (pinfunction "D0") (pintype "passive"))
    (pad "8" smd roundrect (at -5.6133 -1.30625) (size 2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "~{XI}") (pintype "passive"))
    (pad "9" smd roundrect (at -5.6133 -0.015) (size 2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "/Full") (pinfunction "~{FF}") (pintype "passive"))
    (pad "10" smd roundrect (at -5.6133 1.27625) (size 2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/Q0") (pinfunction "Q0") (pintype "passive"))
    (pad "11" smd roundrect (at -5.6133 2.5675) (size 2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/Q1") (pinfunction "Q1") (pintype "passive"))
    (pad "12" smd roundrect (at -5.6133 3.85875) (size 2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "unconnected-(U3-NC_2-Pad12)") (pinfunction "NC_2") (pintype "passive+no_connect"))
    (pad "13" smd roundrect (at -5.6133 5.15) (size 2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/Q2") (pinfunction "Q2") (pintype "passive"))
    (pad "14" smd roundrect (at -3.875 6.8375) (size 0.65 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/Q3") (pinfunction "Q3") (pintype "passive"))
    (pad "15" smd roundrect (at -2.595834 6.8375) (size 0.65 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "unconnected-(U3-Q8-Pad15)") (pinfunction "Q8") (pintype "passive+no_connect"))
    (pad "16" smd roundrect (at -1.316668 6.8375) (size 0.65 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "17" smd roundrect (at -0.037502 6.8375) (size 0.65 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "unconnected-(U3-NC_3-Pad17)") (pinfunction "NC_3") (pintype "passive+no_connect"))
    (pad "18" smd roundrect (at 1.241664 6.8375) (size 0.65 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "/Clk_{pixel}") (pinfunction "~{R}") (pintype "passive"))
    (pad "19" smd roundrect (at 2.52083 6.8375) (size 0.65 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "/Q4") (pinfunction "Q4") (pintype "passive"))
    (pad "20" smd roundrect (at 3.8 6.8375) (size 0.65 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/Q5") (pinfunction "Q5") (pintype "passive"))
    (pad "21" smd roundrect (at 5.5117 5.15) (size 2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/Q6") (pinfunction "Q6") (pintype "passive"))
    (pad "22" smd roundrect (at 5.5117 3.85875) (size 2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/Q7") (pinfunction "Q7") (pintype "passive"))
    (pad "23" smd roundrect (at 5.5117 2.5675) (size 2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "/HalfFull") (pinfunction "~{XO}/~{HF}") (pintype "passive"))
    (pad "24" smd roundrect (at 5.5117 1.27625) (size 2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "/Empty") (pinfunction "~{EF}") (pintype "passive"))
    (pad "25" smd roundrect (at 5.5117 -0.015) (size 2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/~{StartFrame}") (pinfunction "~{RS}") (pintype "passive"))
    (pad "26" smd roundrect (at 5.5117 -1.30625) (size 2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "~{FL}/~{RT}") (pintype "passive"))
    (pad "27" smd roundrect (at 5.5117 -2.5975) (size 2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "unconnected-(U3-NC_4-Pad27)") (pinfunction "NC_4") (pintype "passive+no_connect"))
    (pad "28" smd roundrect (at 5.5117 -3.88875) (size 2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "/L7") (pinfunction "D7") (pintype "passive"))
    (pad "29" smd roundrect (at 5.5117 -5.18) (size 2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "/L6") (pinfunction "D6") (pintype "passive"))
    (pad "30" smd roundrect (at 3.8 -6.8375) (size 0.65 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "/L5") (pinfunction "D5") (pintype "passive"))
    (pad "31" smd roundrect (at 2.52083 -6.8375) (size 0.65 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "/L4") (pinfunction "D4") (pintype "passive"))
    (pad "32" smd roundrect (at 1.241664 -6.8375) (size 0.65 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "VCC") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 135.382 83.058 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Product" "https://www.mouser.com/ProductDetail/Samsung-Electro-Mechanics/CL21B106KPQNNNG?qs=yOVawPpwOwmi1gAJqK4H6Q%3D%3D")
    (property "Sheetfile" "vgaterm-schematics.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C1" (at -3.048 0) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 2.188) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 103.886 78.2535 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "vgaterm-schematics.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x15_P2.54mm_Vertical" (layer "F.Cu")
    (at 102.955 51.562 -90)
    (descr "Through hole straight socket strip, 1x15, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x15 2.54mm single row")
    (property "Sheetfile" "vgaterm-schematics.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x15, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J4" (at 2.54 -0.169 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x15_Socket" (at 0 38.33 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 17.78) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "unconnected-(J4-Pin_2-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "unconnected-(J4-Pin_3-Pad3)") (pinfunction "Pin_3") (pintype "passive+no_connect"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "/Rst") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "/SIO3") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "/SIO2") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "/SCLK") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "/SIO0") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "unconnected-(J4-Pin_11-Pad11)") (pinfunction "Pin_11") (pintype "passive+no_connect"))
    (pad "12" thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 20 "unconnected-(J4-Pin_12-Pad12)") (pinfunction "Pin_12") (pintype "passive+no_connect"))
    (pad "13" thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_15") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x15_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (at 139 80)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (property "Sheetfile" "vgaterm-schematics.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 2.54 0) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 137 60 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Product" "https://www.mouser.com/ProductDetail/Samsung-Electro-Mechanics/CL10B104KA85PNC?qs=xZ%2FP%252Ba9zWqabsWCtlKJ0Xw%3D%3D")
    (property "Sheetfile" "vgaterm-schematics.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C7" (at 0.96 -1.938 -180) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.68 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (at 68 80)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (property "Sheetfile" "vgaterm-schematics.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at -1.016 -2.032) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 68.5585 64.262 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "vgaterm-schematics.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C3" (at -3.048 0) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (at 102.616 60.198 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Pruduct" "https://www.mouser.com/ProductDetail/Samsung-Electro-Mechanics/CL10B104KA85PNC?qs=xZ%2FP%252Ba9zWqabsWCtlKJ0Xw%3D%3D")
    (property "Sheetfile" "vgaterm-schematics.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C8" (at 2.8155 -0.508) (layer "B.SilkS"))
    (fp_text value "100nF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 2 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-24_W7.62mm_Socket" (layer "B.Cu")
    (at 68.157 60.198 -90)
    (descr "24-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (property "Sheetfile" "vgaterm-schematics.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Programmable Logic Array, DIP-20/SOIC-20/PLCC-20")
    (property "ki_keywords" "GAL PLD 22V10")
    (attr through_hole)
    (fp_text reference "U1" (at 10.414 0.085 90) (layer "B.SilkS"))
    (fp_text value "GAL22V10" (at 3.81 -30.27 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 -13.97 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "/SCLK") (pinfunction "I1/CLK") (pintype "input"))
    (pad "2" thru_hole oval (at 0 -2.54 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "/Vis") (pinfunction "I2") (pintype "input"))
    (pad "3" thru_hole oval (at 0 -5.08 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "/Clk") (pinfunction "I3") (pintype "input"))
    (pad "4" thru_hole oval (at 0 -7.62 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "/~{StartFrame}") (pinfunction "I4/PD") (pintype "input"))
    (pad "5" thru_hole oval (at 0 -10.16 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "/SIO0") (pinfunction "I5") (pintype "input"))
    (pad "6" thru_hole oval (at 0 -12.7 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "/SIO1") (pinfunction "I6") (pintype "input"))
    (pad "7" thru_hole oval (at 0 -15.24 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "/SIO2") (pinfunction "I7") (pintype "input"))
    (pad "8" thru_hole oval (at 0 -17.78 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "/SIO3") (pinfunction "I8") (pintype "input"))
    (pad "9" thru_hole oval (at 0 -20.32 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "I9") (pintype "input"))
    (pad "10" thru_hole oval (at 0 -22.86 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "I10") (pintype "input"))
    (pad "11" thru_hole oval (at 0 -25.4 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "I11") (pintype "input"))
    (pad "12" thru_hole oval (at 0 -27.94 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "13" thru_hole oval (at 7.62 -27.94 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "I12") (pintype "input"))
    (pad "14" thru_hole oval (at 7.62 -25.4 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 24 "/D7") (pinfunction "IO10") (pintype "tri_state"))
    (pad "15" thru_hole oval (at 7.62 -22.86 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "/D6") (pinfunction "IO9") (pintype "tri_state"))
    (pad "16" thru_hole oval (at 7.62 -20.32 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 26 "/D5") (pinfunction "IO8") (pintype "tri_state"))
    (pad "17" thru_hole oval (at 7.62 -17.78 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "/D4") (pinfunction "IO7") (pintype "tri_state"))
    (pad "18" thru_hole oval (at 7.62 -15.24 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 28 "/D3") (pinfunction "IO6") (pintype "tri_state"))
    (pad "19" thru_hole oval (at 7.62 -12.7 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 29 "/D2") (pinfunction "IO5") (pintype "tri_state"))
    (pad "20" thru_hole oval (at 7.62 -10.16 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "/D1") (pinfunction "IO4") (pintype "tri_state"))
    (pad "21" thru_hole oval (at 7.62 -7.62 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "/D0") (pinfunction "I03") (pintype "tri_state"))
    (pad "22" thru_hole oval (at 7.62 -5.08 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 50 "/Clk_{pixel}") (pinfunction "IO2") (pintype "tri_state"))
    (pad "23" thru_hole oval (at 7.62 -2.54 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "/Half") (pinfunction "IO1") (pintype "tri_state"))
    (pad "24" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-24_W7.62mm_Socket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 65.278 53.34) (end 65.278 49.276)
    (layer "Edge.Cuts"))
  (gr_line (start 143.002 84.836) (end 144.018 83.82)
    (layer "Edge.Cuts"))
  (gr_line (start 65.278 49.276) (end 66.04 48.514)
    (layer "Edge.Cuts"))
  (gr_line (start 65.278 83.82) (end 66.294 84.836)
    (layer "Edge.Cuts"))
  (gr_line (start 144.018 49.022) (end 143.51 48.514)
    (layer "Edge.Cuts"))
  (gr_line (start 143.51 48.514) (end 66.04 48.514)
    (layer "Edge.Cuts"))
  (gr_line (start 65.278 53.34) (end 65.278 83.82)
    (layer "Edge.Cuts"))
  (gr_line (start 144.018 83.82) (end 144.018 49.022)
    (layer "Edge.Cuts"))
  (gr_line (start 143.002 84.836) (end 66.294 84.836)
    (layer "Edge.Cuts"))
  (gr_text "~{Full}" (at 136.144 70.104) (layer "B.SilkS"))
  (gr_text "~{Empty}" (at 136.144 64.516) (layer "B.SilkS"))
  (gr_text "DO- U0Txd  VCC VCC U-\nDO+ GND U0Rxd GND U+" (at 118.364 75.946 180) (layer "B.SilkS"))
  (gr_text "P0 P1 P2 P3 P4 P5 P6 P7 KbRx KbTx Clk Vis ~{Start} GND Vcc" (at 105.664 49.276 180) (layer "B.SilkS"))
  (gr_text "~{HalfFull}" (at 136.144 67.31) (layer "B.SilkS"))
  (gr_text "VCC" (at 70.866 83.82) (layer "F.SilkS"))
  (gr_text "To Dev \nBoard\nUSB" (at 77.724 84.582) (layer "F.SilkS"))
  (gr_text "C" (at 137.414 56.642) (layer "F.SilkS"))
  (gr_text "Designed by Seth & Eric\nof Rustbox" (at 84.074 84.074) (layer "F.SilkS"))
  (gr_text "DO-" (at 74.168 83.82) (layer "F.SilkS"))
  (gr_text "Vgaterm - 2023-10-07" (at 81.026 77.47) (layer "F.SilkS"))
  (gr_text "DO+" (at 74.168 76.962) (layer "F.SilkS"))
  (gr_text "A" (at 117.856 83.82) (layer "F.SilkS"))
  (gr_text "GND" (at 70.866 76.962) (layer "F.SilkS"))
  (gr_text "B" (at 110.744 84.074) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 142.24 52.832) (xy 144.018 52.832))
    (height -12.192)
    (gr_text "1.7780 mm" (at 143.129 39.49) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 65.278 48.514) (xy 106.68 48.514))
    (height -7.62)
    (gr_text "41.4020 mm" (at 85.979 39.744) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 65.278 84.836) (xy 144.018 84.836))
    (height 3.047999)
    (gr_text "78.7400 mm" (at 104.648 86.733999) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 144.018 84.328) (xy 131.318 84.328))
    (height -5.842)
    (gr_text "12.7000 mm" (at 137.668 89.02) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 147.574 48.514) (xy 147.574 84.836))
    (height -1.733691)
    (gr_text "36.3220 mm" (at 148.157691 66.675 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 2) (net_name "VCC") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 58.928 92.964)
        (xy 148.082 92.71)
        (xy 148.082 37.592)
        (xy 59.69 37.846)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 58.928 92.456)
        (xy 147.828 92.71)
        (xy 147.828 37.592)
        (xy 59.436 37.846)
      )
    )
  )
)
