(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~87~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 101)
    (zones 0)
    (modules 5)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.85 0.85)
    (pad_drill 0.5)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 152.4 101.6)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 /MAG~RST)
  (net 4 /SDA)
  (net 5 /SCL)
  (net 6 /INT)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /INT)
    (add_net /MAG~RST)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
  )
  (module KwanSystems:LGA-14L (layer F.Cu) (tedit 5F3D6253)
    (at 154.686 98.425 90)
    (fp_text reference U103 (at -0.4 -0.15 270) (layer F.Fab))
    (fp_text value LSM6DSO (at 2.54 0 90) (layer F.Fab) hide)
    (fp_text user Z (at -0.45 0.25 90) (layer Dwgs.User))
    (fp_text user X (at 0.35 0.25 90) (layer Dwgs.User))
    (fp_text user Y (at -0.4 -0.5 90) (layer Dwgs.User))
    (pad 1 smd rect (at -1.1625 -0.75 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 2 smd rect (at -1.1625 -0.25 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 3 smd rect (at -1.1625 0.25 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 4 smd rect (at -1.1625 0.75 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 /INT) (solder_mask_margin 0.0508))
    (pad 5 smd rect (at -0.5 0.9125 180) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3) (solder_mask_margin 0.0508))
    (pad 6 smd rect (at 0 0.9125 180) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 7 smd rect (at 0.5 0.9125 180) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 8 smd rect (at 1.1625 0.75 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3) (solder_mask_margin 0.0508))
    (pad 9 smd rect (at 1.1625 0.25 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.0508))
    (pad 10 smd rect (at 1.1625 -0.25 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.0508))
    (pad 11 smd rect (at 1.1625 -0.75 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.0508))
    (pad 12 smd rect (at 0.5 -0.9125) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3) (solder_mask_margin 0.0508))
    (pad 13 smd rect (at 0 -0.9125) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 /SCL) (solder_mask_margin 0.0508))
    (pad 14 smd rect (at -0.5 -0.9125) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /SDA) (solder_mask_margin 0.0508))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/Bosch_LGA-14_3x2.5mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 154.432 96.266 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C101 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 2.2u (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KwanSystems:BME280 (layer F.Cu) (tedit 5F3D9117)
    (at 157.353 98.425 90)
    (fp_text reference U102 (at 0 0 90) (layer F.Fab))
    (fp_text value BME280 (at 0 -2.5 90) (layer F.Fab))
    (pad 6 smd rect (at -1.025 0.325 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 7 smd rect (at -1.025 -0.325 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -1.025 0.975 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.025 0.975 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 5 /SCL))
    (pad 1 smd rect (at 1.025 -0.975 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.025 0.325 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 4 /SDA))
    (pad 8 smd rect (at -1.025 -0.975 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 1.025 -0.325 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model /home/jeppesen/workspace/kicad/KwanSystems.pretty/BME280--3DModel-STEP-56544.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module Connector_PinHeader_1.00mm:PinHeader_1x06_P1.00mm_Vertical (layer F.Cu) (tedit 5F514583)
    (at 152.4 95.8342)
    (descr "Through hole straight pin header, 1x06, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x06 1.00mm single row")
    (fp_text reference J101 (at 0 -1.56) (layer F.SilkS) hide)
    (fp_text value 01x06 (at 0 6.56) (layer F.Fab) hide)
    (fp_text user %R (at 4.0132 3.937 90) (layer F.Fab) hide)
    (pad 6 thru_hole oval (at 0 5) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 /MAG~RST))
    (pad 5 thru_hole oval (at 0 4) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 /INT))
    (pad 4 thru_hole oval (at 0 3) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 /SDA))
    (pad 3 thru_hole oval (at 0 2) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 /SCL))
    (pad 2 thru_hole oval (at 0 1) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 +3V3))
  )
  (module KwanSystems:AK09970 (layer B.Cu) (tedit 5F3D3F3B)
    (at 156.21 98.552)
    (fp_text reference U101 (at 0 -0.3) (layer Dwgs.User))
    (fp_text value AK09970 (at 0.2 0.3) (layer Dwgs.User))
    (fp_text user Z (at -0.6 -0.7) (layer Dwgs.User))
    (fp_text user Y (at -0.7 0.9) (layer Dwgs.User))
    (fp_text user X (at 0.8 -0.7) (layer Dwgs.User))
    (pad 16 smd rect (at -1.5375 -0.75 90) (size 0.3 0.575) (layers B.Cu B.Paste B.Mask)
      (net 3 /MAG~RST))
    (pad 15 smd rect (at -1.5375 -0.25 90) (size 0.3 0.575) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 14 smd rect (at -1.5375 0.25 90) (size 0.3 0.575) (layers B.Cu B.Paste B.Mask))
    (pad 13 smd rect (at -1.5375 0.75 90) (size 0.3 0.575) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 12 smd rect (at -0.75 1.5375 180) (size 0.3 0.575) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 11 smd rect (at -0.25 1.5375 180) (size 0.3 0.575) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd rect (at 0.25 1.5375 180) (size 0.3 0.575) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at 0.75 1.5375 180) (size 0.3 0.575) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at 1.5375 0.75 270) (size 0.3 0.575) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at 1.5375 0.25 270) (size 0.3 0.575) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at 1.5375 -0.25 270) (size 0.3 0.575) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 1.5375 -0.75 270) (size 0.3 0.575) (layers B.Cu B.Paste B.Mask)
      (net 4 /SDA))
    (pad 4 smd rect (at 0.75 -1.5375) (size 0.3 0.575) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at 0.25 -1.5375) (size 0.3 0.575) (layers B.Cu B.Paste B.Mask)
      (net 5 /SCL))
    (pad 2 smd rect (at -0.25 -1.5375) (size 0.3 0.575) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 1 smd rect (at -0.75 -1.5375) (size 0.3 0.575) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/Bosch_LGA-8_3x3mm_P0.8mm_ClockwisePinNumbering.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (gr_line (start 152.4 95.25) (end 152.4 101.6) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 158.75 101.6) (end 152.4 101.6) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 158.75 95.25) (end 158.75 101.6) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 152.4 95.25) (end 158.75 95.25) (layer Edge.Cuts) (width 0.0254))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.75 101.6) (xy 152.4 101.6) (xy 152.4 95.25) (xy 158.75 95.25)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.75 101.6) (xy 152.4 101.6) (xy 152.4 95.25) (xy 158.75 95.25)
      )
    )
  )
)
