(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 143)
    (no_connects 1)
    (area 120.926099 87.428599 176.076101 122.578601)
    (thickness 1.6)
    (drawings 429)
    (tracks 629)
    (zones 0)
    (modules 58)
    (nets 102)
  )
  (page A4)
  (title_block
    (title "\"Cameo\" 5V level adapter cape for PocketBeagle")
    (date 2018-04-10)
    (rev NaN)
    (comment 1 London)
    (comment 2 stepleton@gmail.com)
    (comment 3 "Tom Stepleton")
    (comment 4 "Forfeited into the public domain with NO WARRANTY")
  )
  (layers
    (0 Top signal)
    (1 VDD signal hide)
    (2 DigitalGND signal hide)
    (31 Bottom signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.015)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.27 1.27)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0254)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x0103c_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory plots))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 USB_DC)
  (net 3 VDD_5V)
  (net 4 VDD_3V3B)
  (net 5 SYS_5V)
  (net 6 VIN.BAT)
  (net 7 "/(U1.P12)PWM1A")
  (net 8 "/(U1.T16)")
  (net 9 "/(U1.P5)GPIO-0.23")
  (net 10 "/(U1.R15)")
  (net 11 "/(U1.P15)UART4.RX")
  (net 12 "/(U1.T15)")
  (net 13 "/(U1.R16)UART4.TX")
  (net 14 "/(U1.N14)")
  (net 15 "/(U1.B11)I2C1.SCL")
  (net 16 "/(U1.R13)")
  (net 17 "/(U1.A11)I2C1.SDA")
  (net 18 "/(U1.T11)PWR.BTN")
  (net 19 /BAT.TEMP)
  (net 20 "/(U1.T7)")
  (net 21 "/(U1.P7)PRU-0.15")
  (net 22 "/(U1.T5)")
  (net 23 "/(U1.R7)")
  (net 24 "/(U1.T6)PRU-0.14")
  (net 25 "/(U1.P6)")
  (net 26 "/(U1.C13)SPI1.MOSI")
  (net 27 "/(U1.R11)RESET#")
  (net 28 "/(U1.C12)SPI1.MISO")
  (net 29 "/(U1.C3)PRU-0.6")
  (net 30 "/(U1.C5)SPI1.CLK")
  (net 31 "/(U1.B1)PRU-0.3")
  (net 32 "/(U1.A4)SPI1.CS")
  (net 33 "/(U1.B2)PRU-0.2")
  (net 34 "/(U1.R6)")
  (net 35 "/(U1.B3)PRU-0.5")
  (net 36 "/(U1.F3)AIN5~3.3V")
  (net 37 "/(U1.N13)AIN7~1.8V")
  (net 38 "/(U1.A1)PWM0A")
  (net 39 "/(U1.F1)")
  (net 40 "/(U1.R5)GPIO-0.26")
  (net 41 "/(U1.A2)PRU-0.1")
  (net 42 "/(U1.A12)UART0.RX")
  (net 43 "/(U1.A3)PRU-0.4")
  (net 44 "/(U1.B12)UART0.TX")
  (net 45 "/(U1.C4)PRU-0.7")
  (net 46 "/(U1.A10)I2C2.SCL")
  (net 47 "/(U1.C7)AIN4~1.8V")
  (net 48 "/(U1.B10)I2C2.SDA")
  (net 49 "/(U1.C6)AIN3~1.8V")
  (net 50 "/(U1.B6)AIN2~1.8V")
  (net 51 "/(U1.B8)AIN1~1.8V")
  (net 52 "/(U1.B4)PRU-0.16")
  (net 53 "/(U1.A8)AIN0~1.8V")
  (net 54 "/(U1.B7)VREF+")
  (net 55 "/(U1.B9)VREF-")
  (net 56 "/(U1.L14)USB1.ID")
  (net 57 "/(U1.B14)SPI0.MOSI")
  (net 58 "/(U1.L15)USB1.D+")
  (net 59 "/(U1.B13)SPI0.MISO")
  (net 60 "/(U1.L16)USB1.D-")
  (net 61 "/(U1.A13)SPI0.CLK")
  (net 62 "/(U1.A14)SPI0.CS")
  (net 63 "/(U1.M15)USB1.VBUS")
  (net 64 "/(U1.E1)")
  (net 65 "/(U1.M14)USB1.DRVVBUS")
  (net 66 "/(U1.F2)AIN6~3.3V")
  (net 67 /PEX1)
  (net 68 "Net-(JP1-Pad2)")
  (net 69 /PEX2)
  (net 70 "Net-(JP18-Pad2)")
  (net 71 /PR/~W)
  (net 72 "Net-(JP19-Pad2)")
  (net 73 /PD0)
  (net 74 "Net-(JP20-Pad2)")
  (net 75 /PD1)
  (net 76 "Net-(JP21-Pad2)")
  (net 77 /PD2)
  (net 78 "Net-(JP22-Pad2)")
  (net 79 /PD5)
  (net 80 "Net-(JP23-Pad2)")
  (net 81 /PD6)
  (net 82 "Net-(JP24-Pad2)")
  (net 83 /PD7)
  (net 84 "Net-(JP25-Pad2)")
  (net 85 "Net-(JP10-Pad1)")
  (net 86 /PD4)
  (net 87 "Net-(JP11-Pad1)")
  (net 88 /PD3)
  (net 89 "Net-(JP12-Pad1)")
  (net 90 /~PPARITY)
  (net 91 "Net-(JP13-Pad1)")
  (net 92 /~PCMD)
  (net 93 "Net-(JP14-Pad1)")
  (net 94 /~PBSY)
  (net 95 "Net-(JP15-Pad1)")
  (net 96 /~PSTRB)
  (net 97 "Net-(JP16-Pad1)")
  (net 98 /PEX3)
  (net 99 "Net-(P3-Pad1)")
  (net 100 "Net-(P3-Pad13)")
  (net 101 "Net-(P3-Pad16)")
  (net_class Default "This is the default net class."
    (clearance 0.015)
    (trace_width 0.254)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "/(U1.A1)PWM0A")
    (add_net "/(U1.A10)I2C2.SCL")
    (add_net "/(U1.A11)I2C1.SDA")
    (add_net "/(U1.A12)UART0.RX")
    (add_net "/(U1.A13)SPI0.CLK")
    (add_net "/(U1.A14)SPI0.CS")
    (add_net "/(U1.A2)PRU-0.1")
    (add_net "/(U1.A3)PRU-0.4")
    (add_net "/(U1.A4)SPI1.CS")
    (add_net "/(U1.A8)AIN0~1.8V")
    (add_net "/(U1.B1)PRU-0.3")
    (add_net "/(U1.B10)I2C2.SDA")
    (add_net "/(U1.B11)I2C1.SCL")
    (add_net "/(U1.B12)UART0.TX")
    (add_net "/(U1.B13)SPI0.MISO")
    (add_net "/(U1.B14)SPI0.MOSI")
    (add_net "/(U1.B2)PRU-0.2")
    (add_net "/(U1.B3)PRU-0.5")
    (add_net "/(U1.B4)PRU-0.16")
    (add_net "/(U1.B6)AIN2~1.8V")
    (add_net "/(U1.B7)VREF+")
    (add_net "/(U1.B8)AIN1~1.8V")
    (add_net "/(U1.B9)VREF-")
    (add_net "/(U1.C12)SPI1.MISO")
    (add_net "/(U1.C13)SPI1.MOSI")
    (add_net "/(U1.C3)PRU-0.6")
    (add_net "/(U1.C4)PRU-0.7")
    (add_net "/(U1.C5)SPI1.CLK")
    (add_net "/(U1.C6)AIN3~1.8V")
    (add_net "/(U1.C7)AIN4~1.8V")
    (add_net "/(U1.E1)")
    (add_net "/(U1.F1)")
    (add_net "/(U1.F2)AIN6~3.3V")
    (add_net "/(U1.F3)AIN5~3.3V")
    (add_net "/(U1.L14)USB1.ID")
    (add_net "/(U1.L15)USB1.D+")
    (add_net "/(U1.L16)USB1.D-")
    (add_net "/(U1.M14)USB1.DRVVBUS")
    (add_net "/(U1.M15)USB1.VBUS")
    (add_net "/(U1.N13)AIN7~1.8V")
    (add_net "/(U1.N14)")
    (add_net "/(U1.P12)PWM1A")
    (add_net "/(U1.P15)UART4.RX")
    (add_net "/(U1.P5)GPIO-0.23")
    (add_net "/(U1.P6)")
    (add_net "/(U1.P7)PRU-0.15")
    (add_net "/(U1.R11)RESET#")
    (add_net "/(U1.R13)")
    (add_net "/(U1.R15)")
    (add_net "/(U1.R16)UART4.TX")
    (add_net "/(U1.R5)GPIO-0.26")
    (add_net "/(U1.R6)")
    (add_net "/(U1.R7)")
    (add_net "/(U1.T11)PWR.BTN")
    (add_net "/(U1.T15)")
    (add_net "/(U1.T16)")
    (add_net "/(U1.T5)")
    (add_net "/(U1.T6)PRU-0.14")
    (add_net "/(U1.T7)")
    (add_net /BAT.TEMP)
    (add_net /PD0)
    (add_net /PD1)
    (add_net /PD2)
    (add_net /PD3)
    (add_net /PD4)
    (add_net /PD5)
    (add_net /PD6)
    (add_net /PD7)
    (add_net /PEX1)
    (add_net /PEX2)
    (add_net /PEX3)
    (add_net /PR/~W)
    (add_net /~PBSY)
    (add_net /~PCMD)
    (add_net /~PPARITY)
    (add_net /~PSTRB)
    (add_net GND)
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(JP10-Pad1)")
    (add_net "Net-(JP11-Pad1)")
    (add_net "Net-(JP12-Pad1)")
    (add_net "Net-(JP13-Pad1)")
    (add_net "Net-(JP14-Pad1)")
    (add_net "Net-(JP15-Pad1)")
    (add_net "Net-(JP16-Pad1)")
    (add_net "Net-(JP18-Pad2)")
    (add_net "Net-(JP19-Pad2)")
    (add_net "Net-(JP20-Pad2)")
    (add_net "Net-(JP21-Pad2)")
    (add_net "Net-(JP22-Pad2)")
    (add_net "Net-(JP23-Pad2)")
    (add_net "Net-(JP24-Pad2)")
    (add_net "Net-(JP25-Pad2)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad13)")
    (add_net "Net-(P3-Pad16)")
    (add_net SYS_5V)
    (add_net USB_DC)
    (add_net VDD_3V3B)
    (add_net VDD_5V)
    (add_net VIN.BAT)
  )
  (module "PocketBeagle.pretty:TH-2X18-(35MIL-DIA)-W_O-SILK" (layer Top) (tedit 59924F19)
    (at 148.5011 117.7036)
    (attr virtual)
    (fp_text reference P1 (at -18.68678 3.34518) (layer F.SilkS))
    (fp_text value ~ (at 0 0) (layer F.SilkS))
    (pad 36 thru_hole circle (at 21.59 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 38 "/(U1.A1)PWM0A"))
    (pad 35 thru_hole circle (at 21.59 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 39 "/(U1.F1)"))
    (pad 34 thru_hole circle (at 19.05 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 40 "/(U1.R5)GPIO-0.26"))
    (pad 33 thru_hole circle (at 19.05 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 41 "/(U1.A2)PRU-0.1"))
    (pad 32 thru_hole circle (at 16.51 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 42 "/(U1.A12)UART0.RX"))
    (pad 31 thru_hole circle (at 16.51 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 43 "/(U1.A3)PRU-0.4"))
    (pad 30 thru_hole circle (at 13.97 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 44 "/(U1.B12)UART0.TX"))
    (pad 29 thru_hole circle (at 13.97 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 45 "/(U1.C4)PRU-0.7"))
    (pad 28 thru_hole circle (at 11.43 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 46 "/(U1.A10)I2C2.SCL"))
    (pad 27 thru_hole circle (at 11.43 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 47 "/(U1.C7)AIN4~1.8V"))
    (pad 26 thru_hole circle (at 8.89 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 48 "/(U1.B10)I2C2.SDA"))
    (pad 25 thru_hole circle (at 8.89 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 49 "/(U1.C6)AIN3~1.8V"))
    (pad 24 thru_hole circle (at 6.35 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 SYS_5V))
    (pad 23 thru_hole circle (at 6.35 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 50 "/(U1.B6)AIN2~1.8V"))
    (pad 22 thru_hole circle (at 3.81 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 21 thru_hole circle (at 3.81 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 51 "/(U1.B8)AIN1~1.8V"))
    (pad 20 thru_hole circle (at 1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 52 "/(U1.B4)PRU-0.16"))
    (pad 19 thru_hole circle (at 1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 53 "/(U1.A8)AIN0~1.8V"))
    (pad 18 thru_hole circle (at -1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 54 "/(U1.B7)VREF+"))
    (pad 17 thru_hole circle (at -1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 55 "/(U1.B9)VREF-"))
    (pad 16 thru_hole circle (at -3.81 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 15 thru_hole circle (at -3.81 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 14 thru_hole circle (at -6.35 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 VDD_3V3B))
    (pad 13 thru_hole circle (at -6.35 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 56 "/(U1.L14)USB1.ID"))
    (pad 12 thru_hole circle (at -8.89 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 57 "/(U1.B14)SPI0.MOSI"))
    (pad 11 thru_hole circle (at -8.89 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 58 "/(U1.L15)USB1.D+"))
    (pad 10 thru_hole circle (at -11.43 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 59 "/(U1.B13)SPI0.MISO"))
    (pad 9 thru_hole circle (at -11.43 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 60 "/(U1.L16)USB1.D-"))
    (pad 8 thru_hole circle (at -13.97 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 61 "/(U1.A13)SPI0.CLK"))
    (pad 7 thru_hole circle (at -13.97 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 USB_DC))
    (pad 6 thru_hole circle (at -16.51 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 62 "/(U1.A14)SPI0.CS"))
    (pad 5 thru_hole circle (at -16.51 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 63 "/(U1.M15)USB1.VBUS"))
    (pad 4 thru_hole circle (at -19.05 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 64 "/(U1.E1)"))
    (pad 3 thru_hole circle (at -19.05 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 65 "/(U1.M14)USB1.DRVVBUS"))
    (pad 2 thru_hole circle (at -21.59 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 66 "/(U1.F2)AIN6~3.3V"))
    (pad 1 thru_hole rect (at -21.59 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 VDD_5V))
  )
  (module "PocketBeagle.pretty:TH-2X18-(35MIL-DIA)-W_O-SILK" (layer Top) (tedit 59924F19)
    (at 148.5011 92.3036)
    (attr virtual)
    (fp_text reference P2 (at -18.6055 -3.15468 180) (layer F.SilkS))
    (fp_text value ~ (at 0 0) (layer F.SilkS))
    (pad 36 thru_hole circle (at 21.59 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 37 "/(U1.N13)AIN7~1.8V"))
    (pad 35 thru_hole circle (at 21.59 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 36 "/(U1.F3)AIN5~3.3V"))
    (pad 34 thru_hole circle (at 19.05 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 35 "/(U1.B3)PRU-0.5"))
    (pad 33 thru_hole circle (at 19.05 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 34 "/(U1.R6)"))
    (pad 32 thru_hole circle (at 16.51 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 33 "/(U1.B2)PRU-0.2"))
    (pad 31 thru_hole circle (at 16.51 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 32 "/(U1.A4)SPI1.CS"))
    (pad 30 thru_hole circle (at 13.97 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 31 "/(U1.B1)PRU-0.3"))
    (pad 29 thru_hole circle (at 13.97 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 30 "/(U1.C5)SPI1.CLK"))
    (pad 28 thru_hole circle (at 11.43 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 29 "/(U1.C3)PRU-0.6"))
    (pad 27 thru_hole circle (at 11.43 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 28 "/(U1.C12)SPI1.MISO"))
    (pad 26 thru_hole circle (at 8.89 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 27 "/(U1.R11)RESET#"))
    (pad 25 thru_hole circle (at 8.89 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 26 "/(U1.C13)SPI1.MOSI"))
    (pad 24 thru_hole circle (at 6.35 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 25 "/(U1.P6)"))
    (pad 23 thru_hole circle (at 6.35 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 VDD_3V3B))
    (pad 22 thru_hole circle (at 3.81 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 24 "/(U1.T6)PRU-0.14"))
    (pad 21 thru_hole circle (at 3.81 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 20 thru_hole circle (at 1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 "/(U1.R7)"))
    (pad 19 thru_hole circle (at 1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 22 "/(U1.T5)"))
    (pad 18 thru_hole circle (at -1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 21 "/(U1.P7)PRU-0.15"))
    (pad 17 thru_hole circle (at -1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 20 "/(U1.T7)"))
    (pad 16 thru_hole circle (at -3.81 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 19 /BAT.TEMP))
    (pad 15 thru_hole circle (at -3.81 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 14 thru_hole circle (at -6.35 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 VIN.BAT))
    (pad 13 thru_hole circle (at -6.35 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 SYS_5V))
    (pad 12 thru_hole circle (at -8.89 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 18 "/(U1.T11)PWR.BTN"))
    (pad 11 thru_hole circle (at -8.89 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 "/(U1.A11)I2C1.SDA"))
    (pad 10 thru_hole circle (at -11.43 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 "/(U1.R13)"))
    (pad 9 thru_hole circle (at -11.43 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 15 "/(U1.B11)I2C1.SCL"))
    (pad 8 thru_hole circle (at -13.97 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 "/(U1.N14)"))
    (pad 7 thru_hole circle (at -13.97 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 "/(U1.R16)UART4.TX"))
    (pad 6 thru_hole circle (at -16.51 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 "/(U1.T15)"))
    (pad 5 thru_hole circle (at -16.51 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 "/(U1.P15)UART4.RX"))
    (pad 4 thru_hole circle (at -19.05 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 "/(U1.R15)"))
    (pad 3 thru_hole circle (at -19.05 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 "/(U1.P5)GPIO-0.23"))
    (pad 2 thru_hole circle (at -21.59 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 "/(U1.T16)"))
    (pad 1 thru_hole rect (at -21.59 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 "/(U1.P12)PWM1A"))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer Top) (tedit 5ACD4E9D)
    (at 123.19 113.665 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.524 270) (layer F.SilkS))
    (fp_text value 0.1 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 4 VDD_3V3B))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer Top) (tedit 5ACD4EA4)
    (at 123.444 102.489 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 1.524 90) (layer F.SilkS))
    (fp_text value 0.1 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 5 SYS_5V))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer Top) (tedit 5ACD4EB0)
    (at 168.402 113.665 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.524 270) (layer F.SilkS))
    (fp_text value 0.1 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 4 VDD_3V3B))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer Top) (tedit 5ACD4EB5)
    (at 168.783 102.489 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 1.524 90) (layer F.SilkS))
    (fp_text value 0.1 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 5 SYS_5V))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4C80)
    (at 127.127 99.187 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP1 (at 3.302 -0.381 90) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 67 /PEX1))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 68 "Net-(JP1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4C6A)
    (at 132.461 99.187 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP2 (at 3.302 -0.381 90) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 69 /PEX2))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 70 "Net-(JP18-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4C51)
    (at 137.795 99.187 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP3 (at 3.302 -0.381 90) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 71 /PR/~W))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 72 "Net-(JP19-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4C3E)
    (at 143.002 99.187 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP4 (at 3.302 -0.381 90) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 73 /PD0))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 74 "Net-(JP20-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4C11)
    (at 148.336 99.187 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP5 (at 3.302 -0.381 90) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 75 /PD1))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 76 "Net-(JP21-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4BF7)
    (at 153.67 99.187 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP6 (at 3.302 -0.381 90) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 77 /PD2))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 78 "Net-(JP22-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4BD5)
    (at 159.004 99.187 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP7 (at 3.302 -0.381 90) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 79 /PD5))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 80 "Net-(JP23-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4BBA)
    (at 164.211 99.187 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP8 (at 3.302 -0.381 90) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 81 /PD6))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 82 "Net-(JP24-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4B4F)
    (at 172.72 99.187 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP9 (at 3.048 0.508 90) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 83 /PD7))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 84 "Net-(JP25-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4D33)
    (at 163.83 110.871 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP10 (at -3.683 -0.127 90) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 85 "Net-(JP10-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 86 /PD4))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4DB7)
    (at 158.623 110.871 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP11 (at -3.683 -0.127 90) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 87 "Net-(JP11-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 88 /PD3))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4DFD)
    (at 153.416 110.871 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP12 (at -3.683 0.127 90) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 89 "Net-(JP12-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 90 /~PPARITY))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4E29)
    (at 148.209 110.871 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP13 (at -3.683 0.254 90) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 91 "Net-(JP13-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 92 /~PCMD))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4DDE)
    (at 143.002 110.871 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP14 (at -3.556 0.254 90) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 93 "Net-(JP14-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 94 /~PBSY))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4E65)
    (at 137.795 110.871 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP15 (at -3.556 0.254 90) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 95 "Net-(JP15-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 96 /~PSTRB))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4E8D)
    (at 132.588 110.871 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP16 (at -0.254 -1.27 90) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 97 "Net-(JP16-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 98 /PEX3))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4C75)
    (at 128.778 99.187 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP17 (at -0.254 1.524 90) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 68 "Net-(JP1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4C63)
    (at 134.112 99.187 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP18 (at -0.381 1.524 90) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 70 "Net-(JP18-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4C48)
    (at 139.446 99.187 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP19 (at -0.381 1.524 90) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 72 "Net-(JP19-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4C27)
    (at 144.653 99.187 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP20 (at -0.381 1.524 90) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 74 "Net-(JP20-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4C09)
    (at 149.987 99.187 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP21 (at -0.381 1.524 90) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 76 "Net-(JP21-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4BED)
    (at 155.321 99.187 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP22 (at -0.381 1.524 90) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 78 "Net-(JP22-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4BC7)
    (at 160.655 99.187 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP23 (at -0.381 1.524 90) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 80 "Net-(JP23-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4B7C)
    (at 165.862 99.187 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP24 (at -0.381 1.524 90) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 82 "Net-(JP24-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4B5C)
    (at 171.069 99.187 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP25 (at -0.127 -1.397 90) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 84 "Net-(JP25-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4E18)
    (at 165.481 110.871 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP26 (at -0.254 -1.397 270) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 85 "Net-(JP10-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4E0F)
    (at 160.274 110.871 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP27 (at -0.254 -1.397 270) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 87 "Net-(JP11-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4E0A)
    (at 155.067 110.871 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP28 (at -0.254 -1.397 270) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 89 "Net-(JP12-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4E3F)
    (at 149.86 110.871 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP29 (at -0.254 -1.397 270) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 91 "Net-(JP13-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4E42)
    (at 144.653 110.871 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP30 (at -0.254 -1.397 270) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 93 "Net-(JP14-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4E55)
    (at 139.446 110.871 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP31 (at -0.254 -1.397 270) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 95 "Net-(JP15-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4E71)
    (at 134.239 110.871 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference JP32 (at -0.254 -1.397 270) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 97 "Net-(JP16-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x13 (layer Bottom) (tedit 0)
    (at 133.858 103.759 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 5.1 270) (layer B.SilkS))
    (fp_text value CONN_02X13 (at 0 3.1 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 99 "Net-(P3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 97 "Net-(JP16-Pad1)"))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 68 "Net-(JP1-Pad2)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 95 "Net-(JP15-Pad1)"))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 70 "Net-(JP18-Pad2)"))
    (pad 6 thru_hole oval (at 2.54 -5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 93 "Net-(JP14-Pad1)"))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 72 "Net-(JP19-Pad2)"))
    (pad 8 thru_hole oval (at 2.54 -7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 91 "Net-(JP13-Pad1)"))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 74 "Net-(JP20-Pad2)"))
    (pad 10 thru_hole oval (at 2.54 -10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 89 "Net-(JP12-Pad1)"))
    (pad 11 thru_hole oval (at 0 -12.7 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 76 "Net-(JP21-Pad2)"))
    (pad 12 thru_hole oval (at 2.54 -12.7 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 13 thru_hole oval (at 0 -15.24 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 100 "Net-(P3-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 -15.24 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 15 thru_hole oval (at 0 -17.78 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 78 "Net-(JP22-Pad2)"))
    (pad 16 thru_hole oval (at 2.54 -17.78 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 101 "Net-(P3-Pad16)"))
    (pad 17 thru_hole oval (at 0 -20.32 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 18 thru_hole oval (at 2.54 -20.32 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 87 "Net-(JP11-Pad1)"))
    (pad 19 thru_hole oval (at 0 -22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 20 thru_hole oval (at 2.54 -22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 85 "Net-(JP10-Pad1)"))
    (pad 21 thru_hole oval (at 0 -25.4 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 80 "Net-(JP23-Pad2)"))
    (pad 22 thru_hole oval (at 2.54 -25.4 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 23 thru_hole oval (at 0 -27.94 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 82 "Net-(JP24-Pad2)"))
    (pad 24 thru_hole oval (at 2.54 -27.94 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 25 thru_hole oval (at 0 -30.48 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 84 "Net-(JP25-Pad2)"))
    (pad 26 thru_hole oval (at 2.54 -30.48 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x13.wrl
      (at (xyz 0.05 -0.6 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4E9A)
    (at 129.921 112.268 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0.508 1.397 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 27 "/(U1.R11)RESET#"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4AD7)
    (at 128.778 97.028 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -1.143 -1.524 270) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 5 SYS_5V))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 68 "Net-(JP1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4AD1)
    (at 134.112 97.028 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -0.889 -1.524 270) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 5 SYS_5V))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 70 "Net-(JP18-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4AC8)
    (at 139.446 97.028 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -0.889 -1.524 270) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 5 SYS_5V))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 72 "Net-(JP19-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4ABE)
    (at 144.653 97.028 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -0.889 -1.524 270) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 5 SYS_5V))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 74 "Net-(JP20-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4AB6)
    (at 149.987 97.028 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -0.889 -1.524 270) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 5 SYS_5V))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 76 "Net-(JP21-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4AA9)
    (at 155.321 97.028 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -0.889 -1.524 270) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 5 SYS_5V))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 78 "Net-(JP22-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4AA0)
    (at 160.655 97.028 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -0.889 -1.524 270) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 5 SYS_5V))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 80 "Net-(JP23-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4A8E)
    (at 165.862 97.028 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at -0.889 -1.524 270) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 5 SYS_5V))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 82 "Net-(JP24-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4B29)
    (at 171.069 97.028 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at -1.27 1.397 270) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 5 SYS_5V))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 84 "Net-(JP25-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4E14)
    (at 165.481 113.03 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at -1.143 1.397 90) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 5 SYS_5V))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 85 "Net-(JP10-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4E0D)
    (at 160.274 113.03 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at -1.143 1.397 90) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 5 SYS_5V))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 87 "Net-(JP11-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4E04)
    (at 155.067 113.03 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at -1.143 1.397 90) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 5 SYS_5V))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 89 "Net-(JP12-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4E48)
    (at 149.86 113.03 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at -1.143 1.397 90) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 5 SYS_5V))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 91 "Net-(JP13-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4E4A)
    (at 144.653 113.03 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at -1.143 1.397 90) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 5 SYS_5V))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 93 "Net-(JP14-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4E52)
    (at 139.446 113.03 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at -1.143 1.397 90) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 5 SYS_5V))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 95 "Net-(JP15-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer Top) (tedit 5ACD4D71)
    (at 134.239 113.03 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at -1.143 1.524 90) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 5 SYS_5V))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 97 "Net-(JP16-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints.pretty:TXS0108EPWR (layer Top) (tedit 5ACE8B4E)
    (at 125.857 108.077 90)
    (fp_text reference U1 (at 0 4.191 90) (layer F.SilkS))
    (fp_text value TXS0108E_PW_20 (at 0 0 90) (layer F.Fab))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 1 smd rect (at -2.8194 -2.925 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 25 "/(U1.P6)"))
    (pad 2 smd rect (at -2.8194 -2.274999 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 4 VDD_3V3B))
    (pad 3 smd rect (at -2.8194 -1.625001 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 15 "/(U1.B11)I2C1.SCL"))
    (pad 4 smd rect (at -2.8194 -0.974999 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 36 "/(U1.F3)AIN5~3.3V"))
    (pad 5 smd rect (at -2.8194 -0.325001 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 66 "/(U1.F2)AIN6~3.3V"))
    (pad 6 smd rect (at -2.8194 0.324998 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 64 "/(U1.E1)"))
    (pad 7 smd rect (at -2.8194 0.974999 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 42 "/(U1.A12)UART0.RX"))
    (pad 8 smd rect (at -2.8194 1.624998 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 44 "/(U1.B12)UART0.TX"))
    (pad 9 smd rect (at -2.8194 2.274999 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 39 "/(U1.F1)"))
    (pad 10 smd rect (at -2.8194 2.924998 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 27 "/(U1.R11)RESET#"))
    (pad 11 smd rect (at 2.8194 2.925 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 2.8194 2.275002 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 98 /PEX3))
    (pad 13 smd rect (at 2.8194 1.625001 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 69 /PEX2))
    (pad 14 smd rect (at 2.8194 0.975002 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 67 /PEX1))
    (pad 15 smd rect (at 2.8194 0.325001 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 71 /PR/~W))
    (pad 16 smd rect (at 2.8194 -0.324998 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 92 /~PCMD))
    (pad 17 smd rect (at 2.8194 -0.974999 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 94 /~PBSY))
    (pad 18 smd rect (at 2.8194 -1.624998 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 96 /~PSTRB))
    (pad 19 smd rect (at 2.8194 -2.274999 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 5 SYS_5V))
    (pad 20 smd rect (at 2.8194 -2.924998 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 90 /~PPARITY))
  )
  (module footprints.pretty:TXS0108EPWR (layer Top) (tedit 5ACE8BBD)
    (at 170.815 108.077 90)
    (fp_text reference U2 (at 0.889 -4.064 90) (layer F.SilkS))
    (fp_text value TXS0108E_PW_20 (at 0 0 90) (layer F.Fab))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 1 smd rect (at -2.8194 -2.925 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 38 "/(U1.A1)PWM0A"))
    (pad 2 smd rect (at -2.8194 -2.274999 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 4 VDD_3V3B))
    (pad 3 smd rect (at -2.8194 -1.625001 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 41 "/(U1.A2)PRU-0.1"))
    (pad 4 smd rect (at -2.8194 -0.974999 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 33 "/(U1.B2)PRU-0.2"))
    (pad 5 smd rect (at -2.8194 -0.325001 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 31 "/(U1.B1)PRU-0.3"))
    (pad 6 smd rect (at -2.8194 0.324998 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 43 "/(U1.A3)PRU-0.4"))
    (pad 7 smd rect (at -2.8194 0.974999 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 35 "/(U1.B3)PRU-0.5"))
    (pad 8 smd rect (at -2.8194 1.624998 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 29 "/(U1.C3)PRU-0.6"))
    (pad 9 smd rect (at -2.8194 2.274999 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 45 "/(U1.C4)PRU-0.7"))
    (pad 10 smd rect (at -2.8194 2.924998 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 27 "/(U1.R11)RESET#"))
    (pad 11 smd rect (at 2.8194 2.925 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 2.8194 2.275002 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 83 /PD7))
    (pad 13 smd rect (at 2.8194 1.625001 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 81 /PD6))
    (pad 14 smd rect (at 2.8194 0.975002 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 79 /PD5))
    (pad 15 smd rect (at 2.8194 0.325001 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 86 /PD4))
    (pad 16 smd rect (at 2.8194 -0.324998 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 88 /PD3))
    (pad 17 smd rect (at 2.8194 -0.974999 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 77 /PD2))
    (pad 18 smd rect (at 2.8194 -1.624998 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 75 /PD1))
    (pad 19 smd rect (at 2.8194 -2.274999 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 5 SYS_5V))
    (pad 20 smd rect (at 2.8194 -2.924998 90) (size 1.6764 0.3556) (layers Top F.Paste F.Mask)
      (net 73 /PD0))
  )
  (gr_text 35 (at 171.06138 119.13362) (layer F.SilkS))
  (gr_text 2 (at 125.20168 115.9891) (layer F.SilkS))
  (gr_text 1 (at 125.14072 118.5926) (layer F.SilkS))
  (gr_text 1 (at 125.24232 93.25864) (layer F.SilkS))
  (gr_line (start 131.0011 122.5036) (end 166.0011 122.5036) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.0011 87.5036) (end 131.0011 87.5036) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 131.0011 97.5036) (end 131.0011 87.5036) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.0011 97.5036) (end 121.0011 112.5036) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 131.0011 112.5036) (end 121.0011 112.5036) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 166.0011 112.5036) (end 166.0011 122.5036) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176.0011 112.5036) (end 176.0011 97.5036) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 166.0011 97.5036) (end 176.0011 97.5036) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_text "75 Mils back-->\nTry to move back 75 Mils <---" (at 161.5011 106.7536) (layer Cmts.User))
  (gr_text 2 (at 125.30328 90.65514) (layer F.SilkS))
  (gr_text 36 (at 171.0436 91.059) (layer F.SilkS))
  (gr_text 35 (at 171.1198 93.5736) (layer F.SilkS))
  (gr_text 36 (at 171.1452 116.4336) (layer F.SilkS))
  (gr_text TS:VDD_3V3AUX:1:8::L2 (at 140.4323 107.5174 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3AUX:1:8::L2 (at 141.3213 106.6288 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3AUX:2:8::L2 (at 141.3213 106.6284 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3AUX:2:8::L2 (at 141.3213 100.2788 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3AUX:3:8::L2 (at 141.3213 100.2784 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3AUX:3:8::L2 (at 143.0993 98.5008 310) (layer Eco1.User))
  (gr_text TS:VDD_RTC:4:8::L2 (at 140.4323 102.4374 50) (layer Eco1.User))
  (gr_text TE:VDD_RTC:4:8::L2 (at 140.4323 100.0248 310) (layer Eco1.User))
  (gr_text TS:VDD_RTC:5:8::L2 (at 140.4323 100.0244 50) (layer Eco1.User))
  (gr_text TE:VDD_RTC:5:8::L2 (at 142.7183 97.7388 310) (layer Eco1.User))
  (gr_text TS:VDD_RTC:6:8::L2 (at 142.7183 97.7384 50) (layer Eco1.User))
  (gr_text TE:VDD_RTC:6:8::L2 (at 142.7183 96.9768 310) (layer Eco1.User))
  (gr_text TS:VDD_RTC:7:8::L2 (at 142.7183 96.9764 50) (layer Eco1.User))
  (gr_text TE:VDD_RTC:7:8::L2 (at 140.6863 94.9448 310) (layer Eco1.User))
  (gr_text TS:VDD_RTC:8:8::L2 (at 140.6863 94.9444 50) (layer Eco1.User))
  (gr_text TE:VDD_RTC:8:8::L2 (at 140.6863 93.0398 310) (layer Eco1.User))
  (gr_text V:CGND:1:48 (at 125.62775 108.672375 35) (layer Eco1.User))
  (gr_text V:CGND:2:48 (at 124.68795 108.672375 35) (layer Eco1.User))
  (gr_text V:CGND:3:48 (at 124.68795 107.249975 35) (layer Eco1.User))
  (gr_text V:CGND:4:48 (at 125.62775 107.249975 35) (layer Eco1.User))
  (gr_text V:CGND:5:48 (at 123.21475 108.088175 35) (layer Eco1.User))
  (gr_text V:CGND:6:48 (at 121.99555 108.088175 35) (layer Eco1.User))
  (gr_text V:CGND:7:48 (at 121.99555 109.231175 35) (layer Eco1.User))
  (gr_text V:CGND:8:48 (at 123.21475 106.691175 35) (layer Eco1.User))
  (gr_text V:CGND:9:48 (at 121.99555 106.691175 35) (layer Eco1.User))
  (gr_text V:CGND:10:48 (at 121.99555 105.446575 35) (layer Eco1.User))
  (gr_text V:CGND:11:48 (at 123.21475 105.446575 35) (layer Eco1.User))
  (gr_text V:CGND:12:48 (at 121.99555 104.278175 35) (layer Eco1.User))
  (gr_text V:CGND:13:48 (at 123.21475 104.278175 35) (layer Eco1.User))
  (gr_text V:CGND:14:48 (at 123.21475 103.033575 35) (layer Eco1.User))
  (gr_text V:CGND:15:48 (at 121.99555 103.033575 35) (layer Eco1.User))
  (gr_text V:CGND:16:48 (at 121.99555 101.636575 35) (layer Eco1.User))
  (gr_text V:CGND:17:48 (at 123.21475 101.636575 35) (layer Eco1.User))
  (gr_text V:CGND:18:48 (at 123.21475 100.493575 35) (layer Eco1.User))
  (gr_text V:CGND:19:48 (at 121.99555 100.493575 35) (layer Eco1.User))
  (gr_text V:CGND:20:48 (at 158.80015 97.674175 35) (layer Eco1.User))
  (gr_text V:CGND:21:48 (at 159.48595 97.674175 35) (layer Eco1.User))
  (gr_text V:CGND:22:48 (at 159.48595 98.512375 35) (layer Eco1.User))
  (gr_text V:CGND:23:48 (at 167.94415 96.912175 35) (layer Eco1.User))
  (gr_text V:CGND:24:48 (at 167.94415 97.445575 35) (layer Eco1.User))
  (gr_text V:CGND:25:48 (at 169.46815 96.912175 35) (layer Eco1.User))
  (gr_text V:CGND:26:48 (at 169.46815 97.445575 35) (layer Eco1.User))
  (gr_text V:CGND:27:48 (at 168.70615 97.445575 35) (layer Eco1.User))
  (gr_text V:CGND:28:48 (at 168.70615 96.912175 35) (layer Eco1.User))
  (gr_text V:CGND:29:48 (at 169.46815 112.990375 35) (layer Eco1.User))
  (gr_text V:CGND:30:48 (at 169.46815 112.456975 35) (layer Eco1.User))
  (gr_text V:CGND:31:48 (at 167.94415 112.456975 35) (layer Eco1.User))
  (gr_text V:CGND:32:48 (at 167.94415 112.990375 35) (layer Eco1.User))
  (gr_text V:CGND:33:48 (at 168.70615 112.456975 35) (layer Eco1.User))
  (gr_text V:CGND:34:48 (at 168.70615 112.990375 35) (layer Eco1.User))
  (gr_text V:GND:35:48 (at 143.25535 109.916975 35) (layer Eco1.User))
  (gr_text V:GND:36:48 (at 138.17535 104.836975 35) (layer Eco1.User))
  (gr_text V:GND:37:48 (at 143.25535 99.756975 35) (layer Eco1.User))
  (gr_text V:GND:38:48 (at 148.33535 104.836975 35) (layer Eco1.User))
  (gr_text V:GND:39:48 (at 139.44535 108.646975 35) (layer Eco1.User))
  (gr_text V:GND:40:48 (at 139.44535 101.026975 35) (layer Eco1.User))
  (gr_text V:GND:41:48 (at 147.06535 101.026975 35) (layer Eco1.User))
  (gr_text V:GND:42:48 (at 147.06535 108.646975 35) (layer Eco1.User))
  (gr_text V:GND:43:48 (at 156.89515 103.693975 35) (layer Eco1.User))
  (gr_text V:GND:44:48 (at 127.02475 106.056175 35) (layer Eco1.User))
  (gr_text V:VDD_3V3AUX:45:48 (at 140.58835 107.376975 35) (layer Eco1.User))
  (gr_text V:VDD_3V3B:46:48 (at 145.79535 107.376975 35) (layer Eco1.User))
  (gr_text V:VDD_3V3B:47:48 (at 157.19995 111.161575 35) (layer Eco1.User))
  (gr_text V:VDD_RTC:48:48 (at 140.58835 102.296975 35) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_RTC:1:484 (at 125.34035 96.556537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:2:484 (at 124.34035 96.556537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:7:484 (at 129.92035 103.406537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:8:484 (at 129.92035 102.406537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:9:484 (at 156.89515 105.590937 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:10:484 (at 156.89515 104.590937 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:11:484 (at 156.90695 110.196337 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:12:484 (at 155.20695 110.196337 10) (layer Eco1.User))
  (gr_text FillOverPAD:VBUS.RAW:17:484 (at 127.03835 102.906537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:18:484 (at 128.73835 102.906537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:19:484 (at 172.75655 114.158737 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:20:484 (at 171.05655 114.158737 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:96:484 (at 127.41235 107.490537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:97:484 (at 131.41235 107.490537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3AUX:100:484 (at 124.09035 95.032537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:102:484 (at 124.34035 93.508537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:106:484 (at 128.15035 105.827537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:112:484 (at 123.404269 116.487537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:113:484 (at 123.95535 116.487537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:114:484 (at 124.45535 116.487537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:115:484 (at 125.006431 116.487537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:120:484 (at 155.79495 98.119619 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:123:484 (at 155.79495 96.517456 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:128:484 (at 155.79495 101.701019 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:129:484 (at 155.79495 101.149937 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:130:484 (at 155.79495 100.649937 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:131:484 (at 155.79495 100.098856 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:136:484 (at 155.79495 104.139419 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:137:484 (at 155.79495 103.588337 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:138:484 (at 155.79495 103.088337 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:139:484 (at 155.79495 102.537256 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:144:484 (at 155.79495 106.577819 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:145:484 (at 155.79495 106.026737 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:146:484 (at 155.79495 105.526737 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:147:484 (at 155.79495 104.975656 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:148:484 (at 155.79495 109.016219 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:149:484 (at 155.79495 108.465137 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:150:484 (at 155.79495 107.965137 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:151:484 (at 155.79495 107.414056 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:160:484 (at 162.039631 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:161:484 (at 161.48855 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:162:484 (at 160.98855 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:163:484 (at 160.437469 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:165:484 (at 164.38415 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:166:484 (at 163.88415 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:167:484 (at 163.333069 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:172:484 (at 163.03395 113.853937 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:238:484 (at 143.89035 110.653537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:239:484 (at 142.62035 110.653537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:251:484 (at 147.70035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:252:484 (at 146.43035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:253:484 (at 145.16035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:254:484 (at 143.89035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:255:484 (at 142.62035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:256:484 (at 141.35035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:257:484 (at 140.08035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:258:484 (at 138.81035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:267:484 (at 147.70035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:268:484 (at 146.43035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:269:484 (at 145.16035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:270:484 (at 143.89035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:271:484 (at 142.62035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:272:484 (at 141.35035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3AUX:273:484 (at 140.08035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:274:484 (at 138.81035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:283:484 (at 147.70035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:284:484 (at 146.43035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:285:484 (at 145.16035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:286:484 (at 143.89035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:287:484 (at 142.62035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:288:484 (at 141.35035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3AUX:289:484 (at 140.08035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:290:484 (at 138.81035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:298:484 (at 148.97035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:299:484 (at 147.70035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:301:484 (at 145.16035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:302:484 (at 143.89035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:303:484 (at 142.62035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:304:484 (at 141.35035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:305:484 (at 140.08035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:306:484 (at 138.81035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:307:484 (at 137.54035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:314:484 (at 148.97035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:315:484 (at 147.70035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:317:484 (at 145.16035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:318:484 (at 143.89035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:319:484 (at 142.62035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:320:484 (at 141.35035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:321:484 (at 140.08035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:322:484 (at 138.81035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:323:484 (at 137.54035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:326:484 (at 133.73035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:331:484 (at 147.70035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:SYS_5V:332:484 (at 146.43035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:SYS_5V:333:484 (at 145.16035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:334:484 (at 143.89035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:335:484 (at 142.62035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:336:484 (at 141.35035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_RTC:337:484 (at 140.08035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:338:484 (at 138.81035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:347:484 (at 147.70035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:SYS_5V:348:484 (at 146.43035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:SYS_5V:349:484 (at 145.16035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:350:484 (at 143.89035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:351:484 (at 142.62035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:352:484 (at 141.35035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_RTC:353:484 (at 140.08035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:354:484 (at 138.81035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:363:484 (at 147.70035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:364:484 (at 146.43035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:365:484 (at 145.16035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:366:484 (at 143.89035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:367:484 (at 142.62035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:368:484 (at 141.35035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:369:484 (at 140.08035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:370:484 (at 138.81035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VIN.BAT:381:484 (at 145.16035 99.223537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:382:484 (at 143.89035 99.223537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:383:484 (at 142.62035 99.223537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VIN.BAT:398:484 (at 143.89035 97.953537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:399:484 (at 142.62035 97.953537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_5V:400:484 (at 141.35035 97.953537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VIN.BAT:414:484 (at 143.89035 96.683537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:415:484 (at 142.62035 96.683537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_5V:416:484 (at 141.35035 96.683537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VIN.BAT:430:484 (at 143.89035 95.413537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:431:484 (at 142.62035 95.413537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_5V:432:484 (at 141.35035 95.413537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:441:484 (at 123.74035 99.238537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_RTC:443:484 (at 125.94035 97.938537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:447:484 (at 130.81535 102.406537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:449:484 (at 130.81535 103.406537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:459:484 (at 122.60735 101.164537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:460:484 (at 122.60735 103.764537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:461:484 (at 122.60735 106.164537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:462:484 (at 122.60735 108.764537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:463:484 (at 125.15735 108.064537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:464:484 (at 125.15735 101.864537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:467:484 (at 125.28235 106.264537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VBUS.RAW:469:484 (at 125.28235 103.664537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:473:484 (at 158.62095 106.148538 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:475:484 (at 158.62095 108.348537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:479:484 (at 159.22095 112.808537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:480:484 (at 168.72095 112.798537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:481:484 (at 168.72095 97.298537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:482:484 (at 159.12095 98.198537 10) (layer Eco1.User))
  (gr_text TS:CGND:1:28::L19 (at 158.6441 98.6528 50) (layer Eco1.User))
  (gr_text TE:CGND:1:28::L19 (at 125.4717 101.1932 310) (layer Eco1.User))
  (gr_text TS:GND:2:28::L19 (at 124.6843 97.7384 50) (layer Eco1.User))
  (gr_text TE:GND:2:28::L19 (at 124.4453 99.2778 310) (layer Eco1.User))
  (gr_text TS:GND:3:28::L19 (at 152.3113 93.5734 50) (layer Eco1.User))
  (gr_text TE:GND:3:28::L19 (at 155.1389 95.6814 310) (layer Eco1.User))
  (gr_text TS:GND:4:28::L19 (at 169.7693 114.1976 50) (layer Eco1.User))
  (gr_text TE:GND:4:28::L19 (at 163.6733 113.8932 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3AUX:5:28::L19 (at 140.4323 107.5174 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3AUX:5:28::L19 (at 140.4323 107.5178 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3AUX:6:28::L19 (at 139.9243 108.1524 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3AUX:6:28::L19 (at 140.4323 107.5178 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3AUX:7:28::L19 (at 140.4323 107.5174 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3AUX:7:28::L19 (at 139.9243 108.1528 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3AUX:8:28::L19 (at 139.9243 106.8824 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3AUX:8:28::L19 (at 140.4323 107.5178 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:9:28::L19 (at 145.6393 107.5174 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:9:28::L19 (at 145.6393 107.5178 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:10:28::L19 (at 157.0439 111.302 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:10:28::L19 (at 157.0439 111.3024 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:11:28::L19 (at 157.0439 111.302 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:11:28::L19 (at 145.6393 107.5178 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:12:28::L19 (at 142.1513 116.4334 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:12:28::L19 (at 145.6393 107.5178 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:13:28::L19 (at 145.0043 108.1524 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:13:28::L19 (at 142.1513 116.4338 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:14:28::L19 (at 145.6393 107.5174 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:14:28::L19 (at 145.0043 108.1528 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:15:28::L19 (at 145.0043 106.8824 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:15:28::L19 (at 145.6393 107.5178 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:16:28::L19 (at 146.2743 106.8824 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:16:28::L19 (at 145.6393 107.5178 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:17:28::L19 (at 146.2743 108.1524 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:17:28::L19 (at 145.6393 107.5178 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:18:28::L19 (at 155.6389 106.616681 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:18:28::L19 (at 146.2743 106.8828 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:19:28::L19 (at 155.6389 107.452919 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:19:28::L19 (at 155.6389 106.617081 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:20:28::L19 (at 156.7391 105.6298 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:20:28::L19 (at 155.6389 106.617081 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:21:28::L19 (at 158.4649 106.1874 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:21:28::L19 (at 156.7391 105.6302 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:22:28::L19 (at 156.7509 110.2352 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:22:28::L19 (at 155.6389 107.453319 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:23:28::L19 (at 157.0439 111.302 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:23:28::L19 (at 156.7509 110.2356 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:24:28::L19 (at 156.6081 100.6888 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:24:28::L19 (at 156.7391 105.6302 310) (layer Eco1.User))
  (gr_text TS:VDD_RTC:25:28::L19 (at 140.4323 102.4374 50) (layer Eco1.User))
  (gr_text TE:VDD_RTC:25:28::L19 (at 140.4323 102.4378 310) (layer Eco1.User))
  (gr_text TS:VDD_RTC:26:28::L19 (at 139.9243 103.0724 50) (layer Eco1.User))
  (gr_text TE:VDD_RTC:26:28::L19 (at 140.4323 102.4378 310) (layer Eco1.User))
  (gr_text TS:VDD_RTC:27:28::L19 (at 140.4323 102.4374 50) (layer Eco1.User))
  (gr_text TE:VDD_RTC:27:28::L19 (at 139.9243 103.0728 310) (layer Eco1.User))
  (gr_text TS:VDD_RTC:28:28::L19 (at 139.9243 101.8024 50) (layer Eco1.User))
  (gr_text TE:VDD_RTC:28:28::L19 (at 140.4323 102.4378 310) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_RTC:1:532 (at 125.34035 96.556537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:2:532 (at 124.34035 96.556537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:7:532 (at 129.92035 103.406537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:8:532 (at 129.92035 102.406537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:9:532 (at 156.89515 105.590937 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:10:532 (at 156.89515 104.590937 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:11:532 (at 156.90695 110.196337 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:12:532 (at 155.20695 110.196337 10) (layer Eco1.User))
  (gr_text FillOverPAD:VBUS.RAW:17:532 (at 127.03835 102.906537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:18:532 (at 128.73835 102.906537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:19:532 (at 172.75655 114.158737 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:20:532 (at 171.05655 114.158737 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:96:532 (at 127.41235 107.490537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:97:532 (at 131.41235 107.490537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3AUX:100:532 (at 124.09035 95.032537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:102:532 (at 124.34035 93.508537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:106:532 (at 128.15035 105.827537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:112:532 (at 123.404269 116.487537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:113:532 (at 123.95535 116.487537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:114:532 (at 124.45535 116.487537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:115:532 (at 125.006431 116.487537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:120:532 (at 155.79495 98.119619 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:123:532 (at 155.79495 96.517456 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:128:532 (at 155.79495 101.701019 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:129:532 (at 155.79495 101.149937 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:130:532 (at 155.79495 100.649937 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:131:532 (at 155.79495 100.098856 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:136:532 (at 155.79495 104.139419 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:137:532 (at 155.79495 103.588337 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:138:532 (at 155.79495 103.088337 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:139:532 (at 155.79495 102.537256 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:144:532 (at 155.79495 106.577819 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:145:532 (at 155.79495 106.026737 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:146:532 (at 155.79495 105.526737 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:147:532 (at 155.79495 104.975656 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:148:532 (at 155.79495 109.016219 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:149:532 (at 155.79495 108.465137 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:150:532 (at 155.79495 107.965137 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:151:532 (at 155.79495 107.414056 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:160:532 (at 162.039631 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:161:532 (at 161.48855 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:162:532 (at 160.98855 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:163:532 (at 160.437469 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:165:532 (at 164.38415 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:166:532 (at 163.88415 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:167:532 (at 163.333069 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:172:532 (at 163.03395 113.853937 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:238:532 (at 143.89035 110.653537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:239:532 (at 142.62035 110.653537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:251:532 (at 147.70035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:252:532 (at 146.43035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:253:532 (at 145.16035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:254:532 (at 143.89035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:255:532 (at 142.62035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:256:532 (at 141.35035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:257:532 (at 140.08035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:258:532 (at 138.81035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:267:532 (at 147.70035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:268:532 (at 146.43035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:269:532 (at 145.16035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:270:532 (at 143.89035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:271:532 (at 142.62035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:272:532 (at 141.35035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3AUX:273:532 (at 140.08035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:274:532 (at 138.81035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:283:532 (at 147.70035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:284:532 (at 146.43035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:285:532 (at 145.16035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:286:532 (at 143.89035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:287:532 (at 142.62035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:288:532 (at 141.35035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3AUX:289:532 (at 140.08035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:290:532 (at 138.81035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:298:532 (at 148.97035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:299:532 (at 147.70035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:301:532 (at 145.16035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:302:532 (at 143.89035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:303:532 (at 142.62035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:304:532 (at 141.35035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:305:532 (at 140.08035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:306:532 (at 138.81035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:307:532 (at 137.54035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:314:532 (at 148.97035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:315:532 (at 147.70035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:317:532 (at 145.16035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:318:532 (at 143.89035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:319:532 (at 142.62035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:320:532 (at 141.35035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:321:532 (at 140.08035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:322:532 (at 138.81035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:323:532 (at 137.54035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:326:532 (at 133.73035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:331:532 (at 147.70035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:SYS_5V:332:532 (at 146.43035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:SYS_5V:333:532 (at 145.16035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:334:532 (at 143.89035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:335:532 (at 142.62035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:336:532 (at 141.35035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_RTC:337:532 (at 140.08035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:338:532 (at 138.81035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:347:532 (at 147.70035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:SYS_5V:348:532 (at 146.43035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:SYS_5V:349:532 (at 145.16035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:350:532 (at 143.89035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:351:532 (at 142.62035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:352:532 (at 141.35035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_RTC:353:532 (at 140.08035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:354:532 (at 138.81035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:363:532 (at 147.70035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:364:532 (at 146.43035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:365:532 (at 145.16035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:366:532 (at 143.89035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:367:532 (at 142.62035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:368:532 (at 141.35035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:369:532 (at 140.08035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:370:532 (at 138.81035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VIN.BAT:381:532 (at 145.16035 99.223537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:382:532 (at 143.89035 99.223537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:383:532 (at 142.62035 99.223537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VIN.BAT:398:532 (at 143.89035 97.953537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:399:532 (at 142.62035 97.953537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_5V:400:532 (at 141.35035 97.953537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VIN.BAT:414:532 (at 143.89035 96.683537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:415:532 (at 142.62035 96.683537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_5V:416:532 (at 141.35035 96.683537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VIN.BAT:430:532 (at 143.89035 95.413537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:431:532 (at 142.62035 95.413537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_5V:432:532 (at 141.35035 95.413537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:441:532 (at 123.74035 99.238537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_RTC:443:532 (at 125.94035 97.938537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:447:532 (at 130.81535 102.406537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:449:532 (at 130.81535 103.406537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:507:532 (at 122.60735 101.164537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:508:532 (at 122.60735 103.764537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:509:532 (at 122.60735 106.164537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:510:532 (at 122.60735 108.764537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:511:532 (at 125.15735 108.064537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:512:532 (at 125.15735 101.864537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:515:532 (at 125.28235 106.264537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VBUS.RAW:517:532 (at 125.28235 103.664537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:521:532 (at 158.62095 106.148538 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:523:532 (at 158.62095 108.348537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:527:532 (at 159.22095 112.808537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:528:532 (at 168.72095 112.798537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:529:532 (at 168.72095 97.298537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:530:532 (at 159.12095 98.198537 10) (layer Eco1.User))
  (zone (net 1) (net_name GND) (layer DigitalGND) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.84 85.344) (xy 116.84 125.222) (xy 181.61 125.222) (xy 181.61 85.344)
      )
    )
  )
  (zone (net 5) (net_name SYS_5V) (layer VDD) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.157 126.365) (xy 113.157 82.423) (xy 184.531 82.423) (xy 184.531 126.365)
      )
    )
  )
)
