(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 46)
    (no_connects 1)
    (area 64.696768 32.033281 178.510001 123.265001)
    (thickness 1.6)
    (drawings 49)
    (tracks 204)
    (zones 0)
    (modules 21)
    (nets 54)
  )
  (page USLetter)
  (title_block
    (title "Project Title")
  )
  (layers
    (0 F.Cu jumper)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.1524)
    (edge_width 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3556)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.1524)
    (pcb_text_size 1.016 1.016)
    (mod_edge_width 0.1524)
    (mod_text_size 1.016 1.016)
    (mod_text_width 0.1524)
    (pad_size 10.16 10.16)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0762)
    (solder_mask_min_width 0.1016)
    (pad_to_paste_clearance -0.0762)
    (aux_axis_origin 196.5452 123.5456)
    (grid_origin 81.74812 74.59616)
    (visible_elements FFFEFFFF)
    (pcbplotparams
      (layerselection 0x310fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad2)")
  (net 2 "Net-(J1-Pad3)")
  (net 3 "Net-(J1-Pad4)")
  (net 4 "Net-(J1-Pad5)")
  (net 5 "Net-(J1-Pad6)")
  (net 6 "Net-(J1-Pad7)")
  (net 7 "Net-(J1-Pad8)")
  (net 8 "Net-(J1-Pad9)")
  (net 9 "Net-(J1-Pad10)")
  (net 10 "Net-(J1-Pad12)")
  (net 11 "Net-(J1-Pad18)")
  (net 12 "Net-(J1-Pad19)")
  (net 13 "Net-(J1-Pad20)")
  (net 14 "Net-(J1-Pad21)")
  (net 15 "Net-(J1-Pad22)")
  (net 16 "Net-(C2-Pad1)")
  (net 17 "Net-(C2-Pad2)")
  (net 18 VGH)
  (net 19 PRVGL)
  (net 20 VGL)
  (net 21 VDD)
  (net 22 VSH)
  (net 23 VGH2)
  (net 24 VSL)
  (net 25 VCOM)
  (net 26 GDR)
  (net 27 RESE)
  (net 28 BUSY)
  (net 29 ^RES)
  (net 30 ^D/C)
  (net 31 ^CS)
  (net 32 SCK)
  (net 33 DOUT)
  (net 34 VDDIO)
  (net 35 "Net-(J1-PadVIN)")
  (net 36 GND)
  (net 37 "Net-(J2-Pad2)")
  (net 38 "Net-(J2-Pad1)")
  (net 39 "Net-(J2-Pad3)")
  (net 40 "Net-(J2-Pad4)")
  (net 41 "Net-(J2-Pad5)")
  (net 42 "Net-(J2-Pad30)")
  (net 43 "Net-(J2-Pad31)")
  (net 44 "Net-(J2-Pad32)")
  (net 45 "Net-(J2-Pad33)")
  (net 46 "Net-(J2-Pad34)")
  (net 47 "Net-(J2-Pad6)")
  (net 48 "Net-(J2-Pad11)")
  (net 49 "Net-(J2-Pad12)")
  (net 50 "Net-(CAP1-Pad1)")
  (net 51 "Net-(CAP2-Pad1)")
  (net 52 "Net-(CAP3-Pad1)")
  (net 53 "Net-(J2-Pad24)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3556)
    (uvia_drill 0.254)
    (add_net BUSY)
    (add_net DOUT)
    (add_net GDR)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(CAP1-Pad1)")
    (add_net "Net-(CAP2-Pad1)")
    (add_net "Net-(CAP3-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J1-PadVIN)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad24)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad30)")
    (add_net "Net-(J2-Pad31)")
    (add_net "Net-(J2-Pad32)")
    (add_net "Net-(J2-Pad33)")
    (add_net "Net-(J2-Pad34)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net PRVGL)
    (add_net RESE)
    (add_net SCK)
    (add_net VCOM)
    (add_net VDD)
    (add_net VDDIO)
    (add_net VGH)
    (add_net VGH2)
    (add_net VGL)
    (add_net VSH)
    (add_net VSL)
    (add_net ^CS)
    (add_net ^D/C)
    (add_net ^RES)
  )
  (module hirose-34pos-bigger-gnd-pads:CONN-HEADER-FH34SRJ-34S-0.5SH-BIG-GND (layer F.Cu) (tedit 58E8619F)
    (at 78.85684 60.6298 90)
    (fp_text reference J2 (at -0.225 -0.325 270) (layer F.Fab))
    (fp_text value HEADER-FEMALE-34POS-FFC-SMT-1x34-P0.5MM (at 0 2.9 90) (layer F.Fab) hide)
    (fp_text user %R (at -10.425 -0.075 180) (layer F.SilkS))
    (pad 2 smd rect (at 9.652 -1.778 180) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J2-Pad2)"))
    (pad 1 smd rect (at -8.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at -7.725 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J2-Pad2)"))
    (pad 3 smd rect (at -7.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J2-Pad3)"))
    (pad 4 smd rect (at -6.725 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J2-Pad4)"))
    (pad 5 smd rect (at -6.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J2-Pad5)"))
    (pad 6 smd rect (at -5.725 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(J2-Pad6)"))
    (pad 7 smd rect (at -5.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 GDR))
    (pad 8 smd rect (at -4.725 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 RESE))
    (pad 9 smd rect (at -4.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 VGL))
    (pad 10 smd rect (at -3.725 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 VGH))
    (pad 11 smd rect (at -3.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(J2-Pad11)"))
    (pad 12 smd rect (at -2.725 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(J2-Pad12)"))
    (pad 13 smd rect (at -2.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 14 smd rect (at -1.725 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 28 BUSY))
    (pad 15 smd rect (at -1.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 29 ^RES))
    (pad 16 smd rect (at -0.725 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 30 ^D/C))
    (pad 17 smd rect (at -0.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 31 ^CS))
    (pad 18 smd rect (at 0.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 32 SCK))
    (pad 19 smd rect (at 0.775 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 DOUT))
    (pad 20 smd rect (at 1.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 34 VDDIO))
    (pad 21 smd rect (at 1.775 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 34 VDDIO))
    (pad 22 smd rect (at 2.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 23 smd rect (at 2.775 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 VDD))
    (pad 24 smd rect (at 3.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(J2-Pad24)"))
    (pad 25 smd rect (at 3.775 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 VSH))
    (pad 26 smd rect (at 4.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 VGH2))
    (pad 27 smd rect (at 4.775 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 VSL))
    (pad 28 smd rect (at 5.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 PRVGL))
    (pad 29 smd rect (at 5.775 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 VCOM))
    (pad 30 smd rect (at 6.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(J2-Pad30)"))
    (pad 31 smd rect (at 6.775 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J2-Pad31)"))
    (pad 32 smd rect (at 7.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J2-Pad32)"))
    (pad 33 smd rect (at 7.775 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(J2-Pad33)"))
    (pad 34 smd rect (at 8.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(J2-Pad34)"))
    (pad e smd rect (at -9.652 -1.778 180) (size 2 2) (layers F.Cu F.Paste F.Mask))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58EB4E25)
    (at 86.41812 70.59616 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 1.278 1.726 180) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 20 VGL))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 590B82D3)
    (at 105.87412 40.55816)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 1.274 1.78) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 34 VDDIO))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58EB4E5F)
    (at 80.31734 83.23326)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -3.048 0 90) (layer F.SilkS))
    (fp_text value CAP-CER-2.2UF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58EB4E1C)
    (at 86.93812 75.80616 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -3.556 0 180) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 VGH))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58EB4DE7)
    (at 97.29812 38.12616 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -3.737 0.063 180) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 19 PRVGL))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58EB4E14)
    (at 97.29812 50.77616 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at -3.556 0 180) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 21 VDD))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58EB4E04)
    (at 97.29812 47.57616 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at -3.654 0.106 180) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 22 VSH))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58EB4DFD)
    (at 97.29812 44.32616 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at -3.647 0.038 180) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 23 VGH2))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58EB4DE0)
    (at 97.29812 35.22616 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at -3.717 0.058 180) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 25 VCOM))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58EB4DF3)
    (at 97.29812 41.07616 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at -4.157 0.048 180) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 24 VSL))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 58EB4E4B)
    (at 78.95844 77.36586 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at -3.438 -0.03 360) (layer F.SilkS))
    (fp_text value DIODE (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.635 0 270) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 2 smd rect (at 1.635 0 270) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C2-Pad1)"))
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 58EB4E47)
    (at 82.25536 77.44968 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D2 (at 3.556 0 360) (layer F.SilkS))
    (fp_text value DIODE (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.635 0 270) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 18 VGH))
    (pad 2 smd rect (at 1.635 0 270) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C2-Pad2)"))
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 58EB4E55)
    (at 75.35418 77.44968 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D3 (at -3.126 0.016 180) (layer F.SilkS))
    (fp_text value DIODE (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.635 0 90) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.635 0 90) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 19 PRVGL))
  )
  (module Inductors:Inductor_1212 (layer F.Cu) (tedit 5652586A)
    (at 87.00812 80.83616 90)
    (attr smd)
    (fp_text reference L1 (at 0 2.75 90) (layer F.SilkS))
    (fp_text value INDUCTOR (at 0 -2.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.75 0 90) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 34 VDDIO))
    (pad 2 smd rect (at 1.75 0 90) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C2-Pad2)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 54E9291B)
    (at 95.78812 82.33616 180)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -3.81 180) (layer F.SilkS))
    (fp_text value Q_NMOS_GDS (at 0 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 26 GDR))
    (pad 2 smd rect (at 0.95 1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 27 RESE))
    (pad 3 smd rect (at 0 -1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C2-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 91.66812 82.18616 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value "2.2R 1%" (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 27 RESE))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wickerlib:CAPSENSE-CIRCLE-D10MM (layer B.Cu) (tedit 590046DF)
    (at 138.19812 48.70616 270)
    (fp_text reference CAP1 (at 0 0 270) (layer B.Fab))
    (fp_text value CAPSENSE_CIRCLE (at 0.025 -7.325 270) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0 270) (size 10.16 10.16) (layers B.Cu)
      (net 50 "Net-(CAP1-Pad1)") (clearance 0.508))
  )
  (module Wickerlib:CAPSENSE-CIRCLE-D10MM (layer B.Cu) (tedit 590046EF)
    (at 138.20812 63.79616 270)
    (fp_text reference CAP2 (at 0 0 270) (layer B.Fab))
    (fp_text value CAPSENSE_CIRCLE (at 0.025 -7.325 270) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0 270) (size 10.16 10.16) (layers B.Cu)
      (net 51 "Net-(CAP2-Pad1)") (clearance 0.508))
  )
  (module Wickerlib:CAPSENSE-CIRCLE-D10MM (layer B.Cu) (tedit 59004910)
    (at 138.20812 78.80616 270)
    (fp_text reference A (at 0 0 270) (layer B.Fab))
    (fp_text value CAPSENSE_CIRCLE (at 0.025 -7.325 270) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0 270) (size 10.16 10.16) (layers B.Cu)
      (net 52 "Net-(CAP3-Pad1)") (clearance 0.508))
  )
  (module Wickerlib:TEENSY-3.2-SILK-SIMPLE (layer F.Cu) (tedit 583B5D39)
    (at 117.40812 55.60616)
    (fp_text reference J1 (at -2 0) (layer F.Fab))
    (fp_text value TEENSY3.2-72MHz-SIMPLE (at -2.54 20.32) (layer F.Fab) hide)
    (fp_text user VIN (at 8.382095 -10.16) (layer F.SilkS))
    (fp_text user %R (at 5.08 -12.7) (layer F.SilkS))
    (fp_text user AGND (at 9.144 -7.62) (layer F.SilkS))
    (fp_text user 3.3V (at 8.810666 -5.08) (layer F.SilkS))
    (fp_text user 23 (at 8.144 -2.54) (layer F.SilkS))
    (fp_text user 22 (at 8.144 0) (layer F.SilkS))
    (fp_text user 21 (at 8.144 2.54) (layer F.SilkS))
    (fp_text user 20 (at 8.144 5.08) (layer F.SilkS))
    (fp_text user 19 (at 8.144 7.62) (layer F.SilkS))
    (fp_text user 18 (at 8.144 10.16) (layer F.SilkS))
    (fp_text user 17 (at 8.144 12.7) (layer F.SilkS))
    (fp_text user 16 (at 8.144 15.24) (layer F.SilkS))
    (fp_text user 15 (at 8.144 17.78) (layer F.SilkS))
    (fp_text user 14 (at 8.144 20.32) (layer F.SilkS))
    (fp_text user 13 (at 8.144 22.86) (layer F.SilkS))
    (fp_text user 0 (at -12.668381 -7.62) (layer F.SilkS))
    (fp_text user GND (at -13.716 -10.16) (layer F.SilkS))
    (fp_text user 1 (at -12.668381 -5.08) (layer F.SilkS))
    (fp_text user 2 (at -12.668381 -2.54) (layer F.SilkS))
    (fp_text user 3 (at -12.668381 0) (layer F.SilkS))
    (fp_text user 4 (at -12.668381 2.54) (layer F.SilkS))
    (fp_text user 5 (at -12.668381 5.08) (layer F.SilkS))
    (fp_text user 6 (at -12.668381 7.62) (layer F.SilkS))
    (fp_text user 7 (at -12.668381 10.16) (layer F.SilkS))
    (fp_text user 8 (at -12.668381 12.7) (layer F.SilkS))
    (fp_text user 9 (at -12.668381 15.24) (layer F.SilkS))
    (fp_text user 10 (at -13.144571 17.78) (layer F.SilkS))
    (fp_text user 11 (at -13.144571 20.32) (layer F.SilkS))
    (fp_text user 12 (at -13.144571 22.86) (layer F.SilkS))
    (pad G1 thru_hole circle (at -10.16 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 GND))
    (pad 0 thru_hole circle (at -10.16 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(CAP1-Pad1)"))
    (pad 1 thru_hole circle (at -10.16 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(CAP2-Pad1)"))
    (pad 2 thru_hole circle (at -10.16 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at -10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at -10.16 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at -10.16 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at -10.16 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at -10.16 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at -10.16 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad8)"))
    (pad 9 thru_hole circle (at -10.16 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J1-Pad9)"))
    (pad 10 thru_hole circle (at -10.16 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-Pad10)"))
    (pad 11 thru_hole circle (at -10.16 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 DOUT))
    (pad 12 thru_hole circle (at -10.16 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J1-Pad12)"))
    (pad 13 thru_hole circle (at 5.08 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 SCK))
    (pad 16 thru_hole circle (at 5.08 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 ^D/C))
    (pad 3V2 thru_hole circle (at 5.08 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 VDDIO))
    (pad 18 thru_hole circle (at 5.08 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J1-Pad18)"))
    (pad 17 thru_hole circle (at 5.08 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 ^CS))
    (pad AG thru_hole circle (at 5.08 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 GND))
    (pad 22 thru_hole circle (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J1-Pad22)"))
    (pad VIN thru_hole circle (at 5.08 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(J1-PadVIN)"))
    (pad 21 thru_hole circle (at 5.08 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J1-Pad21)"))
    (pad 20 thru_hole circle (at 5.08 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J1-Pad20)"))
    (pad 19 thru_hole circle (at 5.08 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J1-Pad19)"))
    (pad 23 thru_hole circle (at 5.08 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(CAP3-Pad1)"))
    (pad 14 thru_hole circle (at 5.08 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 ^RES))
    (pad 15 thru_hole circle (at 5.08 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 BUSY))
  )
  (gr_text "Drew Fustini <drew@oshpark.com>" (at 145.84812 63.98616 90) (layer B.SilkS))
  (gr_text "Drew Fustini <drew@oshpark.com>" (at 103.92812 82.58616) (layer B.Mask))
  (gr_text "Drew Fustini <drew@oshpark.com>" (at 103.92812 82.58616) (layer B.Cu))
  (gr_text github.com/pdp7/kicad-teensy-epaper (at 106.44812 36.07616) (layer B.Mask))
  (gr_line (start 143.72812 89.31616) (end 143.94812 89.31616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 133.02812 32.12616) (end 144.00812 32.12616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 132.58812 89.32616) (end 143.76812 89.32616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_text "#" (at 137.88812 78.64616 90) (layer B.SilkS))
  (gr_text + (at 137.82812 63.59616 90) (layer B.SilkS))
  (gr_text * (at 140.08812 48.30616 90) (layer B.SilkS))
  (gr_text "github.com/pdp7/kicad-teensy-epaper\n\nDrew Fustini <drew@oshpark.com>\n" (at 138.35812 64.31616 90) (layer F.SilkS))
  (gr_text github.com/pdp7/kicad-teensy-epaper (at 106.44812 36.07616) (layer B.Cu))
  (gr_circle (center 142.89312 37.41016) (end 141.16812 34.21016) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 148.16812 35.66016) (end 148.16812 35.81016) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 148.16812 85.61016) (end 148.16812 35.81016) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 66.81724 89.32926) (end 133.05028 89.32926) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 68.03898 32.12592) (end 133.07568 32.12592) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 69.3928 72.0598) (end 70.81012 72.0598) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 69.31152 48.68164) (end 70.81266 48.68164) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_circle (center 70.02312 37.37616) (end 68.29812 34.17616) (layer Edge.Cuts) (width 0.1524))
  (gr_circle (center 69.89812 84.27616) (end 68.17312 81.07616) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 64.77312 34.00116) (end 64.77312 87.17616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 66.74812 32.12616) (end 68.19812 32.12616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_arc (start 66.67312 34.02616) (end 64.77312 34.00116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_arc (start 66.84812 87.25116) (end 66.82312 89.32616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_arc (start 144.16742 85.3096) (end 148.16742 85.5596) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_arc (start 144.25642 36.03602) (end 143.89642 32.12602) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_text "2017-05-04\n" (at 77.11812 41.44616 90) (layer F.SilkS))
  (gr_line (start 66.84612 72.05016) (end 69.38612 72.05016) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 66.84612 48.68216) (end 66.84612 72.05016) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 69.38612 48.68216) (end 66.84612 48.68216) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 70.80852 72.13144) (end 70.80852 48.76344) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (zone (net 36) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 65.89812 32.72616) (xy 66.89812 32.27616) (xy 144.86812 32.32616) (xy 147.19812 33.84616) (xy 147.93812 35.60616)
        (xy 147.93812 85.40616) (xy 147.69812 86.58616) (xy 146.92812 87.87616) (xy 146.09812 88.39616) (xy 145.16812 88.94616)
        (xy 139.82812 89.08616) (xy 139.30812 89.09616) (xy 66.95812 89.19616) (xy 66.34812 88.97616) (xy 65.79812 88.82616)
        (xy 65.39812 88.37616) (xy 65.14812 87.97616) (xy 64.99812 87.42616) (xy 64.99812 34.52616) (xy 65.09812 34.07616)
        (xy 65.19812 33.47616) (xy 65.69812 32.87616) (xy 65.79812 32.77616)
      )
    )
  )
  (zone (net 34) (net_name VDDIO) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 65.89812 32.72616) (xy 66.89812 32.27616) (xy 144.15812 32.28616) (xy 146.03812 32.81616) (xy 147.81812 35.11616)
        (xy 147.92812 86.05616) (xy 147.92812 86.08616) (xy 147.72812 86.85616) (xy 147.47812 87.26616) (xy 146.60812 88.34616)
        (xy 143.78812 89.14616) (xy 142.64812 89.11616) (xy 66.62812 89.31616) (xy 66.34812 88.97616) (xy 65.79812 88.82616)
        (xy 65.39812 88.37616) (xy 65.14812 87.97616) (xy 64.99812 87.42616) (xy 64.99812 34.52616) (xy 65.09812 34.07616)
        (xy 65.19812 33.47616) (xy 65.69812 32.87616) (xy 65.79812 32.77616)
      )
    )
  )
)
