(kicad_pcb (version 4) (host pcbnew "(after 2015-may-25 BZR unknown)-product")
  (general
    (links 95)
    (no_connects 0)
    (area 80.0387 27.63 214.1 129.385)
    (thickness 1.6)
    (drawings 23)
    (tracks 670)
    (zones 0)
    (modules 16)
    (nets 62)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 1.6)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory fab/))
  )
  (net 0 "")
  (net 1 Reset)
  (net 2 GND)
  (net 3 VCC5)
  (net 4 /A18)
  (net 5 /A17)
  (net 6 /D4)
  (net 7 /A7)
  (net 8 D12)
  (net 9 /A6)
  (net 10 /D5)
  (net 11 /A5)
  (net 12 D13)
  (net 13 /A4)
  (net 14 /D6)
  (net 15 /A3)
  (net 16 D14)
  (net 17 /A2)
  (net 18 /D7)
  (net 19 /A1)
  (net 20 D15)
  (net 21 /A0)
  (net 22 ~CE)
  (net 23 VPP)
  (net 24 /A16)
  (net 25 ~OE)
  (net 26 /A15)
  (net 27 /D0)
  (net 28 /A14)
  (net 29 D8)
  (net 30 /A13)
  (net 31 /D1)
  (net 32 /A12)
  (net 33 D9)
  (net 34 /A11)
  (net 35 /D2)
  (net 36 /A10)
  (net 37 D10)
  (net 38 /A9)
  (net 39 /D3)
  (net 40 /A8)
  (net 41 D11)
  (net 42 /A19)
  (net 43 /VBAT)
  (net 44 /PC13)
  (net 45 /PC15)
  (net 46 /PA1)
  (net 47 /PA2)
  (net 48 ~BYTE)
  (net 49 Clear)
  (net 50 Clk3)
  (net 51 Clk2)
  (net 52 Clk1)
  (net 53 /PB0)
  (net 54 VCC3)
  (net 55 "Net-(P1-Pad28)")
  (net 56 "Net-(P1-Pad29)")
  (net 57 ~WE)
  (net 58 "Net-(Q1-Pad1)")
  (net 59 "Net-(Q1-Pad2)")
  (net 60 "Net-(Q2-Pad1)")
  (net 61 VCC10)
  (net_class Default "Ceci est la Netclass par défaut"
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A16)
    (add_net /A17)
    (add_net /A18)
    (add_net /A19)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /PA1)
    (add_net /PA2)
    (add_net /PB0)
    (add_net /PC13)
    (add_net /PC15)
    (add_net /VBAT)
    (add_net Clear)
    (add_net Clk1)
    (add_net Clk2)
    (add_net Clk3)
    (add_net D10)
    (add_net D11)
    (add_net D12)
    (add_net D13)
    (add_net D14)
    (add_net D15)
    (add_net D8)
    (add_net D9)
    (add_net GND)
    (add_net "Net-(P1-Pad28)")
    (add_net "Net-(P1-Pad29)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q2-Pad1)")
    (add_net Reset)
    (add_net VCC10)
    (add_net VCC3)
    (add_net VCC5)
    (add_net VPP)
    (add_net ~BYTE)
    (add_net ~CE)
    (add_net ~OE)
    (add_net ~WE)
  )
  (module Wire_Pads:SolderWirePad_2x_2mmDrill (layer F.Cu) (tedit 58B16759)
    (at 119.6 106)
    (fp_text reference IN+ (at -7.2 0.2) (layer F.SilkS))
    (fp_text value "" (at 0.635 3.81) (layer F.Fab))
    (pad IN+ smd rect (at -3.175 0) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC5))
  )
  (module Wire_Pads:SolderWirePad_2x_2mmDrill (layer F.Cu) (tedit 58B16704)
    (at 159.8 124.4)
    (fp_text reference "OUT -" (at 1.6 0) (layer F.SilkS))
    (fp_text value "" (at 0.635 3.81) (layer F.Fab))
    (pad OUT- smd rect (at -3.175 0) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Wire_Pads:SolderWirePad_2x_2mmDrill (layer F.Cu) (tedit 58B166D6)
    (at 159.8 106)
    (fp_text reference OUT+ (at 1.6 0.2) (layer F.SilkS))
    (fp_text value "" (at 0.635 3.81) (layer F.Fab))
    (pad OUT+ smd rect (at -3.175 0) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 61 VCC10))
  )
  (module Wire_Pads:SolderWirePad_2x_2mmDrill (layer F.Cu) (tedit 58B16729)
    (at 119.4 124.6)
    (fp_text reference IN- (at -7.2 0.2) (layer F.SilkS))
    (fp_text value "" (at 0.635 3.81) (layer F.Fab))
    (pad IN- smd rect (at -3.175 0) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module LOGO (layer F.Cu) (tedit 58B09020)
    (at 183.2 48.2)
    (fp_text reference "" (at -1.4 17) (layer F.SilkS) hide)
    (fp_text value "" (at -1.4 12.4) (layer F.SilkS) hide)
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 58AF25E1)
    (at 189.4 97.6 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.08 -2.31 90) (layer F.SilkS))
    (fp_text value 4K7 (at 5.1308 0.2032 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(Q2-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 58AF25FA)
    (at 175.6 112 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 -2.31 90) (layer F.SilkS))
    (fp_text value 1K (at 5.0292 0.0254 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(Q1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 ~BYTE))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Transistors_OldSowjetAera:OldSowjetaera_Transistor_Type-I_SmallPads (layer F.Cu) (tedit 58B1629C)
    (at 177 91.2)
    (fp_text reference PNP (at 0 -7.1) (layer F.SilkS))
    (fp_text value "" (at -4.1783 -12.2809) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 VPP))
    (pad 1 thru_hole circle (at -2 0) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(Q2-Pad1)"))
    (pad 3 thru_hole circle (at 2 0) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 VCC10))
    (model Transistors_OldSowjetAera.3dshapes/OldSowjetaera_Transistor_Type-I_SmallPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_SMALL (layer F.Cu) (tedit 57F0DA47)
    (at 172 119.4 180)
    (fp_text reference Reset (at 2.4 -5.65 180) (layer F.SilkS))
    (fp_text value "" (at 0.635 -5.08 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 8.19 -2.54 180) (size 1.397 1.397) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 8.19 2.54 180) (size 1.397 1.397) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 Reset))
    (pad 1 thru_hole circle (at -3.81 -2.54 180) (size 1.397 1.397) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 2.54 180) (size 1.397 1.397) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module Transistors_OldSowjetAera:OldSowjetaera_Transistor_Type-I_SmallPads (layer F.Cu) (tedit 58AF2614)
    (at 186 112)
    (fp_text reference NPN (at 0 -7.1) (layer F.SilkS))
    (fp_text value "" (at 0.1 7.6) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(Q1-Pad2)"))
    (pad 1 thru_hole circle (at -2 0) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(Q1-Pad1)"))
    (pad 3 thru_hole circle (at 2 0) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Transistors_OldSowjetAera.3dshapes/OldSowjetaera_Transistor_Type-I_SmallPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-42_W15.24mm (layer F.Cu) (tedit 58AF23E0)
    (at 114.236 52.7177 90)
    (descr "42-lead dip package, row spacing 15.24 mm (600 mils)")
    (tags "DIL DIP PDIP 2.54mm 15.24mm 600mil")
    (fp_text reference IC1 (at 7.62 -2.39 90) (layer F.SilkS))
    (fp_text value MX29F1615 (at 7.62 53.19 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /A18))
    (pad 22 thru_hole oval (at 15.24 50.8 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC5))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /A17))
    (pad 23 thru_hole oval (at 15.24 48.26 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /D4))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /A7))
    (pad 24 thru_hole oval (at 15.24 45.72 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 D12))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /A6))
    (pad 25 thru_hole oval (at 15.24 43.18 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /D5))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /A5))
    (pad 26 thru_hole oval (at 15.24 40.64 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 D13))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /A4))
    (pad 27 thru_hole oval (at 15.24 38.1 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /D6))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /A3))
    (pad 28 thru_hole oval (at 15.24 35.56 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 D14))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /A2))
    (pad 29 thru_hole oval (at 15.24 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /D7))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /A1))
    (pad 30 thru_hole oval (at 15.24 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 D15))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /A0))
    (pad 31 thru_hole oval (at 15.24 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 ~CE))
    (pad 32 thru_hole oval (at 15.24 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 VPP))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 33 thru_hole oval (at 15.24 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /A16))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 ~OE))
    (pad 34 thru_hole oval (at 15.24 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /A15))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /D0))
    (pad 35 thru_hole oval (at 15.24 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /A14))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 D8))
    (pad 36 thru_hole oval (at 15.24 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /A13))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /D1))
    (pad 37 thru_hole oval (at 15.24 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /A12))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 D9))
    (pad 38 thru_hole oval (at 15.24 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /A11))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /D2))
    (pad 39 thru_hole oval (at 15.24 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /A10))
    (pad 19 thru_hole oval (at 0 45.72 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 D10))
    (pad 40 thru_hole oval (at 15.24 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /A9))
    (pad 20 thru_hole oval (at 0 48.26 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /D3))
    (pad 41 thru_hole oval (at 15.24 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /A8))
    (pad 21 thru_hole oval (at 0 50.8 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 D11))
    (pad 42 thru_hole oval (at 15.24 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /A19))
    (model Housings_DIP.3dshapes/DIP-42_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib:STM32 (layer F.Cu) (tedit 58B1808A)
    (at 117.475 100.584 90)
    (descr "40-lead dip package, row spacing 15.24 mm (600 mils)")
    (tags "dil dip 2.54 600")
    (fp_text reference P1 (at 0 -5.22 90) (layer F.SilkS))
    (fp_text value DIL40 (at 0 -3.72 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 43 /VBAT))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 44 /PC13))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 45 /PC15))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 ~CE))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 46 /PA1))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 47 /PA2))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 48 ~BYTE))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 49 Clear))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 50 Clk3))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 51 Clk2))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 52 Clk1))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 53 /PB0))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 ~OE))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 20 D15))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 D14))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 Reset))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 54 VCC3))
    (pad 19 thru_hole oval (at 0 45.72 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 20 thru_hole oval (at 0 48.26 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 21 thru_hole oval (at 15.24 48.26 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 D13))
    (pad 22 thru_hole oval (at 15.24 45.72 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 D12))
    (pad 23 thru_hole oval (at 15.24 43.18 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 41 D11))
    (pad 24 thru_hole oval (at 15.24 40.64 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 37 D10))
    (pad 25 thru_hole oval (at 15.24 38.1 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 33 D9))
    (pad 26 thru_hole oval (at 15.24 35.56 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 29 D8))
    (pad 27 thru_hole oval (at 15.24 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 /D7))
    (pad 28 thru_hole oval (at 15.24 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(P1-Pad28)"))
    (pad 29 thru_hole oval (at 15.24 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(P1-Pad29)"))
    (pad 30 thru_hole oval (at 15.24 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 /D6))
    (pad 31 thru_hole oval (at 15.24 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 /D5))
    (pad 32 thru_hole oval (at 15.24 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 /D4))
    (pad 33 thru_hole oval (at 15.24 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 57 ~WE))
    (pad 34 thru_hole oval (at 15.24 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 39 /D3))
    (pad 35 thru_hole oval (at 15.24 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 35 /D2))
    (pad 36 thru_hole oval (at 15.24 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 31 /D1))
    (pad 37 thru_hole oval (at 15.24 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 27 /D0))
    (pad 38 thru_hole oval (at 15.24 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC5))
    (pad 39 thru_hole oval (at 15.24 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 40 thru_hole oval (at 15.24 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (model Housings_DIP.3dshapes/DIP-40_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib:DIP-20_W7.62mm (layer F.Cu) (tedit 58B1AF23)
    (at 118.796 57.7215)
    (descr "20-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U1 (at 0 -5.22) (layer F.SilkS))
    (fp_text value 74LS273 (at 0 -3.72) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 49 Clear))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 /A0))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 27 /D0))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 31 /D1))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A1))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A2))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 35 /D2))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 39 /D3))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 /A3))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 11 thru_hole oval (at 7.62 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 52 Clk1))
    (pad 12 thru_hole oval (at 7.62 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A4))
    (pad 13 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 /D4))
    (pad 14 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 /D5))
    (pad 15 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 /A5))
    (pad 16 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 /A6))
    (pad 17 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 /D6))
    (pad 18 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 /D7))
    (pad 19 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A7))
    (pad 20 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC5))
    (model Housings_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib:DIP-20_W7.62mm (layer F.Cu) (tedit 58B1AF1E)
    (at 136.627 57.5564)
    (descr "20-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U2 (at 0 -5.22) (layer F.SilkS))
    (fp_text value 74LS273 (at 0 -3.72) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 49 Clear))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 40 /A8))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 27 /D0))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 31 /D1))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 38 /A9))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 36 /A10))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 35 /D2))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 39 /D3))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 34 /A11))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 11 thru_hole oval (at 7.62 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 51 Clk2))
    (pad 12 thru_hole oval (at 7.62 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 32 /A12))
    (pad 13 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 /D4))
    (pad 14 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 /D5))
    (pad 15 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 30 /A13))
    (pad 16 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 28 /A14))
    (pad 17 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 /D6))
    (pad 18 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 /D7))
    (pad 19 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 /A15))
    (pad 20 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC5))
    (model Housings_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib:DIP-20_W7.62mm (layer F.Cu) (tedit 58B1AF19)
    (at 154.622 57.7215)
    (descr "20-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U3 (at 0 -5.22) (layer F.SilkS))
    (fp_text value 74LS273 (at 0 -3.72) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 49 Clear))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A16))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 27 /D0))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 31 /D1))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A17))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 /A18))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 35 /D2))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 39 /D3))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 42 /A19))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 11 thru_hole oval (at 7.62 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 50 Clk3))
    (pad 12 thru_hole oval (at 7.62 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 /D4))
    (pad 14 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 /D5))
    (pad 15 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 16 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 17 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 /D6))
    (pad 18 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 /D7))
    (pad 19 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 20 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC5))
    (model Housings_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 58B08AE6)
    (at 179 79)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 -2.31) (layer F.SilkS))
    (fp_text value 4K7 (at 5.2606 0.0005) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(Q2-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 VCC10))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text Flasher (at 184 69.6) (layer F.SilkS))
  (gr_text SWD (at 165 92.6) (layer F.SilkS))
  (dimension 91.45 (width 0.3) (layer Eco1.User)
    (gr_text "91,450 mm" (at 207.45 81.275 90) (layer Eco1.User))
    (feature1 (pts (xy 195.6 35.55) (xy 208.8 35.55)))
    (feature2 (pts (xy 195.6 127) (xy 208.8 127)))
    (crossbar (pts (xy 206.1 127) (xy 206.1 35.55)))
    (arrow1a (pts (xy 206.1 35.55) (xy 206.686421 36.676504)))
    (arrow1b (pts (xy 206.1 35.55) (xy 205.513579 36.676504)))
    (arrow2a (pts (xy 206.1 127) (xy 206.686421 125.873496)))
    (arrow2b (pts (xy 206.1 127) (xy 205.513579 125.873496)))
  )
  (gr_text USB (at 118.6 92.8) (layer F.SilkS))
  (gr_text "\n" (at 80.7887 116.1312) (layer F.SilkS))
  (gr_text "\n" (at 80.1387 114.2712) (layer F.SilkS))
  (gr_text MX29F1615 (at 185 64.2) (layer F.SilkS))
  (gr_line (start 109.22 127) (end 109.22 107.95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.855 127) (end 109.22 127) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110.49 127) (end 109.855 127) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 195.58 127) (end 195.58 107.95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.22 107.95) (end 109.22 87.63) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 195.58 127) (end 110.49 127) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 195.58 86.36) (end 195.58 107.95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 86.36 (width 0.3) (layer Eco1.User)
    (gr_text "86,360 mm" (at 152.4 29.13) (layer Eco1.User))
    (feature1 (pts (xy 195.58 35.56) (xy 195.58 27.78)))
    (feature2 (pts (xy 109.22 35.56) (xy 109.22 27.78)))
    (crossbar (pts (xy 109.22 30.48) (xy 195.58 30.48)))
    (arrow1a (pts (xy 195.58 30.48) (xy 194.453496 31.066421)))
    (arrow1b (pts (xy 195.58 30.48) (xy 194.453496 29.893579)))
    (arrow2a (pts (xy 109.22 30.48) (xy 110.346504 31.066421)))
    (arrow2b (pts (xy 109.22 30.48) (xy 110.346504 29.893579)))
  )
  (gr_line (start 195.58 35.56) (end 195.58 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.22 35.56) (end 195.58 35.56) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.22 38.1) (end 109.22 35.56) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.22 38.1) (end 109.22 87.63) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name VCC5) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 194.818 126.619) (xy 108.839 126.5555) (xy 109.601 35.687) (xy 195.58 35.7505) (xy 195.453 106.934)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 194.31 126.365) (xy 110.49 126.365) (xy 110.49 35.7505) (xy 194.31 35.7505) (xy 194.31 106.68)
      )
    )
  )
)
