<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="20" width="0.0762" layer="46"/>
<wire x1="0" y1="20" x2="6.4" y2="20" width="0.0762" layer="46"/>
<wire x1="6.4" y1="20" x2="6.4" y2="0" width="0.0762" layer="46"/>
<wire x1="6.4" y1="0" x2="0" y2="0" width="0.0762" layer="46"/>
<text>R</text>
<text>+</text>
<text>_</text>
<text>Ground</text>
<text>nSRST</text>
<text>VTref</text>
<text>_</text>
<text>+</text>
<text>Ground</text>
<text>nSRST</text>
<text>VTref</text>
<text>UPDI
Programming
Key</text>
<text>gChart</text>
</plain>
<libraries>
<library name="smd-ipc">
<description>&lt;b&gt;IPC Standard SMD Packages&lt;/b&gt;&lt;p&gt;
This is a package-only library, based on the Surface Mount Design and Land Pattern Standard developed by the 
Institute for Interconnecting and Packaging electronic Circuits (IPC).&lt;p&gt;
Source:&lt;p&gt;
IPC-SM-782&lt;br&gt;
Revision A, August 1993&lt;br&gt;
Includes Amendment 1, October 1996&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="R0805">
<description>&lt;b&gt;Chip RESISTOR, 0805 EIA (2012 Metric)&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R-4K7" library="smd-ipc" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S$7">
</signal>
<signal name="S$12">
</signal>
<signal name="S$13">
</signal>
<signal name="S$1">
</signal>
<signal name="S$2">
</signal>
<signal name="S$4">
</signal>
<signal name="S$5">
</signal>
<signal name="S$6">
</signal>
<signal name="S$8">
</signal>
<signal name="S$9">
</signal>
<signal name="S$10">
</signal>
<signal name="S$11">
</signal>
<signal name="S$14">
</signal>
<signal name="S$15">
</signal>
<signal name="S$16">
</signal>
</signals>
</board>
</drawing>
</eagle>
